============================================================ WARNING =====================================================================
1. At BMC FW Ver 3.07, change the conf to 4MB, so yafuflash and webui does not support BMC upgrade from previous version to newer than v3.07.
Need use SOCFLASH at another package to upgrade it.
2. Befor version 3.05, yafuflash maybe take long time to start the updating process via In-band.
==========================================================================
        S5B serials AST2500(A2) BMC FW Release v3.67.06 (Only for S5Bx/S5Sx)
==========================================================================
Version: 3.67.06
Release Date: 2017.12.01

AMI Subversion Revision: AMI SPX RR11.5

[Utility]:
1. Yafuflash2 (version 4.16.13)

[Firmware Images]:
1. s5bxv3.48.06_rom.ima with checksum          : FFD07508
2. s5bxv3.48.06_rom.ima with MD5 checksum      : 1AA1D41A3C493E3146361E5F033CBD0B
3. s5bxv3.48.06_rom.ima_enc with MD5 checksum  : A825017CD291B75A0084D23FFB2F40AF

[Fan Table]
Version:
S5Bx:
SKU0~2: v12
SKU3~4: v07
SKU5~7: v07

[Change/Add]: 
S5Bx:	
1. Update BMC FW version 3.67.00
2. Change HDS logo at webui


[Bug Fixed]:
S5Bx:
na

[Known issue]: 
na

[Notice]:
	1. Update BMC FW via command line:
		Refer to readme.txt
	2. Update BMC FW via Web UI:
		a) Please select s5bxvXX.YY.ZZ_rom.ima_enc as image file and doesn't upload Signimage key.
	3. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: cmb9.admin
