============================================================ WARNING =====================================================================
1. At BMC FW Ver 3.07, change the conf to 4MB, so yafuflash and webui does not support BMC upgrade from previous version to newer than v3.07.
Need use SOCFLASH at another package to upgrade it.
2. Befor version 3.05, yafuflash maybe take long time to start the updating process via In-band.
==========================================================================
        S5B serials AST2600(A2) BMC FW Release v4.27.06 (Only for S5Bx/S5Sx)
==========================================================================
Version: 4.27.06
Release Date: 2018.11.09

AMI Subversion Revision: AMI SPX RR11.5

[Utility]:
1. Yafuflash2 (version 4.16.21_01)

[Firmware Images]:
1. s5bxv4.27.06_rom.ima with checksum          :   F0D659A4
2. s5bxv4.27.06_rom.ima with MD5 checksum      :   0c766eae3063c384f24c46dcad2e577f
3. s5bxv4.27.06_rom.ima_enc with MD5 checksum  :   94d552937d96e40c204f8f1916e9299c

[Fan Table]
Version:
S5Bx:
SKU0~2: v12
SKU3~4: v07
SKU5~7: v07
SKU8~9: v03

[Change/Add]: 
S5Bx:	
na
 
[Bug Fixed]:
S5Bx:
1. Web page view error - The Help button in System Inventory page cannot be closed. (track-id:256960)
2. Web page view error - It can not be updated the new SSL certificate by refresh BMC WebUI. (track-id:257132)
3. Web page view error - According newest Spec define, Web UI can support User privilege login. (track-id:244824)
4. OpenVas scan Error - There are error found via OpenVas scan. (track-id:247238, 257163)
5. Preserve update Error -  When flashing BMC via redfish with preserve settings, BMC will show "failed to prepare flashing area". (track-id:247238, 257163)

[Known issue]: 
na

[Notice]:
	1. Update BMC FW via command line:
		Refer to readme.txt
	2. Update BMC FW via Web UI:
		a) Please select s5bxvXX.YY.ZZ_rom.ima_enc as image file and doesn't upload Signimage key.
	3. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: cmb9.admin
	4. Please canceling preserve all configuration before upgrading this version BMC (if FW version is less v4.21.06).
	   Because of this version's BMC fixed and add lots of functions (i.e. add some ipmi lib part for Redfish using command to set preserve configuration), 
	   we suggest canceling preserve all configuration before upgrading this version BMC to avoid unexpected defect occured.
	5. Not support GPT image file when using the remote image funciotn. 
	6. please clear browser cache and cookies after finishing upgrades.
	7. Not support BMC FW downgrade with preservation.