==========================================================================
        S5XH/S5XQH series AST2500(A2) BMC FW Release v3.62.06
==========================================================================
Version: 3.62.06
Release Date: 2023.03.20
AMI Subversion Revision: AMI SPX RR12.6
Code Base: 3.60
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.86.28)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.62.06_rom.ima with checksum          : FE8951A0 
2. s5xhv3.62.06_rom.ima with MD5 checksum      : 6fb8a11fe383f3263157ef55aaa56871 
3. s5xhv3.62.06_rom.ima_enc with MD5 checksum  : 9f951509c66db6c88d192051a4dd16f3 

[Fan Table]
Version:
S5X:  
sku0:   S5X_3.5_R06_20210122 .xml
sku1~2: S5X_2.5_R06_20210122 .xml

S5XQ: 
sku3~4: S5XQ_QCT_3p5_FSC_Table_R04_20220422.xml
sku5~8: S5XQ_QCT_2p5_FSC_Table_R04_20220422.xml

[Change/Add/Remove]:
S5XH/S5XQH:
1. [Remove] Remove WEBUI JViewer button. 
2. [Change] Remove power state on WEBUI System Inventory page.
3. [Change][386621] Thermal's request:Intel OCP 3.0 card present but no ASIC reading. System fan duty will be based on AUX mode fan duty table by reading OCP EEPROM.
4. [Change][402306] Sync AMI code base, and removed non-compliant MD5 algorithm support as RMCP+ supports non-compliant MD5 and other algorithm. We Support only Cipher ID 3 & 17 as shown below for security reasons.

[Bug Fixed]:
S5XH/S5XQH:
[Fix] #400041 WebUI menu bar miss 'Host System Diagnostics',  ACD function does not work, can not dump IERR log.
[Fix] #397236 WebUI menu bar is missing 'Host System Diagnostics', does not match SPEC (SPX_User_Guide-RR12_v182.pdf)
[Fix] #397142 Releasenote 'Change/Add' needs detailed listing and 'Bug Fixed' needs listing Symptom
[Fix] #395282 Upper Non-Critical show NA, and compare temperature sensors at S5X serial BMC FW Spec.rev033. Their sensors are different
[Fix] #395276 Fail to reset the factory default after updating BMC 3.50.00, the default account/password can not login
[Fix] #396028 Took more than 8 minutes to change IP address (expected in 3 minutes)
[Fix] #395184 All object in SNMP V3  could not be found by MIB browser nor snmpwalk conmmand.
[Fix] #398380 Items('Retry Interval' and 'Retry Count') were added in WebUI Media Redirection - General Settings of BMC 3.50, not defined in SPX_User_Guide-RR12_v183.
[Fix] #396240 Can not use POSTed session to access Redfish.
[Fix] #396862 Check '@odata.context' after user POST session will find '@odata.context' does not match
[Fix] #396158 LoginInfo SEL did not sync to Redfish.
[Fix] #395928 PATCH LDAP task get Exception status.
[Fix] #398828 The same credential uploaded via WebUI works, but get an error via Redfish(Certificate key length 4096 is out of limited 2048)
[Fix] #386452 GET /redfish/v1?\$expand=.(\$levels=1) should be fail without Account/Password.
[Fix] #395816 The value of /redfish/v1 and /redfish/v1/ with expand are different without Username and Password.
[Fix] #396148 Redfish set ActiveDirectory infomation Task get Exception TaskState and information did not set correctly.
[Fix] #397366 ReadOnly GET some URI failed by insufficient privileges.
[Fix] #397368 Operator GET some URI failed by insufficient privileges.
[Fix] #398074 Used 'Operator' & 'ReadOnly' account can not GET URI other than itself, does not match /redfish/v1/Registries/Redfish_1.0.3_PrivilegeRegistry.json.
[Fix] #398891 GET /Managers/Self/Ethernet Interfaces/ethx, eth0 will show up 'StatelessAddressAuto Config' attribute. Eth0 and eth1 behavior mismatch.
[Fix] #398412 POST /redfish/v1/AccountService/Accounts, the '@odata.id' will lack 'Id' info.
[Fix] #382750 GET /redfish/v1/Chassis/Self/NetworkAdapters/DevType7_NICX, The 'Manufacturer' doesn't display but spec: BMC_Redfish_RTP1.8-API_v1.16.0 has.
[Fix] #396911 MinCollectionInterval of /redfish/v1/TelemetryService not same as spec example.
[Fix] #391003 GET /redfish/v1/TelemetryService, the 'MinCollectionInterval' property mismatch with SPEC defined.
[Fix] #391164 GET /Systems/Self, the 'TotalSystemPersistentMemoryGiB' type mismatch with SPEC defined. (Refer to the latest SPEC: BMC_Redfish_RTP1.8-API_v1.20.pdf)
[Fix] #406049 BMC can't mount SD card after AC cycle randomly. (Fail rate: 5/10)
[Fix] #402544 Reset BMC, the SEL will not 'Management Controller off-line (BMC cold reset) - Asserted' event and Redfish event logged abnormal.
[Fix] #386897 BMC SEL not record 'FAN STB POWER Enable BY OCP - Asserted/ Deasserted' during DC/AC cycle. (Fail rate: 8/100)
[Fix] #402306 Get IPMI lan print, the 'RMCP+ Cipher Suites' info is empty mismatch with previous BMC.
[Fix] #402457 Refresh function on Audit Log page is not workable.
[Fix] #397706 SEL record '[Login Info][Set user info]	User info changed -- User ID: 2 -- Channel: 8'  when user change password first time(Not include CA law). It would not record this event after changing user password again.
[Fix] #390018 GPU-A30 'Upper critical' define not match S5XQ_FSC Table_R03_QCT_20210726.xlsx(PDA#64581)
[Fix] #403957 SNMP get raidDeviceinfoindex failed (timeout).
[Fix] #402450 Set BMC Lan from DHCP to static, the SEL log will record unexpected event about IPv6 addr#01.
[Fix] #403836 The 'BMC image update - Upload BMC image from xx.xx.xx.xx' event sensor type mismatch with SPEC defined.
[Fix] #402828 The 'BIOS image update - Upload BIOS image from xx.xx.xx.xx' event sensor type mismatch with SPEC defined.
[Fix] #402455 The audit log timestamp is wrong.
[Fix] #402401 Sometimes can't click 'Launch H5 Viewer' again after closing rKVM.(Firefox can not reproduce this issue)
[Fix] #396145 After setting AD user and login with WEBUI, would get a total blank web page.
[Fix] #390358 Fail to update BMC preserve configuration via Redfish will return 400 bad request error.
[Fix] #387873 PATCH bond0 MTUSize to 576 task will aborted to exception.
[Fix] #395830 RADIUS NoAccess user GET /redfish/v1/Managers successfully.
[Fix] #396880 When session service set disable then create new session via redfish will find audit log description incorrect.
[Fix] #392823 Redfish change password with original password, the response content is not correct.
[Fix] #391081 After PATCH /redfish/v1/AccountService/Configurations/Oem/Ami/Configurations PAMEnabled to disable, redfish can't GET /redfish/v1/AccountService info.
[Fix] #396914 Some attribute missed in TelemetryService.SubmitTestMetricReport from EventServer.
[Fix] #397196 Use IPMI change bootdev will effect Redfish Systems\Self\SD.
[Fix] #391217 Change the Redfish user password with used password, the Redfish response lacks the 'RelatedProperties' property.
[Fix] #397067 Subscription not deleted after ResumeSubscription and change to TerminateAfterRetries.
[Fix] #403252 Redfish ConfigureManager privilege account POST /Systems/Self/Boot/Certificates, the HTTP status code is 403 not 201.
[Fix] #403248 Redfish ConfigureManager privilege account GET some URI behavior not correct.
[Fix] #403231 Redfish Login privilege account can not GET some URI.
[Fix] #403225 The status code is 200 not match spec definition 202 on POST /redfish/v1/Chassis/Self/Actions/Chassis.Reset.
[Fix] #403203 Can not used ReadOnly and Operator privilege account to GET /Managers/Self/NetworkProtocol/HTTPS/Certificates.
[Fix] #403202 Can not used ReadOnly and Operator privilege account to GET /redfish/v1/AccountService/LDAP/Certificates.
[Fix] #403253 Redfish ConfigureComponents privilege account GET/PATCH/POST some URI behavior not correct.
[Fix] #402681 Redfish set LDAP, the Auditlog content not correct.
[Fix] #402690 Please help to clarify Redfish audit log message content after delete and disable LDAP settings.
[Fix] #401724 GET return code 500 threads dead after PATCH AccountService {'ActiveDirectory': {'RemoteRoleMapping': [null, null, null, null, null]}}.
[Fix] #402825 Redfish set AD, the Auditlog content not correct.
[Fix] #402650 POST or GET /redfish/v1/AccountService/LDAP/Certificates, the response 'Email' attribute type mismatch with SPEC defined.
[Fix] #402648 POST /redfish/v1/AccountService/LDAP/Certificates, the response 'Id' attribute type mismatch with SPEC defined.
[Fix] #391356 The error message of provide EventTimestamp for SubmitTestEvent has escape a sapce.
[Fix] #404306 PATCH /EventService/Subscriptions/1 'DeliveryRetryPolicy' attribute, the Audit event attribute will record empty.
[Fix] #402824 After disable Redfish EventService service, the SSE still keep live.
[Fix] #404291 Trigger the event by PATCH /redfish/v1/Systems/Self. Verify test event from EventService server, the information not correct.
[Fix] #404293 Trigger the event by PATCH /redfish/v1/Chassis/Self. Verify test event from EventService server, the information not correct.
[Fix] #404297 Trigger the event by PATCH /redfish/v1/EventService. Verify test event from EventService server, the information not correct.
[Fix] #404298 Trigger the event by PATCH /redfish/v1/Managers/Self. Verify test event from EventService server, the information not correct.
[Fix] #404295 Trigger the event by POST /redfish/v1/AccountService/Accounts. Verify test event from EventService server, the information not correct.
[Fix] #385102 Redfish will response status code is '500' after POST /redfish/v1/EventService/Subscriptions with invalid request data.
[Fix] #404501 Modify 'IPv6DefaultGateway' attribute will occur 400 Bad Request error.
[Fix] #386914 Base on BMC STD meeting,BMC update via Redfish 1.8 only support preserve all and non-preserve all.
[Fix] #404328 PATCH bond0/eht0/eht1 'InterfaceEnabled' attribute, the feedback message not correct.
[Fix] #405204 redfish/v1/Managers/Self/LogServices/AuditLog/Entries, @odata.id of Links/OriginOfCondition is unreason.
[Fix] #404967 Hostname minimum string size limit in redfish does not match with WebUI.
[Fix] #403956 'InventoryDataStatus': {'@odata.id': '/redfish/v1/Oem/Ami/InventoryData/Status'} didn't expand after expand /redfish/v1?$expand=.($levels=1).
[Fix] #403996 /redfish/v1/Managers/Self/OemSensors data type '#QrtpOemSensor.v1_0_0.OemSensors' did not define on Redfish_1.0.3_PrivilegeRegistry.json
[Fix] #397708 POST /redfish/v1/TelemetryService/MetricReportDefinitions will occur 400 Bad Request error.
[Fix] #402919 Redfish account lockout and retry Audit log message not correct.
[Fix] #397102 Network setting (IPv4/IPv6) changed SEL not logged by BMC.
[Fix] #404014 Redfish 'Login' privilege account GET/HEAD/POST/DELETE some URI behavior not correct.
[Fix] #404048 Redfish 'ConfigureSelf' privilege account GET/HEAD/POST/DELETE some URI behavior not correct.
[Fix] #404056 Redfish 'ConfigureUsers' privilege account GET/HEAD/POST/DELETE some URI behavior not correct.
[Fix] #404107 Redfish 'ConfigureComponents' privilege account GET/HEAD/POST/DELETE some URI behavior not correct.
[Fix] #404260 Redfish 'Operator' role with 'ConfigureComponents', 'ConfigureSelf', 'Login' privilege account GET/HEAD/POST/DELETE some URI behavior not correct.
[Fix] #404257 Redfish 'ReadOnly' role with 'ConfigureSelf', 'Login' privilege account GET/HEAD/POST/DELETE some URI behavior not correct.
[Fix] #383314 BMC SEL record 'System Firmwares #0x8d | Unknown Error | Asserted' during DC cycle 12 hrs(loop: 3)(Similar issue 383009).
[Fix] #383009 BMC logs 'System Firmwares POST Error | Unknown Error | Asserted' event during RHEL 8.3 warm boot cycle test around 126 loops.
[Fix] #404073 Redfish 'ConfigureManager' privilege account GET/HEAD/POST/PATCH some URI behavior not correct.
[Fix] #405462 Redfish set AD service to enable with IPv6 settings.The HTTP status is 202 accepted but response has error message and IPv6 server address not setting success.
[Fix] #404112 WEB and Redfish about IPv6 Prefix Length behavior mismatch.
[Fix] #391349 Redfish SubmitTestEventActionInfo defined EventId and EventTimestamp are required, but actually no need to provide.
[Fix] #405591 PATCH /redfish/v1/AccountService/Accounts/{ID} with invalid data.The HTTP status is 200 OK but response has error message and did not modify success.
[Fix] #397107 Redfish Modify and Verify 'IPv6DefaultGateway' Attribute Failed.
[Fix] #405500 Redfish Enable AD issue clarify.
[Fix] #405662 PATCH /redfish/v1/UpdateService will occur 500 Internal Server Error when 'ServiceEnabled' is true.
[Fix] #402556 Fail to set ServiceEnabled will occur 400 Bad Request.
[Fix] #392053 Password not show in POST SessionService/Session, it's against Spec defined.
[Fix] #405597 Redfish set AD service with invalid data the HTTP status code will return 202 Accepted. The response has error message and the content need to clarify.
[Fix] #405448 After delete AD Role Group, GET /redfish/v1/AccountService has unexpected 'AuthenticationType' attribute.
[Fix] #397710 GET/redfish/v1/Systems/Self, the 'TotalSystemPersistentMemoryGiB' attribute value is null.
[Fix] #392907 POST /redfish/v1/TelemetryService/Triggers, the response will lack 'Links' attribute.
[Fix] #390554 Redfish GET /redfish/v1/Chassis/Self/Power Table 48PowerControl Properties,Table 49Voltages Properties mismatch with SPEC BMC_Redfish_RTP1.8-API_v1.20.
[Fix] #382739 GET /redfish/v1/Systems/Self/NetworkInterfaces/{{NetworkInterface_instnace}}' , The 'Actions'. doesn't display but spec: BMC_Redfish_RTP1.8-API_v1.16.0 has.
[Fix] #391164 GET /Systems/Self, the 'TotalSystemPersistentMemoryGiB' type mismatch with SPEC defined. (Refer to the latest SPEC: BMC_Redfish_RTP1.8-API_v1.20.pdf)
[Fix] #389392 Get /redfish/v1/Systems/Self/BootOptions/{{BootOptions_instance}} response mismatch SPEC defined. (BMC_Redfish_RTP1.8-API_v1.19.0)
[Fix] #395812 GET /redfish/v1/Chassis/Self will lack 'PhysicalSecurity' attribute.
[Fix] #403326 GET /redfish/v1/TelemetryService/Triggers/{Triggers_instance}, the response '@odata.context' not correct and lack 'Links' attribute.
[Fix] #397200 The TaskState of PATCH /Managers/Self/EthernetInterfaces/bond0 'OperatingMode' to 'Stateful' always keep in Pending.
[Fix] #382192 Sometimes Virtual Media did not mount image via redfish success.
[Fix] #391128 Taskstate of POST /redfish/v1/Managers/Self/VirtualMedia/CDX/Actions/VirtualMedia.InsertMedia Started with pending and the get exception result.
[Fix] #398121 AuditLog Entries message content 'transfer protocol' is different with old version of BMC.
[Fix] #404507 Can not PATCH /Managers/Self/EthernetInterfaces/bond0 'OperatingMode' to 'Stateful'.
[Fix] #404513 Modify 'IPv6DefaultGateway', 'IPv6 Network To Stateless/DHCP', 'StaticNameServers'. The Redfish event log message not correct.
[Fix] #404464 Redfish modify 'MTUSize', 'HostName', 'FQDN' attribute. The Redfish event log message not correct.
[Fix] #404495 Redfish modify BMC IPv6 network to static. The Redfish event log message not correct.
[Fix] #390218 The message of Redfish disable eth0/1 while bond0 is enabled are strange and not same as spec example.
[Fix] #405496 Redfish response incorrect odata.context when POST new MetricReportDefinitions.
[Fix] #403881 POST /redfish/v1/UpdateService/Actions/SimpleUpdate, check the Redfish flash state some message change need to clarify this behavior.
[Fix] #386310 GET /redfish/v1/Systems/Self/Boot/Certificates failed via user ReadOnly privilege.
[Fix] #403631 Redfish setting AD General Settings, the response need clarify.
[Fix] #392910 POST /redfish/v1/TelemetryService/Triggers, the response '@odata.context' not correct.
[Fix] #397612 URI /redfish/v1/Managers/Self/VirtualMedia/Oem/Ami/ClientCertificates & /redfish/v1/Managers/Self/VirtualMedia/Oem/Ami/Certificates , can not access in BMC 3.50 but defind in spec v1.21.
[Fix] #402564 Modify /Managers/Self/NetworkProtocol attribute SSDP:ProtocolEnabled, the value will not update immediately.
[Fix] #397543 Addtional Fan SEL event trigger when clear SKU ID and reset BMC.
[Fix] #396013 When create user by WEBUI , missing some event trigger by redfish.
[Fix] #394193 Mount Virtual Media via Redfish, the behavior is not correct.
[Fix] #393190 Mount Virtual Media via Redfish, the behavior is not correct.
[Fix] #391437 Modify some Network Protocol port number. GET /redfish/v1/Managers/Self/NetworkProtocol, the port number will not update immediately.
[Fix] #391109 Via Redfish Flash BMC, some Redfish events will be logged from 'http' not 'https'.
[Fix] #390665 Via Redfish Flash BIOS, some Redfish events will be logged from 'http' not 'https'.
[Fix] #384257 /redfish/v1/EventService/Subscriptions, IPMI SEL did not sync to EventService Subscriptions.
[Fix] #376752 Redfish can't detect Fan sensor number '101' on /redfish/v1/Chassis/Self/Thermal#/Fans/1xx_0/ReadingRPM URI.
[Fix] #372833 The MaxImageSizeBytes attribute value too much change after upload BMC FW image via redfish.
[Fix] #398807 Implementing 'Image Redirection' in WebUI lost some files(CD/DVD and Harddisk)
[Fix] #404458 Due to issue id 403835 which doesn't describe the event ('BIOS image update - Check BIOS image project name') clearly in the spec(QCI_BMC_EventLogTable_v5_93).
[Fix] #386030 Use yafuflash tool flash BMC and preserve ipmi,auth,net,after flash complete can't login BMC webUI.
[Fix] #410083 Follow QCT standard rule to remove function of block login after 3 time wrong password.
[Fix] #410562 BMC cold reset by ipmi command did not be blocked when flash CPLD via Yafuflash tool.
[Fix] #409469 Modify IPv4 of BMC setting via Redfish command, BMC SEL record 'IPv4 of BMC has been changed' via DHCP over 150 seconds(Spec define criteria).
[Fix] #402450 Set BMC Lan from DHCP to static, the SEL log will record unexpected event about IPv6 addr#01.
[Fix] #402716 Set LDAP certificate rekey, the Audit event not correct.
[Fix] #405896 Please help to define /Managers/Self/OemSensors URI complete permission table in Redfish SPEC.
[Fix] #410211 Redfish set ActiveDirectory Authentication account, the old password in the Auditlog content is not hidden.
[Fix] #410266 Redfish record incorrect event when patch SSDP from default true to false under /redfish/v1/Managers/Self/NetworkProtocol.
[Fix] #406022 The "links" value of SSE record log has wrong after POST EventService.SubmitTestEvent via redfish. (EventServer has same issue).
[Fix] #410265 POST data to /redfish/v1/TelemetryService/Triggers will response 500 error.
[Fix] #410281 PATCH "StaticNameServers" to redfish/v1/Managers/Self/EthernetInterfaces/bond0 does not work.
[Fix] #406022 The "links" value of SSE record log has wrong after POST EventService.SubmitTestEvent via redfish. (EventServer has same issue).
[Fix] #403259 Redfish set LDAP role group from 1 to 5, the "RemoteRoleMapping" attribute will lost in /redfish/v1/AccountService.
[Fix] #404438 Modify BMC IPv6 Network "OperatingMode" to "Stateless", the BMC will not disconnect in 1min 10s.
[Fix] #385354 The Redfish will lost some FW update event, it's different with WebUI/IPMI after update BMC FW via redfish with preserve Redfish. (Some event timestamp is wrong).
[Fix] #403167 After inject Strike Timeout Error the SUT doesn't auto power cycle and it still hang on.
[Fix] #409578 After Inject Error Injection(CATERR - IERR), the expected status of SUT is 'reset', but the actual status is 'hangup'.
[Fix] #409411 BMC SEL repeatedly records 'BIOS image update fail-incorrect image file'' event after flash other project's BIOS BIN_enc file via yafuflash.
[Fix] #410664 Update BIOS FW via YAFUFlash tool is fail on the RedHat9(Outband).
[Fix] #413393 The IPMI Main will crash if the user inserts too many SSD in S5XQH and create/delete the Logical device in WEBUI and RESTFul command.(Need to do BMC reboot if the issue occurs)
[Fix] SNMPv3 walk to FRU will timeout if no OCP Card inserted.

[Known issue]:
S5XH/S5XQH:
1.[BMC][373410]LDAP settings ''Encryption Type'' choose ''StartTLS'' with server address is IPv6, the LDAP user cannot login WebUI success. (Server address use IPv4 is pass.)
2.[BMC] Sometimes Audit Log will not record IPMI Power action.
3.[BMC][405366] LDAP account user1 access /Managers, the Status Code will return 401.
4.[BIOS][409722]BMC sensor ''Temp_OCP_ASIC'' and ''Temp_OCP_Trasv'' status is ''na'' during AC cycle/reboot.
5.[BMC][416963]The redfish will response error message and status code is 400 after enable ActiveDirectory Service via redfish.

[Notice]:
1. For S5XQH, only support HW FAB4, FAB6 and FAB7.
2. For S5XQH, before upgrading to v2.11, please use the MB-SKU-Tool to update the MB sku.
3. For S5XQH, updating from 2.18 to 2.21, please use the socflash.
4. The password strength must be set at least 8 letters.
5. For S5XQH, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
6. If upgrade BMC from 2.30 or before version to 3.00, please use the socflash to upgrade BMC.
7. For S5XQH, after updating 3.02, please use the BIOS 3A04 or later.
8. If upgrade BMC from 3.02.06 to ~3.15.06, please use SOCFlash.
9. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.
10. RKVM(H5viewer) on webui might connect fail and then close the window within 5 minutes after AC on/BMC cold reset.
   Please wait for RKVM task reday 5 minute after AC on/BMC cold reset. Then user can use RKVM normally.
   If webui fail to open after RKVM(H5viewer) connection fail, please execute "BMC cold reset" and wait for more than 5 minutes. Then user can use RKVM normally.
11. There is a limitation for bmc downgrade to 3.05 from 3.15, yafuflash tool and update function has update by AMI.
12. Didn't support OEM privilege.
13. Please use Yafuflash version 6.86.05 if your BMC version is after 3.15
14. Please use Yafuflash version 6.86.28 if your BMC version is after 3.34

==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.35.06
==========================================================================
Version: 3.35.06
Release Date: 2023.03.20
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.15
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.86.05)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.35.06_rom.ima with checksum          : 01236872 
2. s5xhv3.35.06_rom.ima with MD5 checksum      : c77823b6e7b2e1e2f17f6b1923bd4801 
3. s5xhv3.35.06_rom.ima_enc with MD5 checksum  : 3afb0b80cad00a30534931fcf78c3c36 

[Fan Table]
Version:
S5X:  
sku0:   S5X_3.5_R06_20210122 .xml
sku1~2: S5X_2.5_R06_20210122 .xml

S5XQ: 
sku3~4: S5XQ_QCT_3p5_FSC_Table_R02_20210420.xml
sku5~8: S5XQ_QCT_2p5_FSC_Table_R02_20210420.xml

[Change/Add]:
S5XH/S5XQH:
N/A

[Bug Fixed]:
S5XH/S5XQH:
1. [Fix] SNMPv3 walk to FRU will timeout if no OCP Card inserted.

[Known issue]:
S5XH/S5XQH:
1. [BMC][373410]LDAP settings ''Encryption Type'' choose ''StartTLS'' with server address is IPv6, the LDAP user cannot login WebUI success. (Server address use IPv4 is pass.)
2. [BMC][389190]Lost RKVM virtual device ''Hard Disk/USB'' during DC cycle over 100 cycles.(Only JViewer has this issue, H5Viewer is pass.)
3. [Redfish][390845]Redfish will not log ''Timestamp clock sync event is first of pair - Asserted'' event after disabled automatic NTP Date & Time via WebUI.
4. [BMC][387117]BMC sensor ''Temp_OCP_ASIC'' status is ''na'' during DC/AC cycle.(INTEL E810 known issue).
5. [BMC][390757]BMC webUI didn't block use root default password(less 8 character) to save SNMPv3 setting.
6. [Redfish][382750]GET /redfish/v1/Chassis/Self/NetworkAdapters/DevType7_NICX, The ''Manufacturer'' doesn't display.
7. [BMC][RAID][413393] The IPMI Main will crash if the user inserts too many SSD in S5XQH and create/delete the Logical device in WEBUI and RESTFul command.(Need to do BMC reboot if the issue occurs)

[Notice]:
1. For S5XQH, only support HW FAB4, FAB6 and FAB7.
2. For S5XQH, before upgrading to v2.11, please use the MB-SKU-Tool to update the MB sku.
3. For S5XQH, updating from 2.18 to 2.21, please use the socflash.
4. The password strength must be set at least 8 letters.
5. For S5XQH, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
6. If upgrade BMC from 2.30 or before version to 3.00, please use the socflash to upgrade BMC.
7. For S5XQH, after updating 3.02, please use the BIOS 3A04 or later.
8. If upgrade BMC from 3.02.06 to ~3.15.06, please use SOCFlash.
9. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.
10. RKVM(H5viewer) on webui might connect fail and then close the window within 5 minutes after AC on/BMC cold reset.
   Please wait for RKVM task reday 5 minute after AC on/BMC cold reset. Then user can use RKVM normally.
   If webui fail to open after RKVM(H5viewer) connection fail, please execute "BMC cold reset" and wait for more than 5 minutes. Then user can use RKVM normally.
11. There is a limitation for bmc downgrade to 3.05 from 3.15, yafuflash tool and update function has update by AMI.
12. Didn't support OEM privilege.
13. Please use Yafuflash version 6.86.05 if your BMC version is after 3.15

==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.34.06
==========================================================================
Version: 3.34.06
Release Date: 2022.12.09
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.15
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.86.05)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.34.06_rom.ima with checksum          : 012A3162 
2. s5xhv3.34.06_rom.ima with MD5 checksum      : 5d96af168755fbebc228d891a0105c4c 
3. s5xhv3.34.06_rom.ima_enc with MD5 checksum  : 0b3d02dc4071b7a28ad04b5f562869f1 

[Fan Table]
Version:
S5X:  
sku0:   S5X_3.5_R06_20210122 .xml
sku1~2: S5X_2.5_R06_20210122 .xml

S5XQ: 
sku3~4: S5XQ_QCT_3p5_FSC_Table_R02_20210420.xml
sku5~8: S5XQ_QCT_2p5_FSC_Table_R02_20210420.xml

[Change/Add]:
S5XH/S5XQH:
N/A

[Bug Fixed]:
S5XH/S5XQH:
1. [Fix-BMC] [390066]BMC webUI system inventory page, power info show ''Limit in Watts'' and ''Limit Exception'' value as NA.
2. [Fix-Redfish] [390711]Use redfish /redfish/v1/UpdateService/upload CPLD,BMC sel log didn't record ''CPLD image update - CPLD image update success''.
3. [Fix-BMC] [390713]BMC should blocked SUT is power on status to update CPLD via redfish /redfish/v1/UpdateService/upload.
4. [Fix-BMC][390997]The SEL ''PCIe Bus Correctable/Uncorrectable/Fatal Error (Bus 16 / Dev 02 / Fun 00)'' & ''ManufacturerID: 000315/ VID: 8086/ DID: 347D/ ErrorID: 24 Slot: Undefined ( 17-02)'' mismatch spec.
5. [Fix-Redfish][382763]GET /redfish/v1/Chassis/Self/NetworkAdapters/DevType7_NICX, The ''FirmwarePackageVersion'' doesn't display version.
6. [Fix-BMC][406049] BMC can't mount SD card after AC cycle randomly. (Fail rate: 5/10)
7. [Fix-BMC] Fix SNMP service will be down if the BMC has inserted RAID Card.
8. [Fix-BMC] Fix CVE-2022-40259, CVE-2022-2827.

[Known issue]:
S5XH/S5XQH:
1. [BMC][373410]LDAP settings ''Encryption Type'' choose ''StartTLS'' with server address is IPv6, the LDAP user cannot login WebUI success. (Server address use IPv4 is pass.)
2. [BMC][389190]Lost RKVM virtual device ''Hard Disk/USB'' during DC cycle over 100 cycles.(Only JViewer has this issue, H5Viewer is pass.)
3. [Redfish][390845]Redfish will not log ''Timestamp clock sync event is first of pair - Asserted'' event after disabled automatic NTP Date & Time via WebUI.
4. [BMC][387117]BMC sensor ''Temp_OCP_ASIC'' status is ''na'' during DC/AC cycle.(INTEL E810 known issue).
5. [BMC][390757]BMC webUI didn't block use root default password(less 8 character) to save SNMPv3 setting.
6. [Redfish][382750]GET /redfish/v1/Chassis/Self/NetworkAdapters/DevType7_NICX, The ''Manufacturer'' doesn't display.


[Notice]:
1. For S5XQH, only support HW FAB4, FAB6 and FAB7.
2. For S5XQH, before upgrading to v2.11, please use the MB-SKU-Tool to update the MB sku.
3. For S5XQH, updating from 2.18 to 2.21, please use the socflash.
4. The password strength must be set at least 8 letters.
5. For S5XQH, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
6. If upgrade BMC from 2.30 or before version to 3.00, please use the socflash to upgrade BMC.
7. For S5XQH, after updating 3.02, please use the BIOS 3A04 or later.
8. If upgrade BMC from 3.02.06 to ~3.15.06, please use SOCFlash.
9. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.
10. RKVM(H5viewer) on webui might connect fail and then close the window within 5 minutes after AC on/BMC cold reset.
   Please wait for RKVM task reday 5 minute after AC on/BMC cold reset. Then user can use RKVM normally.
   If webui fail to open after RKVM(H5viewer) connection fail, please execute "BMC cold reset" and wait for more than 5 minutes. Then user can use RKVM normally.
11. There is a limitation for bmc downgrade to 3.05 from 3.15, yafuflash tool and update function has update by AMI.
12. Didn't support OEM privilege.
13. Please use Yafuflash version 6.86.05 if your BMC version is after 3.15

==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.33.06
==========================================================================
Version: 3.33.06
Release Date: 2022.06.23
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.15
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.86.05)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.33.06_rom.ima with checksum          : 014DFA8E 
2. s5xhv3.33.06_rom.ima with MD5 checksum      : f32ca99fc5238714b828e7d55b8391be 
3. s5xhv3.33.06_rom.ima_enc with MD5 checksum  : 8041f2face8647fee1b5c1c0b9979ebb 

[Fan Table]
Version:
S5X:  
sku0:   S5X_3.5_R06_20210122 .xml
sku1~2: S5X_2.5_R06_20210122 .xml

S5XQ: 
sku3~4: S5XQ_QCT_3p5_FSC_Table_R02_20210420.xml
sku5~8: S5XQ_QCT_2p5_FSC_Table_R02_20210420.xml

[Change/Add]:
S5XH/S5XQH:
1. [Add] [Redfish] Redfish API of Virtual Drive Information.(redfish/v1/Systems/Self/VDR)

[Bug Fixed]:
S5XH/S5XQH:
1.[Fix-BMC] Sometimes S5XQH NVMeSSD Temp or HDD status will shows abnormal reading. 
2.[Fix-BMC] 393198 - Fix WEB UI Services page, lost "solssh" and "ssh" items.

[Known issue]:
S5XH/S5XQH:
1. [BMC][373410]LDAP settings ''Encryption Type'' choose ''StartTLS'' with server address is IPv6, the LDAP user cannot login WebUI success. (Server address use IPv4 is pass.)
2. [BMC][389190]Lost RKVM virtual device ''Hard Disk/USB'' during DC cycle over 100 cycles.(Only JViewer has this issue, H5Viewer is pass.)

[Notice]:
1. For S5XQH, only support HW FAB4, FAB6 and FAB7.
2. For S5XQH, before upgrading to v2.11, please use the MB-SKU-Tool to update the MB sku.
3. For S5XQH, updating from 2.18 to 2.21, please use the socflash.
4. The password strength must be set at least 8 letters.
5. For S5XQH, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
6. If upgrade BMC from 2.30 or before version to 3.00, please use the socflash to upgrade BMC.
7. For S5XQH, after updating 3.02, please use the BIOS 3A04 or later.
8. If upgrade BMC from 3.02.06 to ~3.15.06, please use SOCFlash.
9. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.
10. RKVM(H5viewer) on webui might connect fail and then close the window within 5 minutes after AC on/BMC cold reset.
   Please wait for RKVM task reday 5 minute after AC on/BMC cold reset. Then user can use RKVM normally.
   If webui fail to open after RKVM(H5viewer) connection fail, please execute "BMC cold reset" and wait for more than 5 minutes. Then user can use RKVM normally.
11. There is a limitation for bmc downgrade to 3.05 from 3.15, yafuflash tool and update function has update by AMI.
12. Didn't support OEM privilege.
13. Please use Yafuflash version 6.86.05 if your BMC version is after 3.15

==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.32.06
==========================================================================
Version: 3.32.06
Release Date: 2022.03.31
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.15
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.86.05)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.32.06_rom.ima with checksum          : 01493CB4 
2. s5xhv3.32.06_rom.ima with MD5 checksum      : 13569cb8ed7a5cff5f8c8033809873b2 
3. s5xhv3.32.06_rom.ima_enc with MD5 checksum  : 4be269b6858332537fd08529e7798c7b 

[Fan Table]
Version:
S5X:  
sku0:   S5X_3.5_R06_20210122 .xml
sku1~2: S5X_2.5_R06_20210122 .xml

S5XQ: 
sku3~4: S5XQ_QCT_3p5_FSC_Table_R02_20210420.xml
sku5~8: S5XQ_QCT_2p5_FSC_Table_R02_20210420.xml

[Change/Add]:
S5XH/S5XQH:
1. [CS-BMC] Add IPv6 information in WEB UI System Inventory.
3. [CS-BMC] Add BMC Remote Debug Console function.
4. [BMC] Can read Intel E810 OCP 3.0 Card ASIC temp.  
5. [BMC] External reset function(Use CPLD v8 to varify).

[Bug Fixed]:
S5XH/S5XQH:
1.[Fix] #387151, The jviewer expiry date closer than one month, will pop up SEL every day.
2.[Fix] #383441, SEL didn't record ''BIOS image update fail-incorrect image file'' after flash BIOS bin file via Yafuflash 6.86.05.
3.[Fix] #385202, Fix CPLD success log.
4.[Fix] #387658, Fix BMC "Temp_Inlet Upper Non-Recoverable - Going High" SEL severity.
5.[Fix] #382106#382088, Add mutex on coreAPI to fix watchdog timeout issue.
6.[Fix] #387846, In band linux.sh still preserve config after BMC update.
7.[Fix] #386839, Dashboard UI show sel log classification is abnormal when user login and logout via ipv6.
8.[Fix] #386669  The case in WebUI Services ''Cd-media'' and ''Hd-media'' is different between browser firefox and chrome
9.[Fix] #385387 BMC sel record ''Login success'' event when change user password via WEBUI.la
10.[Fix] #383314, BMC SEL record ''System Firmwares #0x8d | Unknown Error | Asserted'' during DC cycle 12 hrs(loop: 3)(Similar issue 383009)
11.[Fix] #383009, BMC logs ''System Firmwares POST Error | Unknown Error | Asserted'' event during RHEL 8.3 warm boot cycle test around 126 loops
12.[Fix] #386914, Base on BMC STD meeting,BMC update via Redfish 1.8 only support preserve all and non-preserve all.
13.[Fix][371183] BMC shouldn't have "Firmware been update..." message when verify fail with upload other project BMC image.
14.[Fix] CPLD upgrade FW failed.
15.[Fix][363296] Redfish Administrator password did not restore to default after restore default via OEM command.
16.[Fix][382345]POST /redfish/v1/Managers/Self/Actions/Manager.FactoryReset without reset.
17.[Fix][382210] Set Mount CD/DVD and Hard disk in WebUI Media Redirection failed.
18.[Fix][381719] NIC Controller Information page end page have a little edition type problem.
19.[Fix]Power_FANG0 value is double than Power_FANG1 when same duty.
20.[Fix]Receiver second source will trigger many interrupts to make BMC hang up.  
21.[Fix][381612]WebUI System Inventory Thermal tab page Temperature info sensor reading value have wrong value "NaN". 
22.[Fix][384018]IPv4 value change to strange value after BMC not accept invalid value and then refrash page. 
23.[Fix][353835]Dashboard UI show sel log classification is abnormal when user login and logout. 
24.[Fix][384033]Use Firefox to first open BMC web, after accept the unsecure certificate, Firebox will reply session time out (User haven't login) 
25.[Fix][381373]The Board Extra data will disappear in FRU info when Board Extra key-in just one character 
26.[Fix][382494]After BMC cold reset will found an incorrect event "Management controller off-line (undefined event in Data2) - Asserted"
27.[Fix][372751]BMC password will be changed after restore previously-saved configuration file via WebUI, user can't login to BMC 
28.[Fix][383509]BMC can accept 0.0.0.0 as IPv4 default Gateway, It's against help info and SPX_User_Guide-RR12_v170 
29.[Fix][352256]Temp_NVMeSSD & T_SSD_Highest sometimes get ns during system stress (system & iperf & GPU)
30.[Fix][383713]Role group can not save when Group Privilege are "User" and "None"
31.[Fix][382060]intel E810 OCP card temperature sensor no reading
32.[Fix][381437]During AC cycle NVMe temp sensors and T_SSD_Highest sensor will become disabled sensors and get reading value is "NA".
33.[Fix][347346]BMC SEL some items get "Upper Critical - Going High" and reading degree not match sdr during idle overnight.
34.[Fix][382477]SEL ''BMC boot from image-2'' record during 12 hrs DC power cycle.
35.[Fix][382472]BMC reset during DC power cycle in loop6, BMC record Version Change event.
36.[Fix][386803]The case in WebUI Services ''Cd-media'' and ''Hd-media'' is different between browser firefox and chrome.
37.[Fix][385766]BMC sel record ''Login success'' event when change user password via WEBUI.
38.[Fix][383500]BMC SEL record ''System Firmwares #0x8d | Unknown Error | Asserted'' during DC cycle 12 hrs(loop: 3)(Similar issue 383009)
39.[Fix][387124]Base on BMC STD meeting,BMC update via Redfish 1.8 only support preserve all and non-preserve all.
40.[Fix][343421]BMC sel record ''BIOS image update'' events during BIOS update via Yafuflash doesn't defined in event log table. (QCI_BMC_EventLogTable_v5_00
41.[Fix][382763]GET /redfish/v1/Chassis/Self/NetworkAdapters/DevType7_NICX, The ''FirmwarePackageVersion'' doesn't display version
42.[Fix][382750]GET /redfish/v1/Chassis/Self/NetworkAdapters/DevType7_NICX, The ''Manufacturer'' doesn't display
43.[Fix][381612]WebUI System Inventory Thermal tab page Temperature info sensor reading value have wrong value ''NaN''.
44.[Fix][381373]The Board Extra data will disappear in FRU info when Board Extra key-in just one character.
45.[Fix][382250]AuditLog Entries message content ''transfer protocol'' is different with old version of BMC.
46.[Fix][385781]The WebUI SSL info didn't restore to default after update BMC FW via redfish with only preserve redfish.
47.[Fix][385303]The BMC Timezonoe will restore to default value after update BMC FW via redfish with preserve NTP.
48.[Fix][385309]User can't access WebUI/Redfish after update BMC FW via redfish with preserve AUTH.
49.[Fix][385380]The Media Redirection settings will restore to default and WebUI will popup warning message after update BMC FW via redfish with preserve KVM.
50.[Fix][386462]The value of HddWeight with HDD quantity doesn't match spec: FSC Table_R08_20211214_Quartet_Duet.
51.[Fix][386554]Should include "Yafuflash version", ''Code Base'' and ''DMTF Redfish Specification version'' information in release note.
52.[Fix][386818]SMASH service doesn't ready after BMC restore factory defaults 300 seconds, this behavior mismatch with std BMC FW spec definition.
53.[Fix][385784]Setup ''Default Gateway IP'' via IPMITOOL will show strange information and make gateway ip to strange value.

[Known issue]:
S5XH/S5XQH:
1. [Redfish] Hitachi requirements is not ready.(Virtual Drive Information)
2. [BMC][373410]LDAP settings ''Encryption Type'' choose ''StartTLS'' with server address is IPv6, the LDAP user cannot login WebUI success. (Server address use IPv4 is pass.)
3. [BMC][389190]Lost RKVM virtual device ''Hard Disk/USB'' during DC cycle over 100 cycles.(Only JViewer has this issue, H5Viewer is pass.)

[Notice]:
1. For S5XQH, only support HW FAB4, FAB6 and FAB7.
2. For S5XQH, before upgrading to v2.11, please use the MB-SKU-Tool to update the MB sku.
3. For S5XQH, updating from 2.18 to 2.21, please use the socflash.
4. The password strength must be set at least 8 letters.
5. For S5XQH, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
6. If upgrade BMC from 2.30 or before version to 3.00, please use the socflash to upgrade BMC.
7. For S5XQH, after updating 3.02, please use the BIOS 3A04 or later.
8. If upgrade BMC from 3.02.06 to ~3.15.06, please use SOCFlash.
9. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.
10. RKVM(H5viewer) on webui might connect fail and then close the window within 5 minutes after AC on/BMC cold reset.
   Please wait for RKVM task reday 5 minute after AC on/BMC cold reset. Then user can use RKVM normally.
   If webui fail to open after RKVM(H5viewer) connection fail, please execute "BMC cold reset" and wait for more than 5 minutes. Then user can use RKVM normally.
11. There is a limitation for bmc downgrade to 3.05 from 3.15, yafuflash tool and update function has update by AMI.
12. Didn't support OEM privilege.
13. Please use Yafuflash version 6.86.05 if your BMC version is after 3.15

==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.18.06
==========================================================================
Version: 3.18.06
Release Date: 2022.01.28
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.05
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.85.00)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.18.06_rom.ima with checksum          : 196C99AA
2. s5xhv3.18.06_rom.ima with MD5 checksum      : 3107bbabd90ab528d7282af7d20f73b3
3. s5xhv3.18.06_rom.ima_enc with MD5 checksum  : f6e45dfa6e569e399b03a55836dd5d00

[Fan Table]
Version:
S5X:
SKU 0	: R05 (S5X_3.5_R06_20210122 )
SKU 1~2	: R05 (S5X_2.5_R06_20210122 )
S5XQ:
SKU 3~8	: R01 (S5XQ_QCT_2p5_FSC_Table_R01_20201221, S5XQ_QCT_3p5_FSC_Table_R01_20201221)

[Change/Add]:
S5XH/S5XQH:
N/A

[Bug Fixed]:
S5XH/S5XQHS5XQH:
1. [BMC] Sometime NVMeSSD Temp or HDD status will shows abnormal reading.

[Known Issues]:
S5XH/S5XQH:
1. [Redfish] Hitachi requirements is not ready.(Virtual Drive Information)
2. [Redfish] Will get "Unkown" Sensor type via Redfish Logs.
3. [BMC] BMC sometimes will logged "Unknown | sensor of type Unknown | (Unknown OEM D0 SEL)" SEL Log event.

[Notice]:
1. For S5XQH, only support HW FAB4, FAB6 and FAB7.
2. For S5XQH, before upgrading to v2.11, please use the MB-SKU-Tool to update the MB sku.
3. For S5XQH, updating from 2.18 to 2.21, please use the socflash.
4. The password strength must be set at least 8 letters.
5. For S5XQH, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
6. If upgrade BMC from 2.30 or before version to 3.00, please use the socflash to upgrade BMC.
7. For S5XQH, after updating 3.02, please use the BIOS 3A04 or later.
8. If upgrade BMC from 3.02.06 to ~3.15.06, please use SOCFlash.
9. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.
10. RKVM(H5viewer) on webui might connect fail and then close the window within 5 minutes after AC on/BMC cold reset.
   Please wait for RKVM task reday 5 minute after AC on/BMC cold reset. Then user can use RKVM normally.
   If webui fail to open after RKVM(H5viewer) connection fail, please execute "BMC cold reset" and wait for more than 5 minutes. Then user can use RKVM normally.

==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.17.06
==========================================================================
Version: 3.17.06
Release Date: 2021.12.29
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.05
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.85.00)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.17.06_rom.ima with checksum          : 1967BB90
2. s5xhv3.17.06_rom.ima with MD5 checksum      : 53578e293d984327613b09994f4371d6
3. s5xhv3.17.06_rom.ima_enc with MD5 checksum  : 41af6878bbec37ce4b239a1b9bf5d7dd

[Fan Table]
Version:
S5X:
SKU 0	: R05 (S5X_3.5_R06_20210122 )
SKU 1~2	: R05 (S5X_2.5_R06_20210122 )
S5XQ:
SKU 3~8	: R01 (S5XQ_QCT_2p5_FSC_Table_R01_20201221, S5XQ_QCT_3p5_FSC_Table_R01_20201221)

[Change/Add]:
S5XH/S5XQH:
N/A

[Bug Fixed]:
S5XH/S5XQH:
1. [BMC] Add Code to prevent the 2nd source receiver will cause IO Expander to issue abnormal interrupts to make BMC reboot.
2. [BMC] Add code to prevent the LiteON PSU will cause IO Expander to issue abnormal interrupts to make BMC reboot.
3. [BMC][WorkAround] Intel CPU when DC On/Off will have noice and let BMC to Log Fake CATErr SEL Log.

[Known Issues]:
S5XH/S5XQH:
1. [Redfish] Hitachi requirements is not ready.(Virtual Drive Information)
2. [Redfish] Will get "Unkown" Sensor type via Redfish Logs.
3. [BMC] BMC sometimes will logged "Unknown | sensor of type Unknown | (Unknown OEM D0 SEL)" SEL Log event.
4. [S5XQH] Power_FANG0/1 sensor value is not correct.

[Notice]:
1. For S5XQH, only support HW FAB4, FAB6 and FAB7.
2. For S5XQH, before upgrading to v2.11, please use the MB-SKU-Tool to update the MB sku.
3. For S5XQH, updating from 2.18 to 2.21, please use the socflash.
4. The password strength must be set at least 8 letters.
5. For S5XQH, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
6. If upgrade BMC from 2.30 or before version to 3.00, please use the socflash to upgrade BMC.
7. For S5XQH, after updating 3.02, please use the BIOS 3A04 or later.
8. If upgrade BMC from 3.02.06 to ~3.15.06, please use SOCFlash.
9. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.
10. RKVM(H5viewer) on webui might connect fail and then close the window within 5 minutes after AC on/BMC cold reset.
   Please wait for RKVM task reday 5 minute after AC on/BMC cold reset. Then user can use RKVM normally.
   If webui fail to open after RKVM(H5viewer) connection fail, please execute "BMC cold reset" and wait for more than 5 minutes. Then user can use RKVM normally.

==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.16.06
==========================================================================
Version: 3.16.06
Release Date: 2021.11.10
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.05
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.85.00)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.16.06_rom.ima with checksum          : 1968E0CA
2. s5xhv3.16.06_rom.ima with MD5 checksum      : 6a5b04b75a3c80085567a31b5f9692a8
3. s5xhv3.16.06_rom.ima_enc with MD5 checksum  : db3c633d335a88d57c8c286ef9e66945

[Fan Table]
Version:
S5X:
SKU 0	: R05 (S5X_3.5_R06_20210122 )
SKU 1~2	: R05 (S5X_2.5_R06_20210122 )
S5XQ:
SKU 3~8	: R01 (S5XQ_QCT_2p5_FSC_Table_R01_20201221, S5XQ_QCT_3p5_FSC_Table_R01_20201221)

[Change/Add]:
S5XH/S5XQH:
N/A

[Bug Fixed]:
S5XH/S5XQH:
1. [Redfish] Fix customer Redfish unstable issue.(Redfish error code 500, 503)
(Get Power State: - PUMADEV-2894), (Get system drives – PUMADEV-2902), (Clear system logs – PUMADEV-2900), (Get Device UUID – PUMADEV-2901)

[Known Issues]:
S5XH/S5XQH:
1. [Redfish] Hitachi requirements is not ready.(Virtual Drive Information)
2. [Redfish] Will get "Unkown" Sensor type via Redfish Logs.
3. [BMC] BMC sometimes will logged "Unknown | sensor of type Unknown | (Unknown OEM D0 SEL)" SEL Log event.

[Notice]:
1. For S5XQH, only support HW FAB4, FAB6 and FAB7.
2. For S5XQH, before upgrading to v2.11, please use the MB-SKU-Tool to update the MB sku.
3. For S5XQH, updating from 2.18 to 2.21, please use the socflash.
4. The password strength must be set at least 8 letters.
5. For S5XQH, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
6. If upgrade BMC from 2.30 or before version to 3.00, please use the socflash to upgrade BMC.
7. For S5XQH, after updating 3.02, please use the BIOS 3A04 or later.
8. If upgrade BMC from 3.02.06 to ~3.15.06, please use SOCFlash.
9. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.
10. RKVM(H5viewer) on webui might connect fail and then close the window within 5 minutes after AC on/BMC cold reset.
   Please wait for RKVM task reday 5 minute after AC on/BMC cold reset. Then user can use RKVM normally.
   If webui fail to open after RKVM(H5viewer) connection fail, please execute "BMC cold reset" and wait for more than 5 minutes. Then user can use RKVM normally.

==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.15.06
==========================================================================
Version: 3.15.06
Release Date: 2021.09.09
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.05
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.85.00)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.15.06_rom.ima with checksum          : 1963A218
2. s5xhv3.15.06_rom.ima with MD5 checksum      : 04b758b929a7ebc08f9ebb2ec552b2ae
3. s5xhv3.15.06_rom.ima_enc with MD5 checksum  : 490eebe6a5399d929137cc87e22e2b6c

[Fan Table]
Version:
S5X:
SKU 0	: R05 (S5X_3.5_R06_20210122 )
SKU 1~2	: R05 (S5X_2.5_R06_20210122 )
S5XQ:
SKU 3~8	: R01 (S5XQ_QCT_2p5_FSC_Table_R01_20201221, S5XQ_QCT_3p5_FSC_Table_R01_20201221)

[Change/Add]:
S5XH/S5XQH:
1. [CS-BMC] WEB UI UpdateService change the default settings from overwrite to preserved.
2. [CS-BMC] WEB UI Power Control String modify.("ACPI Shutdown" to "Orderly Shutdown")
3. [CS-BMC] Disable IPMI 1.5 and Enable IPMI 2.0 only.(Please remember to add "-I lanplus" parameter in the IPMI command.)
4. [BMC] Define Intel OCP card Device Name in the table.

[Bug Fixed]:
S5XH/S5XQH:
1. [BMC] Fix the controller_name on WebUI RAID Controller Information page to prevent showing the extra space.
2. [BMC] Fix SNMPv3 ask BPS DIMM will not get the correct Memorydevice info.
3. [BMC] Fix Temp_CPU0/1 sensor threshold is not sync between sensor list and sdr list full -v.
4. [Redfish] Fix Redfish password will not restore to default when BMC restore to default.
5. [Restful] Fix RESTful API Error Code 1453 response is inconsistent when set invalid password.

[Known Issues]:
S5XH/S5XQH:
1. [Redfish] Hitachi requirements is not ready.(Virtual Drive Information)
2. [Redfish] Will get "Unkown" Sensor type via Redfish Logs.
3. [BMC] BMC sometimes will logged "Unknown | sensor of type Unknown | (Unknown OEM D0 SEL)" SEL Log event.

[Notice]:
1. For S5XQH, only support HW FAB4, FAB6 and FAB7.
2. For S5XQH, before upgrading to v2.11, please use the MB-SKU-Tool to update the MB sku.
3. For S5XQH, updating from 2.18 to 2.21, please use the socflash.
4. The password strength must be set at least 8 letters.
5. For S5XQH, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
6. If upgrade BMC from 2.30 or before version to 3.00, please use the socflash to upgrade BMC.
7. For S5XQH, after updating 3.02, please use the BIOS 3A04 or later.
8. If upgrade BMC from 3.02.06 to ~3.15.06, please use SOCFlash.
9. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.
10. RKVM(H5viewer) on webui might connect fail and then close the window within 5 minutes after AC on/BMC cold reset.
   Please wait for RKVM task reday 5 minute after AC on/BMC cold reset. Then user can use RKVM normally.
   If webui fail to open after RKVM(H5viewer) connection fail, please execute "BMC cold reset" and wait for more than 5 minutes. Then user can use RKVM normally.

==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.14.06
==========================================================================
Version: 3.14.06
Release Date: 2021.07.23
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.05
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.85.00)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.14.06_rom.ima with checksum          : 196438E6
2. s5xhv3.14.06_rom.ima with MD5 checksum      : c4168f3d0a45f473a50b379493adb29c
3. s5xhv3.14.06_rom.ima_enc with MD5 checksum  : dae4f90c58aa32b083795362e1b03a4c

[Fan Table]
Version:
S5X:
SKU 0	: R05 (S5X_3.5_R06_20210122 )
SKU 1~2	: R05 (S5X_2.5_R06_20210122 )
S5XQ:
SKU 3~8	: R01 (S5XQ_QCT_2p5_FSC_Table_R01_20201221, S5XQ_QCT_3p5_FSC_Table_R01_20201221)

[Change/Add]:
N/A

[Bug Fixed]:
S5XH/S5XQH:
1. [Redfish] Fix Redfish not ready issue.
2. [BMC] When user Local time zone is GMT -X will cause BMC Event Log keep processing.
3. [BMC] WEB UI System Inventory will not show full information.
4. [BMC] WEB UI Settings --> NIC Management will not show NIC Cards Informations.
5. [BMC] Use Yafuflash to update BIOS with preserve script will not preserve BIOS settings.

[Known Issues]:
1. [Redfish] Hitachi requirements is not ready.(Virtual Drive Information)
2. [Redfish] Will get "Unkown" Sensor type via Redfish Logs.
3. [Redfish] Insert Intel NIC Card will let WEB UI System Inventory to need more time to get information. 
4. [BMC] BMC sometimes will logged "Unknown | sensor of type Unknown | (Unknown OEM D0 SEL)" SEL Log event.

[Notice]:
1. For S5XQH, only support HW FAB4, FAB6 and FAB7.
2. For S5XQH, before upgrading to v2.11, please use the MB-SKU-Tool to update the MB sku.
3. For S5XQH, updating from 2.18 to 2.21, please use the socflash.
4. The password strength must be set at least 8 letters.
5. For S5XQH, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
6. If upgrade BMC from 2.30 or before version to 3.00, please use the socflash to upgrade BMC.
7. For S5XQH, after updating 3.02, please use the BIOS 3A04 or later.
8. If upgrade BMC from 3.02.06 to 3.12.06, please use SOCFlash.
9. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.
10. RKVM(H5viewer) on webui might connect fail and then close the window within 5 minutes after AC on/BMC cold reset.
   Please wait for RKVM task reday 5 minute after AC on/BMC cold reset. Then user can use RKVM normally.
   If webui fail to open after RKVM(H5viewer) connection fail, please execute "BMC cold reset" and wait for more than 5 minutes. Then user can use RKVM normally.

==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.13.06
==========================================================================
Version: 3.13.06
Release Date: 2021.06.17
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.05
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.85.00)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.13.06_rom.ima with checksum          : 1962C3E3
2. s5xhv3.13.06_rom.ima with MD5 checksum      : e54375cd403002d20cfe741cb07bb2ba
3. s5xhv3.13.06_rom.ima_enc with MD5 checksum  : 0601213a2963c0853a9a563c43642006

[Fan Table]
Version:
S5X:
SKU 0	: R05 (S5X_3.5_R06_20210122 )
SKU 1~2	: R05 (S5X_2.5_R06_20210122 )
S5XQ:
SKU 3~8	: R01 (S5XQ_QCT_2p5_FSC_Table_R01_20201221, S5XQ_QCT_3p5_FSC_Table_R01_20201221)

[Change/Add]:
N/A

[Bug Fixed]:
S5XH/S5XQH:
1. [BMC] Fix caterr issue.
2. [BMC] Fix conf protect while AC lost.
3. [BMC] Fix Nvme rear temp.
4. [BMC] Fix fan reading overflow.
5. [BMC] Fix AC lost event.
6. [BMC] Fix yafuflash update bmc.

[Known issue]:
1. [Redfish] Hitachi requirements is not ready.(Virtual Drive Information)

[Notice]:
1. For S5XQH, only support HW FAB4, FAB6 and FAB7.
2. For S5XQH, before upgrading to v2.11, please use the MB-SKU-Tool to update the MB sku.
3. For S5XQH, updating from 2.18 to 2.21, please use the socflash.
4. The password strength must be set at least 8 letters.
5. For S5XQH, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
6. If upgrade BMC from 2.30 or before version to 3.00, please use the socflash to upgrade BMC.
7. For S5XQH, after updating 3.02, please use the BIOS 3A04 or later.
8. If upgrade BMC from 3.02.06 to 3.12.06, please follow below method:
	Method 1: follow below step:
	Step1: ipmitool raw 0x32 0x8f 0x01 0x02  
	Step2: ipmitool mc reset cold  
	Step2-1: Wait BMC Ready	
	Step3: ipmitool raw 0x32 0x8f 0x01 0x04  
	Step4: update 3.05 via webui or yafuflash
	If both fail, please use socflash for 3.05.
9. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.
10. RKVM(H5viewer) on webui might connect fail and then close the window within 5 minutes after AC on/BMC cold reset.
   Please wait for RKVM task reday 5 minute after AC on/BMC cold reset. Then user can use RKVM normally.
   If webui fail to open after RKVM(H5viewer) connection fail, please execute "BMC cold reset" and wait for more than 5 minutes. Then user can use RKVM normally.

==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.12.06
==========================================================================
Version: 3.12.06
Release Date: 2021.05.28
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.05
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.85.00)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.12.06_rom.ima with checksum          : 19B2C7F2
2. s5xhv3.12.06_rom.ima with MD5 checksum      : b0bebd631c1128169b93cbd0579c78d4
3. s5xhv3.12.06_rom.ima_enc with MD5 checksum  : 3c224ae3079cf9bcf592db61f182f97f

[Fan Table]
Version:
S5X:
SKU 0	: R05 (S5X_3.5_R06_20210122 )
SKU 1~2	: R05 (S5X_2.5_R06_20210122 )
S5XQ:
SKU 3~8	: R01 (S5XQ_QCT_2p5_FSC_Table_R01_20201221, S5XQ_QCT_3p5_FSC_Table_R01_20201221)

[Change/Add]:
S5XQH:
1. [BMC] Add Fan STB on event by OCP.  

[Bug Fixed]:
N/A

[Known issue]:
1. [BMC] For S5XH, PSU LED and BP LED will be LID if insert Intel OCP 3.0 Card even is Power Off.
2. [BMC] Insert Intel OCP 3.0 Card may cause Redfish and WEB UI can't get Processors information and DIMM Info.
3. [Redfish] Hitachi requirements is not ready.(Virtual Drive Information)

[Notice]:
1. For S5XQH, only support HW FAB4, FAB6 and FAB7.
2. For S5XQH, before upgrading to v2.11, please use the MB-SKU-Tool to update the MB sku.
3. For S5XQH, updating from 2.18 to 2.21, please use the socflash.
4. The password strength must be set at least 8 letters.
5. For S5XQH, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
6. If upgrade BMC from 2.30 or before version to 3.00, please use the socflash to upgrade BMC.
7. For S5XQH, after updating 3.02, please use the BIOS 3A04 or later.
8. If upgrade BMC from 3.02.06 to 3.12.06, please follow below method:
	Method 1: follow below step:
	Step1: ipmitool raw 0x32 0x8f 0x01 0x02  
	Step2: ipmitool mc reset cold  
	Step2-1: Wait BMC Ready	
	Step3: ipmitool raw 0x32 0x8f 0x01 0x04  
	Step4: update 3.05 via webui or yafuflash
	If both fail, please use socflash for 3.05.
9. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.
10. RKVM(H5viewer) on webui might connect fail and then close the window within 5 minutes after AC on/BMC cold reset.
   Please wait for RKVM task reday 5 minute after AC on/BMC cold reset. Then user can use RKVM normally.
   If webui fail to open after RKVM(H5viewer) connection fail, please execute "BMC cold reset" and wait for more than 5 minutes. Then user can use RKVM normally.

==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.10.06
==========================================================================
Version: 3.10.06
Release Date: 2021.05.21
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.05
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.85.00)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.10.06_rom.ima with checksum          : 19BAB2A2
2. s5xhv3.10.06_rom.ima with MD5 checksum      : 30b69341327fcb088fb0237304f4fdd9
3. s5xhv3.10.06_rom.ima_enc with MD5 checksum  : 2bc581b9db436fbebb14baa6ebae5053

[Fan Table]
Version:
S5X:
SKU 0	: R05 (S5X_3.5_R06_20210122 )
SKU 1~2	: R05 (S5X_2.5_R06_20210122 )
S5XQ:
SKU 3~8	: R01 (S5XQ_QCT_2p5_FSC_Table_R01_20201221, S5XQ_QCT_3p5_FSC_Table_R01_20201221)

[Change/Add]:
S5XH/S5XQH:
1. [Redfish] HDS Redfish request: Server FRU(/redfish/v1/Chassis/Self/FRU)

[Bug Fixed]:
S5XH:
1. [BMC] Fix SMASH Functions.
2. [BMC] Set IPv6 static gateway address in BMC WEBUI, the address value is blank after login WEBUI again.
3. [BMC] Fix IERR dump function at CPU amount checking.
4. [BMC] Fix rkvm connect fail then webui also fail issue, BMC will stop user use rkvm when rkvm not ready.
5. [BMC] Fix BMC Image can't boot to the flashed image.
6. [BMC] Set IPv6 static gateway address in BMC WEBUI, the address value is blank after login WEBUI again.
7. [BMC] Fix fan duty will be set to 100% before BMC not ready while OCP card on board.
8. [BMC] Fix dashboard display issue on webui.
S5XQH:
1. [BMC] Fix full fan speed because wrong code judgement by pcie network card.  
2. [BMC] Remove pex polling task on other sku from all flash sku.

[Known Issue]:
1. [BMC] For S5XH, PSU LED and BP LED will be LID if insert Intel OCP 3.0 Card even is Power Off.
2. [BMC] Insert Intel OCP 3.0 Card may cause Redfish and WEB UI can't get Processors information and DIMM Info.
3. [Redfish] Hitachi requirements is not ready.(Virtual Drive Information)

[Notice]:
1. For S5X, only support HW FAB4, FAB6 and FAB7.
2. The password strength must be set at least 8 letters.
3. For S5X, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
4. For S5X and S5XQ, after updating 2.28, please use the BIOS 2A06 or later.
5. If upgrade BMC from 2.30 or before version to 3.00, please use the socflash to upgrade BMC.
6. For S5X and S5XQ, after updating 3.01, please use the BIOS 3A04 or later.
7. If upgrade BMC from 3.02 to 3.07 or after, please follow below method:
8. If upgrade BMC from 3.02~ to 3.07 or after,
	Please follow below step:
	Step1: ipmitool raw 0x32 0x8f 0x01 0x02  
	Step2: ipmitool mc reset cold        
	Step2-1: Wait BMC Ready
	Step3: ipmitool raw 0x32 0x8f 0x01 0x04  
	Step4: update 3.07.06 or after via webui or yafuflash
	If fail, please use socflash for 3.07.06 or after 
9. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.
10.RKVM(H5viewer) on webui might connect fail and then close the window within 5 minutes after AC on/BMC cold reset.
   Please wait for RKVM task reday 5 minute after AC on/BMC cold reset. Then user can use RKVM normally.
   If webui fail to open after RKVM(H5viewer) connection fail, please execute "BMC cold reset" and wait for more than 5 minutes. Then user can use RKVM normally.
   
==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.08.06
==========================================================================
Version: 3.08.06
Release Date: 2021.04.09
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.05
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.85.00)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.08.06_rom.ima with checksum          : 19B978C8
2. s5xhv3.08.06_rom.ima with MD5 checksum      : af7d4b76ddf3452829585025017d9a9b
3. s5xhv3.08.06_rom.ima_enc with MD5 checksum  : 166fca706d36b2e6d74899ce549a2375

[Fan Table]
Version:
S5X:
SKU 0	: R05 (S5X_3.5_R05.0_20201110)
SKU 1~2	: R05 (S5X_2.5_R05.0_20201110)
SKU 3~8	: R01 (S5XQ_QCT_2p5_FSC_Table_R01_20201221, S5XQ_QCT_3p5_FSC_Table_R01_20201221)

[Change/Add]:
S5XH:
1. Revert the LDAP fucntion from common submodule.
2. Fix the SEL parse about the sensor name of "OS".
3. Fix system could not power on when updating bios firmware.
4. Add SMASH Function Support.

[Bug Fixed]:
S5XH :
1. Fix when ac cycle, the conf would be broken.
2. Add the write disable/enable spi when ac cycle.
3. Fix WEB UI Sensor layout(The sensor value information is not fully shown)
4. Redfish Information missing.(Please use mallonex OCP Card)

[Known issue]:
1. PSU LED and BP LED will be LID if insert Intel OCP 3.0 Card even is Power Off.
2. [BMC] Radius function is not ready - Suport Windows Server Radius (NPS).
3. [Redfish] Hitachi requirements is not ready.
 (1)Server FRUs.
 (2)Virtual Drive Information. 
4. Insert Intel OCP 3.0 Card may cause Redfish and WEB UI can't get Processors information and DIMM Info.

[Notice]:
1. For S5X, only support HW FAB4, FAB6 and FAB7.
2. The password strength must be set at least 8 letters.
3. For S5X, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
4. For S5XQ, only support HW FAB6.
5. If upgrade BMC from 2.30 or before version to 3.00, please use the socflash to upgrade BMC.
6. For S5XH and S5XQH, after updating 3.02, please use the BIOS 3A04 or later.
7. If upgrade BMC from 3.02.06 to 3.08.06, please follow below method:
	Method 1: update 3.08.06 via webui or yafuflash twice continuously.
	Method 2: follow below step:
	Step1: ipmitool raw 0x32 0x8f 0x01 0x02  
	Step2: ipmitool mc reset cold        
	Step3: ipmitool raw 0x32 0x8f 0x01 0x04  
	Step3: update 3.08.06 via webui or yafuflash
	If both fail, please use socflash for 3.08.06
8. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.

==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.07.06
==========================================================================
Version: 3.07.06
Release Date: 2021.03.19
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.05
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.85.00)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.07.06_rom.ima with checksum          : 1B6FD0D4
2. s5xhv3.07.06_rom.ima with MD5 checksum      : 33b8d5a4a104720260ac1e5df3292580
3. s5xhv3.07.06_rom.ima_enc with MD5 checksum  : 61054c893811ac17a37114a218e089b8

[Fan Table]
Version:
S5X:
SKU 0	: R05 (S5X_3.5_R05.0_20201110)
SKU 1~2	: R05 (S5X_2.5_R05.0_20201110)
SKU 3~8	: R01 (S5XQ_QCT_2p5_FSC_Table_R01_20201221, S5XQ_QCT_3p5_FSC_Table_R01_20201221)

[Change/Add]:
1. [IPMI] Change to asynchronize for ipmb request
2. [IPMI] Fix the ME failed after DC cycle

[Bug Fixed]:
1. When using WebUI to update the BIOS firmware, the progress bar will go back to the middle after the Upgrade" is completed.
2. Add there should no AC lost event after DC off for 7 seconds flag definition.
3. Fix the HDD device present bounce bug.
4. Fix Pcie temp no reading at multi-card status.
5. The NVMe status doesn't need to change the 0xe2 channel.
6. Fix the nvme temperature and hdd status sensor sometimes show no reading.

[Known issue]:
1. PSU LED and BP LED will be LID if insert OCP 3.0 Card even is Power Off.
2. [BMC] Radius function is not ready - Suport Windows Server Radius (NPS).
3. [Redfish] Hitachi requirements is not ready.
 (1)Server FRUs.
 (2)Virtual Drive Information. 
4. Insert OCP 3.0 Card may cause Redfish and WEB UI can't get Processors information and DIMM Info.

[Notice]:
 1. For S5XH, only support HW FAB4, FAB6 and FAB7.
 2. The password strength must be set at least 8 letters.
 3. For S5XH, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
 4. For S5XQ, only support HW FAB6.
 5. For S5XH and S5XQH, after updating 2.30, please use the BIOS 2A06 or later.
 6. For S5XH, if upgrade BMC from before version to 3.02, please use socflash tool to upgrade to v3.02.
 7. If upgrade BMC from 3.02~ to 3.07,
	Please follow below step:
	Step1: ipmitool raw 0x32 0x8f 0x01 0x02  
	Step2: ipmitool mc reset cold        
	Step3: ipmitool raw 0x32 0x8f 0x01 0x04  
	Step3: update 3.07.06 via webui or yafuflash
	If fail, please use socflash for 3.07.06
 8. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.
 9. For S5XH, after updating 3.01, please use the BIOS 3A04 or later. 	
 
==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.02.06
==========================================================================
Version: 3.02.06
Release Date: 2021.02.04
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.00
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.85.00)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.02.06_rom.ima with checksum          : 139BEEFA
2. s5xhv3.02.06_rom.ima with MD5 checksum      : afddaae384c74979843d9696b02a23c5
3. s5xhv3.02.06_rom.ima_enc with MD5 checksum  : 45685e864eb9bfe90088d5bdf0d6567e

[Fan Table]
Version:
S5XH:
SKU 0	: R5 (S5X_2.5_R05.0_20201110, S5X_3.5_R05.0_20201110)
SKU 1~2	: R5 (S5X_2.5_R05.0_20201110)
SKU 3~8	: R0 (S5XQ_FSC Table_R00_QCT_20200825_thermal)

[Change/Add]:
1. [RR12.3 AMI pure code update] Kernel update to 5.4 from 5.2 
2. Add Web BIOS Firmware update with preserve function. 
3. Redfish properties changed.
	[/redfish/v1/UpdateService/FirmwareInventory/CPLD]
		Add Version
	[/redfish/v1/UpdateService/FirmwareInventory/BIOS]
		Add Version
	[/redfish/v1/Chassis/Self/Power]
		Remove PowerControl-> PowerLimit
	[/redfish/v1/UpdateService]
		Add Oem->BIOS->BIOSPreserveNVRAM
		
[Bug Fixed]:
 1. [WEB]WEB UI can't update BMC.
 2. [REDFISH]In Redfish GET /Managers/Self Firmware version will show 2.30.xxxxx not 2.30.06 
 1. BMC watchdog reset after high inlet temperature to turn off system.
 2. BMC path Settings > System Firewall will change to Settings > Firewall after enter any page under it.
 3. [Web][FW upgrade] Fix CPLD firmware update.
 4. [WEB][Sensor Page] BMC sensor page will appear a lot of ""Chassis"" sensor at ""Discrete Sensor States"" section(Random 4/10).
 5. [WEB][Dashboard] The BMC version on WebUI menu bar is not matched with firmware package release note and IPMI mc info command.
 6. [WEB][Sensor Detail Page] Sensor detail page show multi record at sensor time line.
 7. [Bug] eTrack 349843 SSL certificate did not preserve after restore factory default with preserve all configuration fix again.
 8. Open Settings > IPMI Interfaces with Operator user privilege, WebUI will pup up error message and show incorrect IPMI Interfaces status.
 

[Known issue]:
1. [BMC]Can not read CPU/PCH temperature sometimes.  The fan speed will be Full duty when the CPU temperature disappears.
2. [BMC] Radius function is not ready - Suport Windows Server Radius (NPS).
3. [Redfish] Hitachi requirements is not ready.
 (1)Server FRUs.
 (2)Virtual Drive Information. 

[Notice]:
 1. For S5XH, only support HW FAB4, FAB6 and FAB7.
 2. For S5XH, before upgrading to v2.11, please use the MB-SKU-Tool to update the MB sku.
 3. For S5XH, updating from 2.18 to 2.21, please use the socflash.
 4. The password strength must be set at least 8 letters.
 5. For S5XH, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
 8. For S5XH, after updating 2.28, please use the BIOS 2A06 or later.
 9. If upgrade BMC from 2.30 or before version to 3.00 or after, please use the socflash to upgrade BMC.
10. For S5XH, after updating 3.01, please use the BIOS 3A04 or later. 

==========================================================================
        S5XH series AST2500(A2) BMC FW Release v2.30.06
==========================================================================
Version: 2.30.06
Release Date: 2020.12.31
Code Base: 2.11
DMTF Redfish Specification version: 1.8
AMI Subversion Revision: AMI SPX RR12.3

[Utility]
1. Yafuflash (version 6.78.0)

[Firmware Images]:
1. s5xhv2.30.06_rom.ima with checksum          : A4A259D2
2. s5xhv2.30.06_rom.ima with MD5 checksum      : e8ef1bc7b025d3b1329f30d39e1f3f82
3. s5xhv2.30.06_rom.ima_enc with MD5 checksum  : f2ea3b85c2f98552d3944c49062c1707

[Fan Table]
Version:
S5X:
SKU 0	: R5 (S5X_2.5_R05.0_20201110, S5X_3.5_R05.0_20201110)
SKU 1~2	: R5 (S5X_2.5_R05.0_20201110)
SKU 3~8	: R0 (S5XQ_FSC Table_R00_QCT_20200825_thermal)

[Change/Add]: 
N/A
[Bug Fixed]:
1. Severity or description of MCERR log within BMC SEL is ''Unspecified'' after trigger UPI Failover error by itp,
2. The FRU0 will become garbled text and cause FRU1/10 disappear after system do reboot. (ipmitool fru print)
3. MB FRU has garbage string. (Both of FP and NIC DRU are normal.)
4. The MB-FRU will disappear after system reboot. (DVT system, HW Rev: D2B Rework A / FP board: HW Rev: A1B)

[Known issue]:
1. The Fan_SYS_Status of SEL log on webUI will parse failed.
2. WEB UI can't update BMC. Please use Yafuflash to update BMC Firmware.
3. In Redfish GET /Managers/Self Firmware version will show 2.30.xxxxx not 2.30.06 
4. [Redfish] Hitachi requirements is not ready.
 (1).Server FRUs.
5. [BMC] Radius function is not ready - Suport Windows Server Radius (NPS).
	
[Notice]:
1. Only support HW FAB6 and FAB4.
2. The password strength must be set at least 8 letters.