Intel(R) Network Connection Tools
==========================================
March 24, 2016

Contents
========
- OVERVIEW
- INSTALLING THE TOOLS ON MICROSOFT* WINDOWS*
- INSTALLING THE TOOLS ON DOS
- INSTALLING THE TOOLS ON EFI
- INSTALLING THE TOOLS ON LINUX*
- CUSTOMER SUPPORT


OVERVIEW
========
This document describes how to install the Intel(R) Network Connection Tools. See
the readme provided for each tool for a detailed explanation of the features
available.


INSTALLING THE TOOLS ON MICROSOFT* WINDOWS*
===========================================

The tools' driver can be installed on all versions of Microsoft* Windows* since
Windows 7. To install the tools' drivers on Windows, run install.bat from the
appropriate directory on the CD.

Although the tools are not installed with install.bat, the driver that the tools
require is copied into the local machine Windows driver directory. To run the
tools, launch a Command Prompt window from the Windows Start Menu. Go to the
media and directory where the tools are located and run the tools. The readme
files for each tool are found in the same directory as the tools. These tools
can be manually installed on the local hard drive in any directory.

The tool uses its own driver file (not the same as the system network driver).
If the driver sys file already exists in the drivers directory, install.bat may
fail to copy. Using the /y switch with install.bat will override and copy the
driver file regardless. However, this can be dangerous if an older version of
the driver is being used by another application such as Intel(R) PROSet for
Windows Device Manager. If a driver is already present in the drivers directory,
try running the tool from the command prompt. If it runs, then the driver is
fine. The tool will not run if the driver version present does not match the
driver version expected.

Note that you must have access to the %systemroot%\system32\drivers
directory. Only the administrator account has these privileges. You must be
logged in as administrator or the tools must be run as administrator.

Note that on Windows, any device that is disabled in device manager will not be
accessible by tools due to no memory resources. You would get an error code
0xC86A800E. To solve this problem, you can do one of the following:
1) Re-enable the device in device manager. Never disable this device when
   using tools.
2) Install an NDIS device driver for the device and make sure that it does
   not have a yellow or red bang by it in device manager.
3) Delete the device from device manager and restart the system. The install
   new hardware wizard should appear on next reboot. Do not cancel this. Just
   move the window aside and run the tool(s). Generally, you can click "cancel"
   on the wizard but there are some cases where Windows will disable the memory
   resources causing you to get back into the same state.


INSTALLING THE TOOLS ON EFI
===========================

There is no installation required for EFI tools. The tools can simply be copied
from the appropriate directory to the drive that they will run from. The EFI2
binaries are for use with the UEFI Shell 2.X with the UEFI 2.3 HII protocol.
EFI2 tools will not run on the EFI Shell 1.X or if the UEFI 2.3 HII protocol is
not present.

Note that while EFI supports USB drives, there may be issues running tools
from the USB drive. Whether or not there are issues are BIOS specific. If you
experience issues, run the tool from hard disk instead.


INSTALLING THE TOOLS ON DOS
===========================

The tools support various DOS versions. There is no installation required for
DOS tools. The tools can simply be copied from the DOS directory on the CD to
the drive that they will run from. It is expected that the tools have a clean
boot environment. The tools will not run with memory managers and/or DOS
networking drivers loaded. The tools expect that they have full, unlimited
control of the hardware. The tools *WILL NOT* run properly if EMM386 is present. 
The tools run in protected mode, 32-bit DOS. Therefore, they will not be
compatible with any TSR programs.


INSTALLING THE TOOLS ON LINUX*
==============================

In order to run tools on Linux*, a driver stub must be built and installed on
the system. This driver is not related to the network device driver that is
used to run the network during live traffic. It is a separate driver used
explicitly for tools. Due to the nature of Linux with the number of kernels
that can exist, we provide source for the driver module and an install script
to build/install it.

The tools support Linux distributions based on kernels 2.6.x. Validation is done
randomly on popular distributions such as Red Hat* or Suse*. Configured
kernel source that matches the currently installed kernel is required. A working
GCC is also required. There are some versions of GCC that had a bug which did not
support unnamed structures. These versions of GCC are not supported. If you have
compilation errors, try updating your version of GCC. If you have linker errors
when installing the driver, you should update your kernel - download the latest
stable off www.kernel.org and build/install it.

Note that some distributions such as recent Fedora core versions do not ship
with Kernel source. You must download, install, and configure the source in
order to get the tools' driver built on this OS. Installing the kernel source
RPM does not solve the problem.

This is the installation procedure:
  1. Log in as root and create a temporary directory to build the Intel(R)
     Network Connection Tools driver.
  2. Copy 'install' and 'iqvlinux.tar.gz' to the temporary directory.
     There are 3 versions of Linux supported: Linux32 (x86), Linux_x64 (x64),
     and Linux64 (Itanium). Copies of the above files exist in the appropriate
     directory for your platform.
  3. CD to the temporary directory and run './install.' The driver has been
     installed now, so the files in the temporary directory can be removed.
  4. Copy the tools that you want to use from the appropriate directory of
     the CD.


INSTALLING THE TOOLS ON ORACLE* SOLARIS*
========================================
Iqvsolaris is a separate driver used explicitly for tools and is provided only
in binary form. Iqvsolaris driver and tools are provided for 2 different
architectures: 64s for sparc and 64e for x86_64.

In order to run tools on Solaris*, peform the following steps:

  1. Log in as root.

  2. Manually unload the network device driver.

  3. Copy the binary iqv driver to the local machine driver directory by
     running the './install' script.


INSTALLING THE TOOLS ON FreeBSD*
================================

In order to run tools on FreeBSD*, a driver stub must be built and installed on
the system. This driver is not related to the network device driver that is
used to run the network during live traffic. It is a separate driver used
explicitly for tools. Due to the nature of FreeBSD with the number of kernels
that can exist, we provide source for the driver module and an install script
to build/install it.

The tools support FreeBSD distributions version 10.1 and later.

This is the installation procedure:
  1. Log in as root and create a temporary directory to build the Intel(R)
     Network Connection Tools driver.
  2. Copy 'install' and 'iqvfreebsd.tar' to the temporary directory.
     There are 2 versions of FreeBSD supported: FreeBSD32 (x86) and
     FreeBSD64e (x64). Copies of the above files exist in the appropriate
     directory for your platform.
  3. CD to the temporary directory and run './install' The driver has
     been installed now, so the files in the temporary directory can be
     removed.
  4. Copy the tools that you want to use from the appropriate directory of
     the CD.


CUSTOMER SUPPORT
================
- Main Intel web support site: http://support.intel.com

- Network products information: http://www.intel.com/network


Legal / Disclaimers
===================
Copyright (C) 2002-2016, Intel Corporation. All rights reserved.

Intel Corporation assumes no responsibility for errors or omissions in this
document. Nor does Intel make any commitment to update the information
contained herein.

Intel is a trademark of Intel Corporation in the U.S. and/or other countries.

*Other names and brands may be claimed as the property of others.

This software is furnished under license and may only be used or copied
in accordance with the terms of the license. The information in this
manual is furnished for informational use only, is subject to change
without notice, and should not be construed as a commitment by Intel
Corporation. Intel Corporation assumes no responsibility or liability
for any errors or inaccuracies that may appear in this document or any
software that may be provided in association with this document. Except
as permitted by such license, no part of this document may be reproduced,
stored in a retrieval system, or transmitted in any form or by any means
without the express written consent of Intel Corporation.
