******Note*****
This is X527 NVM image of DA2.

Please use  Tool ˇ§Lanconfˇ¨ can update the NVM image  lanconf -> select one of port -> eeprom/flash -> PHY NVM-> PHY Fw NVM-> Write PHY Flash

Then AC the system.