<6>[    0.000000] Booting Linux on physical CPU 0
<6>[    0.000000] Initializing cgroup subsys cpu
<5>[    0.000000] Linux version 3.4.5 (jwx384541@forge) (gcc version 4.6.x-google 20120106 (prerelease) (GCC) ) #1 PREEMPT Sat Aug 13 18:36:49 CST 2016
<4>[    0.000000] CPU: ARMv7 Processor [414fc091] revision 1 (ARMv7), cr=18c53c7d
<4>[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, VIPT aliasing instruction cache
<4>[    0.000000] Machine: Hisilicon hi6930
<4>[    0.000000] power down charge p:0, pd_charge_flag :0
<4>[    0.000000] softver is normal, softver_factory = 0
<4>[    0.000000] reset type is normal, reset_mode_flag = 0
<4>[    0.000000] run mode is normal, soft_run_mode = 0
<4>[    0.000000] Memory policy: ECC disabled, Data cache writeback
<7>[000002579ms] On node 0 totalpages: 13312
<7>[000002580ms] free_area_init_node: node 0, pgdat c0866924, node_mem_map c0af0000
<7>[000002580ms]   Normal zone: 104 pages used for memmap
<7>[000002580ms]   Normal zone: 0 pages reserved
<7>[000002580ms]   Normal zone: 13208 pages, LIFO batch:3
<4>[000002584ms] [clk]: <hi6930_clock_init> clk init success!
<7>[000002584ms] pcpu-alloc: s0 r0 d32768 u32768 alloc=1*32768
<7>[000002584ms] pcpu-alloc: [0] 0 
<4>[000002584ms] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 13208
<5>[000002584ms] Kernel command line: root=/dev/ram0 rw console=ttyAMA0,115200 console=uw_tty0,115200 rdinit=/init loglevel=2 mem=0x3400000 boardid=0x00000000,0x00000000,0x00000000 pd_charge=0 androidboot.swtype=normal reset_type=normal power_mode=normal 
<6>[000002584ms] PID hash table entries: 256 (order: -2, 1024 bytes)
<6>[000002584ms] Dentry cache hash table entries: 8192 (order: 3, 32768 bytes)
<6>[000002584ms] Inode-cache hash table entries: 4096 (order: 2, 16384 bytes)
<6>[000002589ms] Memory: 52MB = 52MB total
<5>[000002589ms] Memory: 41384k/41384k available, 11864k reserved, 0K highmem
<5>[000002589ms] Virtual kernel memory layout:
<5>[000002589ms]     vector  : 0xffff0000 - 0xffff1000   (   4 kB)
<5>[000002589ms]     fixmap  : 0xfff00000 - 0xfffe0000   ( 896 kB)
<5>[000002589ms]     vmalloc : 0xc3800000 - 0xff000000   ( 952 MB)
<5>[000002589ms]     lowmem  : 0xc0000000 - 0xc3400000   (  52 MB)
<5>[000002589ms]     modules : 0xbf000000 - 0xc0000000   (  16 MB)
<5>[000002589ms]       .text : 0xc0008000 - 0xc07a1e38   (7784 kB)
<5>[000002589ms]       .init : 0xc07a2000 - 0xc07ce000   ( 176 kB)
<5>[000002589ms]       .data : 0xc07ce000 - 0xc0872838   ( 659 kB)
<5>[000002589ms]        .bss : 0xc08b6e2c - 0xc0ae9288   (2250 kB)
<6>[000002590ms] SLUB: Genslabs=11, HWalign=64, Order=0-3, MinObjects=0, CPUs=1, Nodes=1
<6>[000002590ms] NR_IRQS:224
<6>[000002591ms] sched_clock: 32 bits at 100 Hz, resolution 10000000ns, wraps every 4294967286ms
<6>[000002591ms] Console: colour dummy device 80x30
<6>[000002591ms] Calibrating delay loop... 1196.85 BogoMIPS (lpj=5984256)
<6>[000002681ms] pid_max: default: 32768 minimum: 301
<6>[000002681ms] Mount-cache hash table entries: 512
<6>[000002682ms] Initializing cgroup subsys debug
<6>[000002682ms] Initializing cgroup subsys cpuacct
<6>[000002682ms] Initializing cgroup subsys freezer
<6>[000002682ms] CPU: Testing write buffer coherency: ok
<6>[000002682ms] hw perfevents: enabled with ARMv7 Cortex-A9 PMU driver, 7 counters available
<6>[000002682ms] Setting up static identity map for 0x5509fa78 - 0x5509fad0
<6>[000002688ms] dummy: 
<4>[000002688ms] [hardtimer]: <adp_timer_init> adp_timer_init ok
<4>[000002688ms] 
<6>[000002689ms] NET: Registered protocol family 16
<6>[000002690ms] hw-breakpoint: found 5 (+1 reserved) breakpoint and 1 watchpoint registers.
<6>[000002690ms] hw-breakpoint: maximum watchpoint size is 4 bytes.
<6>[000002690ms] Serial: BalongV7R2 UART driver
<6>[000002690ms] uart0: ttyAMA0 at MMIO 0x90007000 (irq = 102) is a Balong rev0
<6>[000002690ms] console [ttyAMA0] enabled
<4>[000002691ms] ipc probe success
<4>[000002691ms] [icc]: <bsp_icc_init> ok
<4>[000002691ms] softtimer init success
<4>[000002691ms] [pmu]: <bsp_hi6559_debug_init> bsp_hi6559_debug_init ok!
<6>[000002692ms] designware_i2c0 designware_i2c0.0: tx_fifo_depth: 64, rx_fifo_depth: 64
<6>[000002692ms] designware_i2c1 designware_i2c1.1: tx_fifo_depth: 64, rx_fifo_depth: 64
<6>[000002696ms] bio: create slab <bio-0> at 0
<6>[000002697ms] V711_MTCMOS1: 
<6>[000002697ms] V711_MTCMOS2: 
<6>[000002697ms] V711_MTCMOS3: 
<6>[000002697ms] V711_MTCMOS4: 
<6>[000002698ms] V711_MTCMOS5: 
<6>[000002698ms] V711_MTCMOS6: 
<6>[000002698ms] V711_MTCMOS7: 
<6>[000002698ms] V711_MTCMOS8: 
<6>[000002698ms] V711_MTCMOS9: 
<6>[000002698ms] V711_MTCMOS10: 
<6>[000002698ms] V711_MTCMOS11: 
<6>[000002699ms] V711_MTCMOS12: 
<4>[000002699ms] [regulator]: <balong_regulator_probe> <961>v711 mtcmos register ok
<6>[000002699ms] PMIC_HI6559_BUCK0: 900 <--> 4050 mV at 1500 mV at 1500 mA 
<6>[000002699ms] PMIC_HI6559_BUCK3: 700 <--> 1204 mV at 900 mV at 900 mA 
<6>[000002699ms] PMIC_HI6559_BUCK4: 1200 <--> 1575 mV at 1225 mV at 1225 mA 
<6>[000002699ms] PMIC_HI6559_BUCK5: 1500 <--> 3300 mV at 2200 mV at 2200 mA 
<6>[000002699ms] PMIC_HI6559_BUCK6: 1800 <--> 2175 mV at 1800 mV at 1800 mA 
<6>[000002700ms] PMIC_HI6559_LDO01: 1800 <--> 3000 mV at 2500 mV at 2500 mA 
<6>[000002700ms] PMIC_HI6559_LDO03: 825 <--> 1000 mV at 900 mV at 900 mA 
<6>[000002700ms] PMIC_HI6559_LDO06: 1500 <--> 2800 mV at 2800 mV at 2800 mA 
<6>[000002700ms] PMIC_HI6559_LDO07: 1800 <--> 3300 mV at 2850 mV at 2850 mA 
<6>[000002700ms] PMIC_HI6559_LDO08: 1100 <--> 1375 mV at 1300 mV at 1300 mA 
<6>[000002700ms] PMIC_HI6559_LDO09: 1800 <--> 3050 mV at 1800 mV at 1800 mA 
<6>[000002701ms] PMIC_HI6559_LDO10: 2800 <--> 3300 mV at 2800 mV at 2800 mA 
<6>[000002701ms] PMIC_HI6559_LDO11: 1800 <--> 3300 mV at 3300 mV at 3300 mA 
<6>[000002701ms] PMIC_HI6559_LDO12: 3000 <--> 3350 mV at 3300 mV at 3300 mA 
<6>[000002701ms] PMIC_HI6559_LDO13: 1800 <--> 3000 mV at 2850 mV at 2850 mA 
<6>[000002701ms] PMIC_HI6559_LDO14: 1800 <--> 3000 mV at 2850 mV at 2850 mA 
<6>[000002702ms] PMIC_HI6559_LDO22: 1200 <--> 1500 mV at 1200 mV at 1200 mA 
<6>[000002702ms] PMIC_HI6559_LDO23: 1500 <--> 2850 mV at 1800 mV at 1800 mA 
<6>[000002702ms] PMIC_HI6559_LDO24: 2800 <--> 3150 mV at 3000 mV at 3000 mA 
<6>[000002702ms] PMIC_HI6559_LVS07: 1800 mV at 1800 mA 
<6>[000002702ms] PMIC_HI6559_LVS09: 1800 mV at 1800 mA 
<4>[000002702ms] [regulator]: <balong_regulator_probe> <972>hi6559 regulator register ok
<6>[000002703ms] PMIC_HI6559_DR01: 3 <--> 24 mV at 3 mV 3 <--> 24 mA at 3 mA 
<6>[000002703ms] PMIC_HI6559_DR02: 3 <--> 24 mV at 3 mV 3 <--> 24 mA at 3 mA 
<6>[000002703ms] PMIC_HI6559_DR03: 1 <--> 4 mV at 1 mV 1 <--> 45 mA at 1 mA 
<6>[000002703ms] PMIC_HI6559_DR04: 1 <--> 4 mV at 1 mV 1 <--> 45 mA at 1 mA 
<6>[000002703ms] PMIC_HI6559_DR05: 1 <--> 4 mV at 1 mV 1 <--> 45 mA at 1 mA 
<4>[000002704ms] [regulator]: <dummy_get_voltage> <112>dummy_get_voltage id:9999 
<4>[000002704ms] [regulator]: <dummy_get_voltage> <112>dummy_get_voltage id:9999 
<6>[000002704ms] common_for_useless: 1 <--> 9000 mV 1 <--> 45 mA 
<4>[000002704ms] [regulator]: <dummy_get_voltage> <112>dummy_get_voltage id:9999 
<4>[000002704ms] [regulator]: <balong_regulator_probe> <982>hi6559 dr regulator register ok
<5>[000002704ms] SCSI subsystem initialized
<4>[000002705ms] [gpio]:  gpio init in acore.
<6>[000002705ms] gpiochip_add: registered GPIOs 0 to 31 on device: balongv7r2
<6>[000002705ms] gpiochip_add: registered GPIOs 32 to 63 on device: balongv7r2
<6>[000002705ms] gpiochip_add: registered GPIOs 64 to 95 on device: balongv7r2
<6>[000002705ms] gpiochip_add: registered GPIOs 96 to 127 on device: balongv7r2
<4>[000002705ms] [gpio]: gpiochip_add over.
<4>[000002705ms] [gpio]:  gpio init over.
<6>[000002706ms] gpiochip_add: registered GPIOs 128 to 143 on device: tca6416
<6>[000002707ms] gpiochip_add: registered GPIOs 144 to 159 on device: tca6416
<4>[000002707ms] [gpio_ex]: gpio ex init ok.
<4>[000002707ms] [pmu]: <hi6559_irq_probe> hi6559_irq_probe ok !
<6>[000002708ms] usbcore: registered new interface driver usbfs
<6>[000002708ms] usbcore: registered new interface driver hub
<6>[000002708ms] usbcore: registered new device driver usb
<6>[000002709ms] Switching to clocksource balong clk cs
<6>[000002740ms] bq27510-battery 0-0055: Normal Mode and read Firmware version=1146
<6>[000002740ms] bq27510-battery 0-0055: bq27510 support ver. 1.0.0 enabled
<4>[000002740ms] i2c-core: driver [bq27510-battery] using legacy suspend method
<4>[000002740ms] i2c-core: driver [bq27510-battery] using legacy resume method
<6>[000002740ms] NET: Registered protocol family 2
<6>[000002741ms] IP route cache hash table entries: 1024 (order: 0, 4096 bytes)
<6>[000002741ms] TCP established hash table entries: 2048 (order: 2, 16384 bytes)
<6>[000002741ms] TCP bind hash table entries: 2048 (order: 1, 8192 bytes)
<6>[000002741ms] TCP: Hash tables configured (established 2048 bind 2048)
<6>[000002741ms] TCP: reno registered
<6>[000002741ms] UDP hash table entries: 256 (order: 0, 4096 bytes)
<6>[000002741ms] UDP-Lite hash table entries: 256 (order: 0, 4096 bytes)
<6>[000002742ms] NET: Registered protocol family 1
<6>[000002742ms] Trying to unpack rootfs image as initramfs...
<6>[000002753ms] Freeing initrd memory: 116K
<6>[000002754ms] cpuidle: using governor ladder
<4>[000002754ms] Enter ecall init
<4>[000002754ms] Finish ecall init
<4>[000002754ms] [Lowpower_mntn]: <bsp_lowpower_mntn_init_acore> NV_ID_DRV_DUMP:D111 read success!
<4>[000002755ms] perf_watchpoint_debugfs_init ok
<6>[000002762ms] jffs2: version 2.2. (NAND) (SUMMARY)  © 2001-2006 Red Hat, Inc.
<6>[000002762ms] fuse init (API version 7.18)
<7>[000002763ms] yaffs: yaffs built Aug 13 2016 18:36:39 Installing.
<6>[000002763ms] msgmni has been set to 81
<6>[000002764ms] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 253)
<6>[000002764ms] io scheduler noop registered
<6>[000002764ms] io scheduler deadline registered
<6>[000002764ms] io scheduler cfq registered (default)
<7>[000002765ms] Registered led device: lcd-backlight
<3>[000002765ms] spp:spi_init
<6>[000002765ms] PS:spi_clk_enable
<4>[000002775ms] gpio_request :2-08.
<6>[000002781ms] brd: module loaded
<6>[000002784ms] loop: module loaded
<4>[000002784ms] Hisilicon Nand Flash Controller Driver, Version 1.00
<4>[000002784ms] Hisilicon NANDC_V6.00 initialize...
<4>[000002785ms] ecctype_onfi 4,writesize 800,oobsize 40,erasesize 20000,chipsize 8000000 spec_shmem->ecc_type 4
<6>[000002785ms] NAND device: Manufacturer ID: 0x01, Chip ID: 0xa1 (AMD/Spansion (null))
<4>[000002785ms] NAND_ECC_NONE selected by board driver. This is not recommended!
<5>[000002785ms] Creating 32 MTD partitions on "NANDC_V6.00":
<5>[000002785ms] 0x000000000000-0x000000040000 : "m3boot"
<5>[000002787ms] 0x000000040000-0x000000100000 : "fastboot"
<5>[000002790ms] 0x000000100000-0x000000280000 : "nvbacklte"
<5>[000002796ms] 0x000000280000-0x000000400000 : "nvdefault"
<5>[000002802ms] 0x000000400000-0x000000800000 : "nvimg"
<5>[000002817ms] 0x000000800000-0x000000b00000 : "nvdload"
<5>[000002828ms] 0x000000b00000-0x000000c40000 : "oeminfo"
<5>[000002833ms] 0x000000c40000-0x0000012c0000 : "kernel"
<5>[000002855ms] 0x0000012c0000-0x000001940000 : "kernelbk"
<5>[000002878ms] 0x000001940000-0x0000019c0000 : "m3image"
<5>[000002881ms] 0x0000019c0000-0x000001d00000 : "dsp"
<5>[000002893ms] 0x000001d00000-0x000002700000 : "vxworks"
<5>[000002927ms] 0x000002700000-0x000002800000 : "wbdata"
<5>[000002932ms] 0x000002800000-0x000002c00000 : "om"
<7>[000002932ms] [*DLOAD_MTD*] fixed_fs_partitions:760: Partition om position fixed, Offset:2800000 Size:0x400000
<7>[000002932ms] 
<5>[000002946ms] 0x000002c00000-0x000003100000 : "app"
<7>[000002947ms] [*DLOAD_MTD*] fixed_fs_partitions:760: Partition app position fixed, Offset:2c00000 Size:0x500000
<7>[000002947ms] 
<5>[000002965ms] 0x000003100000-0x000003900000 : "webui"
<7>[000002965ms] [*DLOAD_MTD*] fixed_fs_partitions:760: Partition webui position fixed, Offset:3100000 Size:0x800000
<7>[000002965ms] 
<5>[000002993ms] 0x000003900000-0x000004800000 : "system"
<7>[000002994ms] [*DLOAD_MTD*] fixed_fs_partitions:760: Partition system position fixed, Offset:3900000 Size:0xf00000
<7>[000002994ms] 
<5>[000003045ms] 0x000004800000-0x000004c00000 : "userdata"
<7>[000003046ms] [*DLOAD_MTD*] fixed_fs_partitions:760: Partition userdata position fixed, Offset:4800000 Size:0x400000
<7>[000003046ms] 
<5>[000003060ms] 0x000004c00000-0x000007580000 : "online"
<7>[000003060ms] [*DLOAD_MTD*] fixed_fs_partitions:760: Partition online position fixed, Offset:4c00000 Size:0x2980000
<7>[000003060ms] 
<5>[000003201ms] 0x000007580000-0x000008000000 : "cdromiso"
<7>[000003202ms] [*DLOAD_MTD*] fixed_fs_partitions:760: Partition cdromiso position fixed, Offset:7580000 Size:0xa80000
<7>[000003202ms] 
<5>[000003238ms] 0x000000000000-0x000000000000 : "nullMTD"
<5>[000003239ms] 0x000000000000-0x000000000000 : "nullMTD"
<5>[000003240ms] 0x000000000000-0x000000000000 : "nullMTD"
<5>[000003241ms] 0x000000000000-0x000000000000 : "nullMTD"
<5>[000003242ms] 0x000000000000-0x000000000000 : "nullMTD"
<5>[000003242ms] 0x000000000000-0x000000000000 : "nullMTD"
<5>[000003243ms] 0x000000000000-0x000000000000 : "nullMTD"
<5>[000003244ms] 0x000000000000-0x000000000000 : "nullMTD"
<5>[000003245ms] 0x000000000000-0x000000000000 : "nullMTD"
<5>[000003246ms] 0x000000000000-0x000000000000 : "nullMTD"
<5>[000003247ms] 0x000000000000-0x000000000000 : "nullMTD"
<5>[000003247ms] 0x000000000000-0x000000000000 : "nullMTD"
<4>[000003248ms] nandc_mtd_dload_proc_deal start 
<4>[000003248ms] smem_data->smem_dload_flag = 0x72a11ef3!
<4>[000003248ms] nandc_mtd_dload_proc_deal end err = 0 
<4>[000003249ms] socp_init: succeed
<3>[000003249ms] start mount early partition
<7>[000003249ms] going to mount /dev/block/mtdblock13  mount point /modem_log/
<6>[000003249ms] yaffs: dev is 32505869 name is "mtdblock13" rw
<6>[000003249ms] yaffs: passed flags ""
<7>[000003249ms] yaffs: yaffs: Attempting MTD mount of 31.13,"mtdblock13"
<7>[000003317ms] yaffs: yaffs_read_super: is_checkpointed 0
<7>[000003317ms] going to mount /dev/block/mtdblock4  mount point /mnvm2:0/
<6>[000003317ms] yaffs: dev is 32505860 name is "mtdblock4" rw
<6>[000003318ms] yaffs: passed flags ""
<7>[000003318ms] yaffs: yaffs: Attempting MTD mount of 31.4,"mtdblock4"
<7>[000003319ms] yaffs: start ecc scan thread fn 
<7>[000003387ms] yaffs: yaffs_read_super: is_checkpointed 0
<4>[000003387ms] Balong nv init  start!
<7>[000003389ms] yaffs: start ecc scan thread fn 
<4>[000003409ms] load from /mnvm2:0/nv.bin
<4>[000003697ms] nvchar init end! major: 0xfc
<4>[000003697ms] Balong nv init ok!
<4>[000003698ms] smem_data->smem_online_upgrade_flag :0x1f70b1dd
<4>[000003698ms] smem_data->smem_multiupg_flag :0x9243f0a8
<4>[000003709ms] kernel_thread begin to  iRet =3 ++++++++++++
<4>[000003709ms]  bq27510_coul_firmware_update_init version =289800361 ++++++++++++
<4>[000003709ms] kernel_thread end to  iRet =3 ++++++++++++
<6>[000003709ms] hi6559_rtc0 hi6559_rtc0.0: rtc core: registered hi6559_rtc0 as rtc0
<4>[000003709ms] hi6559 RTC[0] init OK!
<6>[000003710ms] hi6559_rtc1 hi6559_rtc1.1: rtc core: registered hi6559_rtc1 as rtc1
<4>[000003710ms] hi6559 RTC[1] init OK!
<6>[000003710ms] hi6559_rtc2 hi6559_rtc2.2: rtc core: registered hi6559_rtc2 as rtc2
<4>[000003710ms] hi6559 RTC[2] init OK!
<6>[000003711ms] hi6559_rtc3 hi6559_rtc3.3: rtc core: registered hi6559_rtc3 as rtc3
<4>[000003711ms] hi6559 RTC[3] init OK!
<6>[000003711ms] hi6559_rtc4 hi6559_rtc4.4: rtc core: registered hi6559_rtc4 as rtc4
<4>[000003711ms] hi6559 RTC[4] init OK!
<6>[000003711ms] hi6559_rtc5 hi6559_rtc5.5: rtc core: registered hi6559_rtc5 as rtc5
<4>[000003711ms] hi6559 RTC[5] init OK!
<4>[000003712ms] [tem]: temperature init is ok.
<6>[000003712ms]  initialize thermal device.
<6>[000003712ms] Succeedded to initialize thermal device.
<4>[000003712ms] his_modem_load_vxworks:69: >>loading:vxworks.....
<4>[000004742ms] his_modem_load_vxworks:131: >>start to decompress vxworks image ...
<4>[000006357ms] his_modem_load_vxworks:156: >>load vxworks ok, entey 0x50d10000, length 0x846ef7
<4>[000006359ms] his_modem_probe:403: load ccore image succeed
<6>[000006542ms] succeed to load dsp image, address: 0x50b00000, size: 0x200000
<6>[000006575ms] succeed to load TD config data, address: 0x54ac0000, size: 0x40000
<4>[000006575ms] [version]: <bsp_productinfo_init> bsp version init OK!
<4>[000006575ms] [efuse]: efuse init ok.
<4>[000006575ms] [efuse]: efuse comm init ok.
<4>[000006575ms] [key]: v7r2 gpio key init!
<4>[000006576ms] [key]: v7r2 key driver probes start!
<6>[000006576ms] input: v7r2_gpio_key as /devices/platform/v7r2_gpio_key/input/input0
<4>[000006576ms] [key]: <gpio_keys_gpio_report_event> <298> menu key is release. 
<4>[000006576ms] [key]: <gpio_keys_gpio_report_event> <298> reset key is release. 
<4>[000006576ms] [key]: <report_power_key_up> <238> power key is release. 
<4>[000006576ms] [key]: v7r2 gpio key driver probes end!
<4>[000006576ms] [anten]:  anten init over.
<4>[000006576ms] [om]: <bsp_om_record_resetlog> system reboot reason: NORMAL POWER ON 
<4>[000006577ms] [om]: <bsp_om_fs_check> om fs is ready
<4>[000006577ms] [om]: <bsp_om_save_resetlog> save reset log:system reboot reason: NORMAL POWER ON 
<4>[000006577ms] 
<4>[000006581ms] [dump]: <dump_init_phase2> dump init success!
<4>[000006582ms] [om]: <bsp_om_server_init> bsp om init ok
<4>[000006582ms] [rfile]: <bsp_rfile_init> success.
<4>[000006582ms] ------special_timer wakelock init ok ----------!
<4>[000006582ms] ------special_timer misc register leave!
<4>[000006582ms] [mem]: <bsp_mem_init> memory init OK!
<3>[000006582ms] cshell cann't be init for security
<4>[000006582ms] A:logger_init start 
<6>[000006582ms] logger: created 64K log 'cshell_log'
<4>[000006583ms] [IPF]  ipf init success
<4>[000006589ms] [pmu]: <bsp_hi6559_exc_init> hi6559 exc init ok!
<4>[000006590ms] set eth wakelock timeout 180
<4>[000007599ms] AR8035 phy driver register
<4>[000007600ms] clk:gmac_aclk enable OK!!
<4>[000007600ms] clk:gmac_swclk enable OK!!
<4>[000007600ms] clk:gmac_gtx enable OK!!
<4>[000007600ms] clk:gmac_tx enable OK!!
<4>[000007600ms] clk:gmac_rx enable OK!!
<4>[000007600ms] Get ETH MacAddr:9C:B2:B2:DC:A7:64
<4>[000007720ms] AR8035 start phy reset PIN:140
<6>[000007720ms] stmmac: probed
<4>[000007720ms] AR8035 phy driver configinit
<6>[000007721ms] PPP generic driver version 2.4.2
<6>[000007721ms] PPP BSD Compression module registered
<6>[000007721ms] PPP Deflate Compression module registered
<6>[000007722ms] PPP MPPE Compression module registered
<6>[000007722ms] NET: Registered protocol family 24
<6>[000007722ms] SLIP: version 0.8.4-NET3.019-NEWTTY (dynamic channels, max=256).
<4>[000007722ms] fastip ver:2013-12-05 10:32 v1.0
<4>[000007722ms] fastip_module_init: fastip_kattach kfastip_handle:c0ad73f8
<4>[000007722ms] rmnet2 fastip init
<4>[000007722ms] rmnet2 fastip devname rmnet2
<4>[000007722ms] _fastip_attach: name:rmnet2 fastip handle:c306d3c0
<4>[000007722ms] 
<4>[000007722ms]  rmnet2_fastip_handle attach ok !!!!!! cih = 0xc306d3c0 
<4>[000007723ms] rmnet2 fastip register ok
<6>[000007723ms] bq24192 0-006b: chargeIC_probe: Begin:*******chargeIC_probe*********
<3>[000007723ms] bq24192 0-006b: chargeIC_probe: device tree information missing
<1>[000007724ms]  chargeIC_probe: ********creat proc filesystem********
<6>[000007731ms] read(0x6B)=0xFF
<6>[000007731ms] bq24192 0-006b: chargeIC_probe: chargeIC probed successfully, pn_rev=7, devreg_rev=3
<6>[000007731ms] bq24192 0-006b: chargeIC_probe: g_i2c_client->addr 107
<1>[000007731ms]  begin creat debugfs
<1>[000007734ms]  end creat debugfs den -1030596992 
<3>[000007738ms] [hisi coul]hisi_coul_init
<3>[000007746ms] huawei,bq_bci_battery huawei,bq_bci_battery: bq_bci probe ok!
<3>[000007750ms] huawei,bq_bci_battery huawei,bq_bci_battery: batt soc changed, new soc=77 
<4>[000008385ms] read calibrate value successs! max=4200,min=3400
<4>[000008394ms] CHG_PLT:chg_send_stat_to_app->deviceid 3, eventid 255 
<4>[000008394ms]  read calibrate value successs! max=4200,min=3400
<4>[000008822ms]  chg_task_create: Thread create success!!!
<4>[000008822ms]  
<6>[000008822ms] Initializing USB Mass Storage driver...
<6>[000008822ms] usbcore: registered new interface driver usb-storage
<6>[000008822ms] USB Mass Storage support registered.
<3>[000008822ms] U_ALL:(U_INFO)rndis_webapp_init():rndis_webapp_init success,ret = 0
<3>[000008822ms] U_NV:(U_TRACE)usb_nv_get():NV = 26, ret=0 nv_status=0 
<3>[000008822ms] U_NV:(U_TRACE)usb_nv_get():NV = 50108, ret=0 nv_status=0
<3>[000008822ms] U_NV:(U_TRACE)usb_nv_get():NV = 50109, ret=0 nv_status=0
<4>[000008822ms] 
<4>[000008822ms] [nv_readEx]:can not find 0xc3e7 !
<3>[000008822ms] U_NV:(U_TRACE)usb_nv_get():NV = 50498, ret=269484054 nv_status=0
<3>[000008822ms] U_NV:(U_TRACE)usb_nv_get():Winblue: profile nv val: Huawei Mobile, 0, 0, 1, 3, 1500, 1500
<4>[000008822ms] 
<4>[000008822ms] [nv_readEx]:can not find 0xc542 !
<3>[000008822ms] U_NV:(U_TRACE)usb_nv_get():NV = 50498, ret=269484054 nv_status=0
<3>[000008822ms] U_NV:(U_TRACE)usb_nv_get():NV = 26, ret=0 nv_status=0 
<3>[000008822ms] U_NV:(U_TRACE)usb_nv_get():NV = 50108, ret=0 nv_status=0
<3>[000008822ms] U_NV:(U_TRACE)usb_nv_get():NV = 50109, ret=0 nv_status=0
<4>[000008822ms] 
<4>[000008823ms] [nv_readEx]:can not find 0xc3e7 !
<3>[000008823ms] U_NV:(U_TRACE)usb_nv_get():NV = 50498, ret=269484054 nv_status=0
<3>[000008823ms] U_NV:(U_TRACE)usb_nv_get():Winblue: profile nv val: Huawei Mobile, 0, 0, 1, 3, 1500, 1500
<4>[000008823ms] 
<4>[000008823ms] [nv_readEx]:can not find 0xc542 !
<3>[000008823ms] U_NV:(U_TRACE)usb_nv_get():NV = 50498, ret=269484054 nv_status=0
<4>[000008823ms] CHG_TASK:chg_main_task->start_creart!!!
<3>[000008828ms] U_HOTPLUG:(U_TRACE)bsp_usb_status_change():status 1
<3>[000008828ms] U_HOTPLUG:(U_TRACE)bsp_usb_status_change():status 1
<3>[000008828ms] U_NET:(U_TRACE)usb_prealloc_eth_rx_mem():type:0->3, size:0->2048, num:0->412, ptr=  (null)
<3>[000008828ms] U_NET:(U_TRACE)usb_prealloc_eth_rx_mem():usb_prealloc_eth_rx_mem : allocmem num=412, size=2048
<4>[000008830ms] [wdt]: <hi6930_wdt_probe> <284>wdt init ok
<6>[000008830ms] cpufreq: balongv7r2 CPU frequency driver.
<6>[000008830ms] cpufreq: balong_cpufreq_cpu_init.
<4>[000008832ms] Hi DWC mmc probe ok
<4>[000008832ms] Hi DWC mmc0 probe ok
<3>[000008832ms] U_ALL:(U_INFO)usb_notify_syswatch():U_EVENT: usb_notify_syswatch<5,1>
<4>[000008834ms] Hi DWC mmc probe ok
<4>[000008834ms] Hi DWC mmc1 probe ok
<4>[000008834ms] mshci_wifi_GPIO_init:gpio_request wifi_gpio_addr fail!
<4>[000008834ms] mshci_wifi_power_off:enter!
<3>[000008834ms] ----ebul----[mshci_wifi_power_off:2108] buk3_flags =   (null), BUCK3_ONOFF_FLAG = f4e00278, buk3 from 1 to 0
<3>[000009019ms] U_HOTPLUG:(U_TRACE)usb_notify_handler():old_status 0,status1
<3>[000009019ms] U_HOTPLUG:(U_TRACE)usb_notify_handler():task of cur_status 0 status:1:start.
<3>[000009019ms] U_CHARGER:(U_ERROR)usb_charger_type_detect_event():usb_charger_type_detect_event -val: 1 ,charger_type:0
<3>[000009019ms] U_ALL:(U_INFO)usb_notify_syswatch():U_EVENT: usb_notify_syswatch<4,0>
<3>[000009020ms] U_PNP:(U_TRACE)usb_balong_init():entermshci_wifi_power_on:enter!
<3>[000009040ms] [MBB CHG]battery_monitor_blocking_notifier_call_chain :1 0.
<6>[000009040ms] CHG_DEBUG: wake lock timeout is 6s!
<3>[000009040ms] ----ebul----[mshci_wifi_power_on:2048] buk3_flags = 00000002, BUCK3_ONOFF_FLAG = f4e00278, buk3 from 0 to 1
<3>[000009040ms] 
<3>[000009040ms]  [Mbb Common Drv] Mbb_Common_Probe!
<6>[000009040ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(28),read len(124),len(124),lv=(8),msg: SCI_EVENT_SCI_INIT_SUCCESS
<6>[000009040ms] .
<4>[000009040ms] bsp_sci_init gpio_request failed! 
<3>[000009040ms] Wi-Fi<INFO>[wifi_netlink_chunnel_init:1238]: enter
<3>[000009040ms] Wi-Fi<INFO>[wifi_netlink_chunnel_init:1260]: exit
<3>[000009040ms] Wi-Fi<INFO>[wlan_reg_driver_lock:1456]: Exit, wifi driver lock Register
<3>[000009040ms] Wi-Fi<INFO>[wlan_stus_timer_start:476]: wlan_stus_timer_started!!!!
<3>[000009040ms] Wi-Fi<INFO>[wlan_at_init_rtl_def:2226]: enter
<3>[000009040ms] Wi-Fi<INFO>[wlan_at_reg_chip:771]: chip 8 = (rtl8192) reg   (null) to c0884b40
<3>[000009040ms] Wi-Fi<INFO>[wlan_at_reg_chip:777]: Exit, g_cur_chip= 8
<3>[000009040ms] 
<3>[000009040ms] Wi-Fi<INFO>[wlan_at_init_rtl_def:2232]: exit
<3>[000009040ms] Wi-Fi<INFO>[wlan_wt_init:810]: enter curr_chip 8 = (rtl8192)
<3>[000009040ms] Wi-Fi<INFO>[wlan_wt_init:816]: chip 8 = (rtl8192) reg to c0884b40
<3>[000009041ms] Wi-Fi<INFO>[wlan_wt_init:820]: exit
<3>[000009041ms] init stat time proc_mlog_log_init 389 
<7>[000009041ms] [*DLOAD_NARK_API*] nark_api_init:749: nark api module init.
<3>[000009041ms] 
<3>[000009041ms]  [HARDWARE TEST] init...
<6>[000009041ms] oprofile: using arm/armv7-ca9
<6>[000009041ms] u32 classifier
<6>[000009041ms]     Performance counters on
<6>[000009041ms] Netfilter messages via NETLINK v0.30.
<6>[000009041ms] nf_conntrack version 0.5.0 (648 buckets, 2592 max)
<6>[000009042ms] ctnetlink v0.93: registering with nfnetlink.
<4>[000009042ms] nf_conntrack_rtsp v0.6.21 loading
<4>[000009042ms] nf_nat_http_init <*********** start ************>
<7>[000009042ms]  [/home/jwx384541/E5770s-923_c778/vendor/hisi/modem/system/android/android_4.2_r1/kernel/net/netfilter/proc.c] [273] [atp_proc_init] /proc/app_proc NOT exist !
<7>[000009042ms] 
<7>[000009042ms]  [/home/jwx384541/E5770s-923_c778/vendor/hisi/modem/system/android/android_4.2_r1/kernel/net/netfilter/proc.c] [234] [atp_proc_create_prsite] /proc/app_proc/prsite NOT exist !!!
<7>[000009042ms] 
<7>[000009042ms]  [/home/jwx384541/E5770s-923_c778/vendor/hisi/modem/system/android/android_4.2_r1/kernel/net/netfilter/proc.c] [76] [atp_proc_create_file] will create file: rand
<6>[000009043ms] IPVS: Registered protocols ()
<6>[000009043ms] IPVS: Connection hash table configured (size=4096, memory=32Kbytes)
<6>[000009043ms] IPVS: Creating netns size=808 id=0
<6>[000009043ms] IPVS: ipvs loaded.
<4>[000009043ms] nf_nat_rtsp v0.6.21 loading
<6>[000009043ms] ip_tables: (C) 2000-2006 Netfilter Core Team
<6>[000009044ms] arp_tables: (C) 2002 David S. Miller
<6>[000009044ms] TCP: cubic registered
<6>[000009045ms] NET: Registered protocol family 10
<6>[000009046ms] ip6_tables: (C) 2000-2006 Netfilter Core Team
<6>[000009046ms] NET: Registered protocol family 17
<5>[000009046ms] Bridge firewalling registered
<6>[000009046ms] Ebtables v2.0 registered
<6>[000009047ms] L2TP core driver, V2.0
<6>[000009047ms] PPPoL2TP kernel driver, V2.0
<6>[000009047ms] VFP support v0.3: implementor 41 architecture 3 part 30 variant 9 rev 4
<4>[000009047ms] REB_DFT:reb_init exec...
<4>[000009047ms] Reb_DFT thread create success!
<4>[000009048ms]  INIT REB TEST MOUDLE !
<4>[000009048ms] [regulator]: <dummy_is_enabled> <117>dummy_is_enabled id:9999 
<6>[000009048ms] PMIC_HI6559_LVS09: incomplete constraints, leaving on
<6>[000009048ms] PMIC_HI6559_LDO24: incomplete constraints, leaving on
<6>[000009048ms] PMIC_HI6559_LDO22: incomplete constraints, leaving on
<6>[000009048ms] PMIC_HI6559_LDO14: incomplete constraints, leaving on
<6>[000009048ms] PMIC_HI6559_LDO12: incomplete constraints, leaving on
<6>[000009048ms] PMIC_HI6559_LDO11: incomplete constraints, leaving on
<6>[000009048ms] PMIC_HI6559_LDO08: incomplete constraints, leaving on
<6>[000009048ms] PMIC_HI6559_LDO07: incomplete constraints, leaving on
<6>[000009048ms] PMIC_HI6559_LDO03: incomplete constraints, leaving on
<6>[000009048ms] PMIC_HI6559_LDO01: incomplete constraints, leaving on
<6>[000009048ms] PMIC_HI6559_BUCK6: incomplete constraints, leaving on
<6>[000009048ms] PMIC_HI6559_BUCK4: incomplete constraints, leaving on
<6>[000009048ms] PMIC_HI6559_BUCK3: incomplete constraints, leaving on
<6>[000009048ms] V711_MTCMOS12: incomplete constraints, leaving on
<6>[000009048ms] V711_MTCMOS10: incomplete constraints, leaving on
<7>[000009048ms] his_boot_init.
<4>[000009048ms] #########  power_on_reboot_flag_set = 0xFFFFFFFF ######## 
<4>[000009048ms] #########  power_on_start_reason_get = 0x504F504B ######## 
<4>[000009048ms] system power on time:  70-00-01 00:00:06
<3>[000009050ms] [MBB CHG]charge_event_work :1 0.
<6>[000009050ms] efuse read start group 4 length 4.
<6>[000009050ms] efuse read end group 4 length 4.
<6>[000009050ms] efuse buf[0] is 0x0.
<6>[000009050ms] efuse buf[1] is 0x0.
<6>[000009050ms] efuse buf[2] is 0x0.
<6>[000009050ms] efuse buf[3] is 0x0.
<6>[000009050ms] efuse read ret 0
<7>[000009051ms] power on log save.
<7>[000009051ms]  
<4>[000009052ms] !!!!! VOS_Startup Begin !!!!!
<4>[000009058ms] 
<4>[000009058ms] OM_AcpuSelfTaskReg: Reg the OMPrintf Task[reset]: <ccorereset_regcbfunc> is stub
<4>[000009058ms] [reset]: <ccorereset_regcbfunc> is stub
<4>[000009058ms] TTF_MEMCTRL_AddrInit::Addrs were already initialized!
<4>[000009058ms] TTF_MEMCTRL_AddrInit::Addrs were already initialized!
<4>[000009058ms] TTF_MEMCTRL_AddrInit::Addrs were already initialized!
<4>[000009058ms] TTF_MEMCTRL_AddrInit::Addrs were already initialized!
<4>[000009058ms] TTF_MEMCTRL_AddrInit::Addrs were already initialized!
<4>[000009058ms] TTF_MEMCTRL_AddrInit::Addrs were already initialized!
<4>[000009058ms] TTF_MEMCTRL_AddrInit::Addrs were already initialized!
<4>[000009058ms] TTF_MEMCTRL_AddrInit::Addrs were already initialized!
<4>[000009058ms] TTF_MEMCTRL_AddrInit::Addrs were already initialized!
<4>[000009058ms] TTF_MEMCTRL_AddrInit::Addrs were already initialized!
<4>[000009058ms] TTF_MEMCTRL_AddrInit::Addrs were already initialized!
<4>[000009058ms] TTF_MEMCTRL_AddrInit::Addrs were already initialized!
<6>[000009059ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(27),read len(124),len(124),lv=(8),msg: SCI_EVENT_API_RESET_START
<6>[000009059ms] .
<6>[000009059ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(26),read len(124),len(124),lv=(8),msg: SCI_EVENT_LOW_POWER_EXIT
<6>[000009059ms] .
<6>[000009059ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(24),read len(124),len(124),lv=(8),msg: SCI_EVENT_REGULATOR_UP
<6>[000009059ms] .
<6>[000009061ms] efuse read start group 4 length 4.
<6>[000009061ms] efuse read end group 4 length 4.
<6>[000009061ms] efuse buf[0] is 0x0.
<6>[000009061ms] efuse buf[1] is 0x0.
<6>[000009061ms] efuse buf[2] is 0x0.
<6>[000009061ms] efuse buf[3] is 0x0.
<6>[000009061ms] efuse read ret 0
<4>[000009067ms] mmc0: card claims to support voltages below the defined range. These will be ignored.
<4>[000009068ms] 
<4>[000009068ms] OM_CreateTraceBuffer: real addr=0x57300000, virt addr==0xffd00000
<4>[000009069ms] [reset]: <ccorereset_regcbfunc> is stub
<4>[000009069ms] [reset]: <ccorereset_regcbfunc> is stub
<4>[000009069ms] [reset]: <ccorereset_regcbfunc> is stub
<4>[000009070ms] [reset]: <ccorereset_regcbfunc> is stub
<4>[000009070ms] [reset]: <ccorereset_regcbfunc> is stub
<4>[000009070ms] diag_CreateLogBuf: real addr=0x57f80000, virt addr==0xc3980000
<4>[000009070ms] diag_CreateLogBuf: real addr=0x57f90000, virt addr==0xc3990000
<4>[000009071ms] 
<4>[000009071ms] !!!!! VOS_Startup End !!!!!
<4>[000009073ms] mmc0: host->ocr= 0x010C0000, ocr = 0x91FC00FF.
<6>[000009074ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(46),read len(124),len(124),lv=(8),msg: SCI_EVENT_CARD_ACTIVE_START. eCurrentState=4
<6>[000009074ms] .
<6>[000009074ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(48),read len(124),len(124),lv=(8),msg: SCI_EVENT_REGISTER_COLD_RESET. eCurrentState=4
<6>[000009074ms] .
<6>[000009074ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(48),read len(124),len(124),lv=(8),msg: SCI_EVENT_CARD_ACTIVE_SUCCESS. eCurrentState=4
<6>[000009074ms] .
<6>[000009074ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(14),read len(124),len(124),lv=(2),msg: SIM_CARD_OUT
<6>[000009074ms] .
<6>[000009074ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(47),read len(124),len(124),lv=(8),msg: SCI_EVENT_API_RESET_FINISH. eCurrentState = 4
<6>[000009074ms] .
<6>[000009074ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(43),read len(124),len(124),lv=(8),msg: SCI_EVENT_API_GET_STATUS. eCurrentState=4
<6>[000009074ms] .
<6>[000009080ms] hi6559_rtc0 hi6559_rtc0.0: setting system clock to 1970-01-01 00:00:10 UTC (10)
<6>[000009081ms] Freeing init memory: 176K
<6>[000009086ms] mmc0: new ultra high speed SDR50 SDIO card at address 0001
<6>[000009094ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(43),read len(124),len(124),lv=(8),msg: SCI_EVENT_API_GET_STATUS. eCurrentState=4
<6>[000009094ms] .
<6>[000009108ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(41),read len(124),len(124),lv=(8),msg: SCI_EVENT_INTR_CARD_UP. eCurrentState=4
<6>[000009108ms] .
<6>[000009115ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(43),read len(124),len(124),lv=(8),msg: SCI_EVENT_API_GET_STATUS. eCurrentState=5
<6>[000009115ms] .
<6>[000009119ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(46),read len(124),len(124),lv=(8),msg: bsPL131_REGINTMASK_ATRSTOUT. eCurrentState=5
<6>[000009119ms] .
<6>[000009119ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(43),read len(124),len(124),lv=(8),msg: SCI_EVENT_INTR_CARD_DOWN. eCurrentState=4
<6>[000009119ms] .
<6>[000009119ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(26),read len(124),len(124),lv=(8),msg: SCI_EVENT_REGULATOR_DOWN
<6>[000009119ms] .
<6>[000009134ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(29),read len(124),len(124),lv=(8),msg: SCI_EVENT_VOLTAGE_CLASS_C2B
<6>[000009134ms] .
<6>[000009134ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(24),read len(124),len(124),lv=(8),msg: SCI_EVENT_REGULATOR_UP
<6>[000009134ms] .
<6>[000009135ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(43),read len(124),len(124),lv=(8),msg: SCI_EVENT_API_GET_STATUS. eCurrentState=4
<6>[000009135ms] .
<6>[000009150ms] mmc_attach_sd:in
<6>[000009154ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(46),read len(124),len(124),lv=(8),msg: SCI_EVENT_CARD_ACTIVE_START. eCurrentState=4
<6>[000009154ms] .
<6>[000009154ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(48),read len(124),len(124),lv=(8),msg: SCI_EVENT_REGISTER_COLD_RESET. eCurrentState=4
<6>[000009154ms] .
<6>[000009154ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(48),read len(124),len(124),lv=(8),msg: SCI_EVENT_CARD_ACTIVE_SUCCESS. eCurrentState=4
<6>[000009154ms] .
<6>[000009155ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(43),read len(124),len(124),lv=(8),msg: SCI_EVENT_API_GET_STATUS. eCurrentState=4
<6>[000009155ms] .
<6>[000009175ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(43),read len(124),len(124),lv=(8),msg: SCI_EVENT_API_GET_STATUS. eCurrentState=4
<6>[000009175ms] .
<6>[000009188ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(41),read len(124),len(124),lv=(8),msg: SCI_EVENT_INTR_CARD_UP. eCurrentState=4
<6>[000009188ms] .
<6>[000009195ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(43),read len(124),len(124),lv=(8),msg: SCI_EVENT_API_GET_STATUS. eCurrentState=5
<6>[000009195ms] .
<6>[000009199ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(46),read len(124),len(124),lv=(8),msg: bsPL131_REGINTMASK_ATRSTOUT. eCurrentState=5
<6>[000009199ms] .
<6>[000009199ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(43),read len(124),len(124),lv=(8),msg: SCI_EVENT_INTR_CARD_DOWN. eCurrentState=5
<6>[000009199ms] .
<6>[000009199ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(26),read len(124),len(124),lv=(8),msg: SCI_EVENT_REGULATOR_DOWN
<6>[000009199ms] .
<6>[000009208ms] mmc1: new high speed SDHC card at address 0001
<6>[000009210ms] mmcblk0: mmc1:0001 ASTC 3.72 GiB 
<6>[000009211ms]  mmcblk0: p1
<3>[000009212ms] U_ALL:(U_INFO)usb_notify_syswatch():U_EVENT: usb_notify_syswatch<5,0>
<3>[000009212ms] U_MASS:(U_TRACE)mass_storage_set_sd_card_status():sd_card attach usb can open sd
<6>[000009212ms] ============= mmc_attach_sd ========= 
<6>[000009215ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(43),read len(124),len(124),lv=(8),msg: SCI_EVENT_API_GET_STATUS. eCurrentState=3
<6>[000009215ms] .
<6>[000009262ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(47),read len(124),len(124),lv=(2),msg: USIMM_InitCardTypeByATR: Reset Card is Failed
<6>[000009262ms] .
<6>[000009262ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(47),read len(124),len(124),lv=(2),msg: USIMM_InitCard: USIMM_InitCardFirstStep Error
<6>[000009262ms] .
<3>[000009263ms] [MDOEM:0][TICK:256][TAF_MMA_SndMmcStartReq][LINE:144] Send Msg!
<4>[000009264ms] Reg PCSC Func.
<4>[000009264ms] Update Card Status: 0 .
<6>[000009265ms] efuse read start group 4 length 4.
<6>[000009265ms] efuse read end group 4 length 4.
<6>[000009265ms] efuse buf[0] is 0x0.
<6>[000009265ms] efuse buf[1] is 0x0.
<6>[000009267ms] efuse buf[2] is 0x0.
<6>[000009267ms] efuse buf[3] is 0x0.
<6>[000009267ms] efuse read ret 0
<6>[000009270ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(38),read len(124),len(124),lv=(2),msg: SCI_EVENT_CLK_ERROR. eCurrentState=3
<6>[000009270ms] .
<6>[000009270ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(38),read len(124),len(124),lv=(2),msg: SCI_EVENT_CLK_ERROR. eCurrentState=3
<6>[000009270ms] .
<6>[000009270ms] [Mbb Common Drv] module=(UICC),mlogbuf.len =(38),read len(124),len(124),lv=(2),msg: SCI_EVENT_CLK_ERROR. eCurrentState=3
<6>[000009270ms] .
<3>[000009270ms] [MDOEM:0][TICK:257][NAS_MMC_SndRatModeSwitchOnReq_SwitchOn][LINE:2791] Send start req to GAS!
<6>[000009275ms] efuse read start group 4 length 4.
<6>[000009275ms] efuse read end group 4 length 4.
<6>[000009275ms] efuse buf[0] is 0x0.
<6>[000009275ms] efuse buf[1] is 0x0.
<6>[000009275ms] efuse buf[2] is 0x0.
<6>[000009275ms] efuse buf[3] is 0x0.
<6>[000009275ms] efuse read ret 0
<3>[000009281ms] [MDOEM:0][TICK:258][NAS_MMC_RcvGasStartCnf_SwitchOn_WaitGasStartCnf][LINE:917] ulResult = 0
<3>[000009281ms] [MDOEM:0][TICK:258][NAS_MMC_SndRatModeSwitchOnReq_SwitchOn][LINE:2761] Send start req to LTE!
<6>[000009283ms] efuse read start group 4 length 4.
<6>[000009283ms] efuse read end group 4 length 4.
<6>[000009283ms] efuse buf[0] is 0x0.
<6>[000009283ms] efuse buf[1] is 0x0.
<6>[000009283ms] efuse buf[2] is 0x0.
<6>[000009283ms] efuse buf[3] is 0x0.
<6>[000009283ms] efuse read ret 0
<3>[000009426ms] [MDOEM:0][TICK:273][NAS_MMC_RcvLmmStartCnf_SwitchOn_WaitLStartCnf][LINE:1290] ulResult = 0
<3>[000009426ms] [MDOEM:0][TICK:273][NAS_MMC_SndRatModeSwitchOnReq_SwitchOn][LINE:2777] Send start req to WRRC!
<6>[000009433ms] efuse read start group 4 length 4.
<6>[000009433ms] efuse read end group 4 length 4.
<6>[000009433ms] efuse buf[0] is 0x0.
<6>[000009433ms] efuse buf[1] is 0x0.
<6>[000009433ms] efuse buf[2] is 0x0.
<6>[000009433ms] efuse buf[3] is 0x0.
<6>[000009433ms] efuse read ret 0
<3>[000009434ms] [MDOEM:0][TICK:274][NAS_MMC_RcvWasStartCnf_SwitchOn_WaitWasStartCnf][LINE:1055] FDD ulResult = 0
<3>[000009435ms] [MDOEM:0][TICK:274][NAS_Mmc_SndMmaStartCnf][LINE:1636] Send Msg!
<4>[000009435ms] bsp_power_ctrl_read_cb 0x0
<6>[000009437ms] [Mbb Common Drv] module=(MMC),mlogbuf.len =(57),read len(124),len(124),lv=(2),msg: the rat is 2!,the search type is MMC_LMM_PLMN_SRCH_ANY!
<6>[000009437ms] .
<6>[000009678ms] [Mbb Common Drv] module=(MMC),mlogbuf.len =(66),read len(124),len(124),lv=(2),msg: the fast search cnf type is RRC_PLMN_SEARCH_RLT_SPEC,rat is lte!
<6>[000009678ms] .
<4>[000010186ms] CHG_PLT:chg_send_stat_to_app->deviceid 3, eventid 255 
<4>[000010186ms]  CHG_TASK:chg_main_task->charger_input!!!
<4>[000010270ms]  CHG_PLT:chg_send_stat_to_app->deviceid 4, eventid 255 
<4>[000010315ms]  CHG_STM:set_cur_chg_mode=0
<4>[000010315ms] CHG_PLT: wired charger but chg type unknow force to TRANSIT_ST!
<4>[000010315ms]  
<3>[000010686ms] 
<3>[000010686ms]  [HARDWARE TEST] get mode: mode=0, option = -1158739328!
<3>[000010686ms] 
<3>[000010686ms]  [HARDWARE TEST] mode=0
<3>[000010686ms] init: /init.rc: 118: invalid command 'if'
<3>[000010686ms] init: /init.rc: 120: invalid command 'fi'
<3>[000010840ms] init: /dev/hw_random not found
<3>[000010841ms] init: cannot open '/initlogo.rle'
<5>[000010957ms] jffs2: notice: (1) jffs2_build_xattr_subsystem: complete building xattr subsystem, 0 of xdatum (0 unchecked, 0 orphan) and 0 of xref (0 dead, 0 orphan) found.
<6>[000010960ms] yaffs: dev is 32505873 name is "mtdblock17" rw
<6>[000010960ms] yaffs: passed flags ""
<7>[000010960ms] yaffs: yaffs: Attempting MTD mount of 31.17,"mtdblock17"
<7>[000011025ms] yaffs: start ecc scan thread fn 
<7>[000011025ms] yaffs: yaffs_read_super: is_checkpointed 0
<5>[000011099ms] jffs2: notice: (1) jffs2_build_xattr_subsystem: complete building xattr subsystem, 0 of xdatum (0 unchecked, 0 orphan) and 0 of xref (0 dead, 0 orphan) found.
<5>[000011311ms] jffs2: notice: (1) jffs2_build_xattr_subsystem: complete building xattr subsystem, 0 of xdatum (0 unchecked, 0 orphan) and 0 of xref (0 dead, 0 orphan) found.
<6>[000011314ms] yaffs: dev is 32505874 name is "mtdblock18" rw
<6>[000011314ms] yaffs: passed flags ""
<7>[000011314ms] yaffs: yaffs: Attempting MTD mount of 31.18,"mtdblock18"
<7>[000011319ms] yaffs: yaffs_read_super: is_checkpointed 1
<7>[000011320ms] yaffs: start ecc scan thread fn 
<3>[000011530ms] init: /dev/hw_random not found
<3>[000011540ms] init: skipping insecure file '/system/build.prop'
<6>[000011545ms] lcd_suspend_early
<7>[000011681ms] udc dwc3: registering UDC driver [android_usb]
<3>[000011686ms] U_ACM:(U_ERROR)acm_function_init():acm_function_init has been init
<3>[000011686ms] U_ACM:(U_ERROR)acm_function_init():acm_function_init has been init
<3>[000011686ms] U_ACM:(U_ERROR)acm_function_init():acm_function_init has been init
<3>[000011686ms] U_ACM:(U_ERROR)acm_function_init():acm_function_init has been init
<3>[000011686ms] U_ACM:(U_ERROR)acm_function_init():acm_function_init has been init
<3>[000011686ms] U_ACM:(U_ERROR)acm_function_init():acm_function_init has been init
<3>[000011687ms] U_ACM:(U_ERROR)acm_function_init():acm_function_init has been init
<3>[000011687ms] U_ACM:(U_ERROR)acm_function_init():acm_function_init has been init
<3>[000011687ms] U_ACM:(U_ERROR)acm_function_init():acm_function_init has been init
<3>[000011687ms] U_ACM:(U_ERROR)acm_function_init():acm_function_init has been init
<3>[000011687ms] U_ACM:(U_ERROR)acm_function_init():acm_function_init has been init
<3>[000011687ms] U_PNP:(U_ERROR)composite_bind():android_usb ready
<3>[000011688ms] U_NV:(U_TRACE)usb_nv_get():NV = 26, ret=0 nv_status=0 
<3>[000011688ms] U_NV:(U_TRACE)usb_nv_get():NV = 50108, ret=0 nv_status=0
<3>[000011688ms] U_NV:(U_TRACE)usb_nv_get():NV = 50109, ret=0 nv_status=0
<4>[000011688ms] 
<4>[000011688ms] [nv_readEx]:can not find 0xc3e7 !
<3>[000011688ms] U_NV:(U_TRACE)usb_nv_get():NV = 50498, ret=269484054 nv_status=0
<3>[000011688ms] U_NV:(U_TRACE)usb_nv_get():Winblue: profile nv val: Huawei Mobile, 0, 0, 1, 3, 1500, 1500
<4>[000011688ms] 
<4>[000011688ms] [nv_readEx]:can not find 0xc542 !
<3>[000011688ms] U_NV:(U_TRACE)usb_nv_get():NV = 50498, ret=269484054 nv_status=0
<6>[000011688ms] [*DLOAD_NARK_CORE*] dload_report_port_status:373: Info: port mode is 0
<3>[000011688ms] U_PNP:(U_TRACE)pnp_status_rewind_before(): COMPLETE
<3>[000011688ms] U_CHARGER:(U_ERROR)usb_charger_type_detect_event():usb_charger_type_detect_event -val: 2 ,charger_type:2
<3>[000011688ms] U_HOTPLUG:(U_TRACE)usb_notify_handler():recheck
<3>[000011688ms] U_HOTPLUG:(U_TRACE)usb_notify_handler():task of cur_status 1 status:1:start.
<3>[000011688ms] U_HOTPLUG:(U_TRACE)usb_notify_handler():task of 1 end.
<3>[000011688ms] dwc3 dwc3: request c1d02800 was not queued to ep0out
<3>[000011688ms] U_PNP:(U_TRACE)pnp_check_daynamic_sn_flag(): auto sn
<3>[000011688ms] U_PNP:(U_ERROR)usb_add_config():adding config #1 'android_usb'/c1d22a80
<6>[000011688ms] android_usb gadget: Mass Storage Function, version: GADGET 2.0
<6>[000011688ms] android_usb gadget: Number of LUNs=1
<3>[000011688ms] U_PNP:(U_ERROR)usb_add_function():adding 'Mass Storage Function'/c1d05100 to config 'android_usb'/c1d22a80
<3>[000011689ms] U_PNP:(U_ERROR)usb_add_config():cfg 1/c1d22a80 support speeds: super high full
<7>[000012302ms] dwc3 dwc3: dwc3_gadget_linksts_change_interrupt: link state:5 -> 3
<4>[000012510ms] CHG_STM:form transit_state to fast_stste!
<4>[000012550ms] CHG_PLT:chg_send_stat_to_app->deviceid 3, eventid 0 
<4>[000012550ms]  
<6>[000012610ms] android_work: sent uevent USB_STATE=CONNECTED
<6>[000012630ms] android_work: sent uevent USB_STATE=DISCONNECTED
<3>[000012689ms] U_PNP:(U_ERROR)composite_setup():HNP inactive
<3>[000012689ms] U_PNP:(U_ERROR)set_config():high-speed config #1: android_usb
<3>[000012689ms] U_CHARGER:(U_ERROR)usb_charger_type_detect_event():usb_charger_type_detect_event -val: 2 ,charger_type:3
<3>[000012689ms] U_CHARGER:(U_ERROR)usb_charger_type_detect_event():current_chg_type 2
<3>[000012689ms] U_ALL:(U_INFO)usb_notify_syswatch():U_EVENT: usb_notify_syswatch<1,0>
<3>[000012690ms] U_PNP:(U_ERROR)usb_composite_setup_continue():usb_composite_setup_continue
<3>[000012690ms] U_PNP:(U_ERROR)usb_composite_setup_continue():usb_composite_setup_continue: Completing delayed status
<3>[000012690ms] [MBB CHG]battery_monitor_blocking_notifier_call_chain :1 2.
<6>[000012690ms] CHG_DEBUG: wake lock timeout is 6s!
<3>[000012690ms] [MBB CHG]charge_event_work :1 2.
<6>[000012750ms] android_work: sent uevent USB_STATE=CONFIGURED
<7>[000013162ms] received shell ioctl cmd=0xcafa0000
<7>[000013162ms] , arg=0x00
<7>[000013162ms] received shell ioctl cmd=0xcafa0001
<7>[000013162ms] , arg=0xbeee4be0
<4>[000013168ms] normal mode
<4>[000013168ms] Call bsp_get_factory_mode return, value = 0x1
<6>[000013231ms] yaffs: dev is 32505875 name is "mtdblock19" rw
<6>[000013231ms] yaffs: passed flags ""
<7>[000013231ms] yaffs: yaffs: Attempting MTD mount of 31.19,"mtdblock19"
<7>[000013246ms] [*DLOAD_NARK_API*] visit_dload_smem:302: dload visit smem  vist = 8.
<3>[000013260ms] [hisi coul]charger event = 0x2 
<3>[000013261ms] huawei,bq_bci_battery huawei,bq_bci_battery: bq_charger_event_rcv charger event=2
<4>[000013261ms] CHG_TASK:chg_main_task->charger_input!!!
<4>[000013261ms]  CHG_PLT:chg_send_stat_to_app->deviceid 1, eventid 255 
<4>[000013300ms]  CHG_STM:set_cur_chg_mode=0
<4>[000013300ms] usb2.0 charger insert!
<4>[000013300ms]  
<3>[000013321ms] U_CHARGER:(U_TRACE)usb_speed_work_mode():CHG_CURRENT_HS
<7>[000013360ms] yaffs: yaffs_read_super: is_checkpointed 1
<7>[000013370ms] yaffs: start ecc scan thread fn 
<7>[000013404ms] ISO 9660 Extensions: Microsoft Joliet Level 1
<7>[000013406ms] ISOFS: changing to secondary root
<3>[000013408ms] U_MASS:(U_TRACE)fsg_store_file():fsg_store_file!
<7>[000013420ms] received shell ioctl cmd=0xcafa0000
<7>[000013420ms] , arg=0x00
<7>[000013420ms] received shell ioctl cmd=0xcafa0001
<7>[000013420ms] , arg=0xbecddbe0
<4>[000013426ms] Call bsp_get_product_hw_board_type return, value = 0x0
<3>[000013617ms] [kernel space] data receive from user_pid 198 are 0x1
<3>[000013760ms] U_MASS:(U_TRACE)do_scsi_command():do rewind receive!
<3>[000013760ms] U_MASS:(U_TRACE)do_rewind():do_rewind command
<3>[000013760ms] 00000000: 11 06 20 00 00 01 01 00 01 00 00 00 00 00 00 00
<3>[000013760ms] dwc3 dwc3: request c1d02800 was not queued to ep0out
<3>[000013760ms] dwc3 dwc3: request c1d02800 was not queued to ep0out
<3>[000013760ms] U_PNP:(U_ERROR)reset_config():reset config
<3>[000013760ms] U_PNP:(U_ERROR)unbind_config():unbind function 'Mass Storage Function'/c1d05100
<3>[000013760ms] U_PNP:(U_ERROR)unbind_config():unbind config 'android_usb'/c1d22a80
<3>[000013760ms] U_PNP:(U_TRACE)android_unbind_enabled_functions():unbind android_usb_func 'mass      '
<3>[000013760ms] U_PNP:(U_TRACE)pnp_check_daynamic_sn_flag(): auto sn
<3>[000013760ms] U_PNP:(U_ERROR)usb_add_config():adding config #1 'android_usb'/c1eba900
<3>[000013760ms] U_NET:(U_TRACE)gether_setup_name():gether_setup_name : netname=ecm, cdc_type=1, bypass=0, net_param=40,2048,122880,0
<4>[000013761ms] _fastip_attach: name:usb0 fastip handle:c1ebae40
<3>[000013761ms] U_ECM:(U_TRACE)ecm_bind_config():ecm_bind_config
<3>[000013761ms] U_PNP:(U_ERROR)usb_add_function():adding 'cdc_ethernet'/c1e68400 to config 'android_usb'/c1eba900
<3>[000013761ms] U_ECM:(U_TRACE)ecm_bind():ecm_bind
<3>[000013761ms] U_PNP:(U_ERROR)usb_add_config():cfg 1/c1eba900 support speeds: super high full
<3>[000013773ms] init: untracked pid 207 exited
<6>[000013989ms] CHG_DEBUG: poweron_chg_proc_read poweron state 0!
<7>[000014118ms] dwc3 dwc3: dwc3_gadget_linksts_change_interrupt: link state:5 -> 3
<6>[000014340ms] android_work: sent uevent USB_STATE=DISCONNECTED
<6>[000014401ms] android_work: sent uevent USB_STATE=CONNECTED
<6>[000014414ms] android_work: sent uevent USB_STATE=DISCONNECTED
<6>[000014480ms] android_work: sent uevent USB_STATE=CONNECTED
<3>[000014481ms] U_PNP:(U_ERROR)composite_setup():HNP inactive
<3>[000014481ms] U_PNP:(U_ERROR)set_config():high-speed config #1: android_usb
<3>[000014481ms] U_ECM:(U_TRACE)ecm_set_alt():ecm_set_alt: intf=0, alt=0, ctrl_id=0, data_id=1
<3>[000014481ms] U_HOTPLUG:(U_TRACE)bsp_usb_status_change():status 3
<3>[000014481ms] U_ALL:(U_INFO)usb_notify_syswatch():U_EVENT: usb_notify_syswatch<1,2>
<3>[000014481ms] U_NET: set link status = 1 
<3>[000014481ms] U_ECM:(U_TRACE)ecm_set_alt():ecm_set_alt: intf=1, alt=0, ctrl_id=0, data_id=1
<3>[000014481ms] U_NET:(U_TRACE)gether_connect():gether_connect
<3>[000014482ms] U_NET:(U_TRACE)usb_prealloc_eth_rx_mem():type:3->1, size:2048->2048, num:412->412, ptr=c306c3c0
<3>[000014482ms] U_ECM:(U_TRACE)ecm_close():ecm_close
<3>[000014482ms] U_ALL:(U_INFO)usb_notify_syswatch():U_EVENT: usb_notify_syswatch<1,2>
<3>[000014482ms] U_NET: set link status = 1 
<3>[000014482ms] U_CHARGER:(U_ERROR)usb_charger_type_detect_event():usb_charger_type_detect_event -val: 2 ,charger_type:3
<3>[000014482ms] U_CHARGER:(U_ERROR)usb_charger_type_detect_event():current_chg_type 2
<3>[000014482ms] U_ALL:(U_INFO)usb_notify_syswatch():U_EVENT: usb_notify_syswatch<1,0>
<3>[000014482ms] U_ECM:(U_TRACE)ecm_set_alt():ecm_set_alt: intf=1, alt=0, ctrl_id=0, data_id=1
<3>[000014483ms] U_NET:(U_TRACE)gether_disconnect():gether_disconnect
<3>[000014483ms] U_NET:(U_TRACE)gether_connect():gether_connect
<3>[000014483ms] U_NET:(U_TRACE)usb_prealloc_eth_rx_mem():type:1->1, size:2048->2048, num:412->412, ptr=c306c3c0
<3>[000014483ms] U_ECM:(U_TRACE)ecm_close():ecm_close
<3>[000014483ms] U_ALL:(U_INFO)usb_notify_syswatch():U_EVENT: usb_notify_syswatch<1,2>
<3>[000014483ms] U_NET: set link status = 1 
<3>[000014490ms] U_HOTPLUG:(U_TRACE)usb_notify_handler():old_status 1,status3
<3>[000014490ms] U_HOTPLUG:(U_TRACE)usb_notify_handler():task of cur_status 1 status:3:start.
<3>[000014490ms] U_HOTPLUG:(U_TRACE)bsp_usb_enum_done_process():balong usb enum done,it works well.
<4>[000014490ms] [bq27510_sync_coulupdate_port_control]: LINE [2067] not need to delay notify port enum done 
<4>[000014490ms] slUartHd is ok!
<4>[000014490ms] dmsVcomAtPcuiOpen success!
<3>[000014490ms] [MBB CHG]battery_monitor_blocking_notifier_call_chain :1 2.
<6>[000014490ms] CHG_DEBUG: wake lock timeout is 6s!
<3>[000014490ms] U_NCM:(U_TRACE)ncm_vendor_open():ncm_vendor_open: type=1, id=0
<3>[000014490ms] U_NCM:(U_ERROR)ncm_vendor_open():ncm_vendor_open line 321:module not init.
<4>[000014490ms] diag_UsbCtrlOpen failed.
<4>[000014490ms] diag_UsbAppOpen failed.
<3>[000014490ms] U_NCM:(U_TRACE)ncm_vendor_open():ncm_vendor_open: type=0, id=0
<3>[000014490ms] U_NCM:(U_ERROR)ncm_vendor_open():ncm_vendor_open line 321:module not init.
<3>[000014490ms] U_CHARGER:(U_ERROR)usb_charger_type_detect_event():usb_charger_type_detect_event -val: 3 ,charger_type:2
<3>[000014490ms] U_HOTPLUG:(U_TRACE)usb_notify_handler():recheck
<3>[000014490ms] U_HOTPLUG:(U_TRACE)usb_notify_handler():task of cur_status 3 status:3:start.
<3>[000014490ms] U_HOTPLUG:(U_TRACE)usb_notify_handler():task of 3 end.
<3>[000014490ms] [MBB CHG]charge_event_work: plug event report same plug=1,chg_type=2!!!
<6>[000014942ms] CHG_DEBUG: poweron_chg_proc_read poweron state 0!
<3>[000014980ms] init: untracked pid 206 exited
<7>[000015188ms] kern_path /proc/wifinet don't exist !
<7>[000015188ms] kern_path /proc/wifinet/ssid2 don't exist !
<7>[000015333ms] kern_path /proc/wifinet don't exist !
<7>[000015333ms] kern_path /proc/wifinet/ssid2 don't exist !
<6>[000015344ms] device rmnet2 entered promiscuous mode
<6>[000015345ms] br0: port 1(rmnet2) entered forwarding state
<6>[000015345ms] br0: port 1(rmnet2) entered forwarding state
<4>[000015628ms] device_event_input entry
<4>[000015628ms] PROCESS_ADD_MONITORED
<4>[000015628ms] notify_server ats webserver router device sms oled dhcps call dns
<4>[000015630ms] device_event_send: queue is NOT empty
<1>[000015630ms] device_event_send: msg send over
<4>[000015634ms] device_event_send: queue is NOT empty
<1>[000015634ms] device_event_send: msg send over
<4>[000015638ms] device_event_send: queue is NOT empty
<1>[000015638ms] device_event_send: msg send over
<4>[000015672ms] device_event_send: queue is NOT empty
<1>[000015672ms] device_event_send: msg send over
<4>[000015676ms] device_event_send: queue is NOT empty
<1>[000015676ms] device_event_send: msg send over
<4>[000015680ms] device_event_send: queue is NOT empty
<1>[000015680ms] device_event_send: msg send over
<4>[000015684ms] device_event_send: queue is NOT empty
<1>[000015684ms] device_event_send: msg send over
<4>[000015688ms] device_event_send: queue is NOT empty
<1>[000015688ms] device_event_send: msg send over
<3>[000015735ms] ***realtek*** [__rtl8192cd_init:12184]: Realtek WLAN driver - version 1.7 (2014-11-20)
<3>[000015735ms] ***realtek*** [__rtl8192cd_init:12192]: Adaptivity function - version 8.3
<3>[000015735ms] ***realtek*** [__rtl8192cd_init:12205]:  wlan_index:0  1, 10,0x8179024c,0x0,0
<3>[000015736ms] ***realtek*** [rtw_drv_init:57]: rtw_drv_init: sdio_func_id is "mmc0:0001:1"
<3>[000015736ms] ***realtek*** [rtw_drv_init:60]: Begin to Load NORMAL Mode *******
<3>[000015736ms] ***realtek*** [rtl8192cd_init_one:9177]: =====>>INSIDE rtl8192cd_init_one <<=====
<3>[000015736ms] ***realtek*** [rtl8192cd_init_one:9258]: [alloc] (dot11q cache) new = c1c5c000, cur_idx = 0 of array 3, buf_len = 12512
<3>[000015736ms] ***realtek*** [rtl8192cd_init_one:9321]: [alloc] (shared cache) new = c2208000, cur_idx = 0 of array 6, buf_len = 21216
<3>[000015736ms] ***realtek*** [rtl8192cd_init_one:9341]: [alloc] (shared cache) new = c2010000, cur_idx = 1 of array 6, buf_len = 49156
<3>[000015736ms] ***realtek*** [rtl8192cd_init_one:9361]: [alloc] (shared cache) new = c2300000, cur_idx = 2 of array 6, buf_len = 73732
<3>[000015736ms] ***realtek*** [rtl8192cd_init_one:9381]: [alloc] (shared cache) new = c2210000, cur_idx = 3 of array 6, buf_len = 47108
<3>[000015736ms] ***realtek*** [rtl8192cd_init_one:9401]: [alloc] (shared cache) new = c2408000, cur_idx = 4 of array 6, buf_len = 16388
<3>[000015736ms] ***realtek*** [rtl8192cd_init_one:9422]: [alloc] (shared cache) new = c21f8000, cur_idx = 5 of array 6, buf_len = 16388
<4>[000015736ms] device_event_send: queue is NOT empty
<1>[000015736ms] device_event_send: msg send over
<3>[000015743ms] ***realtek*** [rtw_os_xmit_resource_alloc:78]: [alloc] (xmit cache) new = c2020000, cur_idx = 0 of array 16, buf_len = 31232
<3>[000015743ms] ***realtek*** [rtw_os_xmit_resource_alloc:78]: [alloc] (xmit cache) new = c2028000, cur_idx = 1 of array 16, buf_len = 31232
<3>[000015743ms] ***realtek*** [rtw_os_xmit_resource_alloc:78]: [alloc] (xmit cache) new = c2030000, cur_idx = 2 of array 16, buf_len = 31232
<3>[000015743ms] ***realtek*** [rtw_os_xmit_resource_alloc:78]: [alloc] (xmit cache) new = c2038000, cur_idx = 3 of array 16, buf_len = 31232
<3>[000015743ms] ***realtek*** [rtw_os_xmit_resource_alloc:78]: [alloc] (xmit cache) new = c1cc0000, cur_idx = 4 of array 16, buf_len = 31232
<3>[000015743ms] ***realtek*** [rtw_os_xmit_resource_alloc:78]: [alloc] (xmit cache) new = c1cc8000, cur_idx = 5 of array 16, buf_len = 31232
<3>[000015743ms] ***realtek*** [rtw_os_xmit_resource_alloc:78]: [alloc] (xmit cache) new = c1cd0000, cur_idx = 6 of array 16, buf_len = 31232
<3>[000015743ms] ***realtek*** [rtw_os_xmit_resource_alloc:78]: [alloc] (xmit cache) new = c1cd8000, cur_idx = 7 of array 16, buf_len = 31232
<3>[000015743ms] ***realtek*** [rtl8192es_init_recv_priv:397]: [alloc] (recv cache) new = c2420000, cur_idx = 0 of array 1, buf_len = 65536
<3>[000015745ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = ext_lna_gain, value from def 16 to 12 
<3>[000015746ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = rssi_offset, value from def 0 to 2 
<3>[000015746ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = ofdm_rssi_offset, value from def 0 to 3 
<3>[000015746ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = rx_pwr_7, value from def -30 to -34 
<3>[000015746ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = rx_pwr_3, value from def -12 to -11 
<3>[000015746ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = rx_pwr_2, value from def 5 to 2 
<3>[000015746ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = cck_cca_hi, value from def 205 to 131 
<3>[000015746ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = cck_cca_low, value from def 64 to 131 
<3>[000015746ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = lna_rx_low, value from def 26 to 47 
<3>[000015746ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = trswitch, value from def 0 to 1 
<3>[000015746ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_cck_1, value from def 127 to 5 
<3>[000015746ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_cck_2, value from def 127 to 5 
<3>[000015746ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_cck_5, value from def 127 to 5 
<3>[000015746ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_cck_11, value from def 127 to 5 
<3>[000015746ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_ofdm_6, value from def 127 to 3 
<3>[000015746ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_ofdm_9, value from def 127 to 3 
<3>[000015746ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_ofdm_12, value from def 127 to 3 
<3>[000015746ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_ofdm_18, value from def 127 to 3 
<3>[000015747ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_ofdm_24, value from def 127 to 3 
<3>[000015747ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_ofdm_36, value from def 127 to 3 
<3>[000015747ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_ofdm_48, value from def 127 to 3 
<3>[000015747ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_ofdm_54, value from def 127 to 3 
<3>[000015747ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_mcs_0, value from def 127 to 4 
<3>[000015747ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_mcs_1, value from def 127 to 4 
<3>[000015747ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_mcs_2, value from def 127 to 4 
<3>[000015747ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_mcs_3, value from def 127 to 4 
<3>[000015747ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_mcs_4, value from def 127 to 4 
<3>[000015747ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_mcs_5, value from def 127 to 4 
<3>[000015747ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_mcs_6, value from def 127 to 4 
<3>[000015747ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_mcs_7, value from def 127 to 4 
<3>[000015747ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_mcs_8, value from def 127 to 4 
<3>[000015747ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_mcs_9, value from def 127 to 4 
<3>[000015747ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_mcs_10, value from def 127 to 4 
<3>[000015747ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_mcs_11, value from def 127 to 4 
<3>[000015747ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_mcs_12, value from def 127 to 4 
<3>[000015747ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_mcs_13, value from def 127 to 4 
<3>[000015747ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_mcs_14, value from def 127 to 4 
<3>[000015748ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = txPowerPlus_mcs_15, value from def 127 to 4 
<3>[000015748ms] ***realtek*** [set_mib_default:2072]: num= 0, mib_key = adaptivity_enable, value from def 1 to 2 
<3>[000015764ms] ***realtek*** [_CardEnable:155]: InitPON OK
<3>[000015806ms] ***realtek*** [rtl8192cd_init_one:10997]: =====>>EXIT rtl8192cd_init_one (wlan0) <<=====
<3>[000015806ms] ***realtek*** [rtl8192cd_init_one:9177]: =====>>INSIDE rtl8192cd_init_one <<=====
<3>[000015806ms] ***realtek*** [rtl8192cd_init_one:9241]: [alloc] (mib cache) new = c2438000, cur_idx = 0 of array 2, buf_len = 13704
<3>[000015806ms] ***realtek*** [rtl8192cd_init_one:9258]: [alloc] (dot11q cache) new = c243c000, cur_idx = 1 of array 3, buf_len = 12512
<3>[000015870ms] ***realtek*** [rtl8192cd_init_one:10997]: =====>>EXIT rtl8192cd_init_one (WiFi0) <<=====
<3>[000015870ms] ***realtek*** [rtl8192cd_init_one:9177]: =====>>INSIDE rtl8192cd_init_one <<=====
<3>[000015870ms] ***realtek*** [rtl8192cd_init_one:9241]: [alloc] (mib cache) new = c2250000, cur_idx = 1 of array 2, buf_len = 13704
<3>[000015870ms] ***realtek*** [rtl8192cd_init_one:9258]: [alloc] (dot11q cache) new = c2254000, cur_idx = 2 of array 3, buf_len = 12512
<3>[000015874ms] ***realtek*** [rtl8192cd_init_one:10997]: =====>>EXIT rtl8192cd_init_one (wlan1) <<=====
<3>[000015874ms] ***realtek*** [rtw_drv_init:87]: Load NORMAL Mode Successfully! *******
<6>[000015961ms] efuse read start group 4 length 4.
<6>[000015961ms] efuse read end group 4 length 4.
<6>[000015961ms] efuse buf[0] is 0x0.
<6>[000015961ms] efuse buf[1] is 0x0.
<6>[000015961ms] efuse buf[2] is 0x0.
<6>[000015961ms] efuse buf[3] is 0x0.
<6>[000015961ms] efuse read ret 0
<3>[000015971ms] [special_timer] Timer create start, ID  is  2 
<0>[000015971ms] [special_timer] Creat add start special timer sucess, timerID is 3 
<7>[000016074ms] parent_name_ptr =oeminfo 
<4>[000016074ms]  info :mtd->erasesize = 131072 ,mtd->writesize = 2048 
<7>[000016074ms] operation_region[0] = 0 
<4>[000016075ms] [version]: <bsp_get_iso_version> flash_get_share_region_info ture. 
<7>[000016238ms] parent_name_ptr =oeminfo 
<4>[000016238ms]  info :mtd->erasesize = 131072 ,mtd->writesize = 2048 
<7>[000016238ms] operation_region[0] = 0 
<3>[000016244ms] [*DLOAD_NARK_CORE*] flash_web_proc_write:539: Do not need to update version success.
<6>[000016267ms] CHG_DEBUG: poweron_chg_proc_read poweron state 0!
<6>[000016269ms] invalid lcd MainOLED_DispENoff
<3>[000016489ms] U_MASS:(U_TRACE)mass_storage_usb_sd_is_open():mass_storage_usb_sd_is_open ?
<3>[000016489ms] U_MASS:(U_TRACE)mass_storage_usb_sd_is_open():sd_card_status PRESENT 
<3>[000016489ms] U_MASS:(U_TRACE)mass_storage_usb_sd_is_open():usb sd is not open
<3>[000016489ms] U_MASS:(U_TRACE)mass_storage_set_sd_card_workmode():USB
<4>[000016620ms] [lcd]: <lcd_vectid_get> Gpio is busy!!! 
<4>[000016620ms] 
<4>[000016620ms] [lcd]: <lcd_vectid_get> Gpio is busy!!! 
<4>[000016620ms] 
<4>[000016620ms] ------------[ cut here ]------------
<4>[000016620ms] WARNING: at /home/jwx384541/E5770s-923_c778/vendor/hisi/modem/system/android/android_4.2_r1/kernel/drivers/gpio/gpiolib.c:1585 __gpio_get_value+0x54/0x5c()
<4>[000016620ms] Modules linked in: rtl8192es(O)
<4>[000016620ms] [<c00177d0>] (unwind_backtrace+0x0/0x14c) from [<c002387c>] (warn_slowpath_common+0x54/0x6c)
<4>[000016620ms] [<c002387c>] (warn_slowpath_common+0x54/0x6c) from [<c00238b0>] (warn_slowpath_null+0x1c/0x24)
<4>[000016620ms] [<c00238b0>] (warn_slowpath_null+0x1c/0x24) from [<c01a4ba8>] (__gpio_get_value+0x54/0x5c)
<4>[000016620ms] [<c01a4ba8>] (__gpio_get_value+0x54/0x5c) from [<c01aa2e4>] (lcd_vectid_get+0x30/0x198)
<4>[000016620ms] [<c01aa2e4>] (lcd_vectid_get+0x30/0x198) from [<c01aaa30>] (lcd_init+0x18/0x5c)
<4>[000016620ms] [<c01aaa30>] (lcd_init+0x18/0x5c) from [<c01aaa94>] (lcd_pwron+0x20/0x2c)
<4>[000016620ms] [<c01aaa94>] (lcd_pwron+0x20/0x2c) from [<c01ab040>] (stlcdfb_pan_display+0x114/0x138)
<4>[000016620ms] [<c01ab040>] (stlcdfb_pan_display+0x114/0x138) from [<c01a53f0>] (fb_pan_display+0xb4/0x130)
<4>[000016620ms] [<c01a53f0>] (fb_pan_display+0xb4/0x130) from [<c01a6444>] (do_fb_ioctl+0x474/0x5d8)
<4>[000016620ms] [<c01a6444>] (do_fb_ioctl+0x474/0x5d8) from [<c00c5dc0>] (do_vfs_ioctl+0x84/0x5d8)
<4>[000016620ms] [<c00c5dc0>] (do_vfs_ioctl+0x84/0x5d8) from [<c00c634c>] (sys_ioctl+0x38/0x5c)
<4>[000016620ms] [<c00c634c>] (sys_ioctl+0x38/0x5c) from [<c0011180>] (ret_fast_syscall+0x0/0x30)
<4>[000016620ms] ---[ end trace 2829471d8fa0e43f ]---
<4>[000016621ms] ------------[ cut here ]------------
<4>[000016621ms] WARNING: at /home/jwx384541/E5770s-923_c778/vendor/hisi/modem/system/android/android_4.2_r1/kernel/drivers/gpio/gpiolib.c:1585 __gpio_get_value+0x54/0x5c()
<4>[000016621ms] Modules linked in: rtl8192es(O)
<4>[000016621ms] [<c00177d0>] (unwind_backtrace+0x0/0x14c) from [<c002387c>] (warn_slowpath_common+0x54/0x6c)
<4>[000016621ms] [<c002387c>] (warn_slowpath_common+0x54/0x6c) from [<c00238b0>] (warn_slowpath_null+0x1c/0x24)
<4>[000016621ms] [<c00238b0>] (warn_slowpath_null+0x1c/0x24) from [<c01a4ba8>] (__gpio_get_value+0x54/0x5c)
<4>[000016621ms] [<c01a4ba8>] (__gpio_get_value+0x54/0x5c) from [<c01aa2f8>] (lcd_vectid_get+0x44/0x198)
<4>[000016621ms] [<c01aa2f8>] (lcd_vectid_get+0x44/0x198) from [<c01aaa30>] (lcd_init+0x18/0x5c)
<4>[000016621ms] [<c01aaa30>] (lcd_init+0x18/0x5c) from [<c01aaa94>] (lcd_pwron+0x20/0x2c)
<4>[000016621ms] [<c01aaa94>] (lcd_pwron+0x20/0x2c) from [<c01ab040>] (stlcdfb_pan_display+0x114/0x138)
<4>[000016621ms] [<c01ab040>] (stlcdfb_pan_display+0x114/0x138) from [<c01a53f0>] (fb_pan_display+0xb4/0x130)
<4>[000016621ms] [<c01a53f0>] (fb_pan_display+0xb4/0x130) from [<c01a6444>] (do_fb_ioctl+0x474/0x5d8)
<4>[000016621ms] [<c01a6444>] (do_fb_ioctl+0x474/0x5d8) from [<c00c5dc0>] (do_vfs_ioctl+0x84/0x5d8)
<4>[000016621ms] [<c00c5dc0>] (do_vfs_ioctl+0x84/0x5d8) from [<c00c634c>] (sys_ioctl+0x38/0x5c)
<4>[000016621ms] [<c00c634c>] (sys_ioctl+0x38/0x5c) from [<c0011180>] (ret_fast_syscall+0x0/0x30)
<4>[000016621ms] ---[ end trace 2829471d8fa0e440 ]---
<4>[000016621ms] [lcd]: <lcd_vectid_get> 
<4>[000016621ms] lcd ID=0
<4>[000016621ms] 
<3>[000016621ms] lcd_init:oled_MacID = 66742 
<4>[000016945ms] [lcd]: <MainOLED_DispAlloff> lcd MainOLED_DispAlloff
<4>[000016945ms] 
<6>[000016984ms] invalid lcd MainOLED_DispENon
<3>[000017581ms] Wi-Fi<INFO>[wifi_event_input:1044]: enter
<3>[000017581ms] Wi-Fi<INFO>[wifi_event_input:1070]: record user_pid = 0x461!
<3>[000017581ms] Wi-Fi<INFO>[wifi_at_device_store:771]: receive msg from user is 15 msg_pid:461
<3>[000017581ms] Wi-Fi<INFO>[wifi_at_device_store:829]: wifi MONITOR_PID = 461, p = c225eac0
<3>[000017590ms] Wi-Fi<INFO>[wifi_event_send:1098]: enter
<6>[000018653ms] br0: port 1(rmnet2) entered disabled state
<6>[000018694ms] device rmnet2 left promiscuous mode
<6>[000018694ms] br0: port 1(rmnet2) entered disabled state
<7>[000018776ms] kern_path /proc/wifinet don't exist !
<7>[000018776ms] kern_path /proc/wifinet/ssid2 don't exist !
<6>[000018776ms] ADDRCONF(NETDEV_UP): br0: link is not ready
<6>[000018788ms] device rmnet2 entered promiscuous mode
<6>[000018788ms] br0: port 1(rmnet2) entered forwarding state
<6>[000018788ms] br0: port 1(rmnet2) entered forwarding state
<6>[000018788ms] ADDRCONF(NETDEV_CHANGE): br0: link becomes ready
<4>[000019102ms] RNIC_WriteDialEventReportFile:acDialEventTemp 0
<4>[000019102ms]  len is 2
<4>[000019103ms] RNIC_WriteOnDemandFile:buf30 len 2 
<4>[000019103ms] RNIC_WriteOnDemandFile:acModeTemp 0
<4>[000019103ms]  len is 2
<6>[000019114ms] device usb0 entered promiscuous mode
<4>[000019117ms] RNIC_WriteDialEventReportFile:acDialEventTemp 0
<4>[000019117ms]  len is 2
<4>[000019118ms] RNIC_WriteOnDemandFile:buf30 len 2 
<4>[000019118ms] RNIC_WriteOnDemandFile:acModeTemp 0
<4>[000019118ms]  len is 2
<3>[000019233ms] init: untracked pid 346 exited
<4>[000019240ms] device_event_send: queue is NOT empty
<1>[000019240ms] device_event_send: msg send over
<3>[000019352ms] U_NET:(U_TRACE)eth_open():eth_open
<3>[000019352ms] U_NET:(U_TRACE)eth_start():eth_start
<3>[000019352ms] U_ECM:(U_TRACE)ecm_open():ecm_open
<6>[000019353ms] br0: port 2(usb0) entered forwarding state
<6>[000019353ms] br0: port 2(usb0) entered forwarding state
<4>[000019561ms] RNIC_WriteDialEventReportFile:acDialEventTemp 0
<4>[000019561ms]  len is 2
<4>[000019562ms] RNIC_WriteOnDemandFile:buf30 len 2 
<4>[000019562ms] RNIC_WriteOnDemandFile:acModeTemp 0
<4>[000019562ms]  len is 2
<3>[000019956ms] init: untracked pid 588 exited
<6>[000020078ms] CHG_DEBUG: poweron_chg_proc_read poweron state 0!
<3>[000020359ms] init: untracked pid 575 exited
<4>[000020360ms] device_event_send: queue is NOT empty
<1>[000020360ms] device_event_send: msg send over
<3>[000020438ms] Wi-Fi<INFO>[wifi_at_device_store:771]: receive msg from user is 9 timeout:0
<3>[000020438ms] Wi-Fi<INFO>[wifi_timer_start:569]: set timer to 0 seconds,time id = 0
<3>[000020438ms] Wi-Fi<INFO>[wifi_timer_delete:498]:  enter, wlan_timer[0].timer_stus = 0
<3>[000020438ms] Wi-Fi<INFO>[wifi_timer_delete:502]:  timer TIMER_INACTIVE,id = 0
<6>[000020450ms] invalid lcd MainOLED_DispENon
<3>[000020525ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020525ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F4
<3>[000020525ms] ***realtek*** [read_reg:3690]: read byte reg 210=0xea
<3>[000020526ms] Wi-Fi<INFO>[wifi_at_device_store:771]: receive msg from user is 14 fw_type:0
<3>[000020526ms] Wi-Fi<INFO>[wifi_at_device_store:841]: wifi_at_dev: 14 fw_type:0 is not support!
<3>[000020527ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020527ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020527ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020527ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020527ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020527ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020527ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020527ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020527ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020527ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020528ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020528ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020528ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020528ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020528ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020528ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020528ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020528ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020528ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020528ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020528ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020528ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020528ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020528ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020529ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020529ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020529ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020529ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020529ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020529ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020529ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020529ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020529ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020529ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020529ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020529ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020550ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020550ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020550ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020550ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020550ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020550ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020550ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020550ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020551ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020551ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020551ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020551ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020551ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020551ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020551ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020551ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020551ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020551ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020551ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020551ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020552ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020552ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020552ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020552ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020552ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020552ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020552ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020552ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020552ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020552ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020552ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020552ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020552ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020552ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020553ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B0D
<3>[000020553ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 000089F1
<3>[000020567ms] ***realtek*** [map_country_to_reg:418]: domain:12 cn: RU found: 1
<3>[000020567ms] ***realtek*** [checkBand2ndOffset:8809]: is_40m_bw = 0, net_work_type = 0000000b
<6>[000020730ms] invalid lcd MainOLED_DispENon
<3>[000020819ms] ***realtek*** [debug_out:77]: PSK: PMK=
<3>[000020819ms] ***realtek*** [debug_out:77]: PSK: Set RSNIE
<3>[000020828ms] ***realtek*** [rtl8192cd_init_hw_PCI:10531]: InitPON OK
<3>[000020830ms] ***realtek*** [rtl8192cd_init_hw_PCI:10541]: InitMAC OK
<3>[000020830ms] ***realtek*** [rtl8192cd_init_hw_PCI:10615]: 
<4>[000020830ms] 
<4>[000020830ms] ************* Initialize MAC/PHY parameter *************
<3>[000020830ms] ***realtek*** [PHY_ConfigMACWithParaFile:4641]: [alloc] (cfgfile cache) new = c1350000, cur_idx = 2 of array 3, buf_len = 20480
<3>[000020830ms] ***realtek*** [GetHwReg88XX:678]: [MAC_REG_8192Emp]
<3>[000020833ms] ***realtek*** [GetHwReg88XX:899]: [PHY_REG_8192E_extlna]
<3>[000020833ms] ***realtek*** [PHY_ConfigBBWithParaFile:4390]: [alloc] (cfgfile cache) new = c13b0000, cur_idx = 0 of array 3, buf_len = 20480
<3>[000020839ms] ***realtek*** [GetHwReg88XX:1031]: [PHY_REG_PG_8192Emp]
<3>[000020839ms] ***realtek*** [PHY_ConfigBBWithParaFile:4031]: [cache] (cfgfile cache) mem = c13b0000, cur_idx = 0 of array 3, buf_len = 20480
<3>[000020839ms] ***realtek*** [PHY_ConfigBBWithParaFile:4390]: [cache] (cfgfile cache) mem = c13b0000, cur_idx = 0 of array 3, buf_len = 20480
<3>[000020840ms] ***realtek*** [GetHwReg88XX:1474]: [AGC_TAB_8192E_extlna]
<3>[000020840ms] ***realtek*** [PHY_ConfigBBWithParaFile:4390]: [cache] (cfgfile cache) mem = c13b0000, cur_idx = 0 of array 3, buf_len = 20480
<3>[000020847ms] ***realtek*** [GetHwReg88XX:1741]: [RadioA_8192E_extlna]
<3>[000020847ms] ***realtek*** [PHY_ConfigRFWithParaFile:4569]: [alloc] (cfgfile cache) new = c11b8000, cur_idx = 1 of array 3, buf_len = 20480
<3>[000021207ms] ***realtek*** [GetHwReg88XX:1932]: [RadioB_8192E_extlna]
<3>[000021207ms] ***realtek*** [PHY_ConfigRFWithParaFile:4569]: [cache] (cfgfile cache) mem = c11b8000, cur_idx = 1 of array 3, buf_len = 20480
<3>[000021792ms] ***realtek*** [rtl8192cd_init_hw_PCI:11561]: InitDownload FW OK 
<3>[000021792ms] ***realtek*** [GetHwReg88XX:2171]: [TxPowerTrack_AP]
<4>[000021831ms] set eth wakelock timeout 180
<4>[000021831ms] phy power is enabled
<6>[000021885ms] invalid lcd MainOLED_DispENon
<6>[000022198ms] invalid lcd MainOLED_DispENon
<3>[000022382ms] ***realtek*** [rtl8192cd_init_hw_PCI:12681]: 8192E LCK done!!
<3>[000022382ms] ***realtek*** [SwBWMode:13869]: switch to band 0
<3>[000022385ms] ***realtek*** [rtl8192cd_init_hw_PCI:12783]: 8192E ext PA or ext LNA !!!
<3>[000022387ms] ***realtek*** [set_1cca_enable:10396]: switch 1cca enable to 1
<3>[000022387ms] ***realtek*** [fastip_attach_wifi:123]: wifi fastip netif index = 1, devname wlan0
<4>[000022387ms] _fastip_attach: name:wlan0 fastip handle:c22d2f00
<3>[000022387ms] ***realtek*** [fastip_attach_wifi:132]: wifi_fastip_handle attach ok !!!!!! cih = 0xc22d2f00 
<3>[000022388ms] ***realtek*** [fastip_attach_wifi:140]: wifi wifi register ok
<3>[000022388ms] ***realtek*** [start_clnt_ss:12978]: acli: start_ss_t ss_req:0 scanning:0 is_root:1  
<3>[000022388ms] ***realtek*** [SwBWMode:13869]: switch to band 0
<3>[000022395ms] ***realtek*** [start_clnt_ss:13167]: start_clnt_ss trigger NHM 
<3>[000022396ms] Wi-Fi<INFO>[wlan_set_driver_lock:1482]: Exit, wifi driver lock ON
<3>[000022396ms] Wi-Fi<INFO>[wlan_request_wakeup_irq:1401]: Get WiFi WAKEUP BB(0x4080) GPIO irq = 112 Successfully
<3>[000022396ms] ***realtek*** [rtl8192cd_open:7859]: dev_irq = 112
<6>[000022419ms] device wlan0 entered promiscuous mode
<6>[000022419ms] br0: port 3(wlan0) entered forwarding state
<6>[000022419ms] br0: port 3(wlan0) entered forwarding state
<3>[000022448ms] ***realtek*** [rtl8192cd_ioctl:9042]: recv ioctl iface = wlan0, cmd = 00008B9F
<3>[000022453ms] Wi-Fi<INFO>[wifi_at_device_store:771]: receive msg from user is 9 timeout:600
<3>[000022453ms] Wi-Fi<INFO>[wifi_timer_start:569]: set timer to 600 seconds,time id = 0
<3>[000022453ms] Wi-Fi<INFO>[wifi_timer_delete:498]:  enter, wlan_timer[0].timer_stus = 0
<3>[000022453ms] Wi-Fi<INFO>[wifi_timer_delete:502]:  timer TIMER_INACTIVE,id = 0
<3>[000022453ms] Wi-Fi<INFO>[wifi_timer_start:591]: timer add success, time = 600 seconds,wlan_timer[0].timer_stus = 1
<3>[000022520ms] Wi-Fi<INFO>[wifi_at_device_store:771]: receive msg from user is 9 timeout:0
<3>[000022520ms] Wi-Fi<INFO>[wifi_timer_start:569]: set timer to 0 seconds,time id = 0
<3>[000022520ms] Wi-Fi<INFO>[wifi_timer_delete:498]:  enter, wlan_timer[0].timer_stus = 1
<3>[000022520ms] Wi-Fi<INFO>[wifi_timer_delete:511]: exit, timer delete success,wlan_timer[0].timer_stus = 0
<6>[000022524ms] invalid lcd MainOLED_DispENon
<3>[000022555ms] ***realtek*** [rtl8192cd_ss_timer:13719]: nhm_cnt[0] 5---9 
<3>[000022555ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 1, scan 40M = 0, times 0/3
<3>[000022658ms] ***realtek*** [rtl8192cd_ss_timer:13719]: nhm_cnt[1] 5---9 
<3>[000022658ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 2, scan 40M = 0, times 0/3
<3>[000022802ms] ***realtek*** [rtl8192cd_ss_timer:13719]: nhm_cnt[2] 5---9 
<3>[000022802ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 3, scan 40M = 0, times 0/3
<3>[000022859ms] U_MASS:(U_TRACE)mass_storage_usb_sd_is_open():mass_storage_usb_sd_is_open ?
<3>[000022859ms] U_MASS:(U_TRACE)mass_storage_usb_sd_is_open():sd_card_status PRESENT 
<3>[000022859ms] U_MASS:(U_TRACE)mass_storage_usb_sd_is_open():usb sd is not open
<3>[000022859ms] U_MASS:(U_TRACE)mass_storage_set_sd_card_workmode():USB
<3>[000022905ms] ***realtek*** [rtl8192cd_ss_timer:13719]: nhm_cnt[3] 5---9 
<3>[000022905ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 4, scan 40M = 0, times 0/3
<6>[000022913ms] invalid lcd MainOLED_DispENon
<4>[000022927ms] set eth wakelock timeout 180
<4>[000022928ms] phy power is enabled
<4>[000022981ms] set eth wakelock timeout 180
<4>[000022981ms] phy power is enabled
<3>[000023008ms] ***realtek*** [rtl8192cd_ss_timer:13719]: nhm_cnt[4] 5---9 
<3>[000023009ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 5, scan 40M = 0, times 0/3
<6>[000023028ms] invalid lcd MainOLED_DispENon
<3>[000023132ms] ***realtek*** [rtl8192cd_ss_timer:13719]: nhm_cnt[5] 5---9 
<3>[000023132ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 6, scan 40M = 0, times 0/3
<3>[000023235ms] ***realtek*** [rtl8192cd_ss_timer:13719]: nhm_cnt[6] 5---9 
<3>[000023235ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 7, scan 40M = 0, times 0/3
<3>[000023338ms] ***realtek*** [rtl8192cd_ss_timer:13719]: nhm_cnt[7] 5---9 
<3>[000023338ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 8, scan 40M = 0, times 0/3
<3>[000023442ms] ***realtek*** [rtl8192cd_ss_timer:13719]: nhm_cnt[8] 5---9 
<3>[000023442ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 9, scan 40M = 0, times 0/3
<3>[000023545ms] ***realtek*** [rtl8192cd_ss_timer:13719]: nhm_cnt[9] 5---9 
<3>[000023545ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 10, scan 40M = 0, times 0/3
<3>[000023648ms] ***realtek*** [rtl8192cd_ss_timer:13719]: nhm_cnt[10] 5---9 
<3>[000023648ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 11, scan 40M = 0, times 0/3
<3>[000023752ms] ***realtek*** [rtl8192cd_ss_timer:13719]: nhm_cnt[11] 5---9 
<3>[000023752ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 12, scan 40M = 0, times 0/3
<3>[000023780ms] U_PNP:(U_ERROR)soft_reconnect_handler(): soft_reconnect_handler  state:2 
<3>[000023855ms] ***realtek*** [rtl8192cd_ss_timer:13719]: nhm_cnt[12] 5---9 
<3>[000023855ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:1 scan ch = 13, scan 40M = 0, times 0/3
<3>[000023855ms] ***realtek*** [rtl8192cd_ss_timer:13906]: auto_channel_step 2 
<3>[000023958ms] ***realtek*** [rtl8192cd_ss_timer:13730]: nhm_cnt[0] 0---4 
<3>[000023958ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 1, scan 40M = 0, times 0/3
<3>[000024061ms] ***realtek*** [rtl8192cd_ss_timer:13730]: nhm_cnt[1] 0---4 
<3>[000024061ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 2, scan 40M = 0, times 0/3
<3>[000024164ms] ***realtek*** [rtl8192cd_ss_timer:13730]: nhm_cnt[2] 0---4 
<3>[000024164ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 3, scan 40M = 0, times 0/3
<3>[000024267ms] ***realtek*** [rtl8192cd_ss_timer:13730]: nhm_cnt[3] 0---4 
<3>[000024267ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 4, scan 40M = 0, times 0/3
<3>[000024370ms] ***realtek*** [rtl8192cd_ss_timer:13730]: nhm_cnt[4] 0---4 
<3>[000024370ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 5, scan 40M = 0, times 0/3
<3>[000024473ms] ***realtek*** [rtl8192cd_ss_timer:13730]: nhm_cnt[5] 0---4 
<3>[000024473ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 6, scan 40M = 0, times 0/3
<3>[000024576ms] ***realtek*** [rtl8192cd_ss_timer:13730]: nhm_cnt[6] 0---4 
<3>[000024576ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 7, scan 40M = 0, times 0/3
<3>[000024680ms] ***realtek*** [rtl8192cd_ss_timer:13730]: nhm_cnt[7] 0---4 
<3>[000024680ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 8, scan 40M = 0, times 0/3
<3>[000024782ms] ***realtek*** [rtl8192cd_ss_timer:13730]: nhm_cnt[8] 0---4 
<3>[000024782ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 9, scan 40M = 0, times 0/3
<3>[000024885ms] ***realtek*** [rtl8192cd_ss_timer:13730]: nhm_cnt[9] 0---4 
<3>[000024885ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 10, scan 40M = 0, times 0/3
<3>[000024988ms] ***realtek*** [rtl8192cd_ss_timer:13730]: nhm_cnt[10] 0---4 
<3>[000024988ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 11, scan 40M = 0, times 0/3
<3>[000025091ms] ***realtek*** [rtl8192cd_ss_timer:13730]: nhm_cnt[11] 0---4 
<3>[000025091ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:0 scan ch = 12, scan 40M = 0, times 0/3
<3>[000025194ms] ***realtek*** [rtl8192cd_ss_timer:13730]: nhm_cnt[12] 0---4 
<3>[000025194ms] ***realtek*** [rtl8192cd_ss_timer:13802]: ss_req:0 loop_finish:1 scan ch = 13, scan 40M = 0, times 0/3
<3>[000025194ms] ***realtek*** [rtl8192cd_ss_timer:13923]: STOP_BCN  auto_channel_step = 0 
<3>[000025194ms] ***realtek*** [find_clean_channel:8929]: begin 0 end 13 
<3>[000025194ms] ***realtek*** [selectClearChannel:9504]: channel select ch: 1 aborted
<3>[000025194ms] ***realtek*** [selectClearChannel:9504]: channel select ch: 2 aborted
<3>[000025194ms] ***realtek*** [selectClearChannel:9504]: channel select ch: 3 aborted
<3>[000025194ms] ***realtek*** [selectClearChannel:9504]: channel select ch: 4 aborted
<3>[000025195ms] ***realtek*** [selectClearChannel:9504]: channel select ch: 12 aborted
<3>[000025195ms] ***realtek*** [selectClearChannel:9504]: channel select ch: 13 aborted
<3>[000025195ms] ***realtek*** [rtl8192cd_ss_timer:14106]: auto select to channel 8
<3>[000025195ms] ***realtek*** [checkBand2ndOffset:8809]: is_40m_bw = 0, net_work_type = 0000000b
<3>[000025195ms] ***realtek*** [SwBWMode:13869]: switch to band 0
<3>[000026427ms] NOHZ: local_softirq_pending 08
<3>[000026432ms] NOHZ: local_softirq_pending 08
<3>[000026456ms] NOHZ: local_softirq_pending 08
<3>[000027322ms] NOHZ: local_softirq_pending 08
<3>[000027340ms] NOHZ: local_softirq_pending 08
<3>[000027361ms] NOHZ: local_softirq_pending 08
<3>[000027454ms] NOHZ: local_softirq_pending 08
<3>[000027480ms] NOHZ: local_softirq_pending 08
<3>[000028192ms] NOHZ: local_softirq_pending 08
<3>[000028210ms] NOHZ: local_softirq_pending 08
<3>[000032400ms] ***realtek*** [sdio_power_save_timer:6084]: ps_disable = 0, total_num = 0, pwr_state = 0, offload_ctl = 0
<3>[000032400ms] ***realtek*** [sdio_power_save_timer:6107]: starting offload, offload_function_ctrl = 1
<3>[000032445ms] ***realtek*** [fill_powersave_content:7482]: netif = wlan0, bcn_len = 271, rsp_len = 390, bcn_idx = 0, rsp_idx = 2, total_len = 512
<3>[000032446ms] ***realtek*** [fill_powersave_content:7507]: BUF_len = 0, txDesSize = 40, page_size = 256, total_len = 902
<3>[000032446ms] ***realtek*** [update_beacon:8200]: netif = wlan0, pwr_state = 0, offload_function_ctrl = 1
<3>[000032551ms] ***realtek*** [update_beacon:8200]: netif = wlan0, pwr_state = 0, offload_function_ctrl = 2
<3>[000032651ms] ***realtek*** [cmd_set_ap_offload:1254]: netif = wlan0, cmd_set_ap_offload = 1
<3>[000032651ms] ***realtek*** [update_beacon:8200]: netif = wlan0, pwr_state = 0, offload_function_ctrl = 255
<3>[000032652ms] ***realtek*** [callback_ap_offload:1352]: ap_count = 1, netif = wlan0, hidden = 0, bcn_page = 0x00, rsp_page = 0x02
<3>[000032652ms] ***realtek*** [SetAPOffload88XX:1778]: bEn = 1
<3>[000032652ms] ***realtek*** [SetGpioWakePin:1721]: Exit, gpio wakeup=ee, ret = 0
<3>[000032652ms] ***realtek*** [SetBCNRsvdPage88XX:1673]: bcn: [f6] [0] nr_ap=:1
<3>[000032652ms] ***realtek*** [SetProbeRsvdPage88XX:1694]: prob: [f8] [0] nr_ap=:1
<3>[000032652ms] ***realtek*** [SetAPOffloadEnable88XX:1743]: ap_offload = 0x00000108
<3>[000032652ms] ***realtek*** [SetSAPPS88XX:1762]: SetSAPPS88XX H2CCommand[0]=7 H2CCommand[1]=70
<3>[000037555ms] init: untracked pid 704 exited
<6>[000038050ms] invalid lcd MainOLED_DispENon
<4>[000038880ms] CHG_STM:modem_notify_get_batt_info_callback, batt_volt 4005,batt_temp 35!
<4>[000039060ms] REB_DFT: ptable_part_num 20
<4>[000039070ms] Reb_DFT: find suited mtd idx
<4>[000039070ms] Reb_DFT: find suited mtd idx
<4>[000039070ms] Reb_DFT: find suited mtd idx
<4>[000039070ms] Reb_DFT: find suited mtd idx
<4>[000039070ms] Reb_DFT: find suited mtd idx
<4>[000039070ms] Reb_DFT: find suited mtd idx
<4>[000039070ms] Reb_DFT: find suited mtd idx
<4>[000039070ms] Reb_DFT: find suited mtd idx
<4>[000039070ms] Reb_DFT: find suited mtd idx
<4>[000039070ms] Reb_DFT: find suited mtd idx
<4>[000039070ms] Reb_DFT: find suited mtd idx
<4>[000039070ms] Reb_DFT get_random_num 1280275
<4>[000039070ms] Reb_DFT now random is 19, struct_idx is: 14
<4>[000039070ms] Reb_DFT at last random is 5
<4>[000039070ms] Reb_DFT: receive event 0
<4>[000039070ms]  
<3>[000042420ms] ***realtek*** [sdio_power_save_timer:6084]: ps_disable = 0, total_num = 0, pwr_state = 1, offload_ctl = 255
<3>[000042420ms] Wi-Fi<INFO>[wlan_set_driver_lock:1482]: Exit, wifi driver lock OFF
<4>[000045091ms] Reb_DFT:flash ctrl cfg is 0x00000483, flash ecc ctrl is 0x00000002
<4>[000045091ms] Reb_DFT:pt_ecc_bits is 4
<6>[000047095ms] invalid lcd MainOLED_DispENoff
<3>[000052653ms] init: untracked pid 713 exited
<3>[000067729ms] init: untracked pid 716 exited
<4>[000068882ms] CHG_STM:modem_notify_get_batt_info_callback, batt_volt 4008,batt_temp 35!
<4>[000069052ms] power_on_timeout_isr, system had been powered one minute ago
<4>[000069052ms]  #########  power_on_c_status_get = 0x00000003 ######## 
<4>[000069052ms] system power on ok!
<4>[000069052ms]  
<4>[000074498ms] FAT-fs (mmcblk0p1): utf8 is not a recommended IO charset for FAT filesystems, filesystem will be case sensitive!
<3>[000082807ms] init: untracked pid 725 exited
