root@p722:/ # dmesg
<6>[    0.000000] Booting Linux on physical CPU 0x0
<6>[    0.000000] Initializing cgroup subsys cpu
<6>[    0.000000] Initializing cgroup subsys cpuacct
<5>[    0.000000] Linux version 3.10.100+ (jenkins@localhost) (gcc version 4.7 (GCC) ) #1 PREEMPT Tue Dec 26 09:01:37 CST 2017
<4>[    0.000000] CPU: ARMv7 Processor [411fc0e2] revision 2 (ARMv7), cr=10c53c7d
<4>[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, VIPT aliasing instruction cache
<6>[    0.000000] Machine: HI6932 (Flattened Device Tree), model: HISILICON HI6932 board based on udp
<7>[    0.000000] power down charge p:0�, pd_charge_flag :0
<7>[    0.000000] run mode is normal, soft_run_mode = 0
<4>[    0.000000] Memory policy: ECC disabled, Data cache writeback
<7>[    0.000000] On node 0 totalpages: 36352
<7>[    0.000000] free_area_init_node: node 0, pgdat c0b9d0e4, node_mem_map c0f5f000
<7>[    0.000000]   Normal zone: 284 pages used for memmap
<7>[    0.000000]   Normal zone: 0 pages reserved
<7>[    0.000000]   Normal zone: 36352 pages, LIFO batch:7
<7>[    0.000000] pcpu-alloc: s0 r0 d32768 u32768 alloc=1*32768
<7>[    0.000000] pcpu-alloc: [0] 0 
<4>[    0.000000] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 36068
<5>[    0.000000] Kernel command line: root=/dev/ram0 rw console=ttyAMA0,115200 console=uw_tty0,115200 androidboot.hardware=hi6932_E5885Ls-93a loglevel=5 rdinit=/init mem=142m pd_charge=0� exc_flag=0 exc_type=9 save_flag=0 power_mode=normal 
<6>[    0.000000] PID hash table entries: 1024 (order: 0, 4096 bytes)
<6>[    0.000000] Dentry cache hash table entries: 32768 (order: 5, 131072 bytes)
<6>[    0.000000] Inode-cache hash table entries: 16384 (order: 4, 65536 bytes)
<6>[    0.000000] Memory: 142MB = 142MB total
<5>[    0.000000] Memory: 127584k/127584k available, 17824k reserved, 0K highmem
<5>[    0.000000] Virtual kernel memory layout:
<5>[    0.000000]     vector  : 0xffff0000 - 0xffff1000   (   4 kB)
<5>[    0.000000]     fixmap  : 0xfff00000 - 0xfffe0000   ( 896 kB)
<5>[    0.000000]     vmalloc : 0xc9000000 - 0xff000000   ( 864 MB)
<5>[    0.000000]     lowmem  : 0xc0000000 - 0xc8e00000   ( 142 MB)
<5>[    0.000000]     modules : 0xbf000000 - 0xc0000000   (  16 MB)
<5>[    0.000000]       .text : 0xc0008000 - 0xc0a75980   (10679 kB)
<5>[    0.000000]       .init : 0xc0a76000 - 0xc0abba34   ( 279 kB)
<5>[    0.000000]       .data : 0xc0abc000 - 0xc0badf80   ( 968 kB)
<5>[    0.000000]        .bss : 0xc0badf80 - 0xc0f5e1a4   (3777 kB)
<6>[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=1, Nodes=1
<6>[    0.000000] Preemptible hierarchical RCU implementation.
<6>[    0.000000] NR_IRQS:224
<2>[    0.000000] GIC CPU mask not found - kernel will fail to boot.
<2>[    0.000000] GIC CPU mask not found - kernel will fail to boot.
<6>[    0.000000] Architected cp15 timer(s) running at 19.20MHz (phys).
<6>[    0.000000] Switching to timer-based delay loop
<6>[    0.000000] sched_clock: ARM arch timer >56 bits at 19200kHz, resolution 52ns
<6>[    0.000000] sched_clock: 32 bits at 100 Hz, resolution 10000000ns, wraps every 4294967286ms
<6>[    0.000000] Calibrating delay loop (skipped), value calculated using timer frequency.. 38.40 BogoMIPS (lpj=192000)
<6>[    0.000000] pid_max: default: 32768 minimum: 301
<6>[    0.000000] Security Framework initialized
<6>[    0.000000] SELinux:  Disabled at boot.
<6>[    0.000000] Mount-cache hash table entries: 512
<6>[    0.000000] Initializing cgroup subsys debug
<6>[    0.000000] Initializing cgroup subsys freezer
<6>[    0.000000] CPU: Testing write buffer coherency: ok
<6>[    0.000000] Setting up static identity map for 0xc0703180 - 0xc07031d8
<6>[    0.000000] VFP support v0.3: implementor 41 architecture 3 part 30 variant e rev 0
<6>[    0.000000] regulator-dummy: no parameters
<3>[    0.000000] [sc]: <system_status_init> ok
<3>[    0.000000] [sc]: <dt_sysctrl_init> ok
<3>[    0.000000] [s_mem]: <bsp_shared_mem_init> shared_ddr phy=  a6180000, virt=  c9400000, size=    380000
<3>[    0.000000] [s_mem]: <bsp_shared_mem_init> ok!
<3>[    5.366000] timer: <bsp_slice_init> ok.
<6>[    5.375000] NET: Registered protocol family 16
<4>[    5.375000] 
<4>[    5.375000]  kiconconvInit enter 
<3>[    5.375000] [rdr]: <rdr_area_init> line = 293  ok!
<3>[    5.375000] [rdr]: <rdr_debug_init> line = 161  ok!
<3>[    5.375000] [rdr]: <rdr_module_init> line = 415  ok!
<3>[    5.375000] [rdr]: <rdr_core_init> line = 688  ok!
<3>[    5.375000] [rdr]: <rdr_bootcheck_init> line = 176  ok!
<3>[    5.375000] [adump]: <adump_mem_init> line = 347  ok!
<3>[    5.375000] [adump]: <adump_baseinfo_init> line = 156  ok!
<3>[    5.375000] [adump]: <adump_task_name_init> line = 268  ok!
<3>[    5.375000] [adump]: <adump_sche_switch_init> line = 445  ok!
<3>[    5.375000] [adump]: <adump_tasktcb_info_init> line = 162  ok
<3>[    5.375000] [adump]: <adump_lastkmsg_init> line = 80  ok!
<3>[    5.376000] [adump]: <adump_core_init> line = 407  alloc exc task statck buffer success
<3>[    5.376000] [adump]: <adump_core_init> line = 413  alloc user data buffer success
<3>[    5.376000] [adump]: <adump_core_init> line = 433  ok!
<3>[    5.376000] [adump]: <adump_exception_init> line = 184  ok!
<3>[    5.376000] [adump]: <adump_init> line = 454  ok!
<6>[    5.376000] DMA: preallocated 256 KiB pool for atomic coherent allocations
<4>[    5.386000] new_reg: event buffer(0) addr 0xc9061800
<4>[    5.386000] [spe_event_buffers_setup:] spe_event_buffers_setup, restore event lpos:0
<4>[    5.386000] new_reg: event buffer(1) addr 0xc9062000
<4>[    5.386000] [spe_event_buffers_setup:] spe_event_buffers_setup, restore event lpos:512
<4>[    5.386000] [spe_port_alloc:] spe_port_alloc, restore td pos td_free:0, td_busy:0
<4>[    5.386000] [spe_port_alloc:] spe_port_alloc, restore rd pos rd_free:0, rd_busy:0
<4>[    5.386000] new_reg: port 0 sit property to 0x19 write addr 0xc9060308 
<6>[    5.387000] hw-breakpoint: found 5 (+1 reserved) breakpoint and 4 watchpoint registers.
<6>[    5.387000] hw-breakpoint: maximum watchpoint size is 4 bytes.
<7>[    5.387000] gpiochip_add: registered GPIOs 0 to 7 on device: 2003f000.gpio
<7>[    5.388000] gpiochip_add: registered GPIOs 8 to 15 on device: 9002b000.gpio
<7>[    5.388000] gpiochip_add: registered GPIOs 16 to 23 on device: 9002c000.gpio
<7>[    5.388000] gpiochip_add: registered GPIOs 24 to 31 on device: 9002d000.gpio
<7>[    5.388000] gpiochip_add: registered GPIOs 32 to 39 on device: 9002e000.gpio
<7>[    5.388000] gpiochip_add: registered GPIOs 40 to 47 on device: 9002f000.gpio
<7>[    5.388000] gpiochip_add: registered GPIOs 48 to 55 on device: 90030000.gpio
<7>[    5.388000] gpiochip_add: registered GPIOs 56 to 63 on device: 90031000.gpio
<7>[    5.388000] gpiochip_add: registered GPIOs 64 to 71 on device: 90032000.gpio
<7>[    5.388000] gpiochip_add: registered GPIOs 72 to 79 on device: 90033000.gpio
<7>[    5.388000] gpiochip_add: registered GPIOs 80 to 87 on device: 90034000.gpio
<7>[    5.388000] gpiochip_add: registered GPIOs 88 to 95 on device: 90035000.gpio
<6>[    5.388000] Serial: AMBA PL011 UART driver
<6>[    5.389000] 90024000.uart: ttyAMA0 at MMIO 0x90024000 (irq = 102) is a PL011 rev0
<6>[    5.389000] console [ttyAMA0] enabled
<6>[    5.389000] 90025000.uart: ttyAMA1 at MMIO 0x90025000 (irq = 103) is a PL011 rev0
<6>[    5.389000] 90027000.uart: ttyAMA2 at MMIO 0x90027000 (irq = 223) is a PL011 rev0
<3>[    5.390000] [fiq]init OK
<3>[    5.390000] timer: <set_adp_timer_isr_and_pm>  ok
<3>[    5.390000] timer: <bsp_timer_probe> ok
<3>[    5.391000] softtimer init success
<3>[    5.391000] ipc probe success
<3>[    5.391000] [MODEM_DUMP]: <dump_area_init> dump_area_init finish
<3>[    5.391000] [MODEM_DUMP]: <bsp_dump_field_init> virt_area_addr = 0xc9aa0200 phy_area_addr = 0xa6120200 total_length = 0x28000 free_offset = 0x824 free_length=0x277dc
<3>[    5.391000] [MODEM_DUMP]: <bsp_dump_field_init> bsp_dump_field_init finish
<3>[    5.392000] [MODEM_DUMP]: <modem_dump_field_register> modem_dump_field_register finish
<3>[    5.392000] [MODEM_DUMP]: <bsp_dump_mem_init> bsp_dump_mem_init finish
<3>[    5.392000] icc: bsp_icc_init ok
<3>[    5.392000] [socp_logbuffer_mmap]:BufferSize or BufferAddr is invalid!
<3>[    5.392000] [pmu]: <pmu_pmic_init> pmussi addr: 0xc90ac000!
<3>[    5.393000] [pmu]: <pmic_ioshare_init> pmic ioshare init ok!
<3>[    5.394000] [pmu]: <pmic_volt_init> pmic volt init ok!
<3>[    5.394000] [pmu]: <pmic_dr_dts_init> init ok!
<3>[    5.394000] [pmu]: <pmic_dr_init> pmic dr init ok!
<6>[    5.394000] designware_i2c 90022000.i2c0: tx_fifo_depth: 64, rx_fifo_depth: 64
<6>[    5.395000] designware_i2c 90023000.i2c1: tx_fifo_depth: 64, rx_fifo_depth: 64
<6>[    5.399000] bio: create slab <bio-0> at 0
<6>[    5.399000] type tca6416, reg_addr 0x20, i2c_num 0, gpio_base 0x60, invert 0x0, irq_base -1 
<7>[    5.400000] gpiochip_add: registered GPIOs 96 to 111 on device: tca6416
<3>[    5.400000] [gpio_ex]: gpio ex init ok.
<3>[    5.400000] [regulator]: <regulator_pmic_dummy_init> <140>register dummy ops ok
<3>[    5.400000] [regulator]: <regulator_pmic_mtcmos_init> <276>register mtcmos ops ok
<6>[    5.400000] LDO5_VCC: 1800 <--> 2850 mV at 1800 mV 
<6>[    5.400000] LDO10_VCC: 2800 <--> 3300 mV at 2850 mV 
<6>[    5.401000] LDO9_VCC: 1800 <--> 3300 mV at 1800 mV 
<6>[    5.401000] Lvs0_VCC: 1800 mV 
<6>[    5.401000] DR1_VCC: 1 <--> 24 mV at 1 mV 1 <--> 24 mA at 1 mA 
<6>[    5.401000] DR2_VCC: 1 <--> 24 mV at 1 mV 1 <--> 24 mA at 1 mA 
<6>[    5.401000] DR3_VCC: 1 <--> 24 mV at 1 mV 1 <--> 24 mA at 1 mA 
<6>[    5.401000] mtcmos0: no parameters
<6>[    5.401000] mtcmos_usb: no parameters
<6>[    5.401000] adp1_VCC: 3 <--> 3300 mV 
<6>[    5.401000] adp2_VCC: 3 <--> 24 mV 
<6>[    5.402000] regulator_test: 3 <--> 24 mV 
<6>[    5.402000] regulator_test: supplied by adp2_VCC
<3>[    5.402000] [regulator]: <balong_regulator_probe> <559>regulator register ok
<6>[    5.402000] vgaarb: loaded
<1>[    5.402000] [lpm3 agent]: <lpm3_agent_init> line = 281  rdr register lpm3  0x85000001 exception success!
<1>[    5.402000] [lpm3 agent]: <lpm3_agent_init> line = 281  rdr register lpm3  0x85000002 exception success!
<4>[    5.402000] hwadp init ok.
<3>[    5.403000] [edma]:<bsp_edma_probe> <1606> edma 0 of_find_compatible_node not found
<3>[    5.403000] [pmu]: <pmic_irq_probe> pmic_irq_probe ok !
<6>[    5.404000] usbcore: registered new interface driver usbfs
<6>[    5.404000] usbcore: registered new interface driver hub
<6>[    5.404000] usbcore: registered new device driver usb
<6>[    5.404000] pps_core: LinuxPPS API ver. 1 registered
<6>[    5.404000] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
<6>[    5.404000] PTP clock support registered
<6>[    5.405000] cfg80211: Calling CRDA to update world regulatory domain
<1>[    5.640000] [PCIe]: Balong PCIe 0 Info: 2.5-Gbps Gen1, Lane: x1
<6>[    5.640000] PCI host bridge to bus 0000:00
<6>[    5.640000] pci_bus 0000:00: root bus resource [io  0x41000000-0x41ffffff]
<6>[    5.640000] pci_bus 0000:00: root bus resource [mem 0x42000000-0x49ffffff]
<6>[    5.640000] pci_bus 0000:00: No busn resource found for root bus, will use [bus 00-ff]
<7>[    5.640000] pci 0000:00:00.0: [19e5:6932] type 01 class 0x060400
<7>[    5.640000] pci 0000:00:00.0: supports D1 D2
<7>[    5.640000] pci 0000:00:00.0: PME# supported from D0 D1 D2 D3hot
<6>[    5.641000] PCI: bus0: Fast back to back transfers disabled
<6>[    5.641000] pci 0000:00:00.0: bridge configuration invalid ([bus 00-00]), reconfiguring
<7>[    5.641000] pci 0000:01:00.0: [19e5:1151] type 00 class 0x028000
<7>[    5.641000] pci 0000:01:00.0: reg 10: [mem 0x00000000-0x0003ffff]
<7>[    5.641000] pci 0000:01:00.0: supports D1 D2
<7>[    5.641000] pci 0000:01:00.0: PME# supported from D0 D1 D3hot
<6>[    5.659000] PCI: bus1: Fast back to back transfers disabled
<7>[    5.659000] pci_bus 0000:01: busn_res: [bus 01-ff] end is updated to 01
<7>[    5.659000] pci_bus 0000:00: busn_res: [bus 00-ff] end is updated to 01
<6>[    5.659000] pci 0000:00:00.0: BAR 8: assigned [mem 0x42000000-0x420fffff]
<6>[    5.659000] pci 0000:01:00.0: BAR 0: assigned [mem 0x42000000-0x4203ffff]
<6>[    5.659000] pci 0000:00:00.0: PCI bridge to [bus 01]
<6>[    5.659000] pci 0000:00:00.0:   bridge window [mem 0x42000000-0x420fffff]
<4>[    5.659000] PCI: enabling device 0000:00:00.0 (0140 -> 0143)
<6>[    5.659000] Switching to clocksource arch_sys_counter
<6>[    5.680000] bq27510-battery 0-0055: Normal Mode and read Firmware version=2150
<6>[    5.680000] bq27510-battery 0-0055: bq27510 support ver. 1.0.0 enabled
<4>[    5.680000] i2c-core: driver [bq27510-battery] using legacy suspend method
<4>[    5.680000] i2c-core: driver [bq27510-battery] using legacy resume method
<6>[    5.680000] NET: Registered protocol family 2
<6>[    5.681000] TCP established hash table entries: 2048 (order: 2, 16384 bytes)
<6>[    5.681000] TCP bind hash table entries: 2048 (order: 1, 8192 bytes)
<6>[    5.681000] TCP: Hash tables configured (established 2048 bind 2048)
<6>[    5.681000] TCP: reno registered
<6>[    5.681000] UDP hash table entries: 256 (order: 0, 4096 bytes)
<6>[    5.681000] UDP-Lite hash table entries: 256 (order: 0, 4096 bytes)
<6>[    5.681000] NET: Registered protocol family 1
<7>[    5.681000] PCI: CLS 64 bytes, default 64
<6>[    5.682000] (1, swapper)tc_mem_init: tc_mem_init
<3>[    5.683000] (1, swapper)tee_rdr_buffer_init: tee_rdr_buffer enter.
<6>[    5.683000] (1, swapper)tee_rdr_buffer_init: tee_rdr_buffer struct size 0x824.
<6>[    5.683000] (1, swapper)tee_rdr_buffer_init: tee_rdr_buffer log len,0x1f7dc.
<3>[    5.686000] (1, swapper)teeos_register_exception: register exception mem failed.
<6>[    5.687000] Trying to unpack rootfs image as initramfs...
<6>[    5.714000] Freeing initrd memory: 400K (c1208000 - c126c000)
<6>[    5.714000] hw perfevents: enabled with armv7_cortex_a17 PMU driver, 7 counters available
<6>[    5.715000] audit: initializing netlink socket (disabled)
<5>[    5.715000] type=2000 audit(0.349:1): initialized
<6>[    5.719000] exFAT: Version 1.2.9
<6>[    5.719000] fuse init (API version 7.22)
<7>[    5.720000] yaffs: yaffs built Dec 26 2017 08:59:24 Installing.
<6>[    5.720000] msgmni has been set to 249
<6>[    5.721000] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 249)
<6>[    5.721000] io scheduler noop registered
<6>[    5.721000] io scheduler deadline registered
<6>[    5.721000] io scheduler cfq registered (default)
<6>[    5.721000] pcieport 0000:00:00.0: Signaling PME through PCIe PME interrupt
<6>[    5.721000] pci 0000:01:00.0: Signaling PME through PCIe PME interrupt
<7>[    5.721000] pcie_pme 0000:00:00.0:pcie01: service driver pcie_pme loaded
<3>[    5.721000] [lcd]: <bsp_lcd_dts_init> LCD paramter read from dtsi,[lcd_id0:96][lcd_id1:101][lcd_rst:97][lcd_cd:51]
<6>[    5.725000] brd: module loaded
<6>[    5.727000] loop: module loaded
<4>[    5.727000] Hisilicon Nand Flash Controller Driver, Version 1.00
<4>[    5.727000] ecctype_onfi 6,writesize 800,oobsize 80,erasesize 20000,chipsize 10000000 spec_shmem->ecc_type 6
<6>[    5.727000] NAND device: Manufacturer ID: 0x01, Chip ID: 0xaa (AMD/Spansion NAND 256MiB 1,8V 8-bit), 256MiB, page size: 2048, OOB size: 128
<4>[    5.728000] NAND_ECC_NONE selected by board driver. This is not recommended!
<4>[    5.728000] mbb_reb_info_init:ecccorrectability=8!
<5>[    5.728000] Creating 36 MTD partitions on "9102b000.nandc":
<5>[    5.728000] 0x000000000000-0x000000080000 : "m3boot"
<5>[    5.728000] 0x000000080000-0x000000180000 : "fastboot"
<5>[    5.729000] 0x000000180000-0x000000280000 : "fastbootbk"
<5>[    5.729000] 0x000000280000-0x000000480000 : "nvbacklte"
<5>[    5.730000] 0x000000480000-0x000000680000 : "nvdefault"
<5>[    5.730000] 0x000000680000-0x000001080000 : "nvimg"
<5>[    5.730000] 0x000001080000-0x000001380000 : "nvdload"
<5>[    5.731000] 0x000001380000-0x000001680000 : "nvsys"
<5>[    5.731000] 0x000001680000-0x0000017c0000 : "oeminfo"
<5>[    5.732000] 0x0000017c0000-0x0000021c0000 : "kernel"
<5>[    5.732000] 0x0000021c0000-0x000002bc0000 : "kernelbk"
<5>[    5.732000] 0x000002bc0000-0x000002dc0000 : "dts"
<5>[    5.733000] 0x000002dc0000-0x000002fc0000 : "dtsbk"
<5>[    5.733000] 0x000002fc0000-0x0000030c0000 : "m3image"
<5>[    5.733000] 0x0000030c0000-0x0000031c0000 : "m3imagebk"
<5>[    5.734000] 0x0000031c0000-0x0000036c0000 : "teeos"
<5>[    5.734000] 0x0000036c0000-0x000003bc0000 : "teeosbk"
<5>[    5.735000] 0x000003bc0000-0x0000047c0000 : "userdata"
<7>[    5.735000] [*DLOAD_MTD*] fixed_fs_partitions:771: Partition userdata position fixed, Offset:3bc0000 Size:0xc00000
<7>[    5.735000] 
<5>[    5.736000] 0x0000047c0000-0x000008540000 : "online"
<7>[    5.736000] [*DLOAD_MTD*] fixed_fs_partitions:771: Partition online position fixed, Offset:47c0000 Size:0x3d80000
<7>[    5.736000] 
<5>[    5.736000] 0x000008540000-0x000009e40000 : "modem_fw"
<7>[    5.737000] [*DLOAD_MTD*] fixed_fs_partitions:771: Partition modem_fw position fixed, Offset:8540000 Size:0x1900000
<7>[    5.737000] 
<5>[    5.737000] 0x000009e40000-0x000009f40000 : "logo"
<5>[    5.738000] 0x000009f40000-0x00000a140000 : "wbdata"
<5>[    5.738000] 0x00000a140000-0x00000a640000 : "reserve3"
<7>[    5.739000] [*DLOAD_MTD*] fixed_fs_partitions:771: Partition reserve3 position fixed, Offset:a140000 Size:0x500000
<7>[    5.739000] 
<5>[    5.739000] 0x00000a640000-0x00000ae40000 : "om"
<7>[    5.740000] [*DLOAD_MTD*] fixed_fs_partitions:771: Partition om position fixed, Offset:a640000 Size:0x800000
<7>[    5.740000] 
<5>[    5.740000] 0x00000ae40000-0x00000c200000 : "app"
<7>[    5.740000] [*DLOAD_MTD*] fixed_fs_partitions:771: Partition app position fixed, Offset:ae40000 Size:0x13c0000
<7>[    5.740000] 
<5>[    5.741000] 0x00000c200000-0x00000d900000 : "webui"
<7>[    5.741000] [*DLOAD_MTD*] fixed_fs_partitions:771: Partition webui position fixed, Offset:c200000 Size:0x1700000
<7>[    5.741000] 
<5>[    5.742000] 0x00000d900000-0x00000f400000 : "system"
<7>[    5.742000] [*DLOAD_MTD*] fixed_fs_partitions:771: Partition system position fixed, Offset:d900000 Size:0x1b00000
<7>[    5.742000] 
<5>[    5.743000] 0x00000f400000-0x000010000000 : "cdromiso"
<7>[    5.743000] [*DLOAD_MTD*] fixed_fs_partitions:771: Partition cdromiso position fixed, Offset:f400000 Size:0xc00000
<7>[    5.743000] 
<5>[    5.744000] 0x000000000000-0x000000000000 : "nullMTD"
<5>[    5.744000] 0x000000000000-0x000000000000 : "nullMTD"
<5>[    5.744000] 0x000000000000-0x000000000000 : "nullMTD"
<5>[    5.745000] 0x000000000000-0x000000000000 : "nullMTD"
<5>[    5.745000] 0x000000000000-0x000000000000 : "nullMTD"
<5>[    5.746000] 0x000000000000-0x000000000000 : "nullMTD"
<5>[    5.746000] 0x000000000000-0x000000000000 : "nullMTD"
<5>[    5.746000] 0x000000000000-0x000000000000 : "nullMTD"
<4>[    5.747000] nandc_mtd_dload_proc_deal start 
<4>[    5.747000] smem_data->smem_dload_flag = 0x0!
<4>[    5.747000] nandc_mtd_dload_proc_deal end err = 0 
<3>[    5.747000] start mount early partition
<7>[    5.747000] going to mount /dev/block/mtdblock5  mount point /mnvm2:0
<6>[    5.747000] yaffs: dev is 32505861 name is "mtdblock5" rw
<6>[    5.747000] yaffs: passed flags ""
<7>[    5.747000] yaffs: yaffs: Attempting MTD mount of 31.5,"mtdblock5"
<7>[    5.749000] yaffs: yaffs_read_super: is_checkpointed 1
<3>[    5.749000] mount /mnvm2:0 success
<7>[    5.749000] going to mount /dev/block/mtdblock19  mount point /modem_fw
<6>[    5.749000] yaffs: dev is 32505875 name is "mtdblock19" ro
<6>[    5.749000] yaffs: passed flags ""
<7>[    5.749000] yaffs: yaffs: Attempting MTD mount of 31.19,"mtdblock19"
<7>[    5.878000] yaffs: yaffs_read_super: is_checkpointed 1
<3>[    5.878000] mount /modem_fw success
<7>[    5.878000] going to mount /dev/block/mtdblock23  mount point /modem_log
<6>[    5.878000] yaffs: dev is 32505879 name is "mtdblock23" rw
<6>[    5.878000] yaffs: passed flags ""
<7>[    5.878000] yaffs: yaffs: Attempting MTD mount of 31.23,"mtdblock23"
<7>[    5.879000] yaffs: yaffs_read_super: is_checkpointed 1
<3>[    5.879000] mount /modem_log success
<3>[    5.879000] end mount early partition
<4>[    5.879000] ------special_timer wakelock init ok ----------!
<4>[    5.880000] ------special_timer misc register leave!
<3>[    5.880000] [rfile]: <bsp_rfile_init> success.
<3>[    5.880000] loadps: 
<3>[    5.880000] loadps:  his_loadps_probe.
<3>[    5.880000] 
<3>[    5.880000] loadps:  <load_ps_task> entry.
<3>[    5.880000] 
<3>[    5.880000] loadps:  <his_loadps_probe> success.
<3>[    5.880000] 
<3>[    5.881000] socp_ind_delay_init:of_property_read_u32_array get size 0x200000!
<3>[    5.883000] socp_logbuffer_dmalloc success,  ulAddress 0xae400000, pucBuf 0xc9b01000. size 0x200000
<3>[    5.883000] the module has not been initialized!
<3>[    5.883000] [bsp_socp_ind_delay_init]:socp_ind_delay init sucess!
<3>[    5.884000] [socp_init]: succeed, base addr=0xc90ca000, irq num:46 !
<3>[    5.884000] [MODEM_DUMP]: <dump_base_info_init> dump_base_info_init finish
<3>[    5.884000] [MODEM_DUMP]: <dump_save_task_init> dump_save_task_init finish
<3>[    5.884000] [MODEM_DUMP]: <dump_map_mdm_ddr> mdm_ddr= 0,type=0
<3>[    5.884000] [MODEM_DUMP]: <dump_map_mdm_ddr> dump_memmap_modem_ddr finish
<3>[    5.885000] [nv]: <nv_init_dev> line = 3971  init modem nv dev ok
<3>[    5.885000] [nv]: <modem_nv_delay> line = 3805  modem nv wait for nv block device 0 s
<3>[    5.886000] Balong nv init  start! Dec 26 2017 09:00:24
<3>[    5.891000] [nv]: <nv_debug_init> line = 206  [debug info]debug file modem_log/drv/nv/debug_switch.txt not exist, not a error
<3>[    5.968000] load from /mnvm2:0/nv.bin current slice:0x2fbd6
<3>[    5.969000] [19700101000000-0002fc09]:[Normal] System Reboot [Soft Reboot]!
<3>[    5.969000] 
<3>[    5.972000] [rdr]: <rdr_save_file> line = 386  save /modem_log/dump/history.log finished!
<3>[    6.373000] [nv]: <bsp_nvm_kernel_init> line = 3624  reload success!
<4>[    6.374000] nvchar init end! major: 0xf8
<3>[    6.374000] Balong nv init ok!
<7>[    6.375000] parent_name_ptr =oeminfo 
<4>[    6.375000]  info :mtd->erasesize = 131072 ,mtd->writesize = 2048 
<7>[    6.375000] operation region index = 0 start_addr = 0 
<3>[    6.376000] smem_data->smem_online_upgrade_flag :0x0
<3>[    6.376000] smem_data->smem_multiupg_flag :0x0
<3>[    6.376000] his_modem_probe.
<6>[    6.382000] [sec]: <get_file_name> loading /modem_fw/sec_lphy.bin  image
<6>[    6.383000] [sec]: <get_file_name> file /modem_fw/sec_lphy.bin can't access, try unsec image
<6>[    6.383000] [sec]: <load_image> find file /modem_fw/lphy.bin, is_sec: 0
<6>[    6.383000] [sec]: <load_data_to_secos> need read file /modem_fw/lphy.bin 0xa00c0000 to 0x278000 though secos from offset 0x0
<6>[    6.421000] [sec]: <load_data_to_secos> trans data ot os: etype 0x2 ,run_addr 0xa00c0000, from 0xc0c0a180 to secos file_offset 0x0, bytes 0x20000 success
<6>[    6.442000] [sec]: <load_data_to_secos> trans data ot os: etype 0x2 ,run_addr 0xa00c0000, from 0xc0c0a180 to secos file_offset 0x20000, bytes 0x20000 success
<6>[    6.463000] [sec]: <load_data_to_secos> trans data ot os: etype 0x2 ,run_addr 0xa00c0000, from 0xc0c0a180 to secos file_offset 0x40000, bytes 0x20000 success
<6>[    6.484000] [sec]: <load_data_to_secos> trans data ot os: etype 0x2 ,run_addr 0xa00c0000, from 0xc0c0a180 to secos file_offset 0x60000, bytes 0x20000 success
<6>[    6.504000] [sec]: <load_data_to_secos> trans data ot os: etype 0x2 ,run_addr 0xa00c0000, from 0xc0c0a180 to secos file_offset 0x80000, bytes 0x20000 success
<6>[    6.525000] [sec]: <load_data_to_secos> trans data ot os: etype 0x2 ,run_addr 0xa00c0000, from 0xc0c0a180 to secos file_offset 0xa0000, bytes 0x20000 success
<6>[    6.546000] [sec]: <load_data_to_secos> trans data ot os: etype 0x2 ,run_addr 0xa00c0000, from 0xc0c0a180 to secos file_offset 0xc0000, bytes 0x20000 success
<6>[    6.567000] [sec]: <load_data_to_secos> trans data ot os: etype 0x2 ,run_addr 0xa00c0000, from 0xc0c0a180 to secos file_offset 0xe0000, bytes 0x20000 success
<6>[    6.588000] [sec]: <load_data_to_secos> trans data ot os: etype 0x2 ,run_addr 0xa00c0000, from 0xc0c0a180 to secos file_offset 0x100000, bytes 0x20000 success
<6>[    6.609000] [sec]: <load_data_to_secos> trans data ot os: etype 0x2 ,run_addr 0xa00c0000, from 0xc0c0a180 to secos file_offset 0x120000, bytes 0x20000 success
<6>[    6.629000] [sec]: <load_data_to_secos> trans data ot os: etype 0x2 ,run_addr 0xa00c0000, from 0xc0c0a180 to secos file_offset 0x140000, bytes 0x20000 success
<6>[    6.650000] [sec]: <load_data_to_secos> trans data ot os: etype 0x2 ,run_addr 0xa00c0000, from 0xc0c0a180 to secos file_offset 0x160000, bytes 0x20000 success
<6>[    6.671000] [sec]: <load_data_to_secos> trans data ot os: etype 0x2 ,run_addr 0xa00c0000, from 0xc0c0a180 to secos file_offset 0x180000, bytes 0x20000 success
<6>[    6.692000] [sec]: <load_data_to_secos> trans data ot os: etype 0x2 ,run_addr 0xa00c0000, from 0xc0c0a180 to secos file_offset 0x1a0000, bytes 0x20000 success
<6>[    6.713000] [sec]: <load_data_to_secos> trans data ot os: etype 0x2 ,run_addr 0xa00c0000, from 0xc0c0a180 to secos file_offset 0x1c0000, bytes 0x20000 success
<6>[    6.734000] [sec]: <load_data_to_secos> trans data ot os: etype 0x2 ,run_addr 0xa00c0000, from 0xc0c0a180 to secos file_offset 0x1e0000, bytes 0x20000 success
<6>[    6.755000] [sec]: <load_data_to_secos> trans data ot os: etype 0x2 ,run_addr 0xa00c0000, from 0xc0c0a180 to secos file_offset 0x200000, bytes 0x20000 success
<6>[    6.775000] [sec]: <load_data_to_secos> trans data ot os: etype 0x2 ,run_addr 0xa00c0000, from 0xc0c0a180 to secos file_offset 0x220000, bytes 0x20000 success
<6>[    6.796000] [sec]: <load_data_to_secos> trans data ot os: etype 0x2 ,run_addr 0xa00c0000, from 0xc0c0a180 to secos file_offset 0x240000, bytes 0x20000 success
<6>[    6.813000] [sec]: <load_data_to_secos> trans data ot os: etype 0x2 ,run_addr 0xa00c0000, from 0xc0c0a180 to secos file_offset 0x260000, bytes 0x18000 success
<3>[    6.813000] [sec]: <load_image> load image /modem_fw/lphy.bin to secos success
<3>[    6.814000] [sec]: <load_image> verify image /modem_fw/lphy.bin success
<6>[    6.814000] [sec]: <get_file_name> loading /modem_fw/sec_balong_modem.bin  image
<6>[    6.814000] [sec]: <get_file_name> file /modem_fw/sec_balong_modem.bin can't access, try unsec image
<6>[    6.814000] [sec]: <load_image> find file /modem_fw/balong_modem.bin, is_sec: 0
<6>[    6.814000] [sec]: <load_data_to_secos> need read file /modem_fw/balong_modem.bin 0xa1400000 to 0x7980ff though secos from offset 0x0
<6>[    6.852000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x0, bytes 0x20000 success
<6>[    6.872000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x20000, bytes 0x20000 success
<6>[    6.893000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x40000, bytes 0x20000 success
<6>[    6.914000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x60000, bytes 0x20000 success
<6>[    6.935000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x80000, bytes 0x20000 success
<6>[    6.956000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0xa0000, bytes 0x20000 success
<6>[    6.977000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0xc0000, bytes 0x20000 success
<6>[    6.997000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0xe0000, bytes 0x20000 success
<6>[    7.018000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x100000, bytes 0x20000 success
<6>[    7.039000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x120000, bytes 0x20000 success
<6>[    7.059000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x140000, bytes 0x20000 success
<6>[    7.080000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x160000, bytes 0x20000 success
<6>[    7.101000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x180000, bytes 0x20000 success
<6>[    7.122000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x1a0000, bytes 0x20000 success
<6>[    7.143000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x1c0000, bytes 0x20000 success
<6>[    7.164000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x1e0000, bytes 0x20000 success
<6>[    7.185000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x200000, bytes 0x20000 success
<6>[    7.205000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x220000, bytes 0x20000 success
<6>[    7.226000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x240000, bytes 0x20000 success
<6>[    7.247000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x260000, bytes 0x20000 success
<6>[    7.268000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x280000, bytes 0x20000 success
<6>[    7.289000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x2a0000, bytes 0x20000 success
<6>[    7.309000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x2c0000, bytes 0x20000 success
<6>[    7.330000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x2e0000, bytes 0x20000 success
<6>[    7.351000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x300000, bytes 0x20000 success
<6>[    7.372000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x320000, bytes 0x20000 success
<6>[    7.393000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x340000, bytes 0x20000 success
<6>[    7.414000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x360000, bytes 0x20000 success
<6>[    7.435000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x380000, bytes 0x20000 success
<6>[    7.455000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x3a0000, bytes 0x20000 success
<6>[    7.476000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x3c0000, bytes 0x20000 success
<6>[    7.497000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x3e0000, bytes 0x20000 success
<6>[    7.518000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x400000, bytes 0x20000 success
<6>[    7.539000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x420000, bytes 0x20000 success
<6>[    7.559000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x440000, bytes 0x20000 success
<6>[    7.580000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x460000, bytes 0x20000 success
<6>[    7.601000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x480000, bytes 0x20000 success
<6>[    7.622000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x4a0000, bytes 0x20000 success
<6>[    7.643000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x4c0000, bytes 0x20000 success
<6>[    7.664000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x4e0000, bytes 0x20000 success
<6>[    7.685000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x500000, bytes 0x20000 success
<6>[    7.705000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x520000, bytes 0x20000 success
<6>[    7.726000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x540000, bytes 0x20000 success
<6>[    7.747000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x560000, bytes 0x20000 success
<6>[    7.768000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x580000, bytes 0x20000 success
<6>[    7.789000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x5a0000, bytes 0x20000 success
<6>[    7.809000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x5c0000, bytes 0x20000 success
<6>[    7.830000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x5e0000, bytes 0x20000 success
<6>[    7.851000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x600000, bytes 0x20000 success
<6>[    7.872000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x620000, bytes 0x20000 success
<6>[    7.893000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x640000, bytes 0x20000 success
<6>[    7.914000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x660000, bytes 0x20000 success
<6>[    7.935000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x680000, bytes 0x20000 success
<6>[    7.955000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x6a0000, bytes 0x20000 success
<6>[    7.976000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x6c0000, bytes 0x20000 success
<6>[    7.997000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x6e0000, bytes 0x20000 success
<6>[    8.018000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x700000, bytes 0x20000 success
<6>[    8.039000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x720000, bytes 0x20000 success
<6>[    8.059000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x740000, bytes 0x20000 success
<6>[    8.080000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x760000, bytes 0x20000 success
<6>[    8.097000] [sec]: <load_data_to_secos> trans data ot os: etype 0x0 ,run_addr 0xa1400000, from 0xc0c0a180 to secos file_offset 0x780000, bytes 0x180ff success
<3>[    8.097000] [sec]: <load_image> load image /modem_fw/balong_modem.bin to secos success
<3>[    8.572000] [sec]: <load_image> verify image /modem_fw/balong_modem.bin success
<3>[    8.573000] load ccore image succeed
<3>[    8.573000] send ipc to unreset ccore succeed
<3>[    8.573000] [version]: <bsp_version_acore_init> bsp version acore init OK!
<4>[    8.573000] Enter ecall init
<4>[    8.573000] Finish ecall init
<3>[    8.573000] [om log]: init ok
<3>[    8.573000] hds_init ok!
<6>[    8.574000] ipf 91003000.ipf1: reset_peri_crg 0, 0, 0
<4>[    8.574000]  ipf version is 0x31333061
<3>[    8.574000] ipf 91003000.ipf1: ipf init success
<6>[    8.574000] psam 91040000.psam1: idle_p_ctrl 90000000, a00, 20
<1>[    8.574000] psam init ok!
<3>[    8.574000] [mem]: <bsp_mem_init> memory init OK!
<3>[    8.575000] notice: cp drx dump is not ready, try again in S/R
<3>[    8.575000] [modem log]: init ok
<3>[    8.575000] [applog]: <applog_init> 490  applog init success!
<3>[    8.575000] [dlock]: <bsp_dlock_init> acore nonsecure,do not operate secure sysctrl!
<3>[    8.575000] [nv]: <nv_readEx> line = 415  can not find 0xd157 !
<4>[    8.575000] balong packet snapshot init ok
<3>[    8.576000] [sci]: <bsp_sci_init> Acore: sci init ok 
<3>[    8.576000] [sci]: <sci_debug_status_print> sci_init_flag is 1 
<3>[    8.576000] [sci]: <sci_debug_status_print> sci0_card_satus is 0 
<3>[    8.576000] [sci]: <sci_debug_status_print> sci0_pmu_hpd_status is 0 
<3>[    8.576000] [sci]: <sci_debug_status_print> sci0_detect_level is 0 
<3>[    8.577000] system start....
<3>[    8.577000] [pmu]: <pmic_exc_probe> pmic exc init ok!
<3>[    8.577000] [pmu]: <pmic_version_get> version:6559
<3>[    8.577000] irq_reg&value:
<3>[    8.577000] 0x220=0x0 0x221=0x0 
<3>[    8.577000] 0x222=0x0 0x223=0x0 
<3>[    8.577000] 0x228=0x0 <3>[    8.577000] 
<3>[    8.577000] [pmu]: <pmic_om_wk_handler> record old reg&value:
<3>[    8.577000] 0x22a=0x0 0x22b=0x1 
<3>[    8.577000] event:hreset_n_f(normal)!
<3>[    8.577000] 0x22c=0x0 
<3>[    8.577000] 0x22d=0x0 0x22e=0x0 
<3>[    8.577000] 0x22f=0x0 0x230=0x0 
<3>[    8.577000] 
<3>[    8.577000] [pmu]: <pmic_om_wk_handler> record new reg&value:
<3>[    8.577000] 0x22a=0x0 0x22b=0x0 
<3>[    8.577000] 0x22c=0x0 0x22d=0x0 
<3>[    8.577000] 0x22e=0x0 0x22f=0x0 
<3>[    8.577000] 0x230=0x0 <3>[    8.577000] 
<6>[    8.610000] pmu_rtc rtc.23: rtc core: registered rtc.23 as rtc0
<3>[    8.610000] [rtc]:[func: pmu_rtc_probe],[line: 468]pmic RTC[0] init OK!
<3>[    8.610000] 
<3>[    8.610000] (1, swapper)tlogger_init: 11-29 tlogcat:start=0xc91c0e64      end=0xc91da200 len=0x1f7dc
<3>[    8.610000] [tem]: temperature init is ok.
<6>[    8.610000]  initialize thermal device.
<6>[    8.611000] Succeedded to initialize thermal device.
<3>[    8.612000] [amon] amon_soc_init:init ok
<3>[    8.612000] [amon] amon_cnt_init:amon_soc cnt init ok
<6>[    8.612000] coresight-tmc 90483000.etf: TMC initialized
<6>[    8.612000] coresight-tmc 904c2000.etf: TMC initialized
<6>[    8.613000] coresight-etm 904bc000.ptm: ETM initialized
<6>[    8.613000] coresight-etm 904fc000.ptm: ETM initialized
<6>[    8.613000] cpuidle: using governor ladder
<3>[    8.614000] [pm]:<pm_wakeup_interrupt_debug_init> <350> gic_dis_base map ok.
<3>[    8.614000] [pm]:<balong_pm_init> <513>  pm init ok 
<4>[    8.614000] APP_VCOM_Init entry,282246APP_VCOM_Init eixt,282254RNIC_InitNetCard: entry, 282254RNIC_InitNetCard: eixt, 282332Write power on log nv 0xd33b success.
<3>[    8.624000] [DMS_RegOmChanDataReadCB][LINE: 921] Invalid channel 1.
<4>[    8.625000] [spe_port_alloc:] spe_port_alloc, restore td pos td_free:0, td_busy:0
<4>[    8.625000] [spe_port_alloc:] spe_port_alloc, restore rd pos rd_free:0, rd_busy:0
<4>[    8.626000] new_reg: port 1 sit property to 0x15 write addr 0xc9060348 
<3>[    8.632000] the ind mode direct is already config!
<4>[    8.632000] SCM_RegCoderDestIndChan.
<4>[    8.632000] SCM_CODER_DST_ERR SCM_CoderDestReadCB: Get RD error , 10001, 0
<4>[    8.632000] Diag PowerOnLog false.
<4>[    8.632000] Diag PowerOnLog is close.
<4>[    8.632000] DMS_NLK_Init,entry,282835DMS_NLK_Init,exit,282836
<3>[    8.632000] [watchpoint]: <bsp_wp_init> line = 614  ok!
<3>[    8.632000] [HISI_SPI]: <hisi_spi_init> line = 696  start
<6>[    8.633000] hisi_spi 9001e000.spi: master is unqueued, this is deprecated
<6>[    8.634000] balong_lcd_spi spi0.0:  spidev_probe begin! 
<4>[    8.634000] lcd_spidev_probe is over!!!
<3>[    8.634000] [HISI_SPI]: <hisi_spi_init> line = 711  end
<3>[    8.634000] [HISI_SPI]: <spi_nor_flash_probe> line = 235  ok
<4>[    8.634000] set eth wakelock timeout 180
<3>[    8.978000] [MDOEM:0][TICK:15][NAS_DYNLOAD_RegLoadCallBack][LINE:454] NAS_DYNLOAD_RegLoadCallBack enRatMode=1, ulPid=139, pfInit=-1585523127, pfUnload=-1585523055
<3>[    8.978000] 
<3>[    8.995000] [MDOEM:0][TICK:17][NAS_DYNLOAD_RegLoadCallBack][LINE:454] NAS_DYNLOAD_RegLoadCallBack enRatMode=1, ulPid=133, pfInit=-1585868283, pfUnload=-1585868219
<3>[    8.995000] 
<3>[    8.999000] [MDOEM:0][TICK:17][NAS_MML_RegisterDumpCallBack][LINE:1710] register call back function finished
<3>[    9.005000] [MDOEM:0][TICK:18][NAS_DYNLOAD_RegLoadCallBack][LINE:454] NAS_DYNLOAD_RegLoadCallBack enRatMode=3, ulPid=217, pfInit=-1581571303, pfUnload=-1581571287
<3>[    9.005000] 
<3>[    9.011000] [MDOEM:0][TICK:18][TAF_MMA_InitTask][LINE:862] ulAutoInitPsFlg = 1
<4>[    9.011000] diag_BspRecvCmdList Rcv ccore cmd list, num: 0x2
<4>[    9.250000] Reg PCSC Func.
<4>[    9.250000] Update Card Status: 0 .
<3>[    9.250000] [MDOEM:0][TICK:42][TAF_MMA_SndATUsimmStatusInd][LINE:3664] 
<3>[    9.250000] TAF_MMA_SndATUsimmStatusInd: CardType: 255 , CardStatus: 0 , ulSenderPid: 157
<3>[    9.250000] 
<3>[    9.250000] AT_RcvAtMmaUsimStatusInd: CardType: 255 , CardStatus: 0 , ulSenderPid: 157
<3>[    9.250000] [MDOEM:0][TICK:42][TAF_MMA_RcvPihUsimStatusInd_PreProc][LINE:1976] MMA Rcv PIH Usim Status Ind, USIM CardType: 255,USIM CardService: 0, FSM ID: 1, FSM STATE = 1
<3>[    9.365000] [MDOEM:0][TICK:54][TAF_MMA_RcvUphyInitStatusInd_PreProc][LINE:1613] UPHY Init Status:0
<3>[    9.365000] [MDOEM:0][TICK:54][NAS_MSCC_SndMmcStartReq][LINE:2195] SEND MSG!
<3>[    9.366000] [MDOEM:0][TICK:54][NAS_MMC_ReadPlatformRatCapNvim][LINE:5840] read en_NV_Item_PLATFORM_RAT_CAP correct, RatNum = 3, aenRatList[0]= 0, aenRatList[1]= 1, aenRatList[2]= 2, aenRatList[3]= 4, aenRatList[4]= 4,aenRatList[5]= 4, aenRatList[6]= 4
<3>[    9.368000] [MDOEM:0][TICK:54][NAS_MMC_SndRatModeSwitchOnReq_SwitchOn][LINE:3988] Send start req to GAS!
<3>[    9.373000] [MDOEM:0][TICK:54][NAS_MMC_RcvGasStartCnf_SwitchOn_WaitGasStartCnf][LINE:1501] ulResult = 0
<3>[    9.373000] [MDOEM:0][TICK:54][NAS_MMC_SndRatModeSwitchOnReq_SwitchOn][LINE:3958] Send start req to LTE!
<3>[    9.380000] [MDOEM:0][TICK:55][NAS_MMC_RcvLmmStartCnf_SwitchOn_WaitLStartCnf][LINE:1924] ulResult = 0
<3>[    9.380000] [MDOEM:0][TICK:55][NAS_MMC_SndRatModeSwitchOnReq_SwitchOn][LINE:3974] Send start req to WRRC!
<3>[    9.383000] [MDOEM:0][TICK:55][NAS_MMC_RcvWasStartCnf_SwitchOn_WaitWasStartCnf][LINE:1664] FDD ulResult = 0
<3>[    9.383000] [MDOEM:0][TICK:55][NAS_Mmc_SndMsccStartCnf][LINE:2183] Send Msg!
<3>[    9.384000] [MDOEM:0][TICK:55][NAS_MSCC_SndMmaSwitchOnRsltCnf][LINE:2868] start result=0
<3>[    9.397000] [MDOEM:0][TICK:57][TAF_MMA_SndMsccStartReq][LINE:341] Send Msg!
<3>[    9.397000] [MDOEM:0][TICK:57][TAF_MMA_RcvMsccStartCnf_PhoneMode_WaitMsccStartCnf][LINE:1600] Rcv Mscc Start Cnf!!!
<3>[    9.397000] [MDOEM:0][TICK:57][TAF_MMA_ProcStartComplete_PhoneMode][LINE:2881] enPsInitRslt=1
<3>[    9.397000] Balong_power mdrv_set_modem_state:83 set state 1 ,time slice 9397.
<4>[    9.749000] AR8035 start phy reset PIN:22
<4>[    9.749000] AR8035 phy driver register
<6>[    9.749000] tun: Universal TUN/TAP device driver, 1.6
<6>[    9.749000] tun: (C) 1999-2004 Max Krasnyansky <maxk@qualcomm.com>
<6>[    9.750000]  Enable RX Mitigation via HW Watchdog Timer
<4>[    9.750000] get_phy_device,phy_id is 4dd072!
<6>[    9.751000] libphy: stmmac: probed
<6>[    9.751000] eth0: PHY ID 004dd072 at 4 IRQ POLL (stmmac-0:04) active
<4>[    9.751000] [spe_port_alloc:] spe_port_alloc, restore td pos td_free:0, td_busy:0
<4>[    9.751000] [spe_port_alloc:] spe_port_alloc, restore rd pos rd_free:0, rd_busy:0
<4>[    9.751000] new_reg: port 2 sit property to 0x1 write addr 0xc9060388 
<6>[    9.751000] PPP generic driver version 2.4.2
<6>[    9.751000] PPP BSD Compression module registered
<6>[    9.751000] PPP Deflate Compression module registered
<6>[    9.751000] PPP MPPE Compression module registered
<6>[    9.751000] NET: Registered protocol family 24
<6>[    9.751000] SLIP: version 0.8.4-NET3.019-NEWTTY (dynamic channels, max=256).
<6>[    9.751000] bq24192 0-006b: CHG_HUAWEI_CHARGER:chargeIC_probe: Begin:***chargeIC_probe***
<4>[    9.752000] CHG_HUAWEI_CHARGER: chargeIC_probe: ***creat proc filesystem***
<6>[    9.752000] bq24192 0-006b: CHG_HUAWEI_CHARGER:chargeIC_probe: chargeIC probed successfully, devreg_rev=3
<6>[    9.752000] bq24192 0-006b: CHG_HUAWEI_CHARGER:chargeIC_probe: g_i2c_client->addr [0x6B]
<3>[    9.970000] read itemid = 36
<3>[    9.971000] [hisi coul]hisi_coul_init
<3>[    9.988000] huawei,bq_bci_battery huawei,bq_bci_battery: bq_bci probe ok!
<3>[    9.989000] read itemid = 36
<3>[    9.990000] set usb_vbus_status 0
<5>[    9.990000] usb is not connect in boot
<4>[    9.990000] bsp_usb_adapter_init line 2015
<3>[    9.990000] U_NET(TRACE) usb_prealloc_eth_rx_mem() line:4020 : usb_prealloc_eth_rx_mem : 0, 2,   (null)
<3>[    9.990000] U_NET(TRACE) usb_prealloc_eth_rx_mem() line:4040 : usb_prealloc_eth_rx_mem : allocmem num=51, size=16384
<4>[    9.990000] [spe_port_alloc:] spe_port_alloc, restore td pos td_free:0, td_busy:0
<4>[    9.990000] [spe_port_alloc:] spe_port_alloc, restore rd pos rd_free:0, rd_busy:0
<4>[    9.990000] new_reg: port 3 sit property to 0x9 write addr 0xc90603c8 
<3>[    9.990000] U_NCM(TRACE) usb_ncm_init() line:4625 : ncm spe port alloc suscess
<3>[    9.990000] U_PNP(ERROR) pnp_register_usb_support_function() line:471 : port'acm' authenticate failed can not be used
<3>[    9.990000] U_PNP(ERROR) pnp_register_usb_support_function() line:471 : port'3g_modem' authenticate failed can not be used
<3>[    9.990000] U_PNP(ERROR) pnp_register_usb_support_function() line:471 : port'3g_diag' authenticate failed can not be used
<3>[    9.990000] U_PNP(ERROR) pnp_register_usb_support_function() line:471 : port'c_shell' authenticate failed can not be used
<3>[    9.990000] U_PNP(ERROR) pnp_register_usb_support_function() line:471 : port'pcsc' authenticate failed can not be used
<3>[    9.990000] U_PNP(ERROR) pnp_register_usb_support_function() line:471 : port'voice' authenticate failed can not be used
<3>[    9.990000] U_PNP(ERROR) pnp_register_usb_support_function() line:471 : port'm2m_gps' authenticate failed can not be used
<3>[    9.991000] U_PNP(TRACE) usb_android_driver_init() line:157 : 
<3>[    9.991000] U_OTG(ERROR) otg_dev_request_source() line:78 : GPIO_OTG_ID_SET or GPIO_OTG_ID_SET is invalid
<3>[    9.991000] U_OTG(ERROR) otg_dev_register_id_irq() line:602 : usb_id_det_gpio is invalid
<3>[    9.991000] U_HOTPLUG(TRACE) mbb_usb_status_change_ex() line:558 : error status:0
<3>[    9.991000] [key]: balong gpio key init!
<3>[    9.991000] [key]: balong key driver probes start!
<6>[    9.991000] input: gpio_keys.30 as /devices/gpio_keys.30/input/input0
<7>[    9.991000] evbug: Connected device: input0 (gpio_keys.30 at unknown)
<3>[    9.991000] [key]: menu key is release. 
<3>[    9.991000] [key]: reset key is release. 
<3>[    9.991000] [key]: power key is release. 
<3>[    9.991000] [key]: balong gpio key driver probes end!
<6>[    9.992000] i2c /dev entries driver
<6>[    9.992000] m24sr02 0-0056: HUAWEI_NFC:huawei_nfc_probe:***huawei_nfc_probe***
<4>[    9.992000] HUAWEI_NFC: trying to request irq: m24sr02-3
<4>[    9.992000] HUAWEI_NFC: Init NFC start!
<3>[   10.004000] huawei,bq_bci_battery huawei,bq_bci_battery: batt soc changed, new soc=22 
<4>[   10.425000] HUAWEI_NFC: Init NFC finish!
<3>[   10.426000] [wdt]:wdt init ok
<6>[   10.426000] cpufreq: balongv7r2 CPU frequency driver.
<3>[   10.426000] [cpufreq]: <balong_cpufreq_cpu_init> <521>cpufreq: balong_cpufreq_cpu_init.
<3>[   10.427000] [cpufreq]: <cpufreq_init> <609>cpufreq init ok
<6>[   10.427000] cpuidle: using governor menu
<6>[   10.427000] Synopsys Designware Multimedia Card Interface Driver
<3>[   10.427000] LDO10_VCC: unsupportable voltage range: 2800000-1800000uV
<6>[   10.427000] dwmmc_balong 910fc000.dwmmc0: fifo-depth property not found, using value of FIFOTH register as default
<4>[   10.428000] resetting block ok
<6>[   10.428000] dwmmc_balong 910fc000.dwmmc0: Using internal DMA controller.
<6>[   10.428000] dwmmc_balong 910fc000.dwmmc0: Version ID is 270a
<6>[   10.428000] dwmmc_balong 910fc000.dwmmc0: DW MMC controller at irq 107, 32 bit host data width, 256 deep fifo
<7>[   10.428000] mmc_host mmc0: card is present
<7>[   10.428000] of_get_named_gpio_flags: can't parse gpios property
<7>[   10.428000] mmc0: clock 0Hz busmode 2 powermode 1 cs 0 Vdd 21 width 0 timing 0
<7>[   10.439000] mmc0: clock 400000Hz busmode 2 powermode 2 cs 0 Vdd 21 width 0 timing 0
<3>[   10.439000] dwmmc_balong 910fc000.dwmmc0: ios->clock: 400000 priv->clock: 0
<6>[   10.441000] mmc_host mmc0: Bus speed (slot 0) = 17500000Hz (slot req 400000Hz, actual 397727HZ div = 22)
<7>[   10.459000] mmc_host mmc0: card is present
<7>[   10.459000] mmc_host mmc0: card is present
<6>[   10.459000] mmc0: mmc_rescan_try_freq: trying to init card at 400000 Hz
<7>[   10.459000] mmc0: starting CMD52 arg 00000c00 flags 00000195
<7>[   10.459000] dwmmc_balong 910fc000.dwmmc0: start command: ARGR=0x00000c00 CMDR=0x2000a174 CMD(52)
<6>[   10.459000] dwmmc_balong 910fc000.dwmmc0: 1 slots initialized
<6>[   10.460000] usbcore: registered new interface driver usbhid
<6>[   10.460000] usbhid: USB HID core driver
<3>[   10.460000] clk_remote_init using icc ok
<3>[   10.460000] 
<3>[   10.460000]  [Mbb Common Drv] Mbb_Common_Probe!
<7>[   10.460000] mmc0: req done (CMD52): -110: 00000000 00000000 00000000 00000000
<7>[   10.460000] mmc0: starting CMD52 arg 80000c08 flags 00000195
<7>[   10.460000] dwmmc_balong 910fc000.dwmmc0: start command: ARGR=0x80000c08 CMDR=0x20002174 CMD(52)
<3>[   10.460000] Wi-Fi<INFO>[wifi_netlink_chunnel_init:1599]: enter
<3>[   10.460000] Wi-Fi<INFO>[wifi_netlink_chunnel_init:1621]: exit
<3>[   10.460000] Wi-Fi<INFO>[wlan_reg_driver_lock:1798]: Exit, wifi driver lock Register
<3>[   10.460000] Wi-Fi<INFO>[wlan_stus_timer_start:804]: wlan_stus_timer_started!!!!
<3>[   10.460000] Wi-Fi<INFO>[wlan_at_reg_chip:1177]: chip 13 = (unknown) reg   (null) to c0b7a444
<3>[   10.461000] Wi-Fi<INFO>[wlan_at_reg_chip:1183]: Exit, g_cur_chip= 13
<3>[   10.461000] 
<3>[   10.461000] Wi-Fi<INFO>[wlan_wt_init:1238]: enter curr_chip 13 = (unknown)
<3>[   10.461000] Wi-Fi<INFO>[wlan_wt_init:1244]: chip 13 = (unknown) reg to c0b7a444
<3>[   10.461000] Wi-Fi<INFO>[wlan_wt_init:1248]: exit
<3>[   10.461000] read itemid = 36
<3>[   10.461000] init stat time proc_mlog_log_init 595 
<7>[   10.461000] [*DLOAD_NARK_API*] nark_api_init:834: nark api module init.
<3>[   10.461000] [subnet_adapter]: status=0 len=0
<3>[   10.461000] loadps:  bsp_load_ps_callback wakeup loadps task
<3>[   10.461000] 
<3>[   10.461000] loadps:  start load_ps_task .
<3>[   10.461000] 
<3>[   10.461000] loadps:  success take g_loadpsMain.task_mutex elapsed wakeuptime 0ms time.
<3>[   10.461000] 
<3>[   10.461000] loadps: icc read addr 0xa3036000 size 0x5735c0.
<3>[   10.461000] 
<3>[   10.461000] loadps:  start load image to sram .
<3>[   10.461000] 
<7>[   10.461000] mmc0: req done (CMD52): -110: 00000000 00000000 00000000 00000000
<6>[   10.464000] [sec]: <get_file_name> loading /modem_fw/sec_was.bin  image
<6>[   10.464000] [sec]: <get_file_name> file /modem_fw/sec_was.bin can't access, try unsec image
<6>[   10.464000] [sec]: <load_image> find file /modem_fw/was.bin, is_sec: 0
<6>[   10.464000] [sec]: <load_data_to_secos> need read file /modem_fw/was.bin 0xa3036000 to 0x2e1b80 though secos from offset 0x0
<7>[   10.498000] mmc0: clock 400000Hz busmode 2 powermode 2 cs 1 Vdd 21 width 0 timing 0
<7>[   10.499000] mmc0: starting CMD0 arg 00000000 flags 000000c0
<7>[   10.499000] dwmmc_balong 910fc000.dwmmc0: start command: ARGR=0x00000000 CMDR=0x20002000 CMD(0)
<7>[   10.499000] mmc0: req done (CMD0): 0: 00000000 00000000 00000000 00000000
<7>[   10.500000] mmc0: clock 400000Hz busmode 2 powermode 2 cs 0 Vdd 21 width 0 timing 0
<7>[   10.501000] mmc0: starting CMD8 arg 000001aa flags 000002f5
<7>[   10.501000] dwmmc_balong 910fc000.dwmmc0: start command: ARGR=0x000001aa CMDR=0x20002148 CMD(8)
<6>[   10.501000] ftyreset module initialized.
<7>[   10.502000] mmc0: req done (CMD8): -110: 00000000 00000000 00000000 00000000
<6>[   10.502000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x0, bytes 0x20000 success
<7>[   10.519000] mmc0: starting CMD5 arg 00000000 flags 000002e1
<7>[   10.519000] dwmmc_balong 910fc000.dwmmc0: start command: ARGR=0x00000000 CMDR=0x20002045 CMD(5)
<6>[   10.519000] [HWLOCK] drv verify simlock init ok!
<6>[   10.519000] oprofile: using timer interrupt.
<6>[   10.520000] u32 classifier
<6>[   10.520000]     Performance counters on
<6>[   10.520000] Netfilter messages via NETLINK v0.30.
<6>[   10.520000] nf_conntrack version 0.5.0 (1999 buckets, 7996 max)
<6>[   10.520000] ctnetlink v0.93: registering with nfnetlink.
<6>[   10.520000] IPVS: Registered protocols ()
<6>[   10.520000] IPVS: Connection hash table configured (size=4096, memory=32Kbytes)
<6>[   10.520000] IPVS: Creating netns size=736 id=0
<6>[   10.520000] IPVS: ipvs loaded.
<6>[   10.521000] ip_tables: (C) 2000-2006 Netfilter Core Team
<6>[   10.521000] arp_tables: (C) 2002 David S. Miller
<6>[   10.521000] TCP: cubic registered
<6>[   10.521000] NET: Registered protocol family 10
<6>[   10.522000] ip6_tables: (C) 2000-2006 Netfilter Core Team
<6>[   10.523000] NET: Registered protocol family 17
<6>[   10.523000] NET: Registered protocol family 15
<6>[   10.523000] Ebtables v2.0 registered
<7>[   10.523000] mmc0: req failed (CMD5): -110, retrying...
<7>[   10.523000] dwmmc_balong 910fc000.dwmmc0: start command: ARGR=0x00000000 CMDR=0x20002045 CMD(5)
<7>[   10.524000] mmc0: req failed (CMD5): -110, retrying...
<7>[   10.524000] dwmmc_balong 910fc000.dwmmc0: start command: ARGR=0x00000000 CMDR=0x20002045 CMD(5)
<6>[   10.524000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x20000, bytes 0x20000 success
<7>[   10.529000] dwmmc_balong 910fc000.dwmmc0: irq mmc debnce 0xffffff ,mmc status0x6,timestamp0x5438f,cd1
<7>[   10.541000] mmc_host mmc0: card is not present
<7>[   10.541000] mmc0: req failed (CMD5): -110, retrying...
<7>[   10.541000] dwmmc_balong 910fc000.dwmmc0: start command: ARGR=0x00000000 CMDR=0x20002045 CMD(5)
<7>[   10.542000] mmc0: req done (CMD5): -110: 00000000 00000000 00000000 00000000
<6>[   10.542000] mmc_attach_sd:in
<7>[   10.542000] mmc0: starting CMD55 arg 00000000 flags 000000f5
<7>[   10.542000] dwmmc_balong 910fc000.dwmmc0: start command: ARGR=0x00000000 CMDR=0x20002177 CMD(55)
<6>[   10.542000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x40000, bytes 0x20000 success
<7>[   10.543000] mmc0: req done (CMD55): -110: 00000000 00000000 00000000 00000000
<7>[   10.559000] mmc0: starting CMD55 arg 00000000 flags 000000f5
<7>[   10.559000] dwmmc_balong 910fc000.dwmmc0: start command: ARGR=0x00000000 CMDR=0x20002177 CMD(55)
<7>[   10.560000] mmc0: req done (CMD55): -110: 00000000 00000000 00000000 00000000
<7>[   10.560000] mmc0: starting CMD55 arg 00000000 flags 000000f5
<7>[   10.560000] dwmmc_balong 910fc000.dwmmc0: start command: ARGR=0x00000000 CMDR=0x20002177 CMD(55)
<6>[   10.560000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x60000, bytes 0x20000 success
<7>[   10.561000] mmc0: req done (CMD55): -110: 00000000 00000000 00000000 00000000
<7>[   10.577000] mmc0: starting CMD55 arg 00000000 flags 000000f5
<7>[   10.577000] dwmmc_balong 910fc000.dwmmc0: start command: ARGR=0x00000000 CMDR=0x20002177 CMD(55)
<6>[   10.577000] l2tp_core: L2TP core driver, V2.0
<6>[   10.577000] l2tp_ppp: PPPoL2TP kernel driver, V2.0
<6>[   10.577000] 8021q: 802.1Q VLAN Support v1.8
<7>[   10.577000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [2290] [atp_proc_init] /proc/app_proc NOT exist !
<7>[   10.577000] 
<7>[   10.577000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [506] [atp_proc_create_prsite] /proc/app_proc/prsite NOT exist !!!
<7>[   10.577000] 
<7>[   10.577000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [50] [atp_proc_create_file] will create file: addr
<7>[   10.577000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [50] [atp_proc_create_file] will create file: mask
<7>[   10.577000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [50] [atp_proc_create_file] will create file: actionmode
<7>[   10.578000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [50] [atp_proc_create_file] will create file: location
<7>[   10.578000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [50] [atp_proc_create_file] will create file: times
<7>[   10.578000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [50] [atp_proc_create_file] will create file: rand
<7>[   10.578000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [50] [atp_proc_create_file] will create file: multiuserenable
<7>[   10.578000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [50] [atp_proc_create_file] will create file: delmac
<7>[   10.578000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [997] [atp_proc_create_dial] /proc/app_proc/dial NOT exist !!!
<7>[   10.578000] 
<7>[   10.578000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [50] [atp_proc_create_file] will create file: wlan_dev_name
<7>[   10.578000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [50] [atp_proc_create_file] will create file: eth_is_lan
<7>[   10.578000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [50] [atp_proc_create_file] will create file: report_timeout
<7>[   10.578000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [1368] [atp_proc_create_guestwifiaccessui] /proc/app_proc/guestwifiaccessui NOT exist !!!
<7>[   10.578000] 
<7>[   10.578000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [50] [atp_proc_create_file] will create file: ifaccess
<6>[   10.578000] ebt_time registered
<7>[   10.578000] mmc0: req done (CMD55): -110: 00000000 00000000 00000000 00000000
<6>[   10.578000] mmc_attach_sd:mmc_send_app_op_cond error!-110
<7>[   10.578000] mmc0: clock 400000Hz busmode 1 powermode 2 cs 0 Vdd 21 width 0 timing 0
<7>[   10.578000] mmc0: starting CMD1 arg 00000000 flags 000000e1
<7>[   10.578000] dwmmc_balong 910fc000.dwmmc0: start command: ARGR=0x00000000 CMDR=0x20002041 CMD(1)
<7>[   10.579000] mmc0: req done (CMD1): -110: 00000000 00000000 00000000 00000000
<7>[   10.579000] mmc0: clock 0Hz busmode 1 powermode 0 cs 0 Vdd 0 width 0 timing 0
<7>[   10.580000] mmc_host mmc0: card is not present
<7>[   10.580000] mmc_host mmc0: card is not present
<7>[   10.580000] mmc_host mmc0: card is not present
<7>[   10.580000] mmc_host mmc0: card is not present
<4>[   10.580000] nf_nat_rtsp v0.6.21 loading
<4>[   10.580000] nf_conntrack_rtsp v0.6.21 loading
<6>[   10.581000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x80000, bytes 0x20000 success
<6>[   10.599000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0xa0000, bytes 0x20000 success
<6>[   10.617000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0xc0000, bytes 0x20000 success
<6>[   10.635000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0xe0000, bytes 0x20000 success
<7>[   10.652000] his_boot_init.
<7>[   10.652000] #########  power_on_reboot_flag_set = 0xFFFFFFFF ######## 
<7>[   10.652000] #########  power_on_start_reason_get = 0x504F5752 ######## 
<4>[   10.652000] system power on time:  70-00-01 00:00:05
<4>[   10.653000] [onoff]bsp_power_ctrl_read_cb is called, msg: 0x0
<4>[   10.653000] bsp_coresight_init: init ok
<6>[   10.653000] pmu_rtc rtc.23: setting system clock to 1970-01-01 01:12:15 UTC (4335)
<6>[   10.656000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x100000, bytes 0x20000 success
<6>[   10.673000] Freeing unused kernel memory: 276K (c0a76000 - c0abb000)
<6>[   10.675000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x120000, bytes 0x20000 success
<11>[   10.693000] init: open touche5 skintype failed 
<6>[   10.700000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x140000, bytes 0x20000 success
<6>[   10.718000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x160000, bytes 0x20000 success
<6>[   10.736000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x180000, bytes 0x20000 success
<6>[   10.754000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x1a0000, bytes 0x20000 success
<6>[   10.772000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x1c0000, bytes 0x20000 success
<6>[   10.790000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x1e0000, bytes 0x20000 success
<6>[   10.808000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x200000, bytes 0x20000 success
<6>[   10.830000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x220000, bytes 0x20000 success
<6>[   10.848000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x240000, bytes 0x20000 success
<6>[   10.870000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x260000, bytes 0x20000 success
<6>[   10.888000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x280000, bytes 0x20000 success
<6>[   10.906000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x2a0000, bytes 0x20000 success
<6>[   10.924000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x2c0000, bytes 0x20000 success
<6>[   10.926000] [sec]: <load_data_to_secos> trans data ot os: etype 0x5 ,run_addr 0xa3036000, from 0xc0c0a180 to secos file_offset 0x2e0000, bytes 0x1b80 success
<3>[   10.926000] [sec]: <load_image> load image /modem_fw/was.bin to secos success
<3>[   10.930000] [sec]: <load_image> verify image /modem_fw/was.bin success
<3>[   10.930000] loadps:  complete load image to sram result 0 total load_ps_image time 469 ms.
<3>[   10.930000] 
<3>[   10.930000] loadps: load image complete.
<3>[   10.930000] 
<6>[   10.943000] [Mbb Common Drv] module=(MMC),mlogbuf.len =(57),read len(124),len(124),lv=(2),msg: the rat is 2!,the search type is MMC_LMM_PLMN_SRCH_ANY!
<6>[   10.943000] .
<11>[   11.980000] init: /init.rc: 23: export requires 2 arguments
<11>[   12.041000] init: /dev/hw_random not found
<6>[   12.043000] yaffs: dev is 32505882 name is "mtdblock26" ro
<6>[   12.043000] yaffs: passed flags ""
<7>[   12.043000] yaffs: yaffs: Attempting MTD mount of 31.26,"mtdblock26"
<7>[   12.162000] yaffs: yaffs_read_super: is_checkpointed 1
<6>[   12.162000] yaffs: dev is 32505880 name is "mtdblock24" ro
<6>[   12.162000] yaffs: passed flags ""
<7>[   12.162000] yaffs: yaffs: Attempting MTD mount of 31.24,"mtdblock24"
<7>[   12.283000] yaffs: yaffs_read_super: is_checkpointed 1
<6>[   12.284000] yaffs: dev is 32505881 name is "mtdblock25" ro
<6>[   12.284000] yaffs: passed flags ""
<7>[   12.284000] yaffs: yaffs: Attempting MTD mount of 31.25,"mtdblock25"
<7>[   12.403000] yaffs: yaffs_read_super: is_checkpointed 1
<6>[   12.403000] yaffs: dev is 32505873 name is "mtdblock17" rw
<6>[   12.403000] yaffs: passed flags ""
<7>[   12.403000] yaffs: yaffs: Attempting MTD mount of 31.17,"mtdblock17"
<7>[   12.405000] yaffs: yaffs_read_super: is_checkpointed 1
<6>[   12.406000] yaffs: dev is 32505878 name is "mtdblock22" rw
<6>[   12.406000] yaffs: passed flags ""
<7>[   12.406000] yaffs: yaffs: Attempting MTD mount of 31.22,"mtdblock22"
<7>[   12.474000] yaffs: 3 blocks to be sorted...
<7>[   12.490000] yaffs: yaffs_read_super: is_checkpointed 0
<6>[   12.491000] yaffs: dev is 32505874 name is "mtdblock18" rw
<6>[   12.491000] yaffs: passed flags ""
<7>[   12.491000] yaffs: yaffs: Attempting MTD mount of 31.18,"mtdblock18"
<7>[   12.494000] yaffs: yaffs_read_super: is_checkpointed 1
<11>[   12.538000] init: /dev/hw_random not found
<11>[   12.554000] init: Unable to open persistent property directory /data/property errno: 2
<3>[   12.780000] [hisi coul]charger event = 0x5 
<6>[   12.896000] yaffs: dev is 32505883 name is "mtdblock27" rw
<6>[   12.896000] yaffs: passed flags ""
<7>[   12.896000] yaffs: yaffs: Attempting MTD mount of 31.27,"mtdblock27"
<7>[   12.950000] [*DLOAD_NARK_API*] visit_dload_smem:374: dload visit smem  vist = 8.
<7>[   13.030000] yaffs: yaffs_read_super: is_checkpointed 1
<6>[   13.412000] [kernel space] data receive from user_pid 162 are 0x0
<6>[   13.920000] CHG_HUAWEI_CHARGER: poweron_chg_proc_read: is_powdown_charging=0!
<4>[   14.223000] [nvdev_read]kbuf->type=35,mac_num=4
<4>[   14.223000] [nvdev_read]kbuf->type=37,mac_num=1
<4>[   14.223000] [nvdev_read]kbuf->type=52,mac_num=0
<4>[   14.223000] [nvdev_read]kbuf->type=51,mac_num=0
<3>[   14.223000] The request nv is not support here or para is err, kbuf->type = 71,count = 16
<4>[   14.594000] device_event_input entry
<3>[   14.594000] device_event_input: event handler is NOT registered
<4>[   15.665000] received netlink message payload from pid 226:0:16:10
<4>[   16.370000] At_QryHFreqinfo:current rat is not LTE.
<6>[   16.397000] IPv6: ADDRCONF(NETDEV_UP): br0: link is not ready
<6>[   16.406000] device rmnet2 entered promiscuous mode
<6>[   16.406000] br0: port 1(rmnet2) entered forwarding state
<6>[   16.406000] br0: port 1(rmnet2) entered forwarding state
<6>[   16.409000] IPv6: ADDRCONF(NETDEV_CHANGE): br0: link becomes ready
<4>[   16.724000] AR8035 phy driver configinit
<4>[   16.724000] ar8035 power on
<4>[   17.012000] ------------[ cut here ]------------
<4>[   17.012000] WARNING: at /usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/drivers/base/core.c:579 device_create_file+0x7c/0x8c()
<4>[   17.012000] Attribute timeout_state: read permission without 'show'
<4>[   17.012000] Modules linked in:
<4>[   17.012000] CPU: 0 PID: 465 Comm: ifconfig Not tainted 3.10.100+ #1
<4>[   17.012000] [<c001552c>] (unwind_backtrace+0x0/0x138) from [<c0012594>] (show_stack+0x10/0x14)
<4>[   17.012000] [<c0012594>] (show_stack+0x10/0x14) from [<c001fcac>] (warn_slowpath_common+0x4c/0x68)
<4>[   17.012000] [<c001fcac>] (warn_slowpath_common+0x4c/0x68) from [<c001fd5c>] (warn_slowpath_fmt+0x30/0x40)
<4>[   17.012000] [<c001fd5c>] (warn_slowpath_fmt+0x30/0x40) from [<c022ec50>] (device_create_file+0x7c/0x8c)
<4>[   17.013000] [<c022ec50>] (device_create_file+0x7c/0x8c) from [<c040a6d0>] (hw_net_sysfs_init+0x9c/0x1f4)
<4>[   17.013000] [<c040a6d0>] (hw_net_sysfs_init+0x9c/0x1f4) from [<c040ac50>] (ar8035_config_init+0xf0/0x100)
<4>[   17.013000] [<c040ac50>] (ar8035_config_init+0xf0/0x100) from [<c040936c>] (phy_init_hw+0x3c/0x48)
<4>[   17.013000] [<c040936c>] (phy_init_hw+0x3c/0x48) from [<c04093c4>] (phy_attach_direct+0x4c/0xe8)
<4>[   17.013000] [<c04093c4>] (phy_attach_direct+0x4c/0xe8) from [<c04094e0>] (phy_connect_direct+0x14/0x50)
<4>[   17.013000] [<c04094e0>] (phy_connect_direct+0x14/0x50) from [<c0409560>] (phy_connect+0x44/0x70)
<4>[   17.013000] [<c0409560>] (phy_connect+0x44/0x70) from [<c040efb0>] (stmmac_init_phy+0xa0/0x190)
<4>[   17.013000] [<c040efb0>] (stmmac_init_phy+0xa0/0x190) from [<c0412024>] (stmmac_open+0x38/0xf48)
<4>[   17.013000] [<c0412024>] (stmmac_open+0x38/0xf48) from [<c0558d38>] (__dev_open+0xa8/0x108)
<4>[   17.013000] [<c0558d38>] (__dev_open+0xa8/0x108) from [<c0558f6c>] (__dev_change_flags+0x8c/0x130)
<4>[   17.013000] [<c0558f6c>] (__dev_change_flags+0x8c/0x130) from [<c055907c>] (dev_change_flags+0x10/0x48)
<4>[   17.013000] [<c055907c>] (dev_change_flags+0x10/0x48) from [<c05eefec>] (devinet_ioctl+0x76c/0x824)
<4>[   17.013000] [<c05eefec>] (devinet_ioctl+0x76c/0x824) from [<c0542020>] (sock_ioctl+0x70/0x2e4)
<4>[   17.013000] [<c0542020>] (sock_ioctl+0x70/0x2e4) from [<c00eb5c4>] (do_vfs_ioctl+0x80/0x5c0)
<4>[   17.013000] [<c00eb5c4>] (do_vfs_ioctl+0x80/0x5c0) from [<c00ebb70>] (SyS_ioctl+0x6c/0x7c)
<4>[   17.013000] [<c00ebb70>] (SyS_ioctl+0x6c/0x7c) from [<c000ec80>] (ret_fast_syscall+0x0/0x38)
<4>[   17.013000] ---[ end trace d505d90b42176295 ]---
<6>[   17.050000] dwmac1000_set_filter: # mcasts 0, # unicast 0
<6>[   17.050000]       Filter: 0x00000010
<6>[   17.050000]       Hash0:0xffffffff, Hash1:0xffffffff
<6>[   17.050000] dwmac1000_set_filter: # mcasts 0, # unicast 0
<6>[   17.050000]       Filter: 0x00000010
<6>[   17.050000]       Hash0:0xffffffff, Hash1:0xffffffff
<6>[   17.050000] dwmac1000_set_filter: # mcasts 1, # unicast 0
<6>[   17.050000]       Filter: 0x00000010
<6>[   17.050000]       Hash0:0xffffffff, Hash1:0xffffffff
<6>[   17.050000] dwmac1000_set_filter: # mcasts 2, # unicast 0
<6>[   17.050000]       Filter: 0x00000010
<6>[   17.050000]       Hash0:0xffffffff, Hash1:0xffffffff
<6>[   17.050000] dwmac1000_set_filter: # mcasts 2, # unicast 0
<6>[   17.050000]       Filter: 0x00000010
<6>[   17.050000]       Hash0:0xffffffff, Hash1:0xffffffff
<6>[   17.050000] dwmac1000_set_filter: # mcasts 3, # unicast 0
<6>[   17.050000]       Filter: 0x00000010
<6>[   17.050000]       Hash0:0xffffffff, Hash1:0xffffffff
<6>[   17.212000] dwmac1000_set_filter: # mcasts 3, # unicast 0
<6>[   17.212000]       Filter: 0x00000010
<6>[   17.212000]       Hash0:0xffffffff, Hash1:0xffffffff
<4>[   17.240000] in stmmac_set_mac_address 
<4>[   17.240000] in spe_port_ioctl 
<4>[   17.252000] AR8035 phy driver configinit
<4>[   17.252000] ar8035 power on
<6>[   17.289000] CHG_HUAWEI_CHARGER: poweron_chg_proc_read: is_powdown_charging=0!
<4>[   17.311000] ------------[ cut here ]------------
<4>[   17.311000] WARNING: at /usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/drivers/gpio/gpiolib.c:1987 __gpio_set_value+0xb0/0x140()
<4>[   17.311000] Modules linked in:
<4>[   17.311000] CPU: 0 PID: 233 Comm: oled Tainted: G        W    3.10.100+ #1
<4>[   17.311000] [<c001552c>] (unwind_backtrace+0x0/0x138) from [<c0012594>] (show_stack+0x10/0x14)
<4>[   17.311000] [<c0012594>] (show_stack+0x10/0x14) from [<c001fcac>] (warn_slowpath_common+0x4c/0x68)
<4>[   17.311000] [<c001fcac>] (warn_slowpath_common+0x4c/0x68) from [<c001fce4>] (warn_slowpath_null+0x1c/0x24)
<4>[   17.311000] [<c001fce4>] (warn_slowpath_null+0x1c/0x24) from [<c01eaaac>] (__gpio_set_value+0xb0/0x140)
<4>[   17.311000] [<c01eaaac>] (__gpio_set_value+0xb0/0x140) from [<c020e0cc>] (lcd_reset+0x1c/0x90)
<4>[   17.311000] [<c020e0cc>] (lcd_reset+0x1c/0x90) from [<c020e230>] (stlcdfb_pan_display+0xf0/0x11c)
<4>[   17.311000] [<c020e230>] (stlcdfb_pan_display+0xf0/0x11c) from [<c0208df8>] (fb_pan_display+0xb4/0x128)
<4>[   17.311000] [<c0208df8>] (fb_pan_display+0xb4/0x128) from [<c0209e3c>] (do_fb_ioctl+0x4cc/0x60c)
<4>[   17.311000] [<c0209e3c>] (do_fb_ioctl+0x4cc/0x60c) from [<c00eb5c4>] (do_vfs_ioctl+0x80/0x5c0)
<4>[   17.311000] [<c00eb5c4>] (do_vfs_ioctl+0x80/0x5c0) from [<c00ebb70>] (SyS_ioctl+0x6c/0x7c)
<4>[   17.311000] [<c00ebb70>] (SyS_ioctl+0x6c/0x7c) from [<c000ec80>] (ret_fast_syscall+0x0/0x38)
<4>[   17.311000] ---[ end trace d505d90b42176296 ]---
<4>[   17.341000] ------------[ cut here ]------------
<4>[   17.341000] WARNING: at /usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/drivers/gpio/gpiolib.c:1987 __gpio_set_value+0xb0/0x140()
<4>[   17.341000] Modules linked in:
<4>[   17.341000] CPU: 0 PID: 233 Comm: oled Tainted: G        W    3.10.100+ #1
<4>[   17.341000] [<c001552c>] (unwind_backtrace+0x0/0x138) from [<c0012594>] (show_stack+0x10/0x14)
<4>[   17.341000] [<c0012594>] (show_stack+0x10/0x14) from [<c001fcac>] (warn_slowpath_common+0x4c/0x68)
<4>[   17.341000] [<c001fcac>] (warn_slowpath_common+0x4c/0x68) from [<c001fce4>] (warn_slowpath_null+0x1c/0x24)
<4>[   17.341000] [<c001fce4>] (warn_slowpath_null+0x1c/0x24) from [<c01eaaac>] (__gpio_set_value+0xb0/0x140)
<4>[   17.342000] [<c01eaaac>] (__gpio_set_value+0xb0/0x140) from [<c020e0f0>] (lcd_reset+0x40/0x90)
<4>[   17.342000] [<c020e0f0>] (lcd_reset+0x40/0x90) from [<c020e230>] (stlcdfb_pan_display+0xf0/0x11c)
<4>[   17.342000] [<c020e230>] (stlcdfb_pan_display+0xf0/0x11c) from [<c0208df8>] (fb_pan_display+0xb4/0x128)
<4>[   17.342000] [<c0208df8>] (fb_pan_display+0xb4/0x128) from [<c0209e3c>] (do_fb_ioctl+0x4cc/0x60c)
<4>[   17.342000] [<c0209e3c>] (do_fb_ioctl+0x4cc/0x60c) from [<c00eb5c4>] (do_vfs_ioctl+0x80/0x5c0)
<4>[   17.342000] [<c00eb5c4>] (do_vfs_ioctl+0x80/0x5c0) from [<c00ebb70>] (SyS_ioctl+0x6c/0x7c)
<4>[   17.342000] [<c00ebb70>] (SyS_ioctl+0x6c/0x7c) from [<c000ec80>] (ret_fast_syscall+0x0/0x38)
<4>[   17.342000] ---[ end trace d505d90b42176297 ]---
<4>[   17.371000] ------------[ cut here ]------------
<4>[   17.371000] WARNING: at /usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/drivers/gpio/gpiolib.c:1987 __gpio_set_value+0xb0/0x140()
<4>[   17.371000] Modules linked in:
<4>[   17.371000] CPU: 0 PID: 233 Comm: oled Tainted: G        W    3.10.100+ #1
<4>[   17.371000] [<c001552c>] (unwind_backtrace+0x0/0x138) from [<c0012594>] (show_stack+0x10/0x14)
<4>[   17.371000] [<c0012594>] (show_stack+0x10/0x14) from [<c001fcac>] (warn_slowpath_common+0x4c/0x68)
<4>[   17.371000] [<c001fcac>] (warn_slowpath_common+0x4c/0x68) from [<c001fce4>] (warn_slowpath_null+0x1c/0x24)
<4>[   17.371000] [<c001fce4>] (warn_slowpath_null+0x1c/0x24) from [<c01eaaac>] (__gpio_set_value+0xb0/0x140)
<4>[   17.371000] [<c01eaaac>] (__gpio_set_value+0xb0/0x140) from [<c020e118>] (lcd_reset+0x68/0x90)
<4>[   17.372000] [<c020e118>] (lcd_reset+0x68/0x90) from [<c020e230>] (stlcdfb_pan_display+0xf0/0x11c)
<4>[   17.372000] [<c020e230>] (stlcdfb_pan_display+0xf0/0x11c) from [<c0208df8>] (fb_pan_display+0xb4/0x128)
<4>[   17.372000] [<c0208df8>] (fb_pan_display+0xb4/0x128) from [<c0209e3c>] (do_fb_ioctl+0x4cc/0x60c)
<4>[   17.372000] [<c0209e3c>] (do_fb_ioctl+0x4cc/0x60c) from [<c00eb5c4>] (do_vfs_ioctl+0x80/0x5c0)
<4>[   17.372000] [<c00eb5c4>] (do_vfs_ioctl+0x80/0x5c0) from [<c00ebb70>] (SyS_ioctl+0x6c/0x7c)
<4>[   17.372000] [<c00ebb70>] (SyS_ioctl+0x6c/0x7c) from [<c000ec80>] (ret_fast_syscall+0x0/0x38)
<4>[   17.372000] ---[ end trace d505d90b42176298 ]---
<6>[   17.583000] dwmac1000_set_filter: # mcasts 0, # unicast 0
<6>[   17.583000]       Filter: 0x00000010
<6>[   17.583000]       Hash0:0xffffffff, Hash1:0xffffffff
<6>[   17.583000] dwmac1000_set_filter: # mcasts 0, # unicast 0
<6>[   17.583000]       Filter: 0x00000010
<6>[   17.583000]       Hash0:0xffffffff, Hash1:0xffffffff
<6>[   17.583000] dwmac1000_set_filter: # mcasts 1, # unicast 0
<6>[   17.583000]       Filter: 0x00000010
<6>[   17.583000]       Hash0:0xffffffff, Hash1:0xffffffff
<6>[   17.583000] IPv6: ADDRCONF(NETDEV_UP): eth0: link is not ready
<6>[   17.583000] dwmac1000_set_filter: # mcasts 1, # unicast 0
<6>[   17.583000]       Filter: 0x00000010
<6>[   17.583000]       Hash0:0xffffffff, Hash1:0xffffffff
<4>[   17.640000] ------------[ cut here ]------------
<4>[   17.640000] WARNING: at /usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/drivers/gpio/gpiolib.c:1904 __gpio_get_value+0x88/0x118()
<4>[   17.640000] Modules linked in:
<4>[   17.640000] CPU: 0 PID: 233 Comm: oled Tainted: G        W    3.10.100+ #1
<4>[   17.640000] [<c001552c>] (unwind_backtrace+0x0/0x138) from [<c0012594>] (show_stack+0x10/0x14)
<4>[   17.640000] [<c0012594>] (show_stack+0x10/0x14) from [<c001fcac>] (warn_slowpath_common+0x4c/0x68)
<4>[   17.640000] [<c001fcac>] (warn_slowpath_common+0x4c/0x68) from [<c001fce4>] (warn_slowpath_null+0x1c/0x24)
<4>[   17.640000] [<c001fce4>] (warn_slowpath_null+0x1c/0x24) from [<c01eabc4>] (__gpio_get_value+0x88/0x118)
<4>[   17.640000] [<c01eabc4>] (__gpio_get_value+0x88/0x118) from [<c020d75c>] (lcd_vectid_get+0x28/0x138)
<4>[   17.640000] [<c020d75c>] (lcd_vectid_get+0x28/0x138) from [<c020dca8>] (lcd_init+0x18/0x68)
<4>[   17.640000] [<c020dca8>] (lcd_init+0x18/0x68) from [<c020dd18>] (lcd_pwron+0x20/0x2c)
<4>[   17.640000] [<c020dd18>] (lcd_pwron+0x20/0x2c) from [<c020e238>] (stlcdfb_pan_display+0xf8/0x11c)
<4>[   17.640000] [<c020e238>] (stlcdfb_pan_display+0xf8/0x11c) from [<c0208df8>] (fb_pan_display+0xb4/0x128)
<4>[   17.640000] [<c0208df8>] (fb_pan_display+0xb4/0x128) from [<c0209e3c>] (do_fb_ioctl+0x4cc/0x60c)
<4>[   17.640000] [<c0209e3c>] (do_fb_ioctl+0x4cc/0x60c) from [<c00eb5c4>] (do_vfs_ioctl+0x80/0x5c0)
<4>[   17.640000] [<c00eb5c4>] (do_vfs_ioctl+0x80/0x5c0) from [<c00ebb70>] (SyS_ioctl+0x6c/0x7c)
<4>[   17.640000] [<c00ebb70>] (SyS_ioctl+0x6c/0x7c) from [<c000ec80>] (ret_fast_syscall+0x0/0x38)
<4>[   17.640000] ---[ end trace d505d90b42176299 ]---
<4>[   17.641000] ------------[ cut here ]------------
<4>[   17.641000] WARNING: at /usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/drivers/gpio/gpiolib.c:1904 __gpio_get_value+0x88/0x118()
<4>[   17.641000] Modules linked in:
<4>[   17.641000] CPU: 0 PID: 233 Comm: oled Tainted: G        W    3.10.100+ #1
<4>[   17.641000] [<c001552c>] (unwind_backtrace+0x0/0x138) from [<c0012594>] (show_stack+0x10/0x14)
<4>[   17.641000] [<c0012594>] (show_stack+0x10/0x14) from [<c001fcac>] (warn_slowpath_common+0x4c/0x68)
<4>[   17.641000] [<c001fcac>] (warn_slowpath_common+0x4c/0x68) from [<c001fce4>] (warn_slowpath_null+0x1c/0x24)
<4>[   17.641000] [<c001fce4>] (warn_slowpath_null+0x1c/0x24) from [<c01eabc4>] (__gpio_get_value+0x88/0x118)
<4>[   17.641000] [<c01eabc4>] (__gpio_get_value+0x88/0x118) from [<c020d768>] (lcd_vectid_get+0x34/0x138)
<4>[   17.641000] [<c020d768>] (lcd_vectid_get+0x34/0x138) from [<c020dca8>] (lcd_init+0x18/0x68)
<4>[   17.641000] [<c020dca8>] (lcd_init+0x18/0x68) from [<c020dd18>] (lcd_pwron+0x20/0x2c)
<4>[   17.641000] [<c020dd18>] (lcd_pwron+0x20/0x2c) from [<c020e238>] (stlcdfb_pan_display+0xf8/0x11c)
<4>[   17.641000] [<c020e238>] (stlcdfb_pan_display+0xf8/0x11c) from [<c0208df8>] (fb_pan_display+0xb4/0x128)
<4>[   17.641000] [<c0208df8>] (fb_pan_display+0xb4/0x128) from [<c0209e3c>] (do_fb_ioctl+0x4cc/0x60c)
<4>[   17.641000] [<c0209e3c>] (do_fb_ioctl+0x4cc/0x60c) from [<c00eb5c4>] (do_vfs_ioctl+0x80/0x5c0)
<4>[   17.641000] [<c00eb5c4>] (do_vfs_ioctl+0x80/0x5c0) from [<c00ebb70>] (SyS_ioctl+0x6c/0x7c)
<4>[   17.641000] [<c00ebb70>] (SyS_ioctl+0x6c/0x7c) from [<c000ec80>] (ret_fast_syscall+0x0/0x38)
<4>[   17.641000] ---[ end trace d505d90b4217629a ]---
<3>[   17.641000] [lcd]: <lcd_vectid_get> 
<3>[   17.641000] lcd ID=0
<3>[   17.641000] 
<3>[   17.641000] [lcd]: <lcd_init> lcd_init:oled_MacID = 0 
<3>[   17.641000] 
<6>[   17.669000] arp uses obsolete (PF_INET,SOCK_PACKET)
<6>[   17.693000] br0: port 1(rmnet2) entered disabled state
<6>[   17.702000] br0: port 1(rmnet2) entered listening state
<6>[   17.702000] br0: port 1(rmnet2) entered listening state
<6>[   17.702000] IPv6: ADDRCONF(NETDEV_UP): br0: link is not ready
<4>[   17.762000] get_muticast_flag = 0
<3>[   17.847000] [special_timer] Timer delete start, user ID  is  3 
<3>[   17.847000] [special_timer] Timer delete end, already deleted!
<4>[   17.878000] At_QryHFreqinfo:current rat is not LTE.
<3>[   17.911000] [special_timer] Timer create start, user ID  is  4 
<6>[   17.911000] [special_timer] Creat add start special timer sucess, kernel timerID is 2 
<3>[   17.921000] [lcd]: <MainOLED_DispAlloff> lcd MainOLED_DispAlloff
<3>[   17.921000] 
<4>[   18.023000] device_event_send: queue is NOT empty
<1>[   18.023000] device_event_send: msg send over
<7>[   18.073000] received shell ioctl cmd=0xcafa0000
<7>[   18.073000] , arg=0x00
<7>[   18.073000] received shell ioctl cmd=0xcafa0001
<7>[   18.073000] , arg=0xbe891b40
<7>[   18.075000] parent_name_ptr =oeminfo 
<4>[   18.075000]  info :mtd->erasesize = 131072 ,mtd->writesize = 2048 
<7>[   18.075000] operation region index = 0 start_addr = 0 
<3>[   18.076000] [version]: <bsp_get_web_version> flash_get_share_region_info ture. 
<4>[   18.121000] Call wifi_power_off_1151 return, value = 0x0
<7>[   18.131000] received shell ioctl cmd=0xcafa0000
<7>[   18.131000] , arg=0x00
<7>[   18.131000] received shell ioctl cmd=0xcafa0001
<7>[   18.131000] , arg=0xbe8ffb40
<4>[   18.161000] Call wifi_power_on_1151 return, value = 0x1
<7>[   18.173000] parent_name_ptr =oeminfo 
<4>[   18.173000]  info :mtd->erasesize = 131072 ,mtd->writesize = 2048 
<7>[   18.173000] operation region index = 0 start_addr = 0 
<3>[   18.174000] [*DLOAD_NARK_CORE*] flash_web_proc_write:634: Do not need to update version success.
<4>[   18.735000] pstPlmnId->Mcc: 0xffffffff, ORI:0xfff
<4>[   18.755000] pstPlmnId->Mcc: 0xffffffff, ORI:0xfff
<3>[   18.797000] U_MASS(ERROR) virtualsd_ioctl() line:64 : ioctl usb_get_mmc_dev_idex error, get mmcblocknum = -123
<7>[   19.206000] PCI driver: driver init start.
<7>[   19.206000] pci probe begin!
<4>[   19.206000] PCI: enabling device 0000:01:00.0 (0140 -> 0142)
<7>[   19.206000] bar0: 0x42000000, len = 0x40000
<7>[   19.206000] bar1: 0x0, len = 0x0
<7>[   19.206000] bar2: 0x0, len = 0x0
<7>[   19.206000] bar3: 0x0, len = 0x0
<7>[   19.206000] bar4: 0x0, len = 0x0
<7>[   19.206000] bar5: 0x0, len = 0x0
<7>[   19.206000] BAR 0: set to [mem 0x42000000, len = 0x40000]
<7>[   19.206000] BAR 0: ioremap addr = 0xcad00000
<7>[   19.206000] pci_resource_start[0x42000000],pci_resource_en[0x4203ffff]
<7>[   19.206000] WITP: pci_dev->irq      : 195.
<7>[   19.206000] PCI driver: probe succ!
<7>[   19.210000] oal_5115_pci_init,OAL_PCIE_SYS_BASE_PHYS=0x90100000,map g_pst_5115_sys_ctl = 0xcacd2000
<4>[   19.223000] l4 port number:
<4>[   19.223000] action = add
<4>[   19.223000] protocol = udp
<4>[   19.223000] set l4 portnum : 53
<7>[   19.300000] INI_DRV:D]ini_cfg_init:1088]ini_file_name@/system/bin/wifi_hisi/cfg_e5_hisi.ini
<7>[   19.300000] 
<6>[   19.699000] br0: port 1(rmnet2) entered learning state
<7>[   19.970000] Tick=4294681906, FileId=1611, LineNo=485, FuncName::hal_board_init, " Support max chip num: 1.
<7>[   19.970000] "
<7>[   19.970000] 
<7>[   19.970000] Tick=4294681906, FileId=1611, LineNo=426, FuncName::hal_chip_init, "Chip version: 0x11510100.
<7>[   19.970000] "
<7>[   19.970000] 
<7>[   19.992000] [PCIe]: PCIe 0 Info: 2.5-Gbps Gen1.1, Lane: x1
<7>[   19.992000] hi1151_soc_set_pcie_l1s:uc_on_off[1]!
<7>[   19.994000] Info:waitting app_sdt start...
<7>[   19.998000] WL_PCIE_RESET_GPIO value=1
<7>[   20.001000] g_aus_tx_pwr_ref_val_2G[0][0]= 8520
<7>[   20.001000] g_aus_tx_pwr_ref_val_2G[1][0]= 6674
<7>[   20.001000] g_aus_tx_pwr_ref_val_2G[0][1]= 8192
<7>[   20.001000] g_aus_tx_pwr_ref_val_2G[1][1]= 8192
<7>[   20.001000] g_aus_tx_pwr_ref_val_2G[0][2]= 7209
<7>[   20.001000] g_aus_tx_pwr_ref_val_2G[1][2]= 6717
<7>[   20.001000] g_aus_tx_pwr_ref_val_2G[0][3]= 7864
<7>[   20.001000] g_aus_tx_pwr_ref_val_2G[1][3]= 7537
<7>[   20.001000] g_aus_tx_pwr_ref_val_2G[0][4]= 8520
<7>[   20.001000] g_aus_tx_pwr_ref_val_2G[1][4]= 7864
<7>[   20.001000] g_aus_tx_pwr_ref_val_2G[0][5]= 8192
<7>[   20.001000] g_aus_tx_pwr_ref_val_2G[1][5]= 8192
<7>[   20.001000] g_aus_tx_pwr_ref_val_2G[0][6]= 7111
<7>[   20.001000] g_aus_tx_pwr_ref_val_2G[1][6]= 6554
<7>[   20.001000] g_aus_tx_pwr_ref_val_2G[0][7]= 7864
<7>[   20.001000] g_aus_tx_pwr_ref_val_2G[1][7]= 8192
<7>[   20.001000] g_aus_tx_pwr_ref_val_2G[0][8]= 7209
<7>[   20.001000] g_aus_tx_pwr_ref_val_2G[1][8]= 7209
<7>[   20.001000] g_aus_tx_pwr_ref_val_2G[0][9]= 6881
<7>[   20.001000] g_aus_tx_pwr_ref_val_2G[1][9]= 7537
<7>[   20.002000] g_aus_tx_pwr_ref_val_2G[0][10]= 6226
<7>[   20.002000] g_aus_tx_pwr_ref_val_2G[1][10]= 7209
<7>[   20.002000] g_aus_tx_pwr_ref_val_2G[0][11]= 8847
<7>[   20.002000] g_aus_tx_pwr_ref_val_2G[1][11]= 8520
<7>[   20.002000] g_aus_tx_pwr_ref_val_2G[0][12]= 7537
<7>[   20.002000] g_aus_tx_pwr_ref_val_2G[1][12]= 8192
<7>[   20.019000] g_al_cali_acc_val_i[8896]
<7>[   20.019000] g_al_cali_acc_val_i[3527]
<7>[   20.030000] g_al_cali_acc_val_i[8552]
<7>[   20.030000] g_al_cali_acc_val_i[3370]
<7>[   20.036000] g_al_cali_acc_val_i[7214]
<7>[   20.044000] g_al_cali_acc_val_i[2878]
<7>[   20.053000] g_al_cali_acc_val_i[8118]
<7>[   20.053000] g_al_cali_acc_val_i[3430]
<7>[   20.062000] g_al_cali_acc_val_i[8720]
<7>[   20.062000] g_al_cali_acc_val_i[3739]
<7>[   20.075000] g_al_cali_acc_val_i[8640]
<7>[   20.075000] g_al_cali_acc_val_i[3686]
<7>[   20.084000] g_al_cali_acc_val_i[7166]
<7>[   20.084000] g_al_cali_acc_val_i[3002]
<7>[   20.094000] g_al_cali_acc_val_i[7981]
<7>[   20.094000] g_al_cali_acc_val_i[3365]
<7>[   20.115000] g_al_cali_acc_val_i[7695]
<7>[   20.115000] g_al_cali_acc_val_i[3156]
<7>[   20.139000] g_al_cali_acc_val_i[7196]
<7>[   20.139000] g_al_cali_acc_val_i[3008]
<7>[   20.160000] g_al_cali_acc_val_i[6617]
<7>[   20.161000] g_al_cali_acc_val_i[2761]
<7>[   20.166000] g_al_cali_acc_val_i[9089]
<7>[   20.166000] g_al_cali_acc_val_i[3825]
<7>[   20.198000] g_al_cali_acc_val_i[7683]
<7>[   20.198000] g_al_cali_acc_val_i[3311]
<7>[   20.206000] g_al_cali_acc_val_i[7056]
<7>[   20.206000] g_al_cali_acc_val_i[2545]
<7>[   20.224000] g_al_cali_acc_val_i[8514]
<7>[   20.224000] g_al_cali_acc_val_i[3592]
<7>[   20.239000] g_al_cali_acc_val_i[6933]
<7>[   20.239000] g_al_cali_acc_val_i[2693]
<7>[   20.254000] g_al_cali_acc_val_i[7574]
<7>[   20.254000] g_al_cali_acc_val_i[3173]
<7>[   20.270000] g_al_cali_acc_val_i[7797]
<7>[   20.270000] g_al_cali_acc_val_i[2988]
<7>[   20.282000] g_al_cali_acc_val_i[8147]
<7>[   20.282000] g_al_cali_acc_val_i[3027]
<7>[   20.303000] g_al_cali_acc_val_i[6188]
<7>[   20.303000] g_al_cali_acc_val_i[2191]
<7>[   20.328000] g_al_cali_acc_val_i[7877]
<7>[   20.328000] g_al_cali_acc_val_i[3344]
<7>[   20.334000] g_al_cali_acc_val_i[7142]
<7>[   20.334000] g_al_cali_acc_val_i[3006]
<7>[   20.360000] g_al_cali_acc_val_i[7669]
<7>[   20.360000] g_al_cali_acc_val_i[3420]
<7>[   20.365000] g_al_cali_acc_val_i[7295]
<7>[   20.366000] g_al_cali_acc_val_i[3072]
<7>[   20.384000] g_al_cali_acc_val_i[8507]
<7>[   20.384000] g_al_cali_acc_val_i[3224]
<7>[   20.402000] g_al_cali_acc_val_i[8247]
<7>[   20.402000] g_al_cali_acc_val_i[3229]
<6>[   20.637000] CHG_HUAWEI_CHARGER: poweron_chg_proc_read: is_powdown_charging=0!
<7>[   20.855000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [1328] [atp_proc_guestwifiaccessui_ifaccess_write] atp_proc_guestwifiaccessui_ifaccess_write 
<7>[   20.855000] 
<11>[   20.939000] init: untracked pid 568 exited
<7>[   20.954000] g_al_cali_acc_val_i[9725]
<7>[   20.960000] g_al_cali_acc_val_i[3858]
<7>[   20.971000] g_al_cali_acc_val_i[7823]
<7>[   20.971000] g_al_cali_acc_val_i[3043]
<7>[   20.982000] g_al_cali_acc_val_i[7612]
<7>[   20.982000] g_al_cali_acc_val_i[3189]
<7>[   20.993000] g_al_cali_acc_val_i[7323]
<7>[   20.993000] g_al_cali_acc_val_i[3145]
<7>[   21.003000] g_al_cali_acc_val_i[7038]
<7>[   21.003000] g_al_cali_acc_val_i[3089]
<7>[   21.016000] g_al_cali_acc_val_i[8379]
<7>[   21.016000] g_al_cali_acc_val_i[3703]
<7>[   21.027000] g_al_cali_acc_val_i[8149]
<7>[   21.027000] g_al_cali_acc_val_i[3550]
<7>[   21.038000] g_al_cali_acc_val_i[7915]
<7>[   21.038000] g_al_cali_acc_val_i[3377]
<7>[   21.049000] g_al_cali_acc_val_i[7212]
<7>[   21.049000] g_al_cali_acc_val_i[2980]
<7>[   21.070000] g_al_cali_acc_val_i[9459]
<7>[   21.070000] g_al_cali_acc_val_i[3575]
<7>[   21.077000] g_al_cali_acc_val_i[8138]
<7>[   21.077000] g_al_cali_acc_val_i[3451]
<7>[   21.083000] g_al_cali_acc_val_i[8040]
<7>[   21.083000] g_al_cali_acc_val_i[3312]
<6>[   21.089000] CHG_HUAWEI_CHARGER: poweron_chg_proc_read: is_powdown_charging=0!
<7>[   21.098000] g_al_cali_acc_val_i[8002]
<7>[   21.098000] g_al_cali_acc_val_i[3642]
<7>[   21.104000] g_al_cali_acc_val_i[7998]
<7>[   21.104000] g_al_cali_acc_val_i[3396]
<7>[   21.120000] g_al_cali_acc_val_i[8211]
<7>[   21.120000] g_al_cali_acc_val_i[3148]
<7>[   21.136000] g_al_cali_acc_val_i[8021]
<7>[   21.136000] g_al_cali_acc_val_i[2947]
<7>[   21.142000] g_al_cali_acc_val_i[8306]
<7>[   21.142000] g_al_cali_acc_val_i[3130]
<7>[   21.158000] g_al_cali_acc_val_i[7891]
<7>[   21.158000] g_al_cali_acc_val_i[2906]
<4>[   21.349000] dynamic switch mode:
<4>[   21.349000] set switch on
<4>[   21.349000] action = set
<7>[   21.362000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [350] [atp_proc_prsite_addr_write] atp_proc_prsite_addr_write 
<7>[   21.362000] 
<3>[   21.362000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [269] [atp_proc_prsite_write] atp_proc_prsite_write: 0,  g_stPrsiteUrlInfo.lEnable:0
<3>[   21.362000] 
<7>[   21.372000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [358] [atp_proc_prsite_mask_write] atp_proc_prsite_mask_write 
<7>[   21.372000] 
<3>[   21.372000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [269] [atp_proc_prsite_write] atp_proc_prsite_write: 0,  g_stPrsiteUrlInfo.lEnable:0
<3>[   21.372000] 
<7>[   21.391000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [366] [atp_proc_prsite_actionmode_write] atp_proc_prsite_actionmode_write 
<7>[   21.391000] 
<3>[   21.391000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [269] [atp_proc_prsite_write] atp_proc_prsite_write: 0,  g_stPrsiteUrlInfo.lEnable:0
<3>[   21.391000] 
<7>[   21.407000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [384] [atp_proc_prsite_location_write] atp_proc_prsite_location_write 
<7>[   21.407000] 
<3>[   21.407000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [269] [atp_proc_prsite_write] atp_proc_prsite_write: 
<3>[   21.407000] ,  g_stPrsiteUrlInfo.lEnable:0
<3>[   21.407000] 
<7>[   21.422000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [402] [atp_proc_prsite_multi_user_enable_write] atp_proc_prsite_multi_user_enable_write 
<7>[   21.422000] 
<3>[   21.422000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [269] [atp_proc_prsite_write] atp_proc_prsite_write: 0,  g_stPrsiteUrlInfo.lEnable:0
<3>[   21.422000] 
<7>[   21.468000] g_al_cali_acc_val_q[1071]
<7>[   21.468000] g_al_cali_acc_val_q[-2795]
<7>[   21.498000] g_al_cali_acc_val_q[1527]
<7>[   21.498000] g_al_cali_acc_val_q[-2048]
<7>[   21.512000] g_al_cali_acc_val_q[761]
<7>[   21.512000] g_al_cali_acc_val_q[-3118]
<7>[   21.526000] g_al_cali_acc_val_q[239]
<7>[   21.526000] g_al_cali_acc_val_q[-3457]
<7>[   21.540000] g_al_cali_acc_val_q[117]
<7>[   21.540000] g_al_cali_acc_val_q[-3583]
<7>[   21.554000] g_al_cali_acc_val_q[36]
<7>[   21.554000] g_al_cali_acc_val_q[-3896]
<7>[   21.571000] g_al_cali_acc_val_q[77]
<7>[   21.571000] g_al_cali_acc_val_q[-3647]
<7>[   21.585000] g_al_cali_acc_val_q[1083]
<7>[   21.585000] g_al_cali_acc_val_q[-2879]
<7>[   21.605000] g_al_cali_acc_val_q[1906]
<7>[   21.605000] g_al_cali_acc_val_q[-1705]
<7>[   21.619000] g_al_cali_acc_val_q[1178]
<7>[   21.619000] g_al_cali_acc_val_q[-2614]
<7>[   21.633000] g_al_cali_acc_val_q[746]
<7>[   21.633000] g_al_cali_acc_val_q[-2861]
<7>[   21.646000] g_al_cali_acc_val_q[730]
<7>[   21.647000] g_al_cali_acc_val_q[-3066]
<7>[   21.660000] g_al_cali_acc_val_q[926]
<7>[   21.660000] g_al_cali_acc_val_q[-2682]
<7>[   21.674000] g_al_cali_acc_val_q[652]
<7>[   21.674000] g_al_cali_acc_val_q[-3306]
<6>[   21.699000] br0: topology change detected, propagating
<6>[   21.699000] br0: port 1(rmnet2) entered forwarding state
<6>[   21.700000] IPv6: ADDRCONF(NETDEV_CHANGE): br0: link becomes ready
<7>[   23.608000] wiphy_register start.
<7>[   23.709000] Tick=4294685636, FileId=1207, LineNo=11748, FuncName::wal_hipriv_sys_write, " Hisilicon0 radartool dfsenable 0
<7>[   23.709000] "
<7>[   23.709000] 
<7>[   19.264000] netlink create succ.
<7>[   23.719000] Tick=4294685646, FileId=1207, LineNo=11748, FuncName::wal_hipriv_sys_write, " Hisilicon0 radartool cacenable 0
<7>[   23.719000] "
<7>[   23.719000] 
<12>[   23.735000] Starting ACS...
<7>[   25.206000] Tick=4294687136, FileId=1207, LineNo=11748, FuncName::wal_hipriv_sys_write, " Hisilicon0 acs sw 1
<7>[   25.206000] "
<7>[   25.206000] 
<7>[   25.206000] set acs sw=1
<7>[   25.206000] set acs sw=1 in dmac
<12>[   25.239000] Stopping WLAN...
<7>[   25.282000] Tick=4294687216, FileId=1207, LineNo=11748, FuncName::wal_hipriv_sys_write, " Hisilicon0 alg dbac stop
<7>[   25.282000] "
<7>[   25.282000] 
<7>[   25.498000] Tick=4294687426, FileId=1207, LineNo=11748, FuncName::wal_hipriv_sys_write, " Hisilicon0 alg dbac disable
<7>[   25.498000] "
<7>[   25.498000] 
<7>[   25.732000] Tick=4294687666, FileId=1207, LineNo=11748, FuncName::wal_hipriv_sys_write, " Hisilicon0 lpm_soc_mode 5 1 0
<7>[   25.732000] "
<7>[   25.732000] 
<7>[   25.743000] Tick=4294687676, FileId=1207, LineNo=11748, FuncName::wal_hipriv_sys_write, " Hisilicon0 lpm_soc_mode 6 1 0
<7>[   25.743000] "
<7>[   25.743000] 
<12>[   25.758000] Starting WLAN... start ap
<7>[   25.777000] Tick=4294687706, FileId=1207, LineNo=11748, FuncName::wal_hipriv_sys_write, " Hisilicon0 create wlan0 ap
<7>[   25.777000] "
<7>[   25.777000] 
<4>[   25.813000] [spe_port_alloc:] spe_port_alloc, restore td pos td_free:0, td_busy:0
<4>[   25.813000] [spe_port_alloc:] spe_port_alloc, restore rd pos rd_free:0, rd_busy:0
<4>[   25.813000] new_reg: port 4 sit property to 0x1 write addr 0xc9060408 
<3>[   25.813000] Wi-Fi<INFO>[wifi_spe_port_alloc:2547]: spe port 4 first alloc;
<3>[   25.813000] 
<7>[   25.816000] wal_netdev_spe_init::vap_id::1;port_num::4
<4>[   25.833000] in spe_port_ioctl 
<7>[   25.833000] Success
<4>[   25.853000] in spe_port_ioctl 
<4>[   25.853000] spe port 4 attached to bridge.
<6>[   25.853000] device wlan0 entered promiscuous mode
<4>[   25.866000] in spe_port_ioctl 
<7>[   25.866000] Success
<4>[   25.866000] delmaclistbydev Multiuser not Enable
<7>[   26.475000] wal_netdev_open,dev_name is:wlan0
<3>[   26.475000] Wi-Fi<INFO>[wlan_set_driver_lock:1824]: Exit, wifi driver lock ON
<6>[   26.475000] br0: port 2(wlan0) entered listening state
<6>[   26.475000] br0: port 2(wlan0) entered listening state
<7>[   26.688000] hmac_config_set_beacon::pst_mac_vap->st_cap_flag.bit_11ac2g=1, bit_disable_2ght40=0
<7>[   26.688000] wal_netdev_open,dev_name is:wlan0
<7>[   26.691000] >>> got=5:do scan mode=0 func=0xb type=1 ch_cnt=12
<7>[   26.692000] Success
<3>[   26.692000] Wi-Fi<INFO>[wlan_set_driver_lock:1824]: Exit, wifi driver lock ON
<7>[   28.130000] <<< rsp=5:scan report ch=12 bss=13 init=1
<7>[   28.134000] got init rank result [0 0 7] -  [0 0 0] init=1 for 0:0
<7>[   28.263000] Tick=4294690196, FileId=1207, LineNo=11748, FuncName::wal_hipriv_sys_write, " wlan0 isolation_mode 4
<7>[   28.263000] "
<7>[   28.263000] 
<7>[   28.278000] Tick=4294690206, FileId=1207, LineNo=11748, FuncName::wal_hipriv_sys_write, " wlan0 isolation_type 2 0
<7>[   28.278000] "
<7>[   28.278000] 
<7>[   28.296000] Tick=4294690226, FileId=1207, LineNo=11748, FuncName::wal_hipriv_sys_write, " wlan0 isolation_fwd 2
<7>[   28.296000] "
<7>[   28.296000] 
<7>[   28.308000] Tick=4294690236, FileId=1207, LineNo=11748, FuncName::wal_hipriv_sys_write, " wlan0 blacklist_mode 0
<7>[   28.308000] "
<7>[   28.308000] 
<7>[   28.327000] Tick=4294690256, FileId=1207, LineNo=11748, FuncName::wal_hipriv_sys_write, " Hisilicon0 pm_enable 1
<7>[   28.327000] "
<7>[   28.327000] 
<7>[   28.328000] Success
<6>[   28.382000] device wlan0 left promiscuous mode
<6>[   28.382000] br0: port 2(wlan0) entered disabled state
<4>[   28.388000] delmaclistbydev Multiuser not Enable
<4>[   28.388000] in spe_port_ioctl 
<4>[   28.414000] in spe_port_ioctl 
<4>[   28.414000] spe port 4 attached to bridge.
<6>[   28.414000] device wlan0 entered promiscuous mode
<6>[   28.415000] br0: port 2(wlan0) entered listening state
<6>[   28.415000] br0: port 2(wlan0) entered listening state
<12>[   28.421000] Setting DFS radar threshold to -52...
<7>[   28.441000] Tick=4294690376, FileId=1207, LineNo=11748, FuncName::wal_hipriv_sys_write, " Hisilicon0 radartool set_radar_th -52
<7>[   28.441000] "
<7>[   28.441000] 
<7>[   28.519000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [841] [atp_proc_dial_wlan_name_write] atp_proc_dial_wlan_name_write 
<7>[   28.519000] 
<3>[   28.712000] [special_timer] Timer create start, user ID  is  3 
<6>[   28.712000] [special_timer] Creat add start special timer sucess, kernel timerID is 3 
<7>[   28.806000]  [/usr1/home/lwx495230/lwx495230_version/V722_E5/1217_release/vendor/hisi/system/kernel/package/atp/network/common/kernel/src/atp_proc.c] [1328] [atp_proc_guestwifiaccessui_ifaccess_write] atp_proc_guestwifiaccessui_ifaccess_write 
<7>[   28.806000] 
<6>[   30.410000] br0: port 2(wlan0) entered learning state
<6>[   32.410000] br0: topology change detected, propagating
<6>[   32.410000] br0: port 2(wlan0) entered forwarding state
<3>[   40.381000] [special_timer] Timer delete start, user ID  is  3 
<6>[   40.381000] Before delete, timerID  is  3 
<4>[   40.640000] REB_DFT: ptable_part_num 28
<4>[   40.641000] Reb_DFT:part_name[kernel],find suited mtd idx
<4>[   40.641000] Reb_DFT:part_name[kernelbk],find suited mtd idx
<4>[   40.641000] Reb_DFT:part_name[m3boot],find suited mtd idx
<4>[   40.641000] Reb_DFT:part_name[m3image],find suited mtd idx
<4>[   40.641000] Reb_DFT:part_name[fastboot],find suited mtd idx
<4>[   40.641000] Reb_DFT:part_name[nvbacklte],find suited mtd idx
<4>[   40.641000] Reb_DFT:part_name[nvdefault],find suited mtd idx
<4>[   40.641000] Reb_DFT:part_name[nvdload],find suited mtd idx
<4>[   40.641000] Reb_DFT:part_name[oeminfo],find suited mtd idx
<3>[   40.836000] [special_timer] Timer delete start, user ID  is  4 
<6>[   40.836000] Before delete, timerID  is  2 
<4>[   41.047000] Reb_DFT: eccability = 0x8