# Static Blackhole Policy

A blackhole task for a specified IP address is manually created on the ATIC to block the traffic destined to the IP address.

#### Procedure

1. Configure the notification mode of second-level blackhole event.
2. Manually create a blackhole policy.
   1. Choose Defense > Policy Settings > Blackhole.
   2. Click .
   3. In the Create Blackhole Policy dialog box, set Blackhole mode to Routing blackhole, select Enable automatically, and set Clean device, VPN, Destination IP address, and Mask. Click OK.

   The manually created static blackhole policy that the blackhole mode is set to Routing blackhole can only be manually decapsulated. For the method of manually decapsulating a blackhole policy, see Manually decapsulating a blackhole policy.

Parent topic: Routing Blackhole

Copyright © Huawei Technologies Co., Ltd.