# Huawei Advanced Anti-DDoS Traffic

#### Function

This report provides visibility into the incoming or attack traffic of a specific Huawei Advanced AntiDDoS.

#### Parameter

Table 1 Query parameters of Advanced Anti-DDoS Traffic
Parameter | Description
--- | ---
Defense IP | Enter the destination IP address. Both IPv4 and IPv6 addresses are applicable. Traffic destined for the IP address is queried.
Time | Click to select the start time and end time of statistics. Or you can change the time values in corresponding text boxes. The end time should be later than the start time and the interval cannot be longer than one year. If the query interval is longer than or equal to seven days and shorter than one year, statistics are collected daily. If the query interval is longer than or equal to one day and shorter than seven days, statistics are collected hourly. If the query interval is shorter than one day, statistics are collected every five minutes.

#### Example

The incoming and attack traffic with a specific defense IP address in a specific period is displayed, as shown in Figure 1.

Figure 1 Incoming and attack traffic with a specific defense IP address

#### Procedure

1. Choose Report > Report > Traffic Analysis.
2. Click the Huawei Advanced AntiDDoS Traffic tab.
3. Set query parameters.
4. Click Search.

   Information about Huawei Advanced AntiDDoS Traffic that matches the query conditions is displayed.

5. Optional: Open or save the query results as files, or send queried reports to the specified email address.

   - Click to open or save the query results as PDF files. A maximum of 10,000 entries can be displayed.
   - Click to open or save the query results as EXCEL files. A maximum of 10,000 entries can be displayed.
   - Click to open or save the query results as CSV files. All data except figures can be displayed.
   - Click to enter a recipient mail address and select an attachment format. Then click OK.

Parent topic: Traffic Analysis

Copyright © Huawei Technologies Co., Ltd.