-- =================================================================
-- Description: IPV6ICMP mib
-- Reference:   This mib was extracted from RFC2466
-- =================================================================
IPV6-ICMP-MIB DEFINITIONS ::= BEGIN

    IMPORTS
        MODULE-IDENTITY, OBJECT-TYPE,
        Counter32, mib-2                 FROM SNMPv2-SMI
        MODULE-COMPLIANCE, OBJECT-GROUP  FROM SNMPv2-CONF
        ipv6IfEntry                      FROM IPV6-MIB;

    ipv6IcmpMIB MODULE-IDENTITY
        LAST-UPDATED "9801082155Z"
        ORGANIZATION "IETF IPv6 Working Group"
        CONTACT-INFO
          "           Dimitry Haskin

              Postal: Bay Networks, Inc.
                      660 Techology Park Drive.
                      Billerica, MA  01821
                      US

                 Tel: +1-978-916-8124
              E-mail: dhaskin@baynetworks.com

                      Steve Onishi

              Postal: Bay Networks, Inc.
                      3 Federal Street
                      Billerica, MA 01821
                      US

                 Tel: +1-978-916-3816
              E-mail: sonishi@baynetworks.com"
        DESCRIPTION
            "The MIB module for entities implementing
             the ICMPv6."
        ::= { mib-2 56 }

    -- the ICMPv6 group

    ipv6IcmpMIBObjects OBJECT IDENTIFIER ::= { ipv6IcmpMIB  1 }


    -- Per-interface ICMPv6 statistics table

    ipv6IfIcmpTable OBJECT-TYPE
        SYNTAX     SEQUENCE OF Ipv6IfIcmpEntry
        MAX-ACCESS not-accessible
        STATUS     current
        DESCRIPTION
            "IPv6 ICMP statistics. This table contains statistics
            of ICMPv6 messages that are received and sourced by
            the entity."
        ::= { ipv6IcmpMIBObjects 1 }

    ipv6IfIcmpEntry OBJECT-TYPE
        SYNTAX     Ipv6IfIcmpEntry
        MAX-ACCESS not-accessible
        STATUS     current
        DESCRIPTION
            "An ICMPv6 statistics entry containing
            objects at a particular IPv6 interface.
            
            Note that a receiving interface is
            the interface to which a given ICMPv6 message
            is addressed which may not be necessarily
            the input interface for the message.
            
            Similarly,  the sending interface is
            the interface that sources a given
            ICMP message which is usually but not
            necessarily the output interface for the message."
        AUGMENTS { ipv6IfEntry }
        ::= { ipv6IfIcmpTable 1 }

    Ipv6IfIcmpEntry ::= SEQUENCE {
        ipv6IfIcmpInMsgs
            Counter32,
        ipv6IfIcmpInErrors
            Counter32,
        ipv6IfIcmpInDestUnreachs
            Counter32,
        ipv6IfIcmpInAdminProhibs
            Counter32,
        ipv6IfIcmpInTimeExcds
            Counter32,
        ipv6IfIcmpInParmProblems
            Counter32,
        ipv6IfIcmpInPktTooBigs
            Counter32,
        ipv6IfIcmpInEchos
            Counter32,
        ipv6IfIcmpInEchoReplies
            Counter32,
        ipv6IfIcmpInRouterSolicits
            Counter32,
        ipv6IfIcmpInRouterAdvertisements
            Counter32,
        ipv6IfIcmpInNeighborSolicits
            Counter32,
        ipv6IfIcmpInNeighborAdvertisements
            Counter32,
        ipv6IfIcmpInRedirects
            Counter32,
        ipv6IfIcmpInGroupMembQueries
            Counter32,
        ipv6IfIcmpInGroupMembResponses
            Counter32,
        ipv6IfIcmpInGroupMembReductions
            Counter32,
        ipv6IfIcmpOutMsgs
            Counter32,
        ipv6IfIcmpOutErrors
            Counter32,
        ipv6IfIcmpOutDestUnreachs
            Counter32,
        ipv6IfIcmpOutAdminProhibs
            Counter32,
        ipv6IfIcmpOutTimeExcds
            Counter32,
        ipv6IfIcmpOutParmProblems
            Counter32,
        ipv6IfIcmpOutPktTooBigs
            Counter32,
        ipv6IfIcmpOutEchos
            Counter32,
        ipv6IfIcmpOutEchoReplies
            Counter32,
        ipv6IfIcmpOutRouterSolicits
            Counter32,
        ipv6IfIcmpOutRouterAdvertisements
            Counter32,
        ipv6IfIcmpOutNeighborSolicits
            Counter32,
        ipv6IfIcmpOutNeighborAdvertisements
            Counter32,
        ipv6IfIcmpOutRedirects
            Counter32,
        ipv6IfIcmpOutGroupMembQueries
            Counter32,
        ipv6IfIcmpOutGroupMembResponses
            Counter32,
        ipv6IfIcmpOutGroupMembReductions
            Counter32
        }

    ipv6IfIcmpInMsgs OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The total number of ICMP messages received
            by the interface which includes all those
            counted by ipv6IfIcmpInErrors. Note that this
            interface is the interface to which the
            ICMP messages were addressed which may not be
            necessarily the input interface for the messages."
        ::= { ipv6IfIcmpEntry 1 }

    ipv6IfIcmpInErrors OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP messages which the interface
            received but determined as having ICMP-specific
            errors (bad ICMP checksums, bad length, etc.)."
        ::= { ipv6IfIcmpEntry 2 }

    ipv6IfIcmpInDestUnreachs OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP Destination Unreachable
            messages received by the interface."
        ::= { ipv6IfIcmpEntry 3 }

    ipv6IfIcmpInAdminProhibs OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP destination
            unreachable/communication administratively
            prohibited messages received by the interface."
        ::= { ipv6IfIcmpEntry 4 }

    ipv6IfIcmpInTimeExcds OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP Time Exceeded messages
             received by the interface."
        ::= { ipv6IfIcmpEntry 5 }

    ipv6IfIcmpInParmProblems OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP Parameter Problem messages
             received by the interface."
        ::= { ipv6IfIcmpEntry 6 }

    ipv6IfIcmpInPktTooBigs OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP Packet Too Big messages
            received by the interface."
        ::= { ipv6IfIcmpEntry 7 }

    ipv6IfIcmpInEchos OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP Echo (request) messages
             received by the interface."
        ::= { ipv6IfIcmpEntry 8 }

    ipv6IfIcmpInEchoReplies OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP Echo Reply messages received
            by the interface."
        ::= { ipv6IfIcmpEntry 9 }

    ipv6IfIcmpInRouterSolicits OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP Router Solicit messages
             received by the interface."
        ::= { ipv6IfIcmpEntry 10 }

    ipv6IfIcmpInRouterAdvertisements OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP Router Advertisement messages
            received by the interface."
        ::= { ipv6IfIcmpEntry 11 }

    ipv6IfIcmpInNeighborSolicits OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP Neighbor Solicit messages
             received by the interface."
        ::= { ipv6IfIcmpEntry 12 }

    ipv6IfIcmpInNeighborAdvertisements OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP Neighbor Advertisement
            messages received by the interface."
        ::= { ipv6IfIcmpEntry 13 }

    ipv6IfIcmpInRedirects OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of Redirect messages received
            by the interface."
        ::= { ipv6IfIcmpEntry 14 }

    ipv6IfIcmpInGroupMembQueries OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMPv6 Group Membership Query
            messages received by the interface."
        ::= { ipv6IfIcmpEntry 15}

    ipv6IfIcmpInGroupMembResponses OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMPv6 Group Membership Response messages
            received by the interface."
        ::= { ipv6IfIcmpEntry 16}

     ipv6IfIcmpInGroupMembReductions OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMPv6 Group Membership Reduction messages
            received by the interface."
        ::= { ipv6IfIcmpEntry 17}

    ipv6IfIcmpOutMsgs OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The total number of ICMP messages which this
            interface attempted to send.  Note that this counter
            includes all those counted by icmpOutErrors."
        ::= { ipv6IfIcmpEntry 18 }

    ipv6IfIcmpOutErrors OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP messages which this interface did
            not send due to problems discovered within ICMP
            such as a lack of buffers.  This value should not
            include errors discovered outside the ICMP layer
            such as the inability of IPv6 to route the resultant
            datagram.  In some implementations there may be no
            types of error which contribute to this counter's
            value."
        ::= { ipv6IfIcmpEntry 19 }

    ipv6IfIcmpOutDestUnreachs OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP Destination Unreachable
            messages sent by the interface."
        ::= { ipv6IfIcmpEntry 20 }

    ipv6IfIcmpOutAdminProhibs OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
             "Number of ICMP dest unreachable/communication
             administratively prohibited messages sent."
        ::= { ipv6IfIcmpEntry 21 }

    ipv6IfIcmpOutTimeExcds OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP Time Exceeded messages sent
            by the interface."
        ::= { ipv6IfIcmpEntry 22 }

    ipv6IfIcmpOutParmProblems OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP Parameter Problem messages
            sent by the interface."
        ::= { ipv6IfIcmpEntry 23 }

    ipv6IfIcmpOutPktTooBigs OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP Packet Too Big messages sent
            by the interface."
        ::= { ipv6IfIcmpEntry 24 }

    ipv6IfIcmpOutEchos OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP Echo (request) messages sent
            by the interface."
        ::= { ipv6IfIcmpEntry 25 }

    ipv6IfIcmpOutEchoReplies OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP Echo Reply messages sent
            by the interface."
        ::= { ipv6IfIcmpEntry 26 }

    ipv6IfIcmpOutRouterSolicits OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP Router Solicitation messages
             sent by the interface."
        ::= { ipv6IfIcmpEntry 27 }

    ipv6IfIcmpOutRouterAdvertisements OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP Router Advertisement messages
            sent by the interface."
        ::= { ipv6IfIcmpEntry 28 }

    ipv6IfIcmpOutNeighborSolicits OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP Neighbor Solicitation
             messages sent by the interface."
        ::= { ipv6IfIcmpEntry 29 }

    ipv6IfIcmpOutNeighborAdvertisements OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMP Neighbor Advertisement
            messages sent by the interface."
        ::= { ipv6IfIcmpEntry 30 }

    ipv6IfIcmpOutRedirects OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of Redirect messages sent. For
            a host, this object will always be zero,
            since hosts do not send redirects."
        ::= { ipv6IfIcmpEntry 31 }

    ipv6IfIcmpOutGroupMembQueries OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMPv6 Group Membership Query
            messages sent."
        ::= { ipv6IfIcmpEntry 32}

    ipv6IfIcmpOutGroupMembResponses OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMPv6 Group Membership Response
            messages sent."
        ::= { ipv6IfIcmpEntry 33}

    ipv6IfIcmpOutGroupMembReductions OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "The number of ICMPv6 Group Membership Reduction
            messages sent."
        ::= { ipv6IfIcmpEntry 34}


    -- conformance information

    ipv6IcmpConformance OBJECT IDENTIFIER ::= { ipv6IcmpMIB 2 }

    ipv6IcmpCompliances OBJECT IDENTIFIER ::= { ipv6IcmpConformance 1 }
    ipv6IcmpGroups      OBJECT IDENTIFIER ::= { ipv6IcmpConformance 2 }

    -- compliance statements

    ipv6IcmpCompliance MODULE-COMPLIANCE
        STATUS  current
        DESCRIPTION
           "The compliance statement for SNMPv2 entities which
           implement ICMPv6."
        MODULE  -- this module
        MANDATORY-GROUPS { ipv6IcmpGroup }
        ::= { ipv6IcmpCompliances 1 }

    ipv6IcmpGroup OBJECT-GROUP
        OBJECTS   {
            ipv6IfIcmpInMsgs,
            ipv6IfIcmpInErrors,
            ipv6IfIcmpInDestUnreachs,
            ipv6IfIcmpInAdminProhibs,
            ipv6IfIcmpInTimeExcds,
            ipv6IfIcmpInParmProblems,
            ipv6IfIcmpInPktTooBigs,
            ipv6IfIcmpInEchos,
            ipv6IfIcmpInEchoReplies,
            ipv6IfIcmpInRouterSolicits,
            ipv6IfIcmpInRouterAdvertisements,
            ipv6IfIcmpInNeighborSolicits,
            ipv6IfIcmpInNeighborAdvertisements,
            ipv6IfIcmpInRedirects,
            ipv6IfIcmpInGroupMembQueries,
            ipv6IfIcmpInGroupMembResponses,
            ipv6IfIcmpInGroupMembReductions,
            ipv6IfIcmpOutMsgs,
            ipv6IfIcmpOutErrors,
            ipv6IfIcmpOutDestUnreachs,
            ipv6IfIcmpOutAdminProhibs,
            ipv6IfIcmpOutTimeExcds,
            ipv6IfIcmpOutParmProblems,
            ipv6IfIcmpOutPktTooBigs,
            ipv6IfIcmpOutEchos,
            ipv6IfIcmpOutEchoReplies,
            ipv6IfIcmpOutRouterSolicits,
            ipv6IfIcmpOutRouterAdvertisements,
            ipv6IfIcmpOutNeighborSolicits,
            ipv6IfIcmpOutNeighborAdvertisements,
            ipv6IfIcmpOutRedirects,
            ipv6IfIcmpOutGroupMembQueries,
            ipv6IfIcmpOutGroupMembResponses,
            ipv6IfIcmpOutGroupMembReductions
            }
        STATUS    current
        DESCRIPTION
            "The ICMPv6 group of objects providing information
             specific to ICMPv6."
        ::= { ipv6IcmpGroups 1 }

END
--                                                                         
--    Copyright (C) The Internet Society (1998).  All Rights Reserved.     
--                                                                         
--    This document and translations of it may be copied and furnished to  
--    others, and derivative works that comment on or otherwise explain it 
--    or assist in its implementation may be prepared, copied, published   
--    and distributed, in whole or in part, without restriction of any     
--    kind, provided that the above copyright notice and this paragraph are
--    included on all such copies and derivative works.  However, this     
--    document itself may not be modified in any way, such as by removing  
--    the copyright notice or references to the Internet Society or other  
--    Internet organizations, except as needed for the purpose of          
--    developing Internet standards in which case the procedures for       
--    copyrights defined in the Internet Standards process must be         
--    followed, or as required to translate it into languages other than   
--    English.                                                             
--                                                                         
--    The limited permissions granted above are perpetual and will not be  
--    revoked by the Internet Society or its successors or assigns.        
--                                                                         
--    This document and the information contained herein is provided on an 
--    "AS IS" basis and THE INTERNET SOCIETY AND THE INTERNET ENGINEERING  
--    TASK FORCE DISCLAIMS ALL WARRANTIES, EXPRESS OR IMPLIED, INCLUDING   
--    BUT NOT LIMITED TO ANY WARRANTY THAT THE USE OF THE INFORMATION      
--    HEREIN WILL NOT INFRINGE ANY RIGHTS OR ANY IMPLIED WARRANTIES OF     
--    MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.                 
                                                                           
                                                                           