--==================================================================
-- Copyright (C) 2022 by  HUAWEI TECHNOLOGIES. All rights reserved.
-- 
-- Description: HUAWEI LINE MIB
-- Reference:
-- Version: V2.17
-- History:
-- <author>,  <date>,  <contents>
-- huxiaolin 2012-12-28 
-- Wang Feng 2014-04-22 Add nodes for wlan npe trusted host
-- ==================================================================


    HUAWEI-LINE-MIB DEFINITIONS ::= BEGIN
 
        IMPORTS
            hwDatacomm
                FROM HUAWEI-MIB
            OBJECT-GROUP, MODULE-COMPLIANCE, NOTIFICATION-GROUP
                FROM SNMPv2-CONF
            IpAddress, Integer32, OBJECT-TYPE, MODULE-IDENTITY, NOTIFICATION-TYPE
                FROM SNMPv2-SMI
            RowStatus
                FROM SNMPv2-TC;
    
-- July 31, 2009 at 16:24 GMT
        -- 1.3.6.1.4.1.2011.5.25.207
        hwLineMIB MODULE-IDENTITY 
            LAST-UPDATED "202201251056Z"        -- Jan 25, 2022 at 10:56 GMT
            ORGANIZATION 
                "Huawei Technologies Co.,Ltd."
            CONTACT-INFO 
                "Huawei Industrial Base
                  Bantian, Longgang
                   Shenzhen 518129
                   People's Republic of China
                   Website: http://www.huawei.com
                   Email: support@huawei.com
                 "
            DESCRIPTION 
                "HUAWEI-LINE-MIB is used to configure and query attributes of connections 
                through management interfaces by users, such as the maximum number of Telnet 
                connections and login information about users.
                "

            REVISION "202201251056Z"
            DESCRIPTION 
                "modify hwConSlotId to hwConSlot  for notification-type hwConAuthModeIncomplete."

            REVISION "202201101628Z"
            DESCRIPTION 
                "modify hwConSlotId to chasisId/slotId for notification-type hwConAuthModeIncomplete."

            REVISION "202110200920Z"
            DESCRIPTION 
                "Add hwConSlotId and hwConAuthMode for notification-type hwConAuthModeIncomplete."

            REVISION "202110131720Z"        
            DESCRIPTION 
                "Add hwConAuthModeIncomplete."
            
            REVISION "201901311239Z"        
            DESCRIPTION 
                "Modify description for hwVtyExceed."

            REVISION "201810241239Z"        
            DESCRIPTION 
                "New Trap added for SSH and Telnet for exceed VTY."

            REVISION "201707251639Z"        
            DESCRIPTION 
                "Modify MAX-ACCESS  of  hwMaxVtyNumber ."

            REVISION "201701181043Z"        
            DESCRIPTION 
                "Modify Trap of  hwVtyHostPermitRowState for compile error."

            REVISION "201603311043Z"        
            DESCRIPTION 
                "Modify Trap of  hwIpUnLocked and hwIpLocked."
 
            REVISION "201603161043Z"        
            DESCRIPTION 
                "New Trap added for hwIpUnLocked."

            REVISION "201603071043Z"        
            DESCRIPTION 
                "New Trap added for hwIpLocked."

            REVISION "201507281520Z"        
            DESCRIPTION 
                "New Trap added for SSH and Telnet for frequent authentication failure."

            REVISION "201405061624Z"        
            DESCRIPTION 
                "New Trap added for SSH login/logout."

            REVISION "201404291624Z"        
            DESCRIPTION 
                "VB description updated"

            REVISION "201404251624Z"        
            DESCRIPTION 
                "New VBs added in HwLoginUserInfoEntry"

            REVISION "201404221624Z"        
            DESCRIPTION 
                "Modified to add nodes for wlan npe trusted host."
		
            REVISION "201404081624Z"        
            DESCRIPTION 
                "Modified to support Trap in VRP V8R8."


            REVISION "200907311624Z"        
            DESCRIPTION 
                "The initial revision of this MIB module ."
            
            ::= { hwDatacomm 207 }

        
    
--
-- Node definitions
--
-- 
        -- 1.3.6.1.4.1.2011.5.25.207.1
        hwLineObjects OBJECT IDENTIFIER ::= { hwLineMIB 1 }

        
        -- 1.3.6.1.4.1.2011.5.25.207.1.1
        hwTelnetSet OBJECT IDENTIFIER ::= { hwLineObjects 1 }

        
        -- 1.3.6.1.4.1.2011.5.25.207.1.1.1
        hwMaxVtyNumber OBJECT-TYPE
            SYNTAX Integer32 (0..15)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the maximum number of Telnet connections. 
                The value ranges from 0 to 15. The default value is 5."
            ::= { hwTelnetSet 1 }

        
        -- 1.3.6.1.4.1.2011.5.25.207.1.2
        hwLoginUserInfo OBJECT IDENTIFIER ::= { hwLineObjects 2 }

        
        -- 1.3.6.1.4.1.2011.5.25.207.1.2.1
        hwLoginUserInfoTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwLoginUserInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table is used to display the user information for login."
            ::= { hwLoginUserInfo 1 }

        
        -- 1.3.6.1.4.1.2011.5.25.207.1.2.1.1
        hwLoginUserInfoEntry OBJECT-TYPE
            SYNTAX HwLoginUserInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table describes information about user login."
            INDEX { hwUserInfoIndex }
            ::= { hwLoginUserInfoTable 1 }

        
        HwLoginUserInfoEntry ::=
            SEQUENCE { 
                hwUserInfoIndex
                    Integer32,
                hwUserInfoName
                    OCTET STRING,
                hwUserInfoIpAddr
                    OCTET STRING,
                hwUserInfoChannel
                    OCTET STRING,
                hwAuthType
                    OCTET STRING,
                hwVpnInstName
                    OCTET STRING
             }

        -- 1.3.6.1.4.1.2011.5.25.207.1.2.1.1.1
        hwUserInfoIndex OBJECT-TYPE
            SYNTAX Integer32 (1..2147483647)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the index of the user information for login."
            ::= { hwLoginUserInfoEntry 1 }

        -- 1.3.6.1.4.1.2011.5.25.207.1.2.1.1.2
        hwUserInfoName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..255))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the name of the user for login."
            ::= { hwLoginUserInfoEntry 2 }

        -- 1.3.6.1.4.1.2011.5.25.207.1.2.1.1.3
        hwUserInfoIpAddr OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..47))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the IP address of the user for login."
            ::= { hwLoginUserInfoEntry 3 }
        
        -- 1.3.6.1.4.1.2011.5.25.207.1.2.1.1.4
        hwUserInfoChannel OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..16))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the channel number of the user for login."
            ::= { hwLoginUserInfoEntry 4 }

        -- 1.3.6.1.4.1.2011.5.25.207.1.2.1.1.5
        hwAuthType OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..20))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the authentication method for login."
            ::= { hwLoginUserInfoEntry 5 }
            
        -- 1.3.6.1.4.1.2011.5.25.207.1.2.1.1.6
        hwVpnInstName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..47))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the VPN name of the user for login."
            ::= { hwLoginUserInfoEntry 6 }

        -- 1.3.6.1.4.1.2011.5.25.207.1.3
        hwUserInterface OBJECT IDENTIFIER ::= { hwLineObjects 3 }

        -- 1.3.6.1.4.1.2011.5.25.207.1.3.1
        hwUserInterfaceTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwUserInterfaceEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table describes information about user Interface."
            ::= { hwUserInterface 1 }

        -- 1.3.6.1.4.1.2011.5.25.207.1.3.1.1
        hwUserInterfaceEntry OBJECT-TYPE
            SYNTAX HwUserInterfaceEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table describes information about user Interface."
            INDEX { hwInterfaceType, hwUserInterfaceIndex }
            ::= { hwUserInterfaceTable 1 }

        HwUserInterfaceEntry ::=
            SEQUENCE { 
                hwInterfaceType
                    INTEGER,
                hwUserInterfaceIndex
                    Integer32,
                hwAuthenticationMode
                    INTEGER,
                hwProtocol
                    INTEGER,
                hwUserInterfaceRowStatus
                    RowStatus
             }

        -- 1.3.6.1.4.1.2011.5.25.207.1.3.1.1.1
        hwInterfaceType OBJECT-TYPE
            SYNTAX INTEGER
                    {
                    vty(1)
                    }
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The type of the user interface."
            ::= { hwUserInterfaceEntry 1 }

        -- 1.3.6.1.4.1.2011.5.25.207.1.3.1.1.2
        hwUserInterfaceIndex OBJECT-TYPE
            SYNTAX Integer32 (0..20)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The index of the user interface."
            ::= { hwUserInterfaceEntry 2 }

        -- 1.3.6.1.4.1.2011.5.25.207.1.3.1.1.3
        hwAuthenticationMode OBJECT-TYPE
            SYNTAX INTEGER
                    {
                    undefined(0),
                    none(1),
                    password(2),
                    aaa(3)
                    }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The authentication mode of the user interface."
            ::= { hwUserInterfaceEntry 3 }

        -- 1.3.6.1.4.1.2011.5.25.207.1.3.1.1.4
        hwProtocol OBJECT-TYPE
            SYNTAX INTEGER
                    {
                    telnet(1),
                    ssh(2),
                    all(3)
                    }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The protocol of the user interface."
            ::= { hwUserInterfaceEntry 4 }

        -- 1.3.6.1.4.1.2011.5.25.207.1.3.1.1.5
        hwUserInterfaceRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "RowStatus for this Table."
            ::= { hwUserInterfaceEntry 5 }

        -- 1.3.6.1.4.1.2011.5.25.207.1.4
        hwVtyHostPermit OBJECT IDENTIFIER ::= { hwLineObjects 4 }
		
        -- 1.3.6.1.4.1.2011.5.25.207.1.4.1
        hwVtyHostPermitTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwVtyHostPermitEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object indicates trusted host table."
            ::= { hwVtyHostPermit 1 }
		
        -- 1.3.6.1.4.1.2011.5.25.207.1.4.1.1
        hwVtyHostPermitEntry OBJECT-TYPE
            SYNTAX HwVtyHostPermitEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object indicates trusted the entry of trusted host table."
            INDEX { hwVtyHostPermitIndex }
            ::= { hwVtyHostPermitTable 1 }
		
        HwVtyHostPermitEntry ::=
            SEQUENCE { 
                hwVtyHostPermitIndex
                Integer32,
                hwVtyHostPermitIpAddress
                IpAddress,
                hwVtyHostPermitMaskAddress
                IpAddress,
                hwVtyHostPermitInformation
                OCTET STRING,
                hwVtyHostPermitRowState
                RowStatus
			 }

        -- 1.3.6.1.4.1.2011.5.25.207.1.4.1.1.1
        hwVtyHostPermitIndex OBJECT-TYPE
            SYNTAX Integer32 (0..7)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The value of this object identifies the index of trusted host table."
            ::= { hwVtyHostPermitEntry 1 }
		
        -- 1.3.6.1.4.1.2011.5.25.207.1.4.1.1.2
        hwVtyHostPermitIpAddress OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The value of this object identifies ip address of trusted host."
            ::= { hwVtyHostPermitEntry 2 }
		
        -- 1.3.6.1.4.1.2011.5.25.207.1.4.1.1.3
        hwVtyHostPermitMaskAddress OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The value of this object identifies mask address of trusted host."
            ::= { hwVtyHostPermitEntry 3 }
		
        -- 1.3.6.1.4.1.2011.5.25.207.1.4.1.1.4
        hwVtyHostPermitInformation OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..127))
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The value of this object identifies the description of trusted host."
            ::= { hwVtyHostPermitEntry 4 }
		
        -- 1.3.6.1.4.1.2011.5.25.207.1.4.1.1.5
        hwVtyHostPermitRowState OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object identifies the status of a row."
            ::= { hwVtyHostPermitEntry 5 }

        -- 1.3.6.1.4.1.2011.5.25.207.1.5
        hwLineMibTrapObjects OBJECT IDENTIFIER ::= { hwLineObjects 5 }
        -- 1.3.6.1.4.1.2011.5.25.207.1.5.1
          hwUserInfoLoginFailedTimes OBJECT-TYPE
                    SYNTAX Integer32
                    MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "Login failed times in the statistic period"
            ::= { hwLineMibTrapObjects 1 }

        -- 1.3.6.1.4.1.2011.5.25.207.1.5.2            
          hwUserInfoStatisticPeriod OBJECT-TYPE
                    SYNTAX Integer32
                    MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "Statistic period to count login failed times"
            ::= { hwLineMibTrapObjects 2 }

       -- 1.3.6.1.4.1.2011.5.25.207.1.5.3 	
          hwUserInfoIpAddress OBJECT-TYPE
                    SYNTAX OCTET STRING (SIZE (0..255))
                    MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "This object indicates the IP address of the user for login."
            ::= { hwLineMibTrapObjects 3 }
			
          -- 1.3.6.1.4.1.2011.5.25.207.1.5.4 	
          hwUserInfoVpnName OBJECT-TYPE
                    SYNTAX OCTET STRING (SIZE (0..255))
                    MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "This object indicates the VPN name of the user for login."
            ::= { hwLineMibTrapObjects 4 }
        -- 1.3.6.1.4.1.2011.5.25.207.1.5.5
          hwCurrentVty OBJECT-TYPE
                    SYNTAX Integer32
                    MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The value of this object identifies the current number of VTY"
            ::= { hwLineMibTrapObjects 5 }

        -- 1.3.6.1.4.1.2011.5.25.207.1.5.6            
          hwMaxVty OBJECT-TYPE
                    SYNTAX Integer32
                    MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The value of this object identifies the maximum number of VTY"
            ::= { hwLineMibTrapObjects 6 }
        -- 1.3.6.1.4.1.2011.5.25.207.1.5.7            
          hwConAuthMode OBJECT-TYPE
                    SYNTAX OCTET STRING (SIZE (0..20))
                    MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The value of this object identifies the authentication mode of console port"
            ::= { hwLineMibTrapObjects 7 }
        -- 1.3.6.1.4.1.2011.5.25.207.1.5.8            
          hwConSlot OBJECT-TYPE
                    SYNTAX OCTET STRING (SIZE (0..32))
                    MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The value of this object identifies the chasis/slot id of console port"
            ::= { hwLineMibTrapObjects 8 }
		 
-- =======================================
-- HUAWEI-LINE-MIB MIB - Notification Information
--=======================================
   
        -- 1.3.6.1.4.1.2011.5.25.207.2
        hwLineNotification OBJECT IDENTIFIER ::= { hwLineMIB 2 }
        
        -- 1.3.6.1.4.1.2011.5.25.207.2.1
        hwVtyNumExceed NOTIFICATION-TYPE
            OBJECTS { hwMaxVtyNumber }
            STATUS current
            DESCRIPTION 
                "This object indicates the alarm reported when the number of Telnet users reaches 
                the maximum number of Telnet connections. In addition, the maximum number of 
                Telnet connections is displayed."
            ::= { hwLineNotification 1 }
        
        -- 1.3.6.1.4.1.2011.5.25.207.2.2
        hwUserLogin NOTIFICATION-TYPE
            OBJECTS { hwUserInfoName, hwUserInfoIpAddr, hwUserInfoChannel, hwAuthType, hwVpnInstName }
            STATUS current
            DESCRIPTION 
                "When a user logs in through Telnet/Stelnet, the user name, IP address for login, 
                used tunnel, authentication type and vpn name are reported."
            ::= { hwLineNotification 2 }
        
        -- 1.3.6.1.4.1.2011.5.25.207.2.3
        hwUserLoginFail NOTIFICATION-TYPE
            OBJECTS { hwUserInfoName, hwUserInfoIpAddr, hwUserInfoChannel, hwAuthType, hwVpnInstName }
            STATUS current
            DESCRIPTION 
                "When a user fails to log in through Telnet/Stelnet, the user name, IP address for login, 
                used tunnel, authentication type and vpn name are reported."
            ::= { hwLineNotification 3 }     

        -- 1.3.6.1.4.1.2011.5.25.207.2.4
        hwUserLogout NOTIFICATION-TYPE
            OBJECTS { hwUserInfoName, hwUserInfoIpAddr, hwUserInfoChannel, hwAuthType, hwVpnInstName }
            STATUS current
            DESCRIPTION 
                "When a user logs out of the Telnet/Stelnet server, the user name, IP address for logout, 
                used tunnel, authentication type and vpn name are reported."
            ::= { hwLineNotification 4 }           

        -- 1.3.6.1.4.1.2011.5.25.207.2.5
        hwUserSshLogin NOTIFICATION-TYPE
            OBJECTS { hwUserInfoName, hwUserInfoIpAddr, hwUserInfoChannel, hwAuthType, hwVpnInstName }
            STATUS current
            DESCRIPTION 
                "When a user logs in to SSH server, the user name, IP address for login, 
                used tunnel, authentication type and vpn name are reported."
            ::= { hwLineNotification 5 } 
            
        -- 1.3.6.1.4.1.2011.5.25.207.2.6
        hwUserSshLogout NOTIFICATION-TYPE
            OBJECTS { hwUserInfoName, hwUserInfoIpAddr, hwUserInfoChannel, hwAuthType, hwVpnInstName }
            STATUS current
            DESCRIPTION 
                "When a user logs out of the SSH server, the user name, IP address for logout, 
                and used tunnel are reported."
            ::= { hwLineNotification 6 } 

        -- 1.3.6.1.4.1.2011.5.25.207.2.7
        hwTelnetLoginFailed NOTIFICATION-TYPE
            OBJECTS { hwUserInfoLoginFailedTimes, hwUserInfoStatisticPeriod }
            STATUS current
            DESCRIPTION
                "When users failed to login telnet server too frequently, login fail times and statistics period are reported."
            ::= { hwLineNotification 7 }

        -- 1.3.6.1.4.1.2011.5.25.207.2.8
        hwSSHLoginFailed NOTIFICATION-TYPE
            OBJECTS { hwUserInfoLoginFailedTimes, hwUserInfoStatisticPeriod }
            STATUS current
            DESCRIPTION
                "When users failed to login ssh server too frequently, login fail times and statistics period are reported."
            ::= { hwLineNotification 8 }

        -- 1.3.6.1.4.1.2011.5.25.207.2.9
        hwTelnetLoginFailedClear NOTIFICATION-TYPE
            OBJECTS { hwUserInfoLoginFailedTimes, hwUserInfoStatisticPeriod }
            STATUS current
            DESCRIPTION
                "When users failed to login telnet server too frequently, login fail times and statistics period are reported."
            ::= { hwLineNotification 9 }

        -- 1.3.6.1.4.1.2011.5.25.207.2.10
        hwSSHLoginFailedClear NOTIFICATION-TYPE
            OBJECTS { hwUserInfoLoginFailedTimes, hwUserInfoStatisticPeriod }
            STATUS current
            DESCRIPTION
                "When users failed to login ssh server too frequently, login fail times and statistics period are reported."
            ::= { hwLineNotification 10 }

        -- 1.3.6.1.4.1.2011.5.25.207.2.11
        hwIpLocked NOTIFICATION-TYPE
            OBJECTS { hwUserInfoIpAddress, hwUserInfoVpnName, hwUserInfoStatisticPeriod }
            STATUS current
            DESCRIPTION
                "when the number of user login failures from the same IP address reaches the threshold, the trap of hwIpLocked is reported."
            ::= { hwLineNotification 11 }

       -- 1.3.6.1.4.1.2011.5.25.207.2.12
        hwIpUnLocked NOTIFICATION-TYPE
            OBJECTS { hwUserInfoIpAddress, hwUserInfoVpnName }
            STATUS current
            DESCRIPTION
                "When the IP is unlocked, the trap of hwIpUnLocked is reported."
            ::= { hwLineNotification 12 }
	   -- 1.3.6.1.4.1.2011.5.25.207.2.13
        hwVtyExceed NOTIFICATION-TYPE
            OBJECTS { hwCurrentVty, hwMaxVty }
            STATUS current
            DESCRIPTION 
                "When the number of available VTY channels was lower than or equal to the threshold value, an alarm is generated."
            ::= { hwLineNotification 13 }
	   -- 1.3.6.1.4.1.2011.5.25.207.2.14
        hwVtyExceedClear NOTIFICATION-TYPE
            OBJECTS { hwCurrentVty, hwMaxVty }
            STATUS current
            DESCRIPTION 
                "When the number of available VTY channels is higher than or equal to the threshold value, the alarm is cleared."
            ::= { hwLineNotification 14 }	
        -- 1.3.6.1.4.1.2011.5.25.207.2.15
        hwConAuthModeIncomplete NOTIFICATION-TYPE
            OBJECTS { hwConSlot, hwConAuthMode }
            STATUS current
            DESCRIPTION 
                "When device startup and check console authentication mode that is not suit for first-login after upgrade, an event is generated."
            ::= { hwLineNotification 15 }
-- =========================================
-- HUAWEI-LINE-MIB MIB - Conformance Information
-- =========================================
        -- 1.3.6.1.4.1.2011.5.25.207.3
        hwLineConformance OBJECT IDENTIFIER ::= { hwLineMIB 3 }

        
        -- 1.3.6.1.4.1.2011.5.25.207.3.1
        hwLineCompliances OBJECT IDENTIFIER ::= { hwLineConformance 1 }

        
        -- 1.3.6.1.4.1.2011.5.25.207.3.1.1
        hwLineCompliance MODULE-COMPLIANCE
            STATUS current
            DESCRIPTION 
                "The compliance statement for 
                entities that support the huawei LINE MIB."
            MODULE      -- this module
            ::= { hwLineCompliances 1 }

        
        -- 1.3.6.1.4.1.2011.5.25.207.3.2
        hwLineGroups OBJECT IDENTIFIER ::= { hwLineConformance 2 }

        -- 1.3.6.1.4.1.2011.5.25.207.3.2.1
        hwLineNotificationGroup NOTIFICATION-GROUP
            NOTIFICATIONS { hwVtyNumExceed, hwUserLogin, hwUserLoginFail, hwUserLogout, hwUserSshLogin, hwUserSshLogout, hwIpLocked, hwIpUnLocked, hwConAuthModeIncomplete   }
            STATUS current
            DESCRIPTION 
                "The collection of notifications in the module."
            ::= { hwLineGroups 1 }
        -- 1.3.6.1.4.1.2011.5.25.207.3.2.2
        hwLineUserInfoGroup OBJECT-GROUP
            OBJECTS { hwUserInfoIndex, hwUserInfoName, hwUserInfoIpAddr, hwUserInfoChannel }
            STATUS current
            DESCRIPTION 
                "A collection of objects on Clock setting level information."
            ::= { hwLineGroups 2 }
        -- 1.3.6.1.4.1.2011.5.25.207.3.2.3
        hwMaxVtyNumberGroup OBJECT-GROUP
            OBJECTS { hwMaxVtyNumber }
            STATUS current
            DESCRIPTION 
                "A collection of objects on vty number information."
            ::= { hwLineGroups 3 }

    END

--
-- HUAWEI-LINE-MIB.mib
--
   
