-- ===========================================================================
-- Description: OSPFv2 MIB
-- Reference:   Module(OSPF-MIB) Extracted from RFC4750.TXT,from 14869 to 169349.Obsoletes: 1850
-- ===========================================================================

OSPF-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Counter32, Gauge32,
    Integer32, Unsigned32, IpAddress, mib-2
                 FROM SNMPv2-SMI
    TEXTUAL-CONVENTION, TruthValue, RowStatus, TimeStamp
                 FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP
                 FROM SNMPv2-CONF
    InterfaceIndexOrZero
                 FROM IF-MIB;

ospf MODULE-IDENTITY
       LAST-UPDATED "200611100000Z" -- November 10, 2006 00:00:00 EST
       ORGANIZATION "IETF OSPF Working Group"
       CONTACT-INFO
       "WG E-Mail: ospf@ietf.org

        WG Chairs: acee@cisco.com
                   rohit@gmail.com

        Editors:   Dan Joyal
                   Nortel
                   600 Technology Park Drive
                   Billerica, MA  01821
                   djoyal@nortel.com

                   Piotr Galecki
                   Airvana
                   19 Alpha Road
                   Chelmsford, MA 01824
                   pgalecki@airvana.com

                   Spencer Giacalone
                   CSFB
                   Eleven Madison Ave
                   New York, NY 10010-3629
                   spencer.giacalone@gmail.com"

       DESCRIPTION
          "The MIB module to describe the OSPF Version 2
          Protocol.  Note that some objects in this MIB
          module may pose a significant security risk.
          Refer to the Security Considerations section
          in RFC 4750 for more information.
          Copyright (C) The IETF Trust (2006).
          This version of this MIB module is part of
          RFC 4750;  see the RFC itself for full legal
          notices."

       REVISION "200611100000Z" -- November 10, 2006 09:00:00 EST
       DESCRIPTION
         "Updated for latest changes to OSPF Version 2:
          - updated the General Group with the new
            ospfRFC1583Compatibility, ospfReferenceBandwidth
            and ospfDiscontinuityTime objects
          - added graceful-restart-related objects
          - added stub-router-related objects
          - updated the Area Table with NSSA-related objects
          - added ospfAreaAggregateExtRouteTag object
          - added Opaque LSA-related objects
          - updates to the Compliances and Security sections
          - added area LSA counter table
          - added section describing translation of notification
            parameters between SNMP versions
          - added ospfComplianceObsolete to contain obsolete
            object groups
          - deprecated ospfExtLsdbTable
          See Appendix B of RFC 4750 for more details.

          This version published as part of RFC 4750"

       REVISION "199501201225Z" -- Fri Jan 20 12:25:50 PST 1995
       DESCRIPTION
          "The initial SMIv2 revision of this MIB module, published
          in RFC 1850."
       ::= { mib-2 14 }

AreaID ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION
          "An OSPF Area Identifier.
           Note that the Area ID, in OSPF, has the same format
           as an IP address, but has the function of defining
           a summarization point for link state advertisements."
       SYNTAX       IpAddress

RouterID ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION
          "A OSPF Router Identifier.
           Note that the Router ID, in OSPF, has the same format
           as an IP address, but identifies the router independent
           of its IP address."
       SYNTAX       IpAddress

Metric ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "d-0"
       STATUS       current
       DESCRIPTION
          "The OSPF internal metric.
           Note that the OSPF metric is defined as an unsigned value
           in the range."
       SYNTAX       Integer32 (0..'FFFF'h)

BigMetric ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "d-0"
       STATUS       current
       DESCRIPTION
          "The OSPF external metric."
       SYNTAX       Integer32 (0..'FFFFFF'h)

Status ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION
          "An indication of the operability of an OSPF
          function or feature.  For example, the status
          of an interface: 'enabled' indicates that
          it is willing to communicate with other OSPF routers,
          and 'disabled' indicates that it is not."
       SYNTAX       INTEGER { enabled (1), disabled (2) }

PositiveInteger ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "d-0"
       STATUS       current
       DESCRIPTION
          "A positive integer.  Values in excess are precluded as
          unnecessary and prone to interoperability issues."
       SYNTAX       Integer32 (0..'7FFFFFFF'h)

HelloRange ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "d-0"
       STATUS       current
       DESCRIPTION
          "The range of intervals in seconds on which Hello messages
          are exchanged."
       SYNTAX       Integer32 (1..'FFFF'h)

UpToMaxAge ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "d-0"
       STATUS       current
       DESCRIPTION
          "The values in seconds that one might find or configure
          for variables bounded by the maximum age of an LSA."
       SYNTAX       Integer32 (0..3600)

DesignatedRouterPriority ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "d-0"
       STATUS       current
       DESCRIPTION
          "The range of values defined for the priority of a system
          for becoming the designated router."
       SYNTAX       Integer32 (0..'FF'h)

TOSType ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "d-0"
       STATUS      current
       DESCRIPTION
        "Type of Service (TOS) is defined as a mapping to the IP
        Type of Service Flags as defined in the IP Forwarding
        Table MIB

            +-----+-----+-----+-----+-----+-----+-----+-----+
            |                 |                       |     |
            |   PRECEDENCE    |    TYPE OF SERVICE    |  0  |
            |                 |                       |     |
            +-----+-----+-----+-----+-----+-----+-----+-----+

                     IP TOS                IP TOS
                Field     Policy      Field     Policy

                Contents    Code      Contents    Code
                0 0 0 0  ==>   0      0 0 0 1  ==>   2
                0 0 1 0  ==>   4      0 0 1 1  ==>   6
                0 1 0 0  ==>   8      0 1 0 1  ==>  10
                0 1 1 0  ==>  12      0 1 1 1  ==>  14
                1 0 0 0  ==>  16      1 0 0 1  ==>  18
                1 0 1 0  ==>  20      1 0 1 1  ==>  22
                1 1 0 0  ==>  24      1 1 0 1  ==>  26
                1 1 1 0  ==>  28      1 1 1 1  ==>  30

         The remaining values are left for future definition."
           SYNTAX       Integer32 (0..30)

OspfAuthenticationType ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION
          "The authentication type."
       SYNTAX       INTEGER {
                       none (0),
                       simplePassword (1),
                       md5 (2)
                       -- reserved for specification by IANA (> 2)
                    }

--  OSPF General Variables

--      Note: These parameters apply globally to the Router's
--      OSPF Process.

ospfGeneralGroup OBJECT IDENTIFIER ::= { ospf 1 }

  ospfRouterId OBJECT-TYPE
       SYNTAX       RouterID
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
          "A 32-bit integer uniquely identifying the
          router in the Autonomous System.
          By convention, to ensure uniqueness, this
          should default to the value of one of the
          router's IP interface addresses.

          This object is persistent and when written
          the entity SHOULD save the change to non-volatile storage."
       REFERENCE
          "OSPF Version 2, C.1 Global parameters"
       ::= { ospfGeneralGroup 1 }

  ospfAdminStat OBJECT-TYPE
       SYNTAX       Status
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
          "The administrative status of OSPF in the
          router.  The value 'enabled' denotes that the
          OSPF Process is active on at least one interface;
          'disabled' disables it on all interfaces.

          This object is persistent and when written
          the entity SHOULD save the change to non-volatile storage."
       ::= { ospfGeneralGroup 2 }

  ospfVersionNumber OBJECT-TYPE
       SYNTAX       INTEGER { version2 (2) }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The current version number of the OSPF protocol is 2."
       REFERENCE
          "OSPF Version 2, Title"
       ::= { ospfGeneralGroup 3 }

  ospfAreaBdrRtrStatus OBJECT-TYPE
       SYNTAX       TruthValue
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "A flag to note whether this router is an Area
          Border Router."
       REFERENCE
          "OSPF Version 2, Section 3 Splitting the AS into
          Areas"
       ::= { ospfGeneralGroup 4 }

  ospfASBdrRtrStatus OBJECT-TYPE
       SYNTAX       TruthValue
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
          "A flag to note whether this router is configured as
           an Autonomous System Border Router.

           This object is persistent and when written the
           entity SHOULD save the change to non-volatile storage."
       REFERENCE
          "OSPF Version 2, Section 3.3 Classification of
          routers"
       ::= { ospfGeneralGroup 5 }

  ospfExternLsaCount OBJECT-TYPE
        SYNTAX       Gauge32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
           "The number of external (LS type-5) link state
           advertisements in the link state database."
        REFERENCE
           "OSPF Version 2, Appendix A.4.5 AS external link
           advertisements"
        ::= { ospfGeneralGroup 6 }

  ospfExternLsaCksumSum OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
           "The 32-bit sum of the LS checksums of
           the external link state advertisements
           contained in the link state database.  This sum
           can be used to determine if there has been a
           change in a router's link state database and
           to compare the link state database of two
           routers.  The value should be treated as unsigned
           when comparing two sums of checksums."
        ::= { ospfGeneralGroup 7 }

  ospfTOSSupport OBJECT-TYPE
       SYNTAX       TruthValue
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
          "The router's support for type-of-service routing.

           This object is persistent and when written
           the entity SHOULD save the change to non-volatile
           storage."
       REFERENCE
          "OSPF Version 2, Appendix F.1.2 Optional TOS
          support"
       ::= { ospfGeneralGroup 8 }

   ospfOriginateNewLsas OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The number of new link state advertisements
          that have been originated.  This number is
          incremented each time the router originates a new
          LSA.

          Discontinuities in the value of this counter can
          occur at re-initialization of the management system,
          and at other times as indicated by the value of
          ospfDiscontinuityTime."
        ::= { ospfGeneralGroup 9 }

  ospfRxNewLsas OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The number of link state advertisements received
          that are determined to be new instantiations.
          This number does not include newer instantiations
          of self-originated link state advertisements.

          Discontinuities in the value of this counter can
          occur at re-initialization of the management system,
          and at other times as indicated by the value of
          ospfDiscontinuityTime."
       ::= { ospfGeneralGroup 10 }

  ospfExtLsdbLimit OBJECT-TYPE
       SYNTAX       Integer32 (-1..'7FFFFFFF'h)
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
          "The maximum number of non-default
          AS-external LSAs entries that can be stored in the
          link state database.  If the value is -1, then
          there is no limit.

          When the number of non-default AS-external LSAs
          in a router's link state database reaches
          ospfExtLsdbLimit, the router enters
          overflow state.  The router never holds more than
          ospfExtLsdbLimit non-default AS-external LSAs
          in its database.  OspfExtLsdbLimit MUST be set
          identically in all routers attached to the OSPF
          backbone and/or any regular OSPF area (i.e.,
          OSPF stub areas and NSSAs are excluded).

          This object is persistent and when written
          the entity SHOULD save the change to non-volatile
          storage."
        DEFVAL { -1 }
        ::= { ospfGeneralGroup 11 }

  ospfMulticastExtensions OBJECT-TYPE
       SYNTAX       Integer32
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
          "A bit mask indicating whether the router is
          forwarding IP multicast (Class D) datagrams
          based on the algorithms defined in the
          multicast extensions to OSPF.

          Bit 0, if set, indicates that the router can
          forward IP multicast datagrams in the router's
          directly attached areas (called intra-area
          multicast routing).

          Bit 1, if set, indicates that the router can
          forward IP multicast datagrams between OSPF
          areas (called inter-area multicast routing).

          Bit 2, if set, indicates that the router can
          forward IP multicast datagrams between
          Autonomous Systems (called inter-AS multicast
          routing).

          Only certain combinations of bit settings are
          allowed, namely: 0 (no multicast forwarding is
          enabled), 1 (intra-area multicasting only), 3
          (intra-area and inter-area multicasting), 5
          (intra-area and inter-AS multicasting), and 7
          (multicasting everywhere).  By default, no
          multicast forwarding is enabled.

          This object is persistent and when written
          the entity SHOULD save the change to non-volatile
          storage."
       DEFVAL { 0 }
       ::= { ospfGeneralGroup 12 }

  ospfExitOverflowInterval OBJECT-TYPE
       SYNTAX       PositiveInteger
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
          "The number of seconds that, after entering
          OverflowState, a router will attempt to leave
          OverflowState.  This allows the router to again
          originate non-default AS-external LSAs.  When
          set to 0, the router will not leave
          overflow state until restarted.

          This object is persistent and when written
          the entity SHOULD save the change to non-volatile
          storage."
       DEFVAL { 0 }
       ::= { ospfGeneralGroup 13 }

  ospfDemandExtensions OBJECT-TYPE
       SYNTAX       TruthValue
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
          "The router's support for demand routing.
           This object is persistent and when written
           the entity SHOULD save the change to non-volatile
           storage."
       REFERENCE
          "Extending OSPF to Support Demand Circuits"
       ::= { ospfGeneralGroup 14 }

  ospfRFC1583Compatibility  OBJECT-TYPE
       SYNTAX       TruthValue
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
          "Indicates metrics used to choose among multiple
          AS-external LSAs.  When RFC1583Compatibility is set to
          enabled, only cost will be used when choosing among
          multiple AS-external LSAs advertising the same
          destination.  When RFC1583Compatibility is set to
          disabled, preference will be driven first by type of
          path using cost only to break ties.

          This object is persistent and when written
          the entity SHOULD save the change to non-volatile
          storage."
        REFERENCE
           "OSPF Version 2, Section 16.4.1 External path
            preferences"
        ::= { ospfGeneralGroup 15 }

 ospfOpaqueLsaSupport  OBJECT-TYPE
       SYNTAX       TruthValue
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The router's support for Opaque LSA types."
       REFERENCE
          "The OSPF Opaque LSA Option"
       ::= { ospfGeneralGroup 16 }

  ospfReferenceBandwidth OBJECT-TYPE
       SYNTAX       Unsigned32
       UNITS        "kilobits per second"
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
          "Reference bandwidth in kilobits/second for
          calculating default interface metrics.  The
          default value is 100,000 KBPS (100 MBPS).

          This object is persistent and when written
          the entity SHOULD save the change to non-volatile
          storage."
       ::= { ospfGeneralGroup 17 }

  ospfRestartSupport OBJECT-TYPE
       SYNTAX       INTEGER { none (1),
                              plannedOnly (2),
                              plannedAndUnplanned (3)
                            }
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
          "The router's support for OSPF graceful restart.
          Options include: no restart support, only planned
          restarts, or both planned and unplanned restarts.

          This object is persistent and when written
          the entity SHOULD save the change to non-volatile
          storage."
       ::= { ospfGeneralGroup 18 }

  ospfRestartInterval OBJECT-TYPE
       SYNTAX       Integer32 (1..1800)
       UNITS        "seconds"
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
          "Configured OSPF graceful restart timeout interval.

           This object is persistent and when written
           the entity SHOULD save the change to non-volatile
           storage."
       ::= { ospfGeneralGroup 19 }

  ospfRestartStrictLsaChecking OBJECT-TYPE
       SYNTAX       TruthValue
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
          "Indicates if strict LSA checking is enabled for
           graceful restart.

           This object is persistent and when written
           the entity SHOULD save the change to non-volatile
           storage."
       ::= { ospfGeneralGroup 20 }


  ospfRestartStatus OBJECT-TYPE
       SYNTAX       INTEGER { notRestarting (1),
                              plannedRestart (2),
                              unplannedRestart (3)
                            }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "Current status of OSPF graceful restart."
       ::= { ospfGeneralGroup 21 }

  ospfRestartAge OBJECT-TYPE
       SYNTAX       Unsigned32
       UNITS        "seconds"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "Remaining time in current OSPF graceful restart
          interval."
       ::= { ospfGeneralGroup 22 }

  ospfRestartExitReason OBJECT-TYPE
       SYNTAX       INTEGER { none (1),           -- none attempted
                              inProgress (2),     -- restart in
                                                  -- progress
                              completed (3),      -- successfully
                                                  -- completed
                              timedOut (4),       -- timed out
                              topologyChanged (5) -- aborted due to
                                                  -- topology change.
                            }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "Describes the outcome of the last attempt at a
          graceful restart.  If the value is 'none', no restart
          has yet been attempted.  If the value is 'inProgress',
          a restart attempt is currently underway."
       ::= { ospfGeneralGroup 23 }

  ospfAsLsaCount OBJECT-TYPE
       SYNTAX       Gauge32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
           "The number of AS-scope link state
           advertisements in the AS-scope link state database."
       ::= { ospfGeneralGroup 24 }

  ospfAsLsaCksumSum OBJECT-TYPE
       SYNTAX       Unsigned32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
           "The 32-bit unsigned sum of the LS checksums of
           the AS link state advertisements contained in the AS-scope
           link state database.  This sum can be used to determine
           if there has been a change in a router's AS-scope link
           state database, and to compare the AS-scope link state
           database of two routers."
       ::= { ospfGeneralGroup 25 }

   ospfStubRouterSupport OBJECT-TYPE
       SYNTAX       TruthValue
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
           "The router's support for stub router functionality."
       REFERENCE
           "OSPF Stub Router Advertisement"
       ::= { ospfGeneralGroup 26 }

   ospfStubRouterAdvertisement OBJECT-TYPE
       SYNTAX       INTEGER {
                          doNotAdvertise (1),
                          advertise(2)
                          }
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
           "This object controls the advertisement of
           stub router LSAs by the router.  The value
           doNotAdvertise will result in the advertisement
           of a standard router LSA and is the default value.

           This object is persistent and when written
           the entity SHOULD save the change to non-volatile
           storage."
       ::= { ospfGeneralGroup 27 }

  ospfDiscontinuityTime OBJECT-TYPE
      SYNTAX     TimeStamp
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
         "The value of sysUpTime on the most recent occasion
          at which any one of this MIB's counters suffered
          a discontinuity.

          If no such discontinuities have occurred since the last
          re-initialization of the local management subsystem,
          then this object contains a zero value."
      ::= { ospfGeneralGroup 28 }


--  OSPF Area Table
--     The OSPF Area Table contains information
--     regarding the various areas.

  ospfAreaTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF OspfAreaEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "Information describing the configured parameters and
          cumulative statistics of the router's attached areas.
          The interfaces and virtual links are configured
          as part of these areas.  Area 0.0.0.0, by definition,
          is the backbone area."
       REFERENCE
          "OSPF Version 2, Section 6 The Area Data Structure"
       ::= { ospf 2 }

  ospfAreaEntry OBJECT-TYPE
       SYNTAX       OspfAreaEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "Information describing the configured parameters and
          cumulative statistics of one of the router's attached areas.
          The interfaces and virtual links are configured as part of
          these areas.  Area 0.0.0.0, by definition, is the backbone
          area.

          Information in this table is persistent and when this object
          is written the entity SHOULD save the change to non-volatile
          storage."
       INDEX { ospfAreaId }
       ::= { ospfAreaTable 1 }
  OspfAreaEntry ::=
        SEQUENCE {
           ospfAreaId
              AreaID,
           ospfAuthType
              OspfAuthenticationType,
           ospfImportAsExtern
              INTEGER,
           ospfSpfRuns
              Counter32,
           ospfAreaBdrRtrCount
              Gauge32,
           ospfAsBdrRtrCount
              Gauge32,
           ospfAreaLsaCount
              Gauge32,
           ospfAreaLsaCksumSum
              Integer32,
           ospfAreaSummary
              INTEGER,
           ospfAreaStatus
              RowStatus,
           ospfAreaNssaTranslatorRole
              INTEGER,
           ospfAreaNssaTranslatorState
              INTEGER,
           ospfAreaNssaTranslatorStabilityInterval
              PositiveInteger,
           ospfAreaNssaTranslatorEvents
              Counter32
           }

  ospfAreaId OBJECT-TYPE
       SYNTAX       AreaID
       MAX-ACCESS   read-only -- read-only since originally
                              -- an SMIv1 index
       STATUS       current
       DESCRIPTION
          "A 32-bit integer uniquely identifying an area.
          Area ID 0.0.0.0 is used for the OSPF backbone."
       REFERENCE
          "OSPF Version 2, Appendix C.2 Area parameters"
       ::= { ospfAreaEntry 1 }

  ospfAuthType OBJECT-TYPE
       SYNTAX       OspfAuthenticationType
       MAX-ACCESS   read-create
       STATUS       obsolete
       DESCRIPTION
          "The authentication type specified for an area."
       REFERENCE
          "OSPF Version 2, Appendix D Authentication"
       DEFVAL { none } -- no authentication, by default
       ::= { ospfAreaEntry 2 }

  ospfImportAsExtern OBJECT-TYPE
       SYNTAX       INTEGER {
                      importExternal (1),
                      importNoExternal (2),
                      importNssa (3)
                      }
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "Indicates if an area is a stub area, NSSA, or standard
          area.  Type-5 AS-external LSAs and type-11 Opaque LSAs are
          not imported into stub areas or NSSAs.  NSSAs import
          AS-external data as type-7 LSAs"
       REFERENCE
          "OSPF Version 2, Appendix C.2 Area parameters"
       DEFVAL { importExternal }
       ::= { ospfAreaEntry 3 }

  ospfSpfRuns OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The number of times that the intra-area route
          table has been calculated using this area's
          link state database.  This is typically done
          using Dijkstra's algorithm.

          Discontinuities in the value of this counter can occur
          at re-initialization of the management system, and at other
          times as indicated by the value of ospfDiscontinuityTime."
       ::= { ospfAreaEntry 4 }

  ospfAreaBdrRtrCount OBJECT-TYPE
       SYNTAX       Gauge32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The total number of Area Border Routers reachable
          within this area.  This is initially zero and is
          calculated in each Shortest Path First (SPF) pass."
       ::= { ospfAreaEntry 5 }

  ospfAsBdrRtrCount OBJECT-TYPE
       SYNTAX       Gauge32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The total number of Autonomous System Border
          Routers reachable within this area.  This is
          initially zero and is calculated in each SPF
          pass."
       ::= { ospfAreaEntry 6 }

  ospfAreaLsaCount OBJECT-TYPE
       SYNTAX       Gauge32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The total number of link state advertisements
          in this area's link state database, excluding
          AS-external LSAs."
       ::= { ospfAreaEntry 7 }

  ospfAreaLsaCksumSum OBJECT-TYPE
       SYNTAX       Integer32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The 32-bit sum of the link state
          advertisements' LS checksums contained in this
          area's link state database.  This sum excludes
          external (LS type-5) link state advertisements.
          The sum can be used to determine if there has
          been a change in a router's link state
          database, and to compare the link state database of
          two routers.  The value should be treated as unsigned
          when comparing two sums of checksums."
       DEFVAL { 0 }
       ::= { ospfAreaEntry 8 }

  ospfAreaSummary OBJECT-TYPE
       SYNTAX       INTEGER {
                       noAreaSummary (1),
                       sendAreaSummary (2)
                       }
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The variable ospfAreaSummary controls the
          import of summary LSAs into stub and NSSA areas.
          It has no effect on other areas.

          If it is noAreaSummary, the router will not
          originate summary LSAs into the stub or NSSA area.
          It will rely entirely on its default route.

          If it is sendAreaSummary, the router will both
          summarize and propagate summary LSAs."
       DEFVAL { noAreaSummary }
       ::= { ospfAreaEntry 9 }

  ospfAreaStatus OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "This object permits management of the table by
          facilitating actions such as row creation,
          construction, and destruction.

          The value of this object has no effect on
          whether other objects in this conceptual row can be
          modified."
       ::= { ospfAreaEntry 10 }

  ospfAreaNssaTranslatorRole OBJECT-TYPE
       SYNTAX       INTEGER { always (1), candidate (2) }
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "Indicates an NSSA border router's ability to
          perform NSSA translation of type-7 LSAs into
          type-5 LSAs."
       DEFVAL { candidate }
       ::= { ospfAreaEntry 11 }

  ospfAreaNssaTranslatorState OBJECT-TYPE
       SYNTAX       INTEGER { enabled (1),
                       elected (2),
                       disabled (3)
                       }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "Indicates if and how an NSSA border router is
          performing NSSA translation of type-7 LSAs into type-5
          LSAs.  When this object is set to enabled, the NSSA Border
          router's OspfAreaNssaExtTranslatorRole has been set to
          always.  When this object is set to elected, a candidate
          NSSA Border router is Translating type-7 LSAs into type-5.
          When this object is set to disabled, a candidate NSSA
          border router is NOT translating type-7 LSAs into type-5."
       ::= { ospfAreaEntry 12 }

  ospfAreaNssaTranslatorStabilityInterval OBJECT-TYPE
       SYNTAX       PositiveInteger
       UNITS        "seconds"
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The number of seconds after an elected translator
          determines its services are no longer required, that
          it should continue to perform its translation duties."
       DEFVAL { 40 }
       ::= { ospfAreaEntry 13 }

  ospfAreaNssaTranslatorEvents OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "Indicates the number of translator state changes
          that have occurred since the last boot-up.

          Discontinuities in the value of this counter can occur
          at re-initialization of the management system, and at other
          times as indicated by the value of ospfDiscontinuityTime."
       ::= { ospfAreaEntry 14 }

--  OSPF Area Default Metric Table

  ospfStubAreaTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF OspfStubAreaEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The set of metrics that will be advertised
          by a default Area Border Router into a stub area."
       REFERENCE
          "OSPF Version 2, Appendix C.2, Area Parameters"
       ::= { ospf 3 }

  ospfStubAreaEntry OBJECT-TYPE
       SYNTAX       OspfStubAreaEntry
       MAX-ACCESS   not-accessible
       STATUS      current
       DESCRIPTION
          "The metric for a given Type of Service that
          will be advertised by a default Area Border
          Router into a stub area.

          Information in this table is persistent and when this object
          is written the entity SHOULD save the change to non-volatile
          storage."
       REFERENCE
          "OSPF Version 2, Appendix C.2, Area Parameters"
       INDEX { ospfStubAreaId, ospfStubTOS }
       ::= { ospfStubAreaTable 1 }

  OspfStubAreaEntry ::=
       SEQUENCE {
          ospfStubAreaId
             AreaID,
          ospfStubTOS
             TOSType,
          ospfStubMetric
             BigMetric,
          ospfStubStatus
             RowStatus,
          ospfStubMetricType
             INTEGER
          }

  ospfStubAreaId OBJECT-TYPE
       SYNTAX       AreaID
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       current
       DESCRIPTION
          "The 32-bit identifier for the stub area.  On
          creation, this can be derived from the
          instance."
       ::= { ospfStubAreaEntry 1 }

  ospfStubTOS OBJECT-TYPE
       SYNTAX       TOSType
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       current
       DESCRIPTION
          "The Type of Service associated with the
          metric.  On creation, this can be derived from
          the instance."
       ::= { ospfStubAreaEntry 2 }

  ospfStubMetric OBJECT-TYPE
       SYNTAX       BigMetric
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The metric value applied at the indicated Type
          of Service.  By default, this equals the least
          metric at the Type of Service among the
          interfaces to other areas."
       ::= { ospfStubAreaEntry 3 }

  ospfStubStatus OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "This object permits management of the table by
          facilitating actions such as row creation,
          construction, and destruction.

          The value of this object has no effect on
          whether other objects in this conceptual row can be
          modified."
       ::= { ospfStubAreaEntry 4 }

  ospfStubMetricType OBJECT-TYPE
       SYNTAX       INTEGER {
                       ospfMetric (1),  -- OSPF Metric
                       comparableCost (2), -- external type 1
                       nonComparable  (3) -- external type 2
                       }
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "This variable displays the type of metric
          advertised as a default route."
       DEFVAL { ospfMetric }
       ::= { ospfStubAreaEntry 5 }

--  OSPF Link State Database

  ospfLsdbTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF OspfLsdbEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The OSPF Process's link state database (LSDB).
           The LSDB contains the link state advertisements
           from throughout the areas that the device is attached to."
       REFERENCE
          "OSPF Version 2, Section 12 Link State Advertisements"
       ::= { ospf 4 }

  ospfLsdbEntry OBJECT-TYPE
       SYNTAX   OspfLsdbEntry
       MAX-ACCESS   not-accessible
       STATUS   current
       DESCRIPTION
          "A single link state advertisement."
       INDEX { ospfLsdbAreaId, ospfLsdbType,
               ospfLsdbLsid, ospfLsdbRouterId }
       ::= { ospfLsdbTable 1 }

  OspfLsdbEntry ::=
       SEQUENCE {
          ospfLsdbAreaId
             AreaID,
          ospfLsdbType
             INTEGER,
          ospfLsdbLsid
             IpAddress,
          ospfLsdbRouterId
             RouterID,
          ospfLsdbSequence
             Integer32,
          ospfLsdbAge
             Integer32,
          ospfLsdbChecksum
             Integer32,
          ospfLsdbAdvertisement
             OCTET STRING
          }

  ospfLsdbAreaId OBJECT-TYPE
       SYNTAX       AreaID
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       current
       DESCRIPTION
          "The 32-bit identifier of the area from which
          the LSA was received."
       REFERENCE
          "OSPF Version 2, Appendix C.2 Area parameters"
       ::= { ospfLsdbEntry 1 }

  ospfLsdbType OBJECT-TYPE
       SYNTAX       INTEGER {
                       routerLink (1),
                       networkLink (2),
                       summaryLink (3),
                       asSummaryLink (4),
                       asExternalLink (5), -- but see ospfAsLsdbTable
                       multicastLink (6),
                       nssaExternalLink (7),
                       areaOpaqueLink (10)
                       }
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       current
       DESCRIPTION
          "The type of the link state advertisement.
          Each link state type has a separate advertisement
          format.

          Note: External link state advertisements are permitted
          for backward compatibility, but should be displayed
          in the ospfAsLsdbTable rather than here."
       REFERENCE
          "OSPF Version 2, Appendix A.4.1 The Link State
          Advertisement header"
       ::= { ospfLsdbEntry 2 }

  ospfLsdbLsid OBJECT-TYPE
       SYNTAX       IpAddress
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       current
       DESCRIPTION
          "The Link State ID is an LS Type Specific field
          containing either a Router ID or an IP address;
          it identifies the piece of the routing domain
          that is being described by the advertisement."
       REFERENCE
          "OSPF Version 2, Section 12.1.4 Link State ID"
       ::= { ospfLsdbEntry 3 }

  ospfLsdbRouterId OBJECT-TYPE
       SYNTAX       RouterID
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       current
       DESCRIPTION
          "The 32-bit number that uniquely identifies the
          originating router in the Autonomous System."
       REFERENCE
          "OSPF Version 2, Appendix C.1 Global parameters"
       ::= { ospfLsdbEntry 4 }

  ospfLsdbSequence OBJECT-TYPE
       SYNTAX       Integer32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The sequence number field is a signed 32-bit
          integer.  It starts with the value '80000001'h,
          or -'7FFFFFFF'h, and increments until '7FFFFFFF'h.
          Thus, a typical sequence number will be very negative.
          It is used to detect old and duplicate Link State
          Advertisements.  The space of sequence numbers is linearly
          ordered.  The larger the sequence number, the more recent
          the advertisement."
       REFERENCE
          "OSPF Version 2, Section 12.1.6 LS sequence
          number"
       ::= { ospfLsdbEntry 5 }

  ospfLsdbAge OBJECT-TYPE
       SYNTAX       Integer32 -- Should be 0..MaxAge, except when
                              -- doNotAge bit is set
       UNITS        "seconds"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "This field is the age of the link state advertisement
          in seconds."
       REFERENCE
          "OSPF Version 2, Section 12.1.1 LS age"
       ::= { ospfLsdbEntry 6 }

  ospfLsdbChecksum OBJECT-TYPE
       SYNTAX       Integer32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "This field is the checksum of the complete contents of
          the advertisement, excepting the age field.  The age field
          is excepted so that an advertisement's age can be
          incremented without updating the checksum.  The checksum
          used is the same that is used for ISO connectionless
          datagrams; it is commonly referred to as the
          Fletcher checksum."
        REFERENCE
           "OSPF Version 2, Section 12.1.7 LS checksum"
        ::= { ospfLsdbEntry 7 }

  ospfLsdbAdvertisement OBJECT-TYPE
       SYNTAX       OCTET STRING (SIZE (1..65535))
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The entire link state advertisement, including
          its header.

          Note that for variable length LSAs, SNMP agents
          may not be able to return the largest string size."
       REFERENCE
          "OSPF Version 2, Section 12 Link State Advertisements"
       ::= { ospfLsdbEntry 8 }

--  Address Range Table

  ospfAreaRangeTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF OspfAreaRangeEntry
       MAX-ACCESS   not-accessible
       STATUS       obsolete
       DESCRIPTION
          "The Address Range Table acts as an adjunct to the Area
           Table.  It describes those Address Range Summaries that
           are configured to be propagated from an Area to reduce
           the amount of information about it that is known beyond
           its borders.  It contains a set of IP address ranges
           specified by an IP address/IP network mask pair.
           For example, class B address range of X.X.X.X
           with a network mask of 255.255.0.0 includes all IP
           addresses from X.X.0.0 to X.X.255.255.

           Note that this table is obsoleted and is replaced
           by the Area Aggregate Table."
       REFERENCE
          "OSPF Version 2, Appendix C.2  Area parameters"
       ::= { ospf 5 }

  ospfAreaRangeEntry OBJECT-TYPE
       SYNTAX       OspfAreaRangeEntry
       MAX-ACCESS   not-accessible
       STATUS       obsolete
       DESCRIPTION
          "A single area address range.

          Information in this table is persistent and when this object
          is written the entity SHOULD save the change to non-volatile
          storage."
       REFERENCE
          "OSPF Version 2, Appendix C.2  Area parameters"
       INDEX { ospfAreaRangeAreaId, ospfAreaRangeNet }
       ::= { ospfAreaRangeTable 1 }

  OspfAreaRangeEntry ::=
       SEQUENCE {
          ospfAreaRangeAreaId
             AreaID,
          ospfAreaRangeNet
             IpAddress,
          ospfAreaRangeMask
             IpAddress,
          ospfAreaRangeStatus
             RowStatus,
          ospfAreaRangeEffect
             INTEGER
          }

  ospfAreaRangeAreaId OBJECT-TYPE
       SYNTAX       AreaID
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       obsolete
       DESCRIPTION
          "The area that the address range is to be found
          within."
       REFERENCE
          "OSPF Version 2, Appendix C.2 Area parameters"
       ::= { ospfAreaRangeEntry 1 }

  ospfAreaRangeNet OBJECT-TYPE
       SYNTAX       IpAddress
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       obsolete
       DESCRIPTION
          "The IP address of the net or subnet indicated
          by the range."
       REFERENCE
          "OSPF Version 2, Appendix C.2 Area parameters"
       ::= { ospfAreaRangeEntry 2 }
  ospfAreaRangeMask OBJECT-TYPE
       SYNTAX       IpAddress
       MAX-ACCESS   read-create
       STATUS       obsolete
       DESCRIPTION
          "The subnet mask that pertains to the net or
          subnet."
       REFERENCE
          "OSPF Version 2, Appendix C.2 Area parameters"
       ::= { ospfAreaRangeEntry 3 }

  ospfAreaRangeStatus OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-create
       STATUS       obsolete
       DESCRIPTION
          "This object permits management of the table by
          facilitating actions such as row creation,
          construction, and destruction.

          The value of this object has no effect on
          whether other objects in this conceptual row can be
          modified."
       ::= { ospfAreaRangeEntry 4 }

  ospfAreaRangeEffect OBJECT-TYPE
       SYNTAX       INTEGER {
                       advertiseMatching (1),
                       doNotAdvertiseMatching (2)
                       }
       MAX-ACCESS   read-create
       STATUS       obsolete
       DESCRIPTION
          "Subnets subsumed by ranges either trigger the
          advertisement of the indicated summary
         (advertiseMatching) or result in the subnet's not
          being advertised at all outside the area."
       DEFVAL { advertiseMatching }
       ::= { ospfAreaRangeEntry 5 }

--  OSPF Host Table

  ospfHostTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF OspfHostEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The Host/Metric Table indicates what hosts are directly
          attached to the router, what metrics and types
          of service should be advertised for them,
          and what areas they are found within."
       REFERENCE
          "OSPF Version 2, Appendix C.7 Host route
          parameters"
       ::= { ospf 6 }

  ospfHostEntry OBJECT-TYPE
       SYNTAX       OspfHostEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "A metric to be advertised, for a given type of
          service, when a given host is reachable.

          Information in this table is persistent and when this object
          is written the entity SHOULD save the change to non-volatile
          storage."
       INDEX { ospfHostIpAddress, ospfHostTOS }
       ::= { ospfHostTable 1 }

  OspfHostEntry ::=
       SEQUENCE {
          ospfHostIpAddress
             IpAddress,
          ospfHostTOS
             TOSType,
          ospfHostMetric
             Metric,
          ospfHostStatus
             RowStatus,
          ospfHostAreaID
             AreaID,
          ospfHostCfgAreaID
             AreaID
          }

  ospfHostIpAddress OBJECT-TYPE
       SYNTAX       IpAddress
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       current
       DESCRIPTION
          "The IP address of the host."
       REFERENCE
          "OSPF Version 2, Appendix C.7 Host route parameters"
       ::= { ospfHostEntry 1 }
  ospfHostTOS OBJECT-TYPE
       SYNTAX       TOSType
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       current
       DESCRIPTION
          "The Type of Service of the route being configured."
       REFERENCE
          "OSPF Version 2, Appendix C.7 Host route parameters"
       ::= { ospfHostEntry 2 }

  ospfHostMetric OBJECT-TYPE
       SYNTAX       Metric
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The metric to be advertised."
       REFERENCE
          "OSPF Version 2, Appendix C.7 Host route parameters"
       ::= { ospfHostEntry 3 }

  ospfHostStatus OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "This object permits management of the table by
          facilitating actions such as row creation,
          construction, and destruction.

          The value of this object has no effect on
          whether other objects in this conceptual row can be
          modified."
       ::= { ospfHostEntry 4 }

  ospfHostAreaID OBJECT-TYPE
       SYNTAX       AreaID
       MAX-ACCESS   read-only
       STATUS       deprecated
       DESCRIPTION
          "The OSPF area to which the host belongs.
          Deprecated by ospfHostCfgAreaID."
       REFERENCE
          "OSPF Version 2, Appendix C.7 Host parameters"
       ::= { ospfHostEntry 5 }

  ospfHostCfgAreaID OBJECT-TYPE
       SYNTAX       AreaID
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "To configure the OSPF area to which the host belongs."
       REFERENCE
          "OSPF Version 2, Appendix C.7 Host parameters"
       ::= { ospfHostEntry 6 }

--  OSPF Interface Table

  ospfIfTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF OspfIfEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The OSPF Interface Table describes the interfaces
          from the viewpoint of OSPF.
          It augments the ipAddrTable with OSPF specific information."
       REFERENCE
          "OSPF Version 2, Appendix C.3  Router interface
          parameters"
       ::= { ospf 7 }

  ospfIfEntry OBJECT-TYPE
       SYNTAX       OspfIfEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The OSPF interface entry describes one interface
          from the viewpoint of OSPF.

          Information in this table is persistent and when this object
          is written the entity SHOULD save the change to non-volatile
          storage."
       INDEX { ospfIfIpAddress, ospfAddressLessIf }
       ::= { ospfIfTable 1 }

  OspfIfEntry ::=
       SEQUENCE {
          ospfIfIpAddress
             IpAddress,
          ospfAddressLessIf
             InterfaceIndexOrZero,
          ospfIfAreaId
             AreaID,
          ospfIfType
             INTEGER,
          ospfIfAdminStat
             Status,
          ospfIfRtrPriority
             DesignatedRouterPriority,
          ospfIfTransitDelay
             UpToMaxAge,
          ospfIfRetransInterval
             UpToMaxAge,
          ospfIfHelloInterval
             HelloRange,
          ospfIfRtrDeadInterval
             PositiveInteger,
          ospfIfPollInterval
             PositiveInteger,
          ospfIfState
             INTEGER,
          ospfIfDesignatedRouter
             IpAddress,
          ospfIfBackupDesignatedRouter
             IpAddress,
          ospfIfEvents
             Counter32,
          ospfIfAuthKey
             OCTET STRING,
          ospfIfStatus
             RowStatus,
          ospfIfMulticastForwarding
             INTEGER,
          ospfIfDemand
             TruthValue,
          ospfIfAuthType
             OspfAuthenticationType,
          ospfIfLsaCount
             Gauge32,
          ospfIfLsaCksumSum
             Unsigned32,
          ospfIfDesignatedRouterId
             RouterID,
          ospfIfBackupDesignatedRouterId
             RouterID
          }

  ospfIfIpAddress OBJECT-TYPE
       SYNTAX       IpAddress
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       current
       DESCRIPTION
          "The IP address of this OSPF interface."
       ::= { ospfIfEntry 1 }

  ospfAddressLessIf OBJECT-TYPE
       SYNTAX       InterfaceIndexOrZero
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       current
       DESCRIPTION
          "For the purpose of easing the instancing of
          addressed and addressless interfaces; this
          variable takes the value 0 on interfaces with
          IP addresses and the corresponding value of
          ifIndex for interfaces having no IP address."
       ::= { ospfIfEntry 2 }

  ospfIfAreaId OBJECT-TYPE
       SYNTAX       AreaID
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "A 32-bit integer uniquely identifying the area
          to which the interface connects.  Area ID
          0.0.0.0 is used for the OSPF backbone."
       DEFVAL { '00000000'H }  -- 0.0.0.0
       ::= { ospfIfEntry 3 }

  ospfIfType OBJECT-TYPE
       SYNTAX       INTEGER {
                       broadcast (1),
                       nbma (2),
                       pointToPoint (3),
                       pointToMultipoint (5)
                       }
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The OSPF interface type.
          By way of a default, this field may be intuited
          from the corresponding value of ifType.
          Broadcast LANs, such as Ethernet and IEEE 802.5,
          take the value 'broadcast', X.25 and similar
          technologies take the value 'nbma', and links
          that are definitively point to point take the
          value 'pointToPoint'."
        ::= { ospfIfEntry 4 }

  ospfIfAdminStat OBJECT-TYPE
       SYNTAX       Status
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The OSPF interface's administrative status.
          The value formed on the interface, and the interface
          will be advertised as an internal route to some area.
          The value 'disabled' denotes that the interface is
          external to OSPF."
       DEFVAL { enabled }
       ::= { ospfIfEntry 5 }

  ospfIfRtrPriority OBJECT-TYPE
       SYNTAX       DesignatedRouterPriority
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The priority of this interface.  Used in
          multi-access networks, this field is used in
          the designated router election algorithm.  The
          value 0 signifies that the router is not eligible
          to become the designated router on this particular
          network.  In the event of a tie in this value,
          routers will use their Router ID as a tie breaker."
        DEFVAL { 1 }
        ::= { ospfIfEntry 6 }

  ospfIfTransitDelay OBJECT-TYPE
        SYNTAX       UpToMaxAge
        UNITS        "seconds"
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION
           "The estimated number of seconds it takes to
           transmit a link state update packet over this
           interface.  Note that the minimal value SHOULD be
           1 second."
        DEFVAL { 1 }
        ::= { ospfIfEntry 7 }

  ospfIfRetransInterval OBJECT-TYPE
       SYNTAX       UpToMaxAge
       UNITS        "seconds"
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The number of seconds between link state advertisement
          retransmissions, for adjacencies belonging to this
          interface.  This value is also used when retransmitting
          database description and Link State request packets.
          Note that minimal value SHOULD be 1 second."
       DEFVAL { 5 }
       ::= { ospfIfEntry 8 }

  ospfIfHelloInterval OBJECT-TYPE
       SYNTAX       HelloRange
       UNITS        "seconds"
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The length of time, in seconds, between the Hello packets
          that the router sends on the interface.  This value must be
          the same for all routers attached to a common network."
       DEFVAL { 10 }
       ::= { ospfIfEntry 9 }

  ospfIfRtrDeadInterval OBJECT-TYPE
       SYNTAX       PositiveInteger
       UNITS        "seconds"
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The number of seconds that a router's Hello packets have
          not been seen before its neighbors declare the router down.
          This should be some multiple of the Hello interval.  This
          value must be the same for all routers attached to a common
          network."
        DEFVAL { 40 }
        ::= { ospfIfEntry 10 }

  ospfIfPollInterval OBJECT-TYPE
       SYNTAX       PositiveInteger
       UNITS        "seconds"
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The larger time interval, in seconds, between the Hello
          packets sent to an inactive non-broadcast multi-access
          neighbor."
       DEFVAL { 120 }
       ::= { ospfIfEntry 11 }

  ospfIfState OBJECT-TYPE
       SYNTAX       INTEGER {
                       down (1),
                       loopback (2),
                       waiting (3),
                       pointToPoint (4),
                       designatedRouter (5),
                       backupDesignatedRouter (6),
                       otherDesignatedRouter (7)
                       }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The OSPF Interface State."
       DEFVAL { down }
       ::= { ospfIfEntry 12 }

  ospfIfDesignatedRouter OBJECT-TYPE
       SYNTAX       IpAddress
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The IP address of the designated router."
       DEFVAL { '00000000'H } -- 0.0.0.0
       ::= { ospfIfEntry 13 }

  ospfIfBackupDesignatedRouter OBJECT-TYPE
       SYNTAX       IpAddress
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The IP address of the backup designated
          router."
       DEFVAL { '00000000'H }  -- 0.0.0.0
       ::= { ospfIfEntry 14 }

  ospfIfEvents OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The number of times this OSPF interface has
          changed its state or an error has occurred.

          Discontinuities in the value of this counter can occur
          at re-initialization of the management system, and at other
          times as indicated by the value of ospfDiscontinuityTime."
       ::= { ospfIfEntry 15 }

  ospfIfAuthKey OBJECT-TYPE
       SYNTAX       OCTET STRING (SIZE (0..256))
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The simple password used as an OSPF
          authentication key when simplePassword security
          is enabled.  This object does not access any OSPF
          cryptogaphic authentication key under
          any circumstance.

          If the key length is shorter than 8 octets, the
          agent will left adjust and zero fill to 8 octets.

          Unauthenticated interfaces need no authentication
          key, and simple password authentication cannot use
          a key of more than 8 octets.

          Note that the use of simplePassword authentication
          is NOT recommended when there is concern regarding
          attack upon the OSPF system.  SimplePassword
          authentication is only sufficient to protect against
          accidental misconfigurations because it re-uses
          simple password. [RFC1704]

          When read, ospfIfAuthKey always returns an octet
          string of length zero."
       REFERENCE
          "OSPF Version 2, Section 9 The Interface Data
          Structure"
       DEFVAL { '0000000000000000'H } -- 0.0.0.0.0.0.0.0
       ::= { ospfIfEntry 16 }

  ospfIfStatus OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "This object permits management of the table by
          facilitating actions such as row creation,
          construction, and destruction.

          The value of this object has no effect on
          whether other objects in this conceptual row can be
          modified."
       ::= { ospfIfEntry 17 }

  ospfIfMulticastForwarding OBJECT-TYPE
       SYNTAX       INTEGER {
                       blocked (1), -- no multicast forwarding
                       multicast (2), -- using multicast address
                       unicast (3) -- to each OSPF neighbor
                       }
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The way multicasts should be forwarded on this
          interface: not forwarded, forwarded as data
          link multicasts, or forwarded as data link
          unicasts.  Data link multicasting is not
          meaningful on point-to-point and NBMA interfaces,
          and setting ospfMulticastForwarding to 0 effectively
          disables all multicast forwarding."
       DEFVAL { blocked }
       ::= { ospfIfEntry 18 }

  ospfIfDemand OBJECT-TYPE
       SYNTAX       TruthValue
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "Indicates whether Demand OSPF procedures (hello
          suppression to FULL neighbors and setting the
          DoNotAge flag on propagated LSAs) should be
          performed on this interface."
       DEFVAL { false }
       ::= { ospfIfEntry 19 }

  ospfIfAuthType OBJECT-TYPE
       SYNTAX       OspfAuthenticationType
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The authentication type specified for an interface.

          Note that this object can be used to engage
          in significant attacks against an OSPF router."
       REFERENCE
          "OSPF Version 2, Appendix D Authentication"
       DEFVAL { none } -- no authentication, by default
       ::= { ospfIfEntry 20 }

  ospfIfLsaCount OBJECT-TYPE
       SYNTAX       Gauge32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The total number of link-local link state advertisements
          in this interface's link-local link state database."
       ::= { ospfIfEntry 21 }
  ospfIfLsaCksumSum OBJECT-TYPE
       SYNTAX       Unsigned32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The 32-bit unsigned sum of the Link State
          Advertisements' LS checksums contained in this
          interface's link-local link state database.
          The sum can be used to determine if there has
          been a change in the interface's link state
          database and to compare the interface link state
          database of routers attached to the same subnet."
       ::= { ospfIfEntry 22 }

  ospfIfDesignatedRouterId OBJECT-TYPE
       SYNTAX       RouterID
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The Router ID of the designated router."
       ::= { ospfIfEntry 23 }

  ospfIfBackupDesignatedRouterId OBJECT-TYPE
       SYNTAX       RouterID
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The Router ID of the backup designated router."
       ::= { ospfIfEntry 24 }

--  OSPF Interface Metric Table

  ospfIfMetricTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF OspfIfMetricEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The Metric Table describes the metrics to be advertised
          for a specified interface at the various types of service.
          As such, this table is an adjunct of the OSPF Interface
          Table.

          Types of service, as defined by RFC 791, have the ability
          to request low delay, high bandwidth, or reliable linkage.

          For the purposes of this specification, the measure of
          bandwidth:
          Metric = referenceBandwidth / ifSpeed

          is the default value.
          The default reference bandwidth is 10^8.
          For multiple link interfaces, note that ifSpeed is the sum
          of the individual link speeds.  This yields a number having
          the following typical values:

          Network Type/bit rate   Metric

          >= 100 MBPS                 1
          Ethernet/802.3             10
          E1                         48
          T1 (ESF)                   65
          64 KBPS                    1562
          56 KBPS                    1785
          19.2 KBPS                  5208
          9.6 KBPS                   10416

          Routes that are not specified use the default
          (TOS 0) metric.

          Note that the default reference bandwidth can be configured
          using the general group object ospfReferenceBandwidth."
       REFERENCE
          "OSPF Version 2, Appendix C.3 Router interface
          parameters"
       ::= { ospf 8 }

  ospfIfMetricEntry OBJECT-TYPE
       SYNTAX       OspfIfMetricEntry
       MAX-ACCESS   not-accessible
       STATUS      current
       DESCRIPTION
          "A particular TOS metric for a non-virtual interface
          identified by the interface index.

          Information in this table is persistent and when this object
          is written the entity SHOULD save the change to non-volatile
          storage."
       REFERENCE
          "OSPF Version 2, Appendix C.3 Router interface
          parameters"
       INDEX { ospfIfMetricIpAddress,
          ospfIfMetricAddressLessIf,
          ospfIfMetricTOS }
       ::= { ospfIfMetricTable 1 }
  OspfIfMetricEntry ::=
       SEQUENCE {
          ospfIfMetricIpAddress
             IpAddress,
          ospfIfMetricAddressLessIf
             InterfaceIndexOrZero,
          ospfIfMetricTOS
             TOSType,
          ospfIfMetricValue
             Metric,
          ospfIfMetricStatus
             RowStatus
          }

  ospfIfMetricIpAddress OBJECT-TYPE
       SYNTAX       IpAddress
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       current
       DESCRIPTION
          "The IP address of this OSPF interface.  On row
          creation, this can be derived from the instance."
       ::= { ospfIfMetricEntry 1 }

  ospfIfMetricAddressLessIf OBJECT-TYPE
       SYNTAX       InterfaceIndexOrZero
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       current
       DESCRIPTION
          "For the purpose of easing the instancing of
          addressed and addressless interfaces; this
          variable takes the value 0 on interfaces with
          IP addresses and the value of ifIndex for
          interfaces having no IP address.  On row
          creation, this can be derived from the instance."
        ::= { ospfIfMetricEntry 2 }

  ospfIfMetricTOS OBJECT-TYPE
       SYNTAX       TOSType
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       current
       DESCRIPTION
          "The Type of Service metric being referenced.
          On row creation, this can be derived from the
          instance."
       ::= { ospfIfMetricEntry 3 }
  ospfIfMetricValue OBJECT-TYPE
       SYNTAX       Metric
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The metric of using this Type of Service on
          this interface.  The default value of the TOS 0
          metric is 10^8 / ifSpeed."
       ::= { ospfIfMetricEntry 4 }

  ospfIfMetricStatus OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "This object permits management of the table by
          facilitating actions such as row creation,
          construction, and destruction.

          The value of this object has no effect on
          whether other objects in this conceptual row can be
          modified."
       ::= { ospfIfMetricEntry 5 }

--  OSPF Virtual Interface Table

  ospfVirtIfTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF OspfVirtIfEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "Information about this router's virtual interfaces
          that the OSPF Process is configured to carry on."
       REFERENCE
          "OSPF Version 2, Appendix C.4  Virtual link
          parameters"
       ::= { ospf 9 }

  ospfVirtIfEntry OBJECT-TYPE
       SYNTAX       OspfVirtIfEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "Information about a single virtual interface.

          Information in this table is persistent and when this object
          is written the entity SHOULD save the change to non-volatile
          storage."
       INDEX { ospfVirtIfAreaId, ospfVirtIfNeighbor }
       ::= { ospfVirtIfTable 1 }

  OspfVirtIfEntry ::=
       SEQUENCE {
          ospfVirtIfAreaId
             AreaID,
          ospfVirtIfNeighbor
             RouterID,
          ospfVirtIfTransitDelay
             UpToMaxAge,
          ospfVirtIfRetransInterval
             UpToMaxAge,
          ospfVirtIfHelloInterval
             HelloRange,
          ospfVirtIfRtrDeadInterval
             PositiveInteger,
          ospfVirtIfState
             INTEGER,
          ospfVirtIfEvents
             Counter32,
          ospfVirtIfAuthKey
             OCTET STRING,
          ospfVirtIfStatus
             RowStatus,
          ospfVirtIfAuthType
             OspfAuthenticationType,
          ospfVirtIfLsaCount
             Gauge32,
          ospfVirtIfLsaCksumSum
             Unsigned32
          }

  ospfVirtIfAreaId OBJECT-TYPE
       SYNTAX       AreaID
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       current
       DESCRIPTION
          "The transit area that the virtual link
          traverses.  By definition, this is not 0.0.0.0."
       ::= { ospfVirtIfEntry 1 }

  ospfVirtIfNeighbor OBJECT-TYPE
       SYNTAX       RouterID
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       current
       DESCRIPTION
          "The Router ID of the virtual neighbor."
       ::= { ospfVirtIfEntry 2 }

  ospfVirtIfTransitDelay OBJECT-TYPE
       SYNTAX       UpToMaxAge
       UNITS        "seconds"
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The estimated number of seconds it takes to
          transmit a Link State update packet over this
          interface.  Note that the minimal value SHOULD be
          1 second."
       DEFVAL { 1 }
       ::= { ospfVirtIfEntry 3 }

  ospfVirtIfRetransInterval OBJECT-TYPE
       SYNTAX       UpToMaxAge
       UNITS        "seconds"
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The number of seconds between link state
          avertisement retransmissions, for adjacencies
          belonging to this interface.  This value is
          also used when retransmitting database
          description and Link State request packets.  This
          value should be well over the expected
          round-trip time.  Note that the minimal value SHOULD be
          1 second."
       DEFVAL { 5 }
       ::= { ospfVirtIfEntry 4 }

  ospfVirtIfHelloInterval OBJECT-TYPE
       SYNTAX       HelloRange
       UNITS        "seconds"
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The length of time, in seconds, between the
          Hello packets that the router sends on the
          interface.  This value must be the same for the
          virtual neighbor."
       DEFVAL { 10 }
       ::= { ospfVirtIfEntry 5 }

  ospfVirtIfRtrDeadInterval OBJECT-TYPE
       SYNTAX       PositiveInteger
       UNITS        "seconds"
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The number of seconds that a router's Hello
          packets have not been seen before its
          neighbors declare the router down.  This should be
          some multiple of the Hello interval.  This
          value must be the same for the virtual neighbor."
       DEFVAL { 60 }
       ::= { ospfVirtIfEntry 6 }

  ospfVirtIfState OBJECT-TYPE
       SYNTAX       INTEGER {
                       down (1), -- these use the same encoding
                       pointToPoint (4) -- as the ospfIfTable
                       }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "OSPF virtual interface states."
       DEFVAL { down }
       ::= { ospfVirtIfEntry 7 }

  ospfVirtIfEvents OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The number of state changes or error events on
          this virtual link.

          Discontinuities in the value of this counter can occur
          at re-initialization of the management system, and at other
          times as indicated by the value of ospfDiscontinuityTime."
       ::= { ospfVirtIfEntry 8 }

  ospfVirtIfAuthKey OBJECT-TYPE
       SYNTAX       OCTET STRING (SIZE(0..256))
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The simple password used as an OSPF
          authentication key when simplePassword security
          is enabled.  This object does not access any OSPF
          cryptogaphic authentication key under
          any circumstance.
          If the key length is shorter than 8 octets, the
          agent will left adjust and zero fill to 8 octets.

          Unauthenticated interfaces need no authentication
          key, and simple password authentication cannot use
          a key of more than 8 octets.

          Note that the use of simplePassword authentication
          is NOT recommended when there is concern regarding
          attack upon the OSPF system.  SimplePassword
          authentication is only sufficient to protect against
          accidental misconfigurations because it re-uses
          simple password.  [RFC1704]

          When read, ospfIfAuthKey always returns an octet
          string of length zero."
       REFERENCE
          "OSPF Version 2, Section 9 The Interface Data
          Structure"
       DEFVAL { '0000000000000000'H } -- 0.0.0.0.0.0.0.0
       ::= { ospfVirtIfEntry 9 }

  ospfVirtIfStatus OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "This object permits management of the table by
          facilitating actions such as row creation,
          construction, and destruction.

          The value of this object has no effect on
          whether other objects in this conceptual row can be
          modified."
        ::= { ospfVirtIfEntry 10 }

  ospfVirtIfAuthType OBJECT-TYPE
       SYNTAX       OspfAuthenticationType
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The authentication type specified for a virtual interface.

          Note that this object can be used to engage
          in significant attacks against an OSPF router."
       REFERENCE
          "OSPF Version 2, Appendix E Authentication"
       DEFVAL { none } -- no authentication, by default
       ::= { ospfVirtIfEntry 11 }

  ospfVirtIfLsaCount OBJECT-TYPE
       SYNTAX       Gauge32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The total number of link-local link state advertisements
          in this virtual interface's link-local link state database."
       ::= { ospfVirtIfEntry 12 }

  ospfVirtIfLsaCksumSum OBJECT-TYPE
       SYNTAX       Unsigned32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The 32-bit unsigned sum of the link state
          advertisements' LS checksums contained in this
          virtual interface's link-local link state database.
          The sum can be used to determine if there has
          been a change in the virtual interface's link state
          database, and to compare the virtual interface
          link state database of the virtual neighbors."
       ::= { ospfVirtIfEntry 13 }

--  OSPF Neighbor Table

  ospfNbrTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF OspfNbrEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "A table describing all non-virtual neighbors
          in the locality of the OSPF router."
       REFERENCE
          "OSPF Version 2, Section 10 The Neighbor Data
          Structure"
       ::= { ospf 10 }

  ospfNbrEntry OBJECT-TYPE
       SYNTAX       OspfNbrEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The information regarding a single neighbor.

          Information in this table is persistent and when this object
          is written the entity SHOULD save the change to non-volatile
          storage."
       REFERENCE
          "OSPF Version 2, Section 10 The Neighbor Data
          Structure"
       INDEX { ospfNbrIpAddr, ospfNbrAddressLessIndex }
       ::= { ospfNbrTable 1 }

  OspfNbrEntry ::=
       SEQUENCE {
          ospfNbrIpAddr
             IpAddress,
          ospfNbrAddressLessIndex
             InterfaceIndexOrZero,
          ospfNbrRtrId
             RouterID,
          ospfNbrOptions
             Integer32,
          ospfNbrPriority
             DesignatedRouterPriority,
          ospfNbrState
             INTEGER,
          ospfNbrEvents
             Counter32,
          ospfNbrLsRetransQLen
             Gauge32,
          ospfNbmaNbrStatus
             RowStatus,
          ospfNbmaNbrPermanence
             INTEGER,
          ospfNbrHelloSuppressed
             TruthValue,
          ospfNbrRestartHelperStatus
             INTEGER,
          ospfNbrRestartHelperAge
             Unsigned32,
          ospfNbrRestartHelperExitReason
             INTEGER
          }

  ospfNbrIpAddr OBJECT-TYPE
       SYNTAX       IpAddress
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       current
       DESCRIPTION
          "The IP address this neighbor is using in its
          IP source address.  Note that, on addressless
          links, this will not be 0.0.0.0 but the
          address of another of the neighbor's interfaces."
       ::= { ospfNbrEntry 1 }

   ospfNbrAddressLessIndex OBJECT-TYPE
       SYNTAX       InterfaceIndexOrZero
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       current
       DESCRIPTION
          "On an interface having an IP address, zero.
          On addressless interfaces, the corresponding
          value of ifIndex in the Internet Standard MIB.
          On row creation, this can be derived from the
          instance."
        ::= { ospfNbrEntry 2 }

  ospfNbrRtrId OBJECT-TYPE
       SYNTAX       RouterID
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "A 32-bit integer (represented as a type
          IpAddress) uniquely identifying the neighboring
          router in the Autonomous System."
       DEFVAL { '00000000'H } -- 0.0.0.0
       ::= { ospfNbrEntry 3 }

  ospfNbrOptions OBJECT-TYPE
       SYNTAX       Integer32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "A bit mask corresponding to the neighbor's
          options field.

          Bit 0, if set, indicates that the system will
          operate on Type of Service metrics other than
          TOS 0.  If zero, the neighbor will ignore all
          metrics except the TOS 0 metric.

          Bit 1, if set, indicates that the associated
          area accepts and operates on external
          information; if zero, it is a stub area.

          Bit 2, if set, indicates that the system is
          capable of routing IP multicast datagrams, that is
          that it implements the multicast extensions to
          OSPF.
          Bit 3, if set, indicates that the associated
          area is an NSSA.  These areas are capable of
          carrying type-7 external advertisements, which
          are translated into type-5 external advertisements
          at NSSA borders."
       REFERENCE
           "OSPF Version 2, Section 12.1.2 Options"
       DEFVAL { 0 }
       ::= { ospfNbrEntry 4 }

   ospfNbrPriority OBJECT-TYPE
       SYNTAX       DesignatedRouterPriority
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The priority of this neighbor in the designated
          router election algorithm.  The value 0 signifies
          that the neighbor is not eligible to become
          the designated router on this particular network."

       DEFVAL { 1 }
       ::= { ospfNbrEntry 5 }

   ospfNbrState OBJECT-TYPE
        SYNTAX       INTEGER {
                         down (1),
                         attempt (2),
                         init (3),
                         twoWay (4),
                         exchangeStart (5),
                         exchange (6),
                         loading (7),
                         full (8)
                         }
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "The state of the relationship with this neighbor."
         REFERENCE
            "OSPF Version 2, Section 10.1 Neighbor States"
         DEFVAL { down }
         ::= { ospfNbrEntry 6 }

  ospfNbrEvents OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The number of times this neighbor relationship
          has changed state or an error has occurred.

          Discontinuities in the value of this counter can occur
          at re-initialization of the management system, and at other
          times as indicated by the value of ospfDiscontinuityTime."
       ::= { ospfNbrEntry 7 }

  ospfNbrLsRetransQLen OBJECT-TYPE
       SYNTAX       Gauge32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The current length of the retransmission
          queue."
       ::= { ospfNbrEntry 8 }

  ospfNbmaNbrStatus OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "This object permits management of the table by
          facilitating actions such as row creation,
          construction, and destruction.

          The value of this object has no effect on
          whether other objects in this conceptual row can be
          modified."
       ::= { ospfNbrEntry 9 }

  ospfNbmaNbrPermanence OBJECT-TYPE
       SYNTAX       INTEGER {
                       dynamic (1), -- learned through protocol
                       permanent (2) -- configured address
                       }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "This variable displays the status of the entry;
          'dynamic' and 'permanent' refer to how the neighbor
          became known."
       DEFVAL { permanent }
       ::= { ospfNbrEntry 10 }

   ospfNbrHelloSuppressed OBJECT-TYPE
       SYNTAX       TruthValue
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "Indicates whether Hellos are being suppressed
          to the neighbor."
       ::= { ospfNbrEntry 11 }

  ospfNbrRestartHelperStatus OBJECT-TYPE
       SYNTAX       INTEGER { notHelping (1),
                              helping (2)
                            }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "Indicates whether the router is acting
          as a graceful restart helper for the neighbor."
          ::= { ospfNbrEntry 12 }

  ospfNbrRestartHelperAge OBJECT-TYPE
       SYNTAX       Unsigned32
       UNITS        "seconds"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "Remaining time in current OSPF graceful restart
          interval, if the router is acting as a restart
          helper for the neighbor."
       ::= { ospfNbrEntry 13 }

  ospfNbrRestartHelperExitReason OBJECT-TYPE
       SYNTAX       INTEGER { none (1),           -- not attempted
                              inProgress (2),     -- restart in
                                                  -- progress
                              completed (3),      -- successfully
                                                  -- completed
                              timedOut (4),       -- timed out
                              topologyChanged (5) -- aborted due to
                                                  -- topology
                                                  -- change.
                            }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "Describes the outcome of the last attempt at acting
           as a graceful restart helper for the neighbor."
       ::= { ospfNbrEntry 14 }

--  OSPF Virtual Neighbor Table
  ospfVirtNbrTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF OspfVirtNbrEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "This table describes all virtual neighbors.
          Since virtual links are configured
          in the Virtual Interface Table, this table is read-only."
       REFERENCE
          "OSPF Version 2, Section 15 Virtual Links"
       ::= { ospf 11 }

  ospfVirtNbrEntry OBJECT-TYPE
       SYNTAX       OspfVirtNbrEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "Virtual neighbor information."
       INDEX { ospfVirtNbrArea, ospfVirtNbrRtrId }
       ::= { ospfVirtNbrTable 1 }

  OspfVirtNbrEntry ::=
       SEQUENCE {
          ospfVirtNbrArea
             AreaID,
          ospfVirtNbrRtrId
             RouterID,
          ospfVirtNbrIpAddr
             IpAddress,
          ospfVirtNbrOptions
             Integer32,
          ospfVirtNbrState
             INTEGER,
          ospfVirtNbrEvents
             Counter32,
          ospfVirtNbrLsRetransQLen
             Gauge32,
          ospfVirtNbrHelloSuppressed
             TruthValue,
          ospfVirtNbrRestartHelperStatus
             INTEGER,
          ospfVirtNbrRestartHelperAge
             Unsigned32,
          ospfVirtNbrRestartHelperExitReason
             INTEGER
          }

  ospfVirtNbrArea OBJECT-TYPE
       SYNTAX       AreaID
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       current
       DESCRIPTION
          "The Transit Area Identifier."
       ::= { ospfVirtNbrEntry 1 }

  ospfVirtNbrRtrId OBJECT-TYPE
       SYNTAX       RouterID
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS      current
       DESCRIPTION
          "A 32-bit integer uniquely identifying the
          neighboring router in the Autonomous System."
       ::= { ospfVirtNbrEntry 2 }

  ospfVirtNbrIpAddr OBJECT-TYPE
       SYNTAX       IpAddress
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The IP address this virtual neighbor is using."
       ::= { ospfVirtNbrEntry 3 }

  ospfVirtNbrOptions OBJECT-TYPE
       SYNTAX       Integer32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "A bit mask corresponding to the neighbor's
          options field.

          Bit 1, if set, indicates that the system will
          operate on Type of Service metrics other than
          TOS 0.  If zero, the neighbor will ignore all
          metrics except the TOS 0 metric.

          Bit 2, if set, indicates that the system is
          network multicast capable, i.e., that it
          implements OSPF multicast routing."
       ::= { ospfVirtNbrEntry 4 }

   ospfVirtNbrState OBJECT-TYPE
       SYNTAX       INTEGER {
                       down (1),
                       attempt (2),
                       init (3),
                       twoWay (4),
                       exchangeStart (5),
                       exchange (6),
                       loading (7),
                       full (8)
                       }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The state of the virtual neighbor relationship."
       ::= { ospfVirtNbrEntry 5 }

  ospfVirtNbrEvents OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The number of times this virtual link has
          changed its state or an error has occurred.

          Discontinuities in the value of this counter can occur
          at re-initialization of the management system, and at other
          times as indicated by the value of ospfDiscontinuityTime."
       ::= { ospfVirtNbrEntry 6 }

  ospfVirtNbrLsRetransQLen OBJECT-TYPE
       SYNTAX       Gauge32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The current length of the retransmission
          queue."
       ::= { ospfVirtNbrEntry 7 }

  ospfVirtNbrHelloSuppressed OBJECT-TYPE
       SYNTAX       TruthValue
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "Indicates whether Hellos are being suppressed
          to the neighbor."
       ::= { ospfVirtNbrEntry 8 }

  ospfVirtNbrRestartHelperStatus OBJECT-TYPE
       SYNTAX       INTEGER { notHelping (1),
                              helping (2)
                            }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "Indicates whether the router is acting
          as a graceful restart helper for the neighbor."
       ::= { ospfVirtNbrEntry 9 }

  ospfVirtNbrRestartHelperAge OBJECT-TYPE
       SYNTAX       Unsigned32
       UNITS        "seconds"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "Remaining time in current OSPF graceful restart
          interval, if the router is acting as a restart
          helper for the neighbor."
       ::= { ospfVirtNbrEntry 10 }

  ospfVirtNbrRestartHelperExitReason OBJECT-TYPE
       SYNTAX       INTEGER { none (1),           -- not attempted
                              inProgress (2),     -- restart in
                                                  -- progress
                              completed (3),      -- successfully
                                                  -- completed
                              timedOut (4),       -- timed out
                              topologyChanged (5) -- aborted due to
                                                  -- topology
                                                  -- change.
                            }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "Describes the outcome of the last attempt at acting
           as a graceful restart helper for the neighbor."
       ::= { ospfVirtNbrEntry 11 }

--  OSPF Link State Database, External

  ospfExtLsdbTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF OspfExtLsdbEntry
       MAX-ACCESS   not-accessible
       STATUS       deprecated
       DESCRIPTION
          "The OSPF Process's external LSA link state database.

          This table is identical to the OSPF LSDB Table
          in format, but contains only external link state
          advertisements.  The purpose is to allow external
          LSAs to be displayed once for the router rather
          than once in each non-stub area.

          Note that external LSAs are also in the AS-scope link state
          database."
       REFERENCE
          "OSPF Version 2, Section 12 Link State Advertisements"
       ::= { ospf 12 }

  ospfExtLsdbEntry OBJECT-TYPE
       SYNTAX       OspfExtLsdbEntry
       MAX-ACCESS   not-accessible
       STATUS       deprecated
       DESCRIPTION
          "A single link state advertisement."
       INDEX { ospfExtLsdbType, ospfExtLsdbLsid, ospfExtLsdbRouterId }
       ::= { ospfExtLsdbTable 1 }

  OspfExtLsdbEntry ::=
       SEQUENCE {
          ospfExtLsdbType
             INTEGER,
          ospfExtLsdbLsid
             IpAddress,
          ospfExtLsdbRouterId
             RouterID,
          ospfExtLsdbSequence
             Integer32,
          ospfExtLsdbAge
             Integer32,
          ospfExtLsdbChecksum
             Integer32,
          ospfExtLsdbAdvertisement
             OCTET STRING
          }

  ospfExtLsdbType OBJECT-TYPE
       SYNTAX      INTEGER {
                      asExternalLink (5)
                      }
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       deprecated
       DESCRIPTION
          "The type of the link state advertisement.
          Each link state type has a separate advertisement
          format."
       REFERENCE
          "OSPF Version 2, Appendix A.4.1 The Link State
          Advertisement header"

       ::= { ospfExtLsdbEntry 1 }

  ospfExtLsdbLsid OBJECT-TYPE
       SYNTAX       IpAddress
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       deprecated
       DESCRIPTION
          "The Link State ID is an LS Type Specific field
          containing either a Router ID or an IP address;
          it identifies the piece of the routing domain
          that is being described by the advertisement."
       REFERENCE
          "OSPF Version 2, Section 12.1.4 Link State ID"
       ::= { ospfExtLsdbEntry 2 }

  ospfExtLsdbRouterId OBJECT-TYPE
       SYNTAX       RouterID
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       deprecated
       DESCRIPTION
          "The 32-bit number that uniquely identifies the
          originating router in the Autonomous System."
       REFERENCE
          "OSPF Version 2, Appendix C.1 Global parameters"
       ::= { ospfExtLsdbEntry 3 }

  ospfExtLsdbSequence OBJECT-TYPE
       SYNTAX       Integer32
       MAX-ACCESS   read-only
       STATUS       deprecated
       DESCRIPTION
          "The sequence number field is a signed 32-bit
          integer.  It starts with the value '80000001'h,
          or -'7FFFFFFF'h, and increments until '7FFFFFFF'h.
          Thus, a typical sequence number will be very negative.
          It is used to detect old and duplicate link state
          advertisements.  The space of sequence numbers is linearly
          ordered.  The larger the sequence number, the more recent
          the advertisement."
       REFERENCE
          "OSPF Version  2,  Section  12.1.6  LS  sequence
          number"
       ::= { ospfExtLsdbEntry 4 }
  ospfExtLsdbAge OBJECT-TYPE
       SYNTAX       Integer32 -- Should be 0..MaxAge, except when
                              -- doNotAge bit is set
       UNITS        "seconds"
       MAX-ACCESS   read-only
       STATUS       deprecated
       DESCRIPTION
          "This field is the age of the link state
          advertisement in seconds."
       REFERENCE
          "OSPF Version 2, Section 12.1.1 LS age"
       ::= { ospfExtLsdbEntry 5 }

  ospfExtLsdbChecksum OBJECT-TYPE
       SYNTAX       Integer32
       MAX-ACCESS   read-only
       STATUS       deprecated
       DESCRIPTION
          "This field is the checksum of the complete
          contents of the advertisement, excepting the
          age field.  The age field is excepted so that
          an advertisement's age can be incremented
          without updating the checksum.  The checksum
          used is the same that is used for ISO
          connectionless datagrams; it is commonly referred
          to as the Fletcher checksum."
       REFERENCE
          "OSPF Version 2, Section 12.1.7 LS checksum"
       ::= { ospfExtLsdbEntry 6 }

  ospfExtLsdbAdvertisement OBJECT-TYPE
       SYNTAX       OCTET STRING (SIZE(36))
       MAX-ACCESS   read-only
       STATUS       deprecated
       DESCRIPTION
          "The entire link state advertisement, including
          its header."
       REFERENCE
          "OSPF Version 2, Section 12  Link State
          Advertisements"
       ::= { ospfExtLsdbEntry 7 }

--  OSPF Use of the CIDR Route Table

  ospfRouteGroup    OBJECT IDENTIFIER ::= { ospf 13 }

--     The IP Forwarding Table defines a number of objects for use by
--     the routing protocol to externalize its information.  Most of
--     the variables (ipForwardDest, ipForwardMask, ipForwardPolicy,
--     ipForwardNextHop, ipForwardIfIndex, ipForwardType,
--     ipForwardProto, ipForwardAge, and ipForwardNextHopAS) are
--     defined there.

--     Those that leave some discretion are defined here.

--     ipCidrRouteProto is, of course, ospf (13).

--     ipCidrRouteAge is the time since the route was first
--     calculated, as opposed to the time since the last SPF run.
--     ipCidrRouteInfo is an OBJECT IDENTIFIER for use by the routing
--     protocol.  The following values shall be found there depending
--     on the way the route was calculated.

  ospfIntraArea      OBJECT IDENTIFIER ::= { ospfRouteGroup 1 }
  ospfInterArea      OBJECT IDENTIFIER ::= { ospfRouteGroup 2 }
  ospfExternalType1  OBJECT IDENTIFIER ::= { ospfRouteGroup 3 }
  ospfExternalType2  OBJECT IDENTIFIER ::= { ospfRouteGroup 4 }

--     ipCidrRouteMetric1 is, by definition, the primary routing
--     metric.  Therefore, it should be the metric that route
--     selection is based on.  For intra-area and inter-area routes,
--     it is an OSPF metric.  For External Type 1 (comparable value)
--     routes, it is an OSPF metric plus the External Metric.  For
--     external Type 2 (non-comparable value) routes, it is the
--     external metric.

--     ipCidrRouteMetric2 is, by definition, a secondary routing
--     metric.  Therefore, it should be the metric that breaks a tie
--     among routes having equal metric1 values and the same
--     calculation rule.  For intra-area, inter-area routes, and
--     External Type 1 (comparable value) routes, it is unused.  For
--     External Type 2 (non-comparable value) routes, it is the metric
--     to the AS border router.

--     ipCidrRouteMetric3, ipCidrRouteMetric4, and ipCidrRouteMetric5
--     are unused.

--  The OSPF Area Aggregate Table
--
--     This table replaces the OSPF Area Summary Table, being an
--     extension of that for CIDR routers.

   ospfAreaAggregateTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF OspfAreaAggregateEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The Area Aggregate Table acts as an adjunct
           to the Area Table.  It describes those address aggregates
           that are configured to be propagated from an area.
           Its purpose is to reduce the amount of information
           that is known beyond an Area's borders.

           It contains a set of IP address ranges
           specified by an IP address/IP network mask pair.
           For example, a class B address range of X.X.X.X
           with a network mask of 255.255.0.0 includes all IP
           addresses from X.X.0.0 to X.X.255.255.

           Note that if ranges are configured such that one range
           subsumes another range (e.g., 10.0.0.0 mask 255.0.0.0
           and 10.1.0.0 mask 255.255.0.0),
           the most specific match is the preferred one."
       REFERENCE
          "OSPF Version 2, Appendix C.2  Area parameters"
       ::= { ospf 14 }

  ospfAreaAggregateEntry OBJECT-TYPE
       SYNTAX   OspfAreaAggregateEntry
       MAX-ACCESS   not-accessible
       STATUS   current
       DESCRIPTION
          "A single area aggregate entry.

          Information in this table is persistent and when this object
          is written the entity SHOULD save the change to non-volatile
          storage."
       REFERENCE
          "OSPF Version 2, Appendix C.2  Area parameters"
       INDEX { ospfAreaAggregateAreaID, ospfAreaAggregateLsdbType,
          ospfAreaAggregateNet, ospfAreaAggregateMask }
       ::= { ospfAreaAggregateTable 1 }

  OspfAreaAggregateEntry ::=
       SEQUENCE {
          ospfAreaAggregateAreaID
             AreaID,
          ospfAreaAggregateLsdbType
             INTEGER,
          ospfAreaAggregateNet
             IpAddress,
          ospfAreaAggregateMask
             IpAddress,
          ospfAreaAggregateStatus
             RowStatus,
          ospfAreaAggregateEffect
             INTEGER,
          ospfAreaAggregateExtRouteTag
             Unsigned32
          }

  ospfAreaAggregateAreaID OBJECT-TYPE
       SYNTAX       AreaID
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       current
       DESCRIPTION
          "The area within which the address aggregate is to be
          found."
       REFERENCE
          "OSPF Version 2, Appendix C.2 Area parameters"
       ::= { ospfAreaAggregateEntry 1 }

  ospfAreaAggregateLsdbType OBJECT-TYPE
       SYNTAX       INTEGER {
                       summaryLink (3),
                       nssaExternalLink (7)
                       }
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS       current
       DESCRIPTION
          "The type of the address aggregate.  This field
          specifies the Lsdb type that this address
          aggregate applies to."
       REFERENCE
          "OSPF Version 2, Appendix A.4.1 The Link State
          Advertisement header"
       ::= { ospfAreaAggregateEntry 2 }

  ospfAreaAggregateNet OBJECT-TYPE
       SYNTAX   IpAddress
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS   current
       DESCRIPTION
          "The IP address of the net or subnet indicated
          by the range."
       REFERENCE
          "OSPF Version 2, Appendix C.2 Area parameters"
       ::= { ospfAreaAggregateEntry 3 }
  ospfAreaAggregateMask OBJECT-TYPE
       SYNTAX       IpAddress
       MAX-ACCESS   read-only -- read-only since originally an
                              -- SMIv1 index
       STATUS      current
       DESCRIPTION
          "The subnet mask that pertains to the net or
          subnet."
       REFERENCE
          "OSPF Version 2, Appendix C.2 Area parameters"
       ::= { ospfAreaAggregateEntry 4 }

  ospfAreaAggregateStatus OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "This object permits management of the table by
          facilitating actions such as row creation,
          construction, and destruction.

          The value of this object has no effect on
          whether other objects in this conceptual row can be
          modified."
       ::= { ospfAreaAggregateEntry 5 }

  ospfAreaAggregateEffect OBJECT-TYPE
       SYNTAX       INTEGER {
                       advertiseMatching (1),
                       doNotAdvertiseMatching (2)
                       }
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "Subnets subsumed by ranges either trigger the
          advertisement of the indicated aggregate
         (advertiseMatching) or result in the subnet's not
          being advertised at all outside the area."
       DEFVAL { advertiseMatching }
       ::= { ospfAreaAggregateEntry 6 }

  ospfAreaAggregateExtRouteTag OBJECT-TYPE
       SYNTAX       Unsigned32
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "External route tag to be included in NSSA (type-7)
           LSAs."
       DEFVAL { 0 }
       ::= { ospfAreaAggregateEntry 7 }

--  OSPF Link State Database, link-local for non-virtual links


  ospfLocalLsdbTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF OspfLocalLsdbEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The OSPF Process's link-local link state database
          for non-virtual links.
          This table is identical to the OSPF LSDB Table
          in format, but contains only link-local Link State
          Advertisements for non-virtual links.  The purpose is
          to allow link-local LSAs to be displayed for each
          non-virtual interface.  This table is implemented to
          support type-9 LSAs that are defined
          in 'The OSPF Opaque LSA Option'."
       REFERENCE
          "OSPF Version 2, Section 12 Link State Advertisements
          and The OSPF Opaque LSA Option"
       ::= { ospf 17 }

  ospfLocalLsdbEntry OBJECT-TYPE
       SYNTAX       OspfLocalLsdbEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "A single link state advertisement."
       INDEX { ospfLocalLsdbIpAddress, ospfLocalLsdbAddressLessIf,
          ospfLocalLsdbType, ospfLocalLsdbLsid, ospfLocalLsdbRouterId
          }
       ::= { ospfLocalLsdbTable 1 }

  OspfLocalLsdbEntry ::=
       SEQUENCE {
          ospfLocalLsdbIpAddress
             IpAddress,
          ospfLocalLsdbAddressLessIf
             InterfaceIndexOrZero,
          ospfLocalLsdbType
             INTEGER,
          ospfLocalLsdbLsid
             IpAddress,
          ospfLocalLsdbRouterId
             RouterID,
          ospfLocalLsdbSequence
             Integer32,
          ospfLocalLsdbAge
             Integer32,
          ospfLocalLsdbChecksum
             Integer32,
          ospfLocalLsdbAdvertisement
             OCTET STRING
          }

  ospfLocalLsdbIpAddress OBJECT-TYPE
       SYNTAX       IpAddress
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The IP address of the interface from
          which the LSA was received if the interface is
          numbered."
       REFERENCE
          "OSPF Version 2, Appendix C.3 Interface parameters"
       ::= { ospfLocalLsdbEntry 1 }

  ospfLocalLsdbAddressLessIf OBJECT-TYPE
       SYNTAX       InterfaceIndexOrZero
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The interface index of the interface from
          which the LSA was received if the interface is
          unnumbered."
       REFERENCE
          "OSPF Version 2, Appendix C.3 Interface parameters"
       ::= { ospfLocalLsdbEntry 2 }

  ospfLocalLsdbType OBJECT-TYPE
       SYNTAX       INTEGER { localOpaqueLink (9) }
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The type of the link state advertisement.
          Each link state type has a separate
          advertisement format."
       REFERENCE
          "OSPF Version 2, Appendix A.4.1 The Link State
          Advertisement header"
       ::= { ospfLocalLsdbEntry 3 }

  ospfLocalLsdbLsid OBJECT-TYPE
       SYNTAX       IpAddress
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The Link State ID is an LS Type Specific field
          containing a 32-bit identifier in IP address format;
          it identifies the piece of the routing domain
          that is being described by the advertisement."
       REFERENCE
         "OSPF Version 2, Section 12.1.4 Link State ID"
       ::= { ospfLocalLsdbEntry 4 }

  ospfLocalLsdbRouterId OBJECT-TYPE
       SYNTAX       RouterID
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The 32-bit number that uniquely identifies the
          originating router in the Autonomous System."
       REFERENCE
          "OSPF Version 2, Appendix C.1 Global parameters"
       ::= { ospfLocalLsdbEntry 5 }

  ospfLocalLsdbSequence OBJECT-TYPE
       SYNTAX       Integer32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The sequence number field is a signed 32-bit
          integer.  It starts with the value '80000001'h,
          or -'7FFFFFFF'h, and increments until '7FFFFFFF'h.
          Thus, a typical sequence number will be very negative.
          It is used to detect old and duplicate link state
          advertisements.  The space of sequence numbers is linearly
          ordered.  The larger the sequence number, the more recent
          the advertisement."
       REFERENCE
          "OSPF Version 2, Section 12.1.6 LS sequence
          number"
       ::= { ospfLocalLsdbEntry 6 }

  ospfLocalLsdbAge OBJECT-TYPE
       SYNTAX       Integer32 -- Should be 0..MaxAge, except when
                              -- doNotAge bit is set
       UNITS        "seconds"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "This field is the age of the link state
          advertisement in seconds."
       REFERENCE
          "OSPF Version 2, Section 12.1.1 LS age"
       ::= { ospfLocalLsdbEntry 7 }

  ospfLocalLsdbChecksum OBJECT-TYPE
       SYNTAX       Integer32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "This field is the checksum of the complete
          contents of the advertisement, excepting the
          age field.  The age field is excepted so that
          an advertisement's age can be incremented
          without updating the checksum.  The checksum
          used is the same that is used for ISO
          connectionless datagrams; it is commonly referred
          to as the Fletcher checksum."
       REFERENCE
          "OSPF Version 2, Section 12.1.7 LS checksum"
       ::= { ospfLocalLsdbEntry 8 }

  ospfLocalLsdbAdvertisement OBJECT-TYPE
       SYNTAX       OCTET STRING (SIZE (1..65535))
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The entire link state advertisement, including
          its header.

          Note that for variable length LSAs, SNMP agents
          may not be able to return the largest string size."
       REFERENCE
          "OSPF Version 2, Section 12 Link State
          Advertisements"
       ::= { ospfLocalLsdbEntry 9 }

--  OSPF Link State Database, link-local for virtual Links

  ospfVirtLocalLsdbTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF OspfVirtLocalLsdbEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The OSPF Process's link-local link state database
          for virtual links.
          This table is identical to the OSPF LSDB Table
          in format, but contains only link-local Link State
          Advertisements for virtual links.  The purpose is to
          allow link-local LSAs to be displayed for each virtual
          interface.  This table is implemented to support type-9 LSAs
          that are defined in 'The OSPF Opaque LSA Option'."
       REFERENCE
          "OSPF Version 2, Section 12 Link State
          Advertisements and The OSPF Opaque LSA Option"
       ::= { ospf 18 }

  ospfVirtLocalLsdbEntry OBJECT-TYPE
       SYNTAX       OspfVirtLocalLsdbEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "A single link state advertisement."
       INDEX { ospfVirtLocalLsdbTransitArea,
          ospfVirtLocalLsdbNeighbor,
          ospfVirtLocalLsdbType,
          ospfVirtLocalLsdbLsid,
          ospfVirtLocalLsdbRouterId
          }
       ::= { ospfVirtLocalLsdbTable 1 }

  OspfVirtLocalLsdbEntry ::=
       SEQUENCE {
          ospfVirtLocalLsdbTransitArea
             AreaID,
          ospfVirtLocalLsdbNeighbor
             RouterID,
          ospfVirtLocalLsdbType
             INTEGER,
          ospfVirtLocalLsdbLsid
             IpAddress,
          ospfVirtLocalLsdbRouterId
             RouterID,
          ospfVirtLocalLsdbSequence
             Integer32,
          ospfVirtLocalLsdbAge
             Integer32,
          ospfVirtLocalLsdbChecksum
             Integer32,
          ospfVirtLocalLsdbAdvertisement
            OCTET STRING
          }

  ospfVirtLocalLsdbTransitArea OBJECT-TYPE
       SYNTAX       AreaID
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The transit area that the virtual link
          traverses.  By definition, this is not 0.0.0.0."
       REFERENCE
          "OSPF Version 2, Appendix C.3 Interface parameters"
       ::= { ospfVirtLocalLsdbEntry 1 }

  ospfVirtLocalLsdbNeighbor OBJECT-TYPE
       SYNTAX       RouterID
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The Router ID of the virtual neighbor."
       REFERENCE
          "OSPF Version 2, Appendix C.3 Interface parameters"
       ::= { ospfVirtLocalLsdbEntry 2 }

  ospfVirtLocalLsdbType OBJECT-TYPE
       SYNTAX       INTEGER  { localOpaqueLink (9) }
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The type of the link state advertisement.
          Each link state type has a separate
          advertisement format."
       REFERENCE
          "OSPF Version 2, Appendix A.4.1 The Link State
          Advertisement header"
       ::= { ospfVirtLocalLsdbEntry 3 }

  ospfVirtLocalLsdbLsid OBJECT-TYPE
       SYNTAX       IpAddress
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The Link State ID is an LS Type Specific field
          containing a 32-bit identifier in IP address format;
          it identifies the piece of the routing domain
          that is being described by the advertisement."
       REFERENCE
          "OSPF Version 2, Section 12.1.4 Link State ID"
       ::= { ospfVirtLocalLsdbEntry 4 }

  ospfVirtLocalLsdbRouterId OBJECT-TYPE
       SYNTAX       RouterID
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The 32-bit number that uniquely identifies the
          originating router in the Autonomous System."
       REFERENCE
          "OSPF Version 2, Appendix C.1 Global parameters"
       ::= { ospfVirtLocalLsdbEntry 5 }

  ospfVirtLocalLsdbSequence OBJECT-TYPE
       SYNTAX       Integer32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The sequence number field is a signed 32-bit
          integer.  It starts with the value '80000001'h,
          or -'7FFFFFFF'h, and increments until '7FFFFFFF'h.
          Thus, a typical sequence number will be very negative.
          It is used to detect old and duplicate link state
          advertisements.  The space of sequence numbers is linearly
          ordered.  The larger the sequence number, the more recent
          the advertisement."
       REFERENCE
          "OSPF Version 2, Section 12.1.6 LS sequence
          number"
       ::= { ospfVirtLocalLsdbEntry 6 }

  ospfVirtLocalLsdbAge OBJECT-TYPE
       SYNTAX       Integer32 -- Should be 0..MaxAge, except when
                              -- doNotAge bit is set
       UNITS        "seconds"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "This field is the age of the link state
          advertisement in seconds."
       REFERENCE
          "OSPF Version 2, Section 12.1.1 LS age"
       ::= { ospfVirtLocalLsdbEntry 7 }

  ospfVirtLocalLsdbChecksum OBJECT-TYPE
       SYNTAX       Integer32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "This field is the checksum of the complete
          contents of the advertisement, excepting the
          age field.  The age field is excepted so that
          an advertisement's age can be incremented
          without updating the checksum.  The checksum
          used is the same that is used for ISO
          connectionless datagrams; it is commonly
          referred to as the Fletcher checksum."
       REFERENCE
          "OSPF Version 2, Section 12.1.7 LS checksum"
       ::= { ospfVirtLocalLsdbEntry 8 }

  ospfVirtLocalLsdbAdvertisement OBJECT-TYPE
       SYNTAX       OCTET STRING (SIZE (1..65535))
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The entire link state advertisement, including
          its header."
       REFERENCE
          "OSPF Version 2, Section 12 Link State
          Advertisements.

          Note that for variable length LSAs, SNMP agents
          may not be able to return the largest string size."
       ::= { ospfVirtLocalLsdbEntry 9 }

--  OSPF Link State Database, AS-scope

  ospfAsLsdbTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF OspfAsLsdbEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The OSPF Process's AS-scope LSA link state database.
           The database contains the AS-scope Link State
           Advertisements from throughout the areas that
           the device is attached to.

           This table is identical to the OSPF LSDB Table
           in format, but contains only AS-scope Link State
           Advertisements.  The purpose is to allow AS-scope
           LSAs to be displayed once for the router rather
           than once in each non-stub area."
       REFERENCE
          "OSPF Version 2, Section 12 Link State
          Advertisements"
       ::= { ospf 19 }

  ospfAsLsdbEntry OBJECT-TYPE
       SYNTAX       OspfAsLsdbEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "A single link state advertisement."
       INDEX { ospfAsLsdbType, ospfAsLsdbLsid, ospfAsLsdbRouterId }
       ::= { ospfAsLsdbTable 1 }

  OspfAsLsdbEntry ::=
       SEQUENCE {
          ospfAsLsdbType
             INTEGER,
          ospfAsLsdbLsid
             IpAddress,
          ospfAsLsdbRouterId
             RouterID,
          ospfAsLsdbSequence
             Integer32,
          ospfAsLsdbAge
             Integer32,
          ospfAsLsdbChecksum
             Integer32,
          ospfAsLsdbAdvertisement
             OCTET STRING
          }

  ospfAsLsdbType OBJECT-TYPE
       SYNTAX      INTEGER {
                      asExternalLink (5),
                      asOpaqueLink   (11)
                      }
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The type of the link state advertisement.
          Each link state type has a separate
          advertisement format."
       REFERENCE
          "OSPF Version 2, Appendix A.4.1 The Link State
          Advertisement header"
       ::= { ospfAsLsdbEntry 1 }

  ospfAsLsdbLsid OBJECT-TYPE
       SYNTAX       IpAddress
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The Link State ID is an LS Type Specific field
          containing either a Router ID or an IP address;
          it identifies the piece of the routing domain
          that is being described by the advertisement."
       REFERENCE
          "OSPF Version 2, Section 12.1.4 Link State ID"
       ::= { ospfAsLsdbEntry 2 }

  ospfAsLsdbRouterId OBJECT-TYPE
       SYNTAX       RouterID
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "The 32-bit number that uniquely identifies the
          originating router in the Autonomous System."
       REFERENCE
          "OSPF Version 2, Appendix C.1 Global parameters"
       ::= { ospfAsLsdbEntry 3 }

  ospfAsLsdbSequence OBJECT-TYPE
       SYNTAX       Integer32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The sequence number field is a signed 32-bit
          integer.  It starts with the value '80000001'h,
          or -'7FFFFFFF'h, and increments until '7FFFFFFF'h.
          Thus, a typical sequence number will be very negative.
          It is used to detect old and duplicate link state
          advertisements.  The space of sequence numbers is linearly
          ordered.  The larger the sequence number, the more recent
          the advertisement."
       REFERENCE
          "OSPF Version  2,  Section  12.1.6  LS  sequence
          number"
       ::= { ospfAsLsdbEntry 4 }

  ospfAsLsdbAge OBJECT-TYPE
       SYNTAX       Integer32 -- Should be 0..MaxAge, except when
                              -- doNotAge bit is set
       UNITS        "seconds"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "This field is the age of the link state
          advertisement in seconds."
       REFERENCE
          "OSPF Version 2, Section 12.1.1 LS age"
       ::= { ospfAsLsdbEntry 5 }
  ospfAsLsdbChecksum OBJECT-TYPE
       SYNTAX       Integer32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "This field is the checksum of the complete
          contents of the advertisement, excepting the
          age field.  The age field is excepted so that
          an advertisement's age can be incremented
          without updating the checksum.  The checksum
          used is the same that is used for ISO
          connectionless datagrams; it is commonly referred
          to as the Fletcher checksum."
       REFERENCE
          "OSPF Version 2, Section 12.1.7 LS checksum"
       ::= { ospfAsLsdbEntry 6 }

  ospfAsLsdbAdvertisement OBJECT-TYPE
       SYNTAX       OCTET STRING (SIZE (1..65535))
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The entire link state advertisement, including
          its header."
       REFERENCE
          "OSPF Version 2, Section 12 Link State
          Advertisements.

          Note that for variable length LSAs, SNMP agents
          may not be able to return the largest string size."
       ::= { ospfAsLsdbEntry 7 }

 --  OSPF Area LSA Counter Table

      ospfAreaLsaCountTable OBJECT-TYPE
          SYNTAX       SEQUENCE OF OspfAreaLsaCountEntry
          MAX-ACCESS   not-accessible
          STATUS       current
          DESCRIPTION
             "This table maintains per-area, per-LSA-type counters"
          ::= { ospf 20 }

      ospfAreaLsaCountEntry OBJECT-TYPE
          SYNTAX       OspfAreaLsaCountEntry
          MAX-ACCESS   not-accessible
          STATUS       current
          DESCRIPTION
             "An entry with a number of link advertisements
              of a given type for a given area."
          INDEX { ospfAreaLsaCountAreaId, ospfAreaLsaCountLsaType }
          ::= { ospfAreaLsaCountTable 1 }

      OspfAreaLsaCountEntry ::=
           SEQUENCE {
              ospfAreaLsaCountAreaId
                 AreaID,
              ospfAreaLsaCountLsaType
                 INTEGER,
              ospfAreaLsaCountNumber
                 Gauge32
           }

      ospfAreaLsaCountAreaId OBJECT-TYPE
          SYNTAX       AreaID
          MAX-ACCESS   not-accessible
          STATUS       current
          DESCRIPTION
             "This entry Area ID."
         ::= { ospfAreaLsaCountEntry 1 }

      ospfAreaLsaCountLsaType OBJECT-TYPE
          SYNTAX       INTEGER {
                          routerLink (1),
                          networkLink (2),
                          summaryLink (3),
                          asSummaryLink (4),
                          multicastLink (6),
                          nssaExternalLink (7),
                          areaOpaqueLink (10)
                       }
          MAX-ACCESS   not-accessible
          STATUS       current
          DESCRIPTION
             "This entry LSA type."
         ::= { ospfAreaLsaCountEntry 2 }

      ospfAreaLsaCountNumber OBJECT-TYPE
          SYNTAX       Gauge32
          MAX-ACCESS   read-only
          STATUS       current
          DESCRIPTION
             "Number of LSAs of a given type for a given area."
         ::= { ospfAreaLsaCountEntry 3 }

-- conformance information
ospfConformance OBJECT IDENTIFIER ::= { ospf 15 }

ospfGroups      OBJECT IDENTIFIER ::= { ospfConformance 1 }
ospfCompliances OBJECT IDENTIFIER ::= { ospfConformance 2 }

-- compliance statements

  ospfCompliance MODULE-COMPLIANCE
       STATUS       deprecated
       DESCRIPTION
          "The compliance statement for OSPF systems
          conforming to RFC 1850."
       MODULE       -- this module
       MANDATORY-GROUPS {
           ospfBasicGroup,
           ospfAreaGroup,
           ospfStubAreaGroup,
           ospfIfGroup,
           ospfIfMetricGroup,
           ospfVirtIfGroup,
           ospfNbrGroup,
           ospfVirtNbrGroup,
           ospfAreaAggregateGroup
           }
       GROUP  ospfHostGroup
          DESCRIPTION
             "This group is mandatory for OSPF systems that support
             attached hosts."
       GROUP  ospfLsdbGroup
          DESCRIPTION
             "This group is mandatory for OSPF systems that display
             their per-area link state database."
       GROUP  ospfExtLsdbGroup
          DESCRIPTION
             "This group is mandatory for OSPF systems that display
             their external link state database."
       ::= { ospfCompliances 1 }

  ospfCompliance2 MODULE-COMPLIANCE
       STATUS       current
       DESCRIPTION
          "The compliance statement."
       MODULE       -- this module
       MANDATORY-GROUPS {
          ospfBasicGroup2,
          ospfAreaGroup2,
          ospfStubAreaGroup,
          ospfIfGroup2,
          ospfIfMetricGroup,
          ospfVirtIfGroup2,
          ospfNbrGroup2,
          ospfVirtNbrGroup2,
          ospfAreaAggregateGroup2
          }
       GROUP  ospfHostGroup2
          DESCRIPTION
             "This group is mandatory for OSPF systems that support
             attached hosts."
       GROUP  ospfLsdbGroup
          DESCRIPTION
             "This group is mandatory for OSPF systems that display
             their per-area link state database."
       GROUP  ospfAsLsdbGroup
          DESCRIPTION
             "This group is mandatory for OSPF systems that display
             their AS-scope link state database."
       GROUP  ospfLocalLsdbGroup
          DESCRIPTION
             "This group is mandatory for OSPF systems that display
             their per-link link state database for non-virtual
             links."
       GROUP  ospfVirtLocalLsdbGroup
          DESCRIPTION
             "This group is mandatory for OSPF systems that display
             their per-link link state database for virtual links."
       GROUP ospfAreaLsaCountGroup
          DESCRIPTION
             "This group is mandatory for OSPF systems that display
             per-area, per-LSA-type counters."
       ::= { ospfCompliances 2 }

  ospfComplianceObsolete MODULE-COMPLIANCE
       STATUS       obsolete
       DESCRIPTION
          "Contains obsolete object groups."
       MODULE       -- this module
       GROUP  ospfAreaRangeGroup
          DESCRIPTION
             "This group is obsolete, and it is mandatory only
             for non-Classless Inter-Domain Routing (CIDR) OSPF
             systems that support multiple areas."
       GROUP  ospfObsoleteGroup
          DESCRIPTION
             "This group contains obsolete objects,
             which are no longer required for OSPF systems."
       ::= { ospfCompliances 3 }
--  units of conformance

  ospfBasicGroup    OBJECT-GROUP
       OBJECTS {
          ospfRouterId,
          ospfAdminStat,
          ospfVersionNumber,
          ospfAreaBdrRtrStatus,
          ospfASBdrRtrStatus,
          ospfExternLsaCount,
          ospfExternLsaCksumSum,
          ospfTOSSupport,
          ospfOriginateNewLsas,
          ospfRxNewLsas,
          ospfExtLsdbLimit,
          ospfMulticastExtensions,
          ospfExitOverflowInterval,
          ospfDemandExtensions
          }
       STATUS      deprecated
       DESCRIPTION
          "These objects are used to monitor/manage
          global OSPF parameters.  This object group
          conforms to RFC 1850."
       ::= { ospfGroups 1 }

  ospfAreaGroup    OBJECT-GROUP
       OBJECTS {
          ospfAreaId,
          ospfImportAsExtern,
          ospfSpfRuns,
          ospfAreaBdrRtrCount,
          ospfAsBdrRtrCount,
          ospfAreaLsaCount,
          ospfAreaLsaCksumSum,
          ospfAreaSummary,
          ospfAreaStatus
          }
       STATUS      deprecated
       DESCRIPTION
          "These objects are used for OSPF systems
          supporting areas per RFC 1850."
       ::= { ospfGroups 2 }

  ospfStubAreaGroup    OBJECT-GROUP
       OBJECTS {
          ospfStubAreaId,
          ospfStubTOS,
          ospfStubMetric,
          ospfStubStatus,
          ospfStubMetricType
          }
       STATUS       current
       DESCRIPTION
          "These objects are used for OSPF systems
          supporting stub areas."
       ::= { ospfGroups 3 }

   ospfLsdbGroup    OBJECT-GROUP
       OBJECTS {
          ospfLsdbAreaId,
          ospfLsdbType,
          ospfLsdbLsid,
          ospfLsdbRouterId,
          ospfLsdbSequence,
          ospfLsdbAge,
          ospfLsdbChecksum,
          ospfLsdbAdvertisement
          }
       STATUS       current
       DESCRIPTION
          "These objects are used for OSPF systems
          that display their link state database."
       ::= { ospfGroups 4 }

   ospfAreaRangeGroup    OBJECT-GROUP
       OBJECTS {
          ospfAreaRangeAreaId,
          ospfAreaRangeNet,
          ospfAreaRangeMask,
          ospfAreaRangeStatus,
          ospfAreaRangeEffect
          }
       STATUS  obsolete
       DESCRIPTION
          "These objects are used for non-CIDR OSPF
          systems that support multiple areas.  This
          object group is obsolete."
       ::= { ospfGroups 5 }

  ospfHostGroup    OBJECT-GROUP
       OBJECTS {
          ospfHostIpAddress,
          ospfHostTOS,
          ospfHostMetric,
          ospfHostStatus,
          ospfHostAreaID
          }
       STATUS       deprecated
       DESCRIPTION
          "These objects are used for OSPF systems
          that support attached hosts."
       ::= { ospfGroups 6 }

  ospfIfGroup    OBJECT-GROUP
       OBJECTS {
          ospfIfIpAddress,
          ospfAddressLessIf,
          ospfIfAreaId,
          ospfIfType,
          ospfIfAdminStat,
          ospfIfRtrPriority,
          ospfIfTransitDelay,
          ospfIfRetransInterval,
          ospfIfHelloInterval,
          ospfIfRtrDeadInterval,
          ospfIfPollInterval,
          ospfIfState,
          ospfIfDesignatedRouter,
          ospfIfBackupDesignatedRouter,
          ospfIfEvents,
          ospfIfAuthType,
          ospfIfAuthKey,
          ospfIfStatus,
          ospfIfMulticastForwarding,
          ospfIfDemand
          }
       STATUS       deprecated
       DESCRIPTION
          "These objects are used to monitor/manage OSPF
          interfaces.  This object group conforms to RFC 1850."
       ::= { ospfGroups 7 }

  ospfIfMetricGroup    OBJECT-GROUP
       OBJECTS {
          ospfIfMetricIpAddress,
          ospfIfMetricAddressLessIf,
          ospfIfMetricTOS,
          ospfIfMetricValue,
          ospfIfMetricStatus
          }
       STATUS       current
       DESCRIPTION
          "These objects are used for OSPF systems for supporting
          interface metrics."
       ::= { ospfGroups 8 }

  ospfVirtIfGroup    OBJECT-GROUP
       OBJECTS {
          ospfVirtIfAreaId,
          ospfVirtIfNeighbor,
          ospfVirtIfTransitDelay,
          ospfVirtIfRetransInterval,
          ospfVirtIfHelloInterval,
          ospfVirtIfRtrDeadInterval,
          ospfVirtIfState,
          ospfVirtIfEvents,
          ospfVirtIfAuthType,
          ospfVirtIfAuthKey,
          ospfVirtIfStatus
          }
        STATUS       deprecated
        DESCRIPTION
          "These objects are used for OSPF systems for supporting
          virtual interfaces.  This object group conforms
          to RFC 1850."
        ::= { ospfGroups 9 }

  ospfNbrGroup    OBJECT-GROUP
       OBJECTS {
          ospfNbrIpAddr,
          ospfNbrAddressLessIndex,
          ospfNbrRtrId,
          ospfNbrOptions,
          ospfNbrPriority,
          ospfNbrState,
          ospfNbrEvents,
          ospfNbrLsRetransQLen,
          ospfNbmaNbrStatus,
          ospfNbmaNbrPermanence,
          ospfNbrHelloSuppressed
          }
       STATUS       deprecated
       DESCRIPTION
          "These objects are used to monitor/manage OSPF neighbors.
          This object group conforms to RFC 1850."
       ::= { ospfGroups 10 }

  ospfVirtNbrGroup    OBJECT-GROUP
       OBJECTS {
          ospfVirtNbrArea,
          ospfVirtNbrRtrId,
          ospfVirtNbrIpAddr,
          ospfVirtNbrOptions,
          ospfVirtNbrState,
          ospfVirtNbrEvents,
          ospfVirtNbrLsRetransQLen,
          ospfVirtNbrHelloSuppressed
          }
       STATUS       deprecated
       DESCRIPTION
          "These objects are used to monitor/manage OSPF virtual
          neighbors.  This object group conforms to RFC 1850."

       ::= { ospfGroups 11 }

  ospfExtLsdbGroup    OBJECT-GROUP
       OBJECTS {
          ospfExtLsdbType,
          ospfExtLsdbLsid,
          ospfExtLsdbRouterId,
          ospfExtLsdbSequence,
          ospfExtLsdbAge,
          ospfExtLsdbChecksum,
          ospfExtLsdbAdvertisement
          }
       STATUS       deprecated
       DESCRIPTION
          "These objects are used for OSPF systems that display
          their link state database.  This object group
          conforms to RFC 1850.

          This object group is replaced by the ospfAsLsdbGroup
          in order to support any AS-scope LSA type in a single
          table."
       ::= { ospfGroups 12 }

  ospfAreaAggregateGroup    OBJECT-GROUP
       OBJECTS {
          ospfAreaAggregateAreaID,
          ospfAreaAggregateLsdbType,
          ospfAreaAggregateNet,
          ospfAreaAggregateMask,
          ospfAreaAggregateStatus,
          ospfAreaAggregateEffect
          }
       STATUS       deprecated
       DESCRIPTION
          "These objects are used for OSPF systems to support
          network prefix aggregation across areas."
       ::= { ospfGroups 13 }

  ospfLocalLsdbGroup    OBJECT-GROUP
       OBJECTS {
          ospfLocalLsdbSequence,
          ospfLocalLsdbAge,
          ospfLocalLsdbChecksum,
          ospfLocalLsdbAdvertisement
          }
       STATUS      current
       DESCRIPTION
          "These objects are used for OSPF systems
          that display their link-local link state databases
          for non-virtual links."
        ::= { ospfGroups 14 }

  ospfVirtLocalLsdbGroup    OBJECT-GROUP
       OBJECTS {
          ospfVirtLocalLsdbSequence,
          ospfVirtLocalLsdbAge,
          ospfVirtLocalLsdbChecksum,
          ospfVirtLocalLsdbAdvertisement
          }
        STATUS       current
        DESCRIPTION
           "These objects are used for OSPF systems
           that display their link-local link state databases
           for virtual links."
         ::= { ospfGroups 15 }

  ospfAsLsdbGroup    OBJECT-GROUP
       OBJECTS {
          ospfAsLsdbSequence,
          ospfAsLsdbAge,
          ospfAsLsdbChecksum,
          ospfAsLsdbAdvertisement
          }
        STATUS       current
        DESCRIPTION
           "These objects are used for OSPF systems
           that display their AS-scope link state database."
         ::= { ospfGroups 16 }

  ospfBasicGroup2    OBJECT-GROUP
       OBJECTS {
          ospfRouterId,
          ospfAdminStat,
          ospfVersionNumber,
          ospfAreaBdrRtrStatus,
          ospfASBdrRtrStatus,
          ospfExternLsaCount,
          ospfExternLsaCksumSum,
          ospfTOSSupport,
          ospfOriginateNewLsas,
          ospfRxNewLsas,
          ospfExtLsdbLimit,
          ospfMulticastExtensions,
          ospfExitOverflowInterval,
          ospfDemandExtensions,
          ospfRFC1583Compatibility,
          ospfOpaqueLsaSupport,
          ospfReferenceBandwidth,
          ospfRestartSupport,
          ospfRestartInterval,
          ospfRestartStrictLsaChecking,
          ospfRestartStatus,
          ospfRestartAge,
          ospfRestartExitReason,
          ospfAsLsaCount,
          ospfAsLsaCksumSum,
          ospfStubRouterSupport,
          ospfStubRouterAdvertisement,
          ospfDiscontinuityTime
          }
       STATUS       current
       DESCRIPTION
          "These objects are used to monitor/manage OSPF global
          parameters."
       ::= { ospfGroups 17 }

  ospfAreaGroup2    OBJECT-GROUP
       OBJECTS {
          ospfAreaId,
          ospfImportAsExtern,
          ospfSpfRuns,
          ospfAreaBdrRtrCount,
          ospfAsBdrRtrCount,
          ospfAreaLsaCount,
          ospfAreaLsaCksumSum,
          ospfAreaSummary,
          ospfAreaStatus,
          ospfAreaNssaTranslatorRole,
          ospfAreaNssaTranslatorState,
          ospfAreaNssaTranslatorStabilityInterval,
          ospfAreaNssaTranslatorEvents
          }
       STATUS       current
       DESCRIPTION
            "These objects are used by OSPF systems
            to support areas."
       ::= { ospfGroups 18 }

  ospfIfGroup2    OBJECT-GROUP
       OBJECTS {
          ospfIfIpAddress,
          ospfAddressLessIf,
          ospfIfAreaId,
          ospfIfType,
          ospfIfAdminStat,
          ospfIfRtrPriority,
          ospfIfTransitDelay,
          ospfIfRetransInterval,
          ospfIfHelloInterval,
          ospfIfRtrDeadInterval,
          ospfIfPollInterval,
          ospfIfState,
          ospfIfDesignatedRouter,
          ospfIfBackupDesignatedRouter,
          ospfIfEvents,
          ospfIfAuthType,
          ospfIfAuthKey,
          ospfIfStatus,
          ospfIfMulticastForwarding,
          ospfIfDemand,
          ospfIfLsaCount,
          ospfIfLsaCksumSum
          }
       STATUS       current
       DESCRIPTION
          "These objects are used to monitor/manage OSPF interfaces."
        ::= { ospfGroups 19 }

  ospfVirtIfGroup2    OBJECT-GROUP
       OBJECTS {
          ospfVirtIfAreaId,
          ospfVirtIfNeighbor,
          ospfVirtIfTransitDelay,
          ospfVirtIfRetransInterval,
          ospfVirtIfHelloInterval,
          ospfVirtIfRtrDeadInterval,
          ospfVirtIfState,
          ospfVirtIfEvents,
          ospfVirtIfAuthType,
          ospfVirtIfAuthKey,
          ospfVirtIfStatus,
          ospfVirtIfLsaCount,
          ospfVirtIfLsaCksumSum,
          ospfIfDesignatedRouterId,
          ospfIfBackupDesignatedRouterId
          }
       STATUS       current
       DESCRIPTION
          "These objects are used to monitor/manage OSPF
          virtual interfaces."
       ::= { ospfGroups 20 }

  ospfNbrGroup2    OBJECT-GROUP
       OBJECTS {
          ospfNbrIpAddr,
          ospfNbrAddressLessIndex,
          ospfNbrRtrId,
          ospfNbrOptions,
          ospfNbrPriority,
          ospfNbrState,
          ospfNbrEvents,
          ospfNbrLsRetransQLen,
          ospfNbmaNbrStatus,
          ospfNbmaNbrPermanence,
          ospfNbrHelloSuppressed,
          ospfNbrRestartHelperStatus,
          ospfNbrRestartHelperAge,
          ospfNbrRestartHelperExitReason
          }
       STATUS       current
       DESCRIPTION
          "These objects are used to monitor/manage OSPF
          neighbors."
       ::= { ospfGroups 21 }

  ospfVirtNbrGroup2    OBJECT-GROUP
       OBJECTS {
          ospfVirtNbrArea,
          ospfVirtNbrRtrId,
          ospfVirtNbrIpAddr,
          ospfVirtNbrOptions,
          ospfVirtNbrState,
          ospfVirtNbrEvents,
          ospfVirtNbrLsRetransQLen,
          ospfVirtNbrHelloSuppressed,
          ospfVirtNbrRestartHelperStatus,
          ospfVirtNbrRestartHelperAge,
          ospfVirtNbrRestartHelperExitReason
          }
       STATUS       current
       DESCRIPTION
          "These objects are used to monitor/manage OSPF
          virtual neighbors."
       ::= { ospfGroups 22 }

  ospfAreaAggregateGroup2    OBJECT-GROUP
       OBJECTS {
          ospfAreaAggregateAreaID,
          ospfAreaAggregateLsdbType,
          ospfAreaAggregateNet,
          ospfAreaAggregateMask,
          ospfAreaAggregateStatus,
          ospfAreaAggregateEffect,
          ospfAreaAggregateExtRouteTag
          }
       STATUS       current
       DESCRIPTION
          "These objects are used for OSPF systems to support
          network prefix aggregation across areas."
       ::= { ospfGroups 23 }

  ospfAreaLsaCountGroup      OBJECT-GROUP
       OBJECTS {
          ospfAreaLsaCountNumber
          }
       STATUS       current
       DESCRIPTION
          "These objects are used for OSPF systems that display
          per-area, per-LSA-type counters."
       ::= { ospfGroups 24 }

  ospfHostGroup2    OBJECT-GROUP
       OBJECTS {
          ospfHostIpAddress,
          ospfHostTOS,
          ospfHostMetric,
          ospfHostStatus,
          ospfHostCfgAreaID
          }
       STATUS       current
       DESCRIPTION
          "These objects are used for OSPF systems
          that support attached hosts."
       ::= { ospfGroups 25 }

--     This object group is included for SMI conformance.  It is not a
--     mandatory group for compliance with this MIB

  ospfObsoleteGroup    OBJECT-GROUP
       OBJECTS {
          ospfAuthType
          }
       STATUS       obsolete
       DESCRIPTION
          "These objects are obsolete and are no longer required for
          OSPF systems.  They are placed into this group for SMI
          conformance."
       ::= { ospfGroups 26 }

END
-- ===========================================================================
-- Full Copyright Statement
-- 
--    Copyright (C) The Internet Society (2004).  This document is subject
--    to the rights, licenses and restrictions contained in BCP 78, and
--    except as set forth therein, the authors retain all their rights.
-- 
--    This document and the information contained herein are provided on an
--    "AS IS" basis and THE CONTRIBUTOR, THE ORGANIZATION HE/SHE REPRESENTS
--    OR IS SPONSORED BY (IF ANY), THE INTERNET SOCIETY AND THE INTERNET
--    ENGINEERING TASK FORCE DISCLAIM ALL WARRANTIES, EXPRESS OR IMPLIED,
--    INCLUDING BUT NOT LIMITED TO ANY WARRANTY THAT THE USE OF THE
--    INFORMATION HEREIN WILL NOT INFRINGE ANY RIGHTS OR ANY IMPLIED
--    WARRANTIES OF MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.
-- 
-- Intellectual Property
-- 
--    The IETF takes no position regarding the validity or scope of any
--    Intellectual Property Rights or other rights that might be claimed to
--    pertain to the implementation or use of the technology described in
--    this document or the extent to which any license under such rights
--    might or might not be available; nor does it represent that it has
--    made any independent effort to identify any such rights.  Information
--    on the procedures with respect to rights in RFC documents can be
--    found in BCP 78 and BCP 79.
-- 
--    Copies of IPR disclosures made to the IETF Secretariat and any
--    assurances of licenses to be made available, or the result of an
--    attempt made to obtain a general license or permission for the use of
--    such proprietary rights by implementers or users of this
--    specification can be obtained from the IETF on-line IPR repository at
--    http://www.ietf.org/ipr.
-- 
--    The IETF invites any interested party to bring to its attention any
--    copyrights, patents or patent applications, or other proprietary
--    rights that may cover technology that may be required to implement
--    this standard.  Please address the information to the IETF at ietf-
--    ipr@ietf.org.
-- 
-- Acknowledgement
-- 
--    Funding for the RFC Editor function is currently provided by the
--    Internet Society.
-- ===========================================================================
