Private MIB files:
HUAWEI-BASE-TRAP-MIB.mib
HUAWEI-CBQOS-MIB.mib
HUAWEI-DHCP-SNOOPING-MIB.mib
HUAWEI-ENTITY-EXTENT-MIB.mib
HUAWEI-ENTITY-TRAP-MIB.mib
HUAWEI-IF-EXT-MIB.mib
HUAWEI-LLDP-MIB.mib
HUAWEI-POE-MIB.mib
HUAWEI-PORT-MIB.mib
HUAWEI-SECURITY-APT-CIS-MIB.mib
HUAWEI-SECURITY-AV-MIB.mib
HUAWEI-SECURITY-CAR-MIB.mib
HUAWEI-SECURITY-CLUSTER-MIB.mib
HUAWEI-SECURITY-CONFIG-MIB.mib
HUAWEI-SECURITY-DDOS-MIB.mib
HUAWEI-SECURITY-DISK-MIB.mib
HUAWEI-SECURITY-DSLITE-MIB.mib
HUAWEI-SECURITY-FAILOVER-MIB.mib
HUAWEI-SECURITY-FULLCONE-MIB.mib
HUAWEI-SECURITY-GTP-MIB.mib
HUAWEI-SECURITY-HEALTHCHECK-MIB.mib
HUAWEI-SECURITY-HRP-MIB.mib
HUAWEI-SECURITY-IPLINK-MIB.mib
HUAWEI-SECURITY-IPS-MIB.mib
HUAWEI-SECURITY-L2T-MIB.mib
HUAWEI-SECURITY-LICENSE-MIB.mib
HUAWEI-SECURITY-LOGIN-MIB.mib
HUAWEI-SECURITY-NAT-MIB.mib
HUAWEI-SECURITY-PPPOE-MIB.mib
HUAWEI-SECURITY-SCALE-MIB.mib
HUAWEI-SECURITY-SESSION-STAT-MIB.mib
HUAWEI-SECURITY-SLB-MIB.mib
HUAWEI-SECURITY-SMARTLINK-MIB.mib
HUAWEI-SECURITY-SSLVPN-MIB.mib
HUAWEI-SECURITY-STAT-MIB.mib
HUAWEI-SECURITY-STATBOARDPHY-MIB.mib
HUAWEI-SECURITY-TDNS-MIB.mib
HUAWEI-SECURITY-UM-MIB.mib
HUAWEI-SECURITY-UPDATE-MIB.mib
HUAWEI-SECURITY-VRFCAR-MIB.mib
HUAWEI-SECURITY-VSYS-MIB.mib
HUAWEI-TC-MIB.mib
HUAWEI-XQoS-MIB.mib

Common MIB Objects
		entPhysicalName
			OID:1.3.6.1.2.1.47.1.1.1.1.7
			Describtion:This object indicates the name of the physical entity.
			MIB:ENTITY-MIB
			
		entPhysicalSoftwareRev
			OID:1.3.6.1.2.1.47.1.1.1.1.10
			Describtion:This object indicates a software version number of a component.
			MIB:ENTITY-MIB
			
		entPhysicalSerialNum
			OID:1.3.6.1.2.1.47.1.1.1.1.11
			Describtion:This object indicates the sequence number.
			MIB:ENTITY-MIB

		hwEntityCpuUsage
			OID:1.3.6.1.4.1.2011.5.25.31.1.1.1.1.5
			Describtion:This object indicates the CPU usage rate.
						The value ranges from 0 to 100.
						The default value is 0.
			MIB:HUAWEI-ENTITY-EXTENT-MIB
			
		hwEntityMemUsage
			OID:1.3.6.1.4.1.2011.5.25.31.1.1.1.1.7
			Describtion:Eudemon8000E-X: This object indicates the memory usage of the MPU and LPU, and VRPIO memory usage of the SPU. The value ranges from 0 to 100 and is 0 by default.
						Eudemon200E-N/1000E-N: This object indicates the memory usage of the device. The value ranges from 0 to 100 and is 0 by default.
			MIB:HUAWEI-ENTITY-EXTENT-MIB

		hwSecStatUsage
			OID:1.3.6.1.4.1.2011.6.122.15.2.1.6
			Describtion:Only the Eudemon8000E-X supports this object.
						This object indicates the CPU usage of the SPU.
			MIB:HUAWEI-SECURITY-STAT-MIB

		hwSecStatPerfTotalMemUsage
			OID:1.3.6.1.4.1.2011.6.122.15.2.1.11
			Describtion:Only the Eudemon8000E-X supports this object.
						This object indicates detailed memory usage information on the SPU.
			MIB:HUAWEI-SECURITY-STAT-MIB
			
		hwSecStatPerfTotalMemUsage
			OID:1.3.6.1.4.1.2011.5.25.31.1.1.1.1.11
			Describtion:This object indicates the temperature.
			MIB:HUAWEI-ENTITY-EXTENT-MIB
			
		hwHardDiskUsage
			OID:1.3.6.1.4.1.2011.5.25.31.1.1.24.1.5
			Describtion:This object indicates the hard disk usage.
			MIB:HUAWEI-ENTITY-EXTENT-MIB
			
		entPhysicalSerialNum
			OID:1.3.6.1.2.1.47.1.1.1.1.11
			Describtion:This object indicates the serial number.
			MIB:ENTITY-MIB

		ifIndex
			OID:1.3.6.1.2.1.2.2.1.1
			Describtion:This object indicates the index of the interface.
			MIB:IF-MIB

		ifPhysAddress
			OID:1.3.6.1.2.1.2.2.1.6
			Describtion:This object indicates the MAC address of the interface.
			MIB:IF-MIB
			
		ifOperStatus
			OID:1.3.6.1.2.1.2.2.1.8
			Describtion:This object indicates the interface status.
			MIB:IF-MIB
			
		ifInOctets
			OID:1.3.6.1.2.1.2.2.1.10
			Describtion:This object indicates the total number of passed bytes in the inbound direction.
			MIB:IF-MIB
			
		ifInUcastPkts
			OID:1.3.6.1.2.1.2.2.1.11
			Describtion:This object indicates the number of unicast packets in the inbound direction.
			MIB:IF-MIB
			
		ifInNUcastPkts
			OID:1.3.6.1.2.1.2.2.1.12
			Describtion:This object indicates the number of non-unicast packets in the inbound direction.
			MIB:IF-MIB

		ifInDiscards
			OID:1.3.6.1.2.1.2.2.1.13
			Describtion:This object indicates the number of packets discarded on the interface in the inbound direction.
			MIB:IF-MIB
			
		ifInErrors
			OID:1.3.6.1.2.1.2.2.1.14
			Describtion:This object indicates the number of error packets in the inbound direction.
			MIB:IF-MIB
			
		ifOutOctets
			OID:1.3.6.1.2.1.2.2.1.16
			Describtion:This object indicates the total number of passed bytes in the outbound direction.
			MIB:IF-MIB
			
		ifOutUcastPkts
			OID:1.3.6.1.2.1.2.2.1.17
			Describtion:This object indicates the number of unicast packets in the outbound direction.
			MIB:IF-MIB
			
		ifOutNUcastPkts
			OID:1.3.6.1.2.1.2.2.1.18
			Describtion:This object indicates the number of non-unicast packets in the outbound direction.
			MIB:IF-MIB
			
		ifOutDiscards
			OID:1.3.6.1.2.1.2.2.1.19
			Describtion:This object indicates the number of packets discarded in the outbound direction.
			MIB:IF-MIB
			
		ifOutErrors
			OID:1.3.6.1.2.1.2.2.1.20
			Describtion:This object indicates the number of error packets in the outbound direction.
			MIB:IF-MIB

			
		hwSecStatMonCurSessSpeed
			OID:1.3.6.1.4.1.2011.6.122.15.1.2.1.3
			Describtion:This object indicates the session establishment rate.
			MIB:HUAWEI-SECURITY-STAT-MIB

		hwSecStatMonTotalSess
			OID:1.3.6.1.4.1.2011.6.122.15.1.2.1.4
			Describtion:This object indicates the total number of existing sessions.
			MIB:HUAWEI-SECURITY-STAT-MIB
			
		hwSecStatMonTcpSess
			OID:1.3.6.1.4.1.2011.6.122.15.1.2.1.6
			Describtion:This object indicates the total number of existing TCP sessions.
			MIB:HUAWEI-SECURITY-STAT-MIB
			
		hwSecStatMonUdpSess
			OID:1.3.6.1.4.1.2011.6.122.15.1.2.1.7
			Describtion:This object indicates the total number of existing UDP sessions.
			MIB:HUAWEI-SECURITY-STAT-MIB
			
		hwSecStatMonIcmpSess
			OID:1.3.6.1.4.1.2011.6.122.15.1.2.1.8
			Describtion:This object indicates the total number of existing ICMP sessions.
			MIB:HUAWEI-SECURITY-STAT-MIB
			
		hwSecStatNoSessTblPkts
			OID:1.3.6.1.4.1.2011.6.122.15.1.2.3.1
			Describtion:This object indicates the number of discarded non-first packets due to the absence of a session table.
			MIB:HUAWEI-SECURITY-STAT-MIB

		hwSecStatSeqErrPkts
			OID:1.3.6.1.4.1.2011.6.122.15.1.2.3.3
			Describtion:This object indicates the total number of packets discarded due to sequence number errors.
			MIB:HUAWEI-SECURITY-STAT-MIB
			
		hwSecStatBlsDenyPkts
			OID:1.3.6.1.4.1.2011.6.122.15.1.2.3.9
			Describtion:This object indicates the total number of packets discarded due to the blacklist.
			MIB:HUAWEI-SECURITY-STAT-MIB
			
		hwSecStatFragExcessDropPkts
			OID:1.3.6.1.4.1.2011.6.122.15.1.2.3.21
			Describtion:This object indicates the number of discarded packets in excess fragments.
			MIB:HUAWEI-SECURITY-STAT-MIB
			
		hwSecStatSessFailDropPkts
			OID:1.3.6.1.4.1.2011.6.122.15.1.2.3.23
			Describtion:This object indicates the total number of packets discarded due to session exhaustion.
			MIB:HUAWEI-SECURITY-STAT-MIB
			
		hwSecStatSecurityPolicyDenyPkts
			OID:1.3.6.1.4.1.2011.6.122.15.1.2.3.39
			Describtion:This object indicates the total number of packets discarded due to security policies.
			MIB:HUAWEI-SECURITY-STAT-MIB
			
		hwSecStatDeviceThroughput
			OID:1.3.6.1.4.1.2011.6.122.15.6.4
			Describtion:This object indicates the throughput of the device.
			MIB:HUAWEI-SECURITY-STAT-MIB
