-- =================================================================
-- Description: VRRP mib
-- Reference:   This mib was extracted from RFC 2787
-- =================================================================

VRRP-MIB DEFINITIONS ::= BEGIN

    IMPORTS
        MODULE-IDENTITY, OBJECT-TYPE,
        NOTIFICATION-TYPE, Counter32,
        Integer32, IpAddress, mib-2         FROM SNMPv2-SMI
    
        TEXTUAL-CONVENTION, RowStatus,
        MacAddress, TruthValue, TimeStamp   FROM SNMPv2-TC
    
        MODULE-COMPLIANCE, OBJECT-GROUP,
        NOTIFICATION-GROUP                  FROM SNMPv2-CONF
        ifIndex                             FROM IF-MIB;
 
 
    
    
    vrrpMIB  MODULE-IDENTITY
        LAST-UPDATED "200003030000Z"
        ORGANIZATION "IETF VRRP Working Group"
        CONTACT-INFO
               "Brian R. Jewell
        Postal: Copper Mountain Networks, Inc.
                2470 Embarcadero Way
                Palo Alto, California 94303
        Tel:    +1 650 687 3367
        E-Mail: bjewell@coppermountain.com"
    
        DESCRIPTION
            "This MIB describes objects used for managing Virtual Router
             Redundancy Protocol (VRRP) routers."
        REVISION "200003030000Z"    -- 03 Mar 2000
        DESCRIPTION "Initial version as published in RFC 2787."
        ::= { mib-2 68 }
    
    -- *******************************************************************
    --  Textual Conventions
    -- *******************************************************************

    VrId ::= TEXTUAL-CONVENTION
        STATUS       current
        DESCRIPTION
            "A number which, along with an interface index (ifIndex),
            serves to uniquely identify a virtual router on a given VRRP
            router. A set of one or more associated addresses is assigned
            to a VRID."
        SYNTAX      Integer32 (1..255)
    
    -- *******************************************************************
    --  VRRP MIB Groups
    -- *******************************************************************

    vrrpOperations      OBJECT IDENTIFIER ::= { vrrpMIB 1 }
    vrrpStatistics      OBJECT IDENTIFIER ::= { vrrpMIB 2 }
    vrrpConformance     OBJECT IDENTIFIER ::= { vrrpMIB 3 }


    -- *******************************************************************
    --  Start of MIB objects
    -- *******************************************************************

    vrrpNodeVersion  OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
           "This value identifies the particular version of the VRRP
            supported by this node."
        ::= { vrrpOperations 1 }
    
    vrrpNotificationCntl  OBJECT-TYPE
        SYNTAX       INTEGER {
            enabled     (1),
            disabled    (2)
        }
        MAX-ACCESS   read-write
        STATUS       current
        DESCRIPTION
           "Indicates whether the VRRP-enabled router will generate
            SNMP traps for events defined in this MIB. 'Enabled'
            results in SNMP traps; 'disabled', no traps are sent."
        DEFVAL { enabled }
        ::= { vrrpOperations 2 }
    
    -- *******************************************************************
    --  VRRP Operations Table
    -- *******************************************************************

    vrrpOperTable OBJECT-TYPE
        SYNTAX       SEQUENCE OF VrrpOperEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "Operations table for a VRRP router which consists of a
             sequence (i.e., one or more conceptual rows) of
             'vrrpOperEntry' items."
        ::= { vrrpOperations 3 }
    
    vrrpOperEntry OBJECT-TYPE
        SYNTAX       VrrpOperEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "An entry in the vrrpOperTable containing the operational
             characteristics of a virtual router. On a VRRP router,
             a given virtual router is identified by a combination
             of the IF index and VRID.
    
             Rows in the table cannot be modified unless the value
             of `vrrpOperAdminState' is `disabled' and the
             `vrrpOperState' has transitioned to `initialize'."
    
        INDEX    { ifIndex, vrrpOperVrId }
        ::= { vrrpOperTable 1 }
    
    VrrpOperEntry ::=
        SEQUENCE {
            vrrpOperVrId
                VrId,
            vrrpOperVirtualMacAddr
                MacAddress,
            vrrpOperState
                INTEGER,
            vrrpOperAdminState
                INTEGER,
            vrrpOperPriority
                Integer32,
            vrrpOperIpAddrCount
                Integer32,
            vrrpOperMasterIpAddr
                IpAddress,
            vrrpOperPrimaryIpAddr
                IpAddress,
            vrrpOperAuthType
                INTEGER,
            vrrpOperAuthKey
                OCTET STRING,
            vrrpOperAdvertisementInterval
                Integer32,
            vrrpOperPreemptMode
                TruthValue,
            vrrpOperVirtualRouterUpTime
                TimeStamp,
            vrrpOperProtocol
                INTEGER,
            vrrpOperRowStatus
                RowStatus
    }
    
    vrrpOperVrId OBJECT-TYPE
        SYNTAX       VrId
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "This object contains the Virtual Router Identifier (VRID)."
        ::= { vrrpOperEntry 1 }
    
    vrrpOperVirtualMacAddr OBJECT-TYPE
        SYNTAX       MacAddress
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The virtual MAC address of the virtual router. Although this
            object can be derived from the 'vrrpOperVrId' object, it is
            defined so that it is easily obtainable by a management
            application and can be included in VRRP-related SNMP traps."
        ::= { vrrpOperEntry 2 }
    
    vrrpOperState OBJECT-TYPE
     SYNTAX       INTEGER {
         initialize(1),
         backup(2),
         master(3)
     }
     MAX-ACCESS   read-only
     STATUS       current

     DESCRIPTION
         "The current state of the virtual router. This object has
         three defined values:
    
              - `initialize', which indicates that all the
                virtual router is waiting for a startup event.
    
              - `backup', which indicates the virtual router is
                monitoring the availability of the master router.
    
              - `master', which indicates that the virtual router
                is forwarding packets for IP addresses that are
                associated with this router.
    
            Setting the `vrrpOperAdminState' object (below) initiates
            transitions in the value of this object."
        ::= { vrrpOperEntry 3 }
    
    vrrpOperAdminState OBJECT-TYPE
        SYNTAX       INTEGER {
            up(1),
            down(2)
        }
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION
            "This object will enable/disable the virtual router
            function. Setting the value to `up', will transition
            the state of the virtual router from `initialize' to `backup'
            or `master', depending on the value of `vrrpOperPriority'.
            Setting the value to `down', will transition  the
            router from `master' or `backup' to `initialize'. State
            transitions may not be immediate; they sometimes depend on
            other factors, such as the interface (IF) state.
    
            The `vrrpOperAdminState' object must be set to `down' prior
            to modifying the other read-create objects in the conceptual
            row. The value of the `vrrpOperRowStatus' object (below)
            must be `active', signifying that the conceptual row
            is valid (i.e., the objects are correctly set),
            in order for this object to be set to `up'."
        DEFVAL    { down }
        ::= { vrrpOperEntry 4 }
    
    vrrpOperPriority OBJECT-TYPE
        SYNTAX       Integer32 (0..255)
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION
            "This object specifies the priority to be used for the
            virtual router master election process. Higher values imply
            higher priority.
    
            A priority of '0', although not settable, is sent by
            the master router to indicate that this router has ceased
            to participate in VRRP and a backup virtual router should
            transition  to become a new master.
    
            A priority of 255 is used for the router that owns the
            associated IP address(es)."
        DEFVAL       { 100 }
        ::= { vrrpOperEntry 5 }
    
    vrrpOperIpAddrCount OBJECT-TYPE
        SYNTAX       Integer32 (0..255)
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The number of IP addresses that are associated with this
            virtual router. This number is equal to the number of rows
            in the vrrpAssoIpAddrTable that correspond to a given IF
            index/VRID pair."
        ::= { vrrpOperEntry 6 }
    
    vrrpOperMasterIpAddr OBJECT-TYPE
        SYNTAX       IpAddress
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The master router's real (primary) IP address. This is
            the IP address listed as the source in VRRP advertisement
            last received by this virtual router."
        ::= { vrrpOperEntry 7 }
    
    vrrpOperPrimaryIpAddr OBJECT-TYPE
        SYNTAX       IpAddress
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION
            "In the case where there is more than one IP address for
            a given `ifIndex', this object is used to specify the IP
            address that will become the `vrrpOperMasterIpAddr', should
            the virtual router transition from backup to master. If
            this object is set to 0.0.0.0, the IP address which is
            numerically lowest will be selected."
        DEFVAL       { '00000000'H } -- 0.0.0.0
        ::= { vrrpOperEntry 8 }
    
    vrrpOperAuthType OBJECT-TYPE
        SYNTAX       INTEGER {
            noAuthentication(1),       -- VRRP protocol exchanges are not
                                       -- authenticated.
            simpleTextPassword(2),     -- Exchanges are authenticated by a
                                       -- clear text password.
            ipAuthenticationHeader(3)  -- Exchanges are authenticated using
                                       -- the IP authentication header.
        }
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION
            "Authentication type used for VRRP protocol exchanges between
            virtual routers. This value of this object is the same for a
            given ifIndex.
    
            New enumerations to this list can only be added via a new
            RFC on the standards track."
        DEFVAL       { noAuthentication }
        ::= { vrrpOperEntry 9 }
    
    vrrpOperAuthKey OBJECT-TYPE
        SYNTAX       OCTET STRING (SIZE (0..16))
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION
            "The Authentication Key. This object is set according to
            the value of the 'vrrpOperAuthType' object
            ('simpleTextPassword' or 'ipAuthenticationHeader'). If the
            length of the value is less than 16 octets, the agent will
            left adjust and zero fill to 16 octets. The value of this
            object is the same for a given ifIndex.
    
            When read, vrrpOperAuthKey always returns an Octet String
            of length zero."
        ::= { vrrpOperEntry 10 }
    
    vrrpOperAdvertisementInterval OBJECT-TYPE
        SYNTAX       Integer32 (1..255)
        UNITS        "seconds"
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION
            "The time interval, in seconds, between sending
            advertisement messages. Only the master router sends
            VRRP advertisements."
        DEFVAL       { 1 }
        ::= { vrrpOperEntry 11 }
    
    vrrpOperPreemptMode OBJECT-TYPE
        SYNTAX       TruthValue
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION
            "Controls whether a higher priority virtual router will
            preempt a lower priority master."
        DEFVAL       { true }
        ::= { vrrpOperEntry 12 }
    
    vrrpOperVirtualRouterUpTime OBJECT-TYPE
        SYNTAX       TimeStamp
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "This is the value of the `sysUpTime' object when this
            virtual router (i.e., the `vrrpOperState') transitioned
            out of `initialized'."
        ::= { vrrpOperEntry 13 }
    
    vrrpOperProtocol OBJECT-TYPE
        SYNTAX   INTEGER {
            ip (1),
            bridge (2),
            decnet (3),
            other (4)
        }
        MAX-ACCESS read-create
        STATUS     current
        DESCRIPTION
            "The particular protocol being controlled by this Virtual
            Router.
    
            New enumerations to this list can only be added via a new
            RFC on the standards track."
        DEFVAL { ip }
        ::= { vrrpOperEntry 14 }
    
    vrrpOperRowStatus OBJECT-TYPE
        SYNTAX       RowStatus
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION
            "The row status variable, used in accordance to installation
            and removal conventions for conceptual rows. The rowstatus of
            a currently active row in the vrrpOperTable is constrained
            by the operational state of the corresponding virtual router.
            When `vrrpOperRowStatus' is set to active(1), no other
            objects in the conceptual row, with the exception of
            `vrrpOperAdminState', can be modified. Prior to setting the
            `vrrpOperRowStatus' object from `active' to a different value,
            the `vrrpOperAdminState' object must be set to `down' and the
            `vrrpOperState' object be transitioned to `initialize'.
    
            To create a row in this table, a manager sets this object
            to either createAndGo(4) or createAndWait(5). Until instances
            of all corresponding columns are appropriately configured,
            the value of the corresponding instance of the `vrrpOperRowStatus'
            column will be read as notReady(3).
            In particular, a newly created row cannot be made active(1)
            until (minimally) the corresponding instance of
            `vrrpOperVrId' has been set and there is at least one active
            row in the `vrrpAssoIpAddrTable' defining an associated
            IP address for the virtual router."
        ::= { vrrpOperEntry 15 }


    -- *******************************************************************
    --  VRRP Associated IP Address Table
    -- *******************************************************************

    vrrpAssoIpAddrTable OBJECT-TYPE
        SYNTAX       SEQUENCE OF VrrpAssoIpAddrEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "The table of addresses associated with this virtual router."
        ::= { vrrpOperations 4 }
    
    vrrpAssoIpAddrEntry OBJECT-TYPE
        SYNTAX       VrrpAssoIpAddrEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "An entry in the table contains an IP address that is
            associated with a virtual router. The number of rows for
            a given ifIndex and VrId will equal the number of IP
            addresses associated (e.g., backed up) by the virtual
            router (equivalent to 'vrrpOperIpAddrCount').
    
            Rows in the table cannot be modified unless the value
            of `vrrpOperAdminState' is `disabled' and the
            `vrrpOperState' has transitioned to `initialize'."
    
        INDEX    { ifIndex, vrrpOperVrId, vrrpAssoIpAddr }
        ::= { vrrpAssoIpAddrTable 1 }
    
    VrrpAssoIpAddrEntry ::=
        SEQUENCE {
            vrrpAssoIpAddr
                IpAddress,
            vrrpAssoIpAddrRowStatus
                RowStatus
    }
    
    vrrpAssoIpAddr OBJECT-TYPE
        SYNTAX       IpAddress
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "The assigned IP addresses that a virtual router is
            responsible for backing up."
        ::= { vrrpAssoIpAddrEntry 1 }
    
    vrrpAssoIpAddrRowStatus OBJECT-TYPE
        SYNTAX       RowStatus
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION
            "The row status variable, used according to installation
            and removal conventions for conceptual rows. Setting this
            object to active(1) or createAndGo(4) results in the
            addition of an associated address for a virtual router.
            Destroying the entry or setting it to notInService(2)
            removes the associated address from the virtual router.
            The use of other values is implementation-dependent."
        ::= { vrrpAssoIpAddrEntry 2 }


    -- *******************************************************************
    --  VRRP Router Statistics
    -- *******************************************************************

    vrrpRouterChecksumErrors OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of VRRP packets received with an invalid
            VRRP checksum value."
        ::= { vrrpStatistics 1 }
    
    vrrpRouterVersionErrors OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of VRRP packets received with an unknown
            or unsupported version number."
        ::= { vrrpStatistics 2 }
    
    vrrpRouterVrIdErrors OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of VRRP packets received with an invalid
            VRID for this virtual router."
        ::= { vrrpStatistics 3 }
    
    -- *******************************************************************
    --  VRRP Router Statistics Table
    -- *******************************************************************

    vrrpRouterStatsTable OBJECT-TYPE
        SYNTAX       SEQUENCE OF VrrpRouterStatsEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "Table of virtual router statistics."
        ::= { vrrpStatistics 4 }
    
    vrrpRouterStatsEntry OBJECT-TYPE
        SYNTAX       VrrpRouterStatsEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "An entry in the table, containing statistics information
            about a given virtual router."
        AUGMENTS    { vrrpOperEntry }
        ::= { vrrpRouterStatsTable 1 }
    
    VrrpRouterStatsEntry ::=
        SEQUENCE {
            vrrpStatsBecomeMaster
                Counter32,
            vrrpStatsAdvertiseRcvd
                Counter32,
            vrrpStatsAdvertiseIntervalErrors
                Counter32,
            vrrpStatsAuthFailures
                Counter32,
            vrrpStatsIpTtlErrors
                Counter32,
            vrrpStatsPriorityZeroPktsRcvd
                Counter32,
            vrrpStatsPriorityZeroPktsSent
                Counter32,
            vrrpStatsInvalidTypePktsRcvd
                Counter32,
            vrrpStatsAddressListErrors
                Counter32,
            vrrpStatsInvalidAuthType
                Counter32,
            vrrpStatsAuthTypeMismatch
                Counter32,
            vrrpStatsPacketLengthErrors
                Counter32
        }
    
    vrrpStatsBecomeMaster OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of times that this virtual router's state
            has transitioned to MASTER."
        ::= { vrrpRouterStatsEntry 1 }
    
    vrrpStatsAdvertiseRcvd OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of VRRP advertisements received by this
            virtual router."
        ::= { vrrpRouterStatsEntry 2 }
    
    vrrpStatsAdvertiseIntervalErrors OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of VRRP advertisement packets received
            for which the advertisement interval is different than the
            one configured for the local virtual router."
        ::= { vrrpRouterStatsEntry 3 }
    
    vrrpStatsAuthFailures OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of VRRP packets received that do not pass
            the authentication check."
        ::= { vrrpRouterStatsEntry 4 }
    
    vrrpStatsIpTtlErrors OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of VRRP packets received by the virtual
            router with IP TTL (Time-To-Live) not equal to 255."
        ::= { vrrpRouterStatsEntry 5 }
    
    vrrpStatsPriorityZeroPktsRcvd OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of VRRP packets received by the virtual
            router with a priority of '0'."
        ::= { vrrpRouterStatsEntry 6 }
    
    vrrpStatsPriorityZeroPktsSent OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of VRRP packets sent by the virtual router
            with a priority of '0'."
        ::= { vrrpRouterStatsEntry 7 }
    
    vrrpStatsInvalidTypePktsRcvd OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The number of VRRP packets received by the virtual router
            with an invalid value in the 'type' field."
        ::= { vrrpRouterStatsEntry 8 }
    
    vrrpStatsAddressListErrors OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of packets received for which the address
            list does not match the locally configured list for the
            virtual router."
        ::= { vrrpRouterStatsEntry 9 }
    
    vrrpStatsInvalidAuthType OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of packets received with an unknown
            authentication type."
        ::= { vrrpRouterStatsEntry 10 }
    
    vrrpStatsAuthTypeMismatch OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of packets received with 'Auth Type' not
            equal to the locally configured authentication method
            (`vrrpOperAuthType')."
        ::= { vrrpRouterStatsEntry 11 }
    
    vrrpStatsPacketLengthErrors OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of packets received with a packet length
            less than the length of the VRRP header."
        ::= { vrrpRouterStatsEntry 12 }

    -- *******************************************************************
    --   Trap Definitions
    -- *******************************************************************

    vrrpNotifications   OBJECT IDENTIFIER ::= { vrrpMIB 0 }
    
    vrrpTrapPacketSrc OBJECT-TYPE
        SYNTAX       IpAddress
        MAX-ACCESS   accessible-for-notify
        STATUS       current
        DESCRIPTION
            "The IP address of an inbound VRRP packet. Used by
             vrrpTrapAuthFailure trap."
        ::= { vrrpOperations 5 }
    
    vrrpTrapAuthErrorType OBJECT-TYPE
        SYNTAX        INTEGER {
            invalidAuthType (1),
            authTypeMismatch (2),
            authFailure (3)
        }
        MAX-ACCESS   accessible-for-notify
        STATUS       current
        DESCRIPTION
            "Potential types of configuration conflicts.
            Used by vrrpAuthFailure trap."
        ::= { vrrpOperations 6 }
    
 
 
 
 
 
 
 
 

    vrrpTrapNewMaster NOTIFICATION-TYPE
        OBJECTS      { vrrpOperMasterIpAddr
 
 
 
                     }
        STATUS       current
        DESCRIPTION
            "The newMaster trap indicates that the sending agent
            has transitioned to 'Master' state."
        ::= { vrrpNotifications 1 }
    
    vrrpTrapAuthFailure NOTIFICATION-TYPE
        OBJECTS      { vrrpTrapPacketSrc,
                       vrrpTrapAuthErrorType
                     }
        STATUS       current
        DESCRIPTION
            "A vrrpAuthFailure trap signifies that a packet has
            been received from a router whose authentication key
            or authentication type conflicts with this router's
            authentication key or authentication type. Implementation
            of this trap is optional."
        ::= { vrrpNotifications 2 }

 
 
 
 
 
 
 
 
 
 
 
 
 

    -- *******************************************************************
    --  Conformance Information
    -- *******************************************************************

    vrrpMIBCompliances  OBJECT IDENTIFIER ::= { vrrpConformance 1 }
    vrrpMIBGroups       OBJECT IDENTIFIER ::= { vrrpConformance 2 }

    -- ...................................................................
    -- Compliance Statements
    -- ...................................................................

    vrrpMIBCompliance MODULE-COMPLIANCE
        STATUS current
        DESCRIPTION
           "The core compliance statement for all VRRP implementations."
        MODULE -- this module
        MANDATORY-GROUPS  {
            vrrpOperGroup,
            vrrpStatsGroup
        }
        OBJECT        vrrpOperPriority
        WRITE-SYNTAX  Integer32 (1..255)
        DESCRIPTION  "SETable values are from 1 to 255."
        ::= { vrrpMIBCompliances 1 }
    
    -- ...................................................................
    -- Conformance Groups
    -- ...................................................................

    vrrpOperGroup  OBJECT-GROUP
        OBJECTS  {
            vrrpNodeVersion,
            vrrpNotificationCntl,
            vrrpOperVirtualMacAddr,
            vrrpOperState,
            vrrpOperAdminState,
            vrrpOperPriority,
            vrrpOperIpAddrCount,
            vrrpOperMasterIpAddr,
            vrrpOperPrimaryIpAddr,
            vrrpOperAuthType,
            vrrpOperAuthKey,
            vrrpOperAdvertisementInterval,
            vrrpOperPreemptMode,
            vrrpOperVirtualRouterUpTime,
            vrrpOperProtocol,
            vrrpOperRowStatus,
            vrrpAssoIpAddrRowStatus
            }
        STATUS current
        DESCRIPTION
           "Conformance group for VRRP operations."
        ::= { vrrpMIBGroups 1 }
    
    vrrpStatsGroup  OBJECT-GROUP
        OBJECTS  {
            vrrpRouterChecksumErrors,
            vrrpRouterVersionErrors,
            vrrpRouterVrIdErrors,
            vrrpStatsBecomeMaster,
            vrrpStatsAdvertiseRcvd,
            vrrpStatsAdvertiseIntervalErrors,
            vrrpStatsAuthFailures,
            vrrpStatsIpTtlErrors,
            vrrpStatsPriorityZeroPktsRcvd,
            vrrpStatsPriorityZeroPktsSent,
            vrrpStatsInvalidTypePktsRcvd,
            vrrpStatsAddressListErrors,
            vrrpStatsInvalidAuthType,
            vrrpStatsAuthTypeMismatch,
            vrrpStatsPacketLengthErrors
            }
        STATUS current
        DESCRIPTION
           "Conformance group for VRRP statistics."
        ::= { vrrpMIBGroups 2 }
    
    vrrpTrapGroup  OBJECT-GROUP
        OBJECTS  {
            vrrpTrapPacketSrc,
            vrrpTrapAuthErrorType            
 
         }
     STATUS current
     DESCRIPTION
        "Conformance group for objects contained in VRRP notifications."
     ::= { vrrpMIBGroups 3 }

 vrrpNotificationGroup NOTIFICATION-GROUP
     NOTIFICATIONS {
         vrrpTrapNewMaster,
            vrrpTrapAuthFailure
 
         }
        STATUS current
        DESCRIPTION
           "The VRRP MIB Notification Group."
     ::= { vrrpMIBGroups 4 }
    
END

-- 
--    Copyright (C) The Internet Society (2000).  All Rights Reserved.
-- 
--    This document and translations of it may be copied and furnished to
--    others, and derivative works that comment on or otherwise explain it
--    or assist in its implementation may be prepared, copied, published
--    and distributed, in whole or in part, without restriction of any
--    kind, provided that the above copyright notice and this paragraph are
--    included on all such copies and derivative works.  However, this
--    document itself may not be modified in any way, such as by removing
--    the copyright notice or references to the Internet Society or other
--    Internet organizations, except as needed for the purpose of
--    developing Internet standards in which case the procedures for
--    copyrights defined in the Internet Standards process must be
--    followed, or as required to translate it into languages other than
--    English.
-- 
--    The limited permissions granted above are perpetual and will not be
--    revoked by the Internet Society or its successors or assigns.
-- 
--    This document and the information contained herein is provided on an
--    "AS IS" basis and THE INTERNET SOCIETY AND THE INTERNET ENGINEERING
--    TASK FORCE DISCLAIMS ALL WARRANTIES, EXPRESS OR IMPLIED, INCLUDING
--    BUT NOT LIMITED TO ANY WARRANTY THAT THE USE OF THE INFORMATION
--    HEREIN WILL NOT INFRINGE ANY RIGHTS OR ANY IMPLIED WARRANTIES OF
--    MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.
-- 

