-- ============================================================================
-- Copyright (C) 2023 by  HUAWEI TECHNOLOGIES. All rights reserved.
-- Description: 
-- Reference: None
-- Version:   V3.86
-- ============================================================================
--
-- HUAWEI-ENTITY-EXTENT-MIB.mib
-- MIB generated by Visual MIB Builder Version 4.0 Build 341
-- Friday, July 15, 2011 at 16:41:48
--

    HUAWEI-ENTITY-EXTENT-MIB DEFINITIONS ::= BEGIN
 
        IMPORTS
            entPhysicalIndex, entPhysicalVendorType, entPhysicalName, entPhysicalClass, PhysicalClass, PhysicalIndex            
                FROM ENTITY-MIB            
            hwDatacomm            
                FROM HUAWEI-MIB            
            InterfaceIndex            
                FROM IF-MIB       
            EnabledStatus            
                FROM P-BRIDGE-MIB            
            SnmpAdminString            
                FROM SNMP-FRAMEWORK-MIB            
            OBJECT-GROUP, MODULE-COMPLIANCE, NOTIFICATION-GROUP            
                FROM SNMPv2-CONF            
            Integer32, Unsigned32, Counter64, OBJECT-TYPE, MODULE-IDENTITY, NOTIFICATION-TYPE            
                FROM SNMPv2-SMI            
            DateAndTime, DisplayString, RowStatus, TEXTUAL-CONVENTION, AutonomousType            
                FROM SNMPv2-TC;


        -- 1.3.6.1.4.1.2011.5.25.31
        hwEntityExtentMIB MODULE-IDENTITY 
            LAST-UPDATED "202309070000Z"
            ORGANIZATION 
                "Huawei Technologies Co.,Ltd."
            CONTACT-INFO 
                "Huawei Industrial Base
  Bantian, Longgang
   Shenzhen 518129
   People's Republic of China
   Website: http://www.huawei.com
   Email: support@huawei.com
 "          
             DESCRIPTION 
                "The private mib file includes the general extent information of the device."

            REVISION     "202309070000Z"                                                                                   
            DESCRIPTION  "V3.86, modify DESCRIPTION of hwEntityOpticalTunableModuleChannel."

            REVISION     "202302140000Z"                                                                                   
            DESCRIPTION  "V3.85, add hwEntityPortType enum value."

            REVISION     "202211240000Z"                                                                                   
            DESCRIPTION  "V3.84 modify hwEntityOpticalType."

            REVISION     "202211180000Z"                                                                                   
            DESCRIPTION  "V3.83 add hwEntityExtHardDiskOnlineFail and  hwEntityExtHardDiskOfflineFail."
            
            REVISION     "202209130000Z"                                                                                   
            DESCRIPTION  "V3.82 modify the description of hwEntityOpticalVoltage, hwEntityOpticalRxPower, hwEntityOpticalTxPower, hwEntityOpticalTemperature."
            
            REVISION     "202205230000Z"                                                                                   
            DESCRIPTION  "V3.81 Add hwIntegratedPowerResetOutput"
            
            REVISION     "202112170000Z"
            DESCRIPTION  "V3.80, modify hwEntityFanName."
            
            REVISION     "202112160000Z" 
            DESCRIPTION  "V3.79, add hwEntityFanName."
            
            REVISION     "202111260000Z" 
            DESCRIPTION  "V3.78, modify DESCRIPTION of hwSystemPowerTable, hwSystemPowerEntry, hwSystemPowerDeviceID, hwSystemPowerTotalPower, hwSystemPowerUsedPower, hwSystemPowerRemainPower, hwSystemPowerReservedPower"

            REVISION     "202111010000Z" 
            DESCRIPTION  "V3.77, modify hwEntityPortType."

            REVISION     "202108070000Z" 
            DESCRIPTION  "V3.76, dd the invalid value description of hwEntityOpticalTemperature, hwEntityOpticalVoltage, hwEntityOpticalBiasCurrent."

            REVISION     "202108070000Z" 
            DESCRIPTION  "V3.75, modify hwEntityOpticalType"

            REVISION     "202107030000Z"
	    DESCRIPTION  "V3.74, add hwBatteryGroupInstallTimeYear, hwBatteryGroupInstallTimeMonth, hwBatteryGroupInstallTimeDay"
            REVISION     "202106290000Z"
	    DESCRIPTION  "V3.73, add hwIntegratedPowerACCurrent, hwIntegratedPower53VDCOutCurrent, hwIntegratedPwrChip1UpgrageStatus,
			hwIntegratedPwrChip2UpgrageStatus, hwIntegratedPwrChip3UpgrageStatus, hwIntegratedPwrChip4UpgrageStatus, hwBatteryChipTable, hwBatteryChipEntry, hwBatteryChipVolt, hwBatteryChipTemp, hwLithiumBatteryVersion"
            REVISION     "202106040000Z" 
            DESCRIPTION  "V3.72, modify hwEntityPortType"

            REVISION     "202105070000Z"
            DESCRIPTION  "V3.71, add hwEntityOpticalFiberType enum value"

            REVISION     "202101130000Z"
            DESCRIPTION  "V3.70, modify hwApInfoTable"

            REVISION     "202012100000Z"
            DESCRIPTION  "V3.69, modify hwCpuUsageTrapSlot"

            REVISION     "202012090000Z"
            DESCRIPTION  "V3.68, add hwIntegratedPowerSoftwareVersionASCII, hwIntegratedPowerCurrentMode, hwIntegratedPowerBusbarVolt, hwIntegratedPowerACVolt, hwIntegratedPowerSolarInputVolt, hwIntegratedPowerSolarInputCurrent, hwIntegratedPower53VDCOutVolt, 
                                       hwIntegratedPowerTotalLoadPower, hwIntegratedPowerDCOverVoltThreshold, hwIntegratedPowerDCUnderVoltThreshold, hwIntegratedPowerLowLoadVoltPowerOffThreshold, hwIntegratedPower53VDCOutVoltLowerThreshold, hwLithiumBatteryGroupTable, 
                                       hwLithiumBatteryGroupEntry, hwBatteryGroupBatteryStatus, hwBatteryGroupBatteryVolt, hwBatteryGroupBatteryCurrent, hwBatteryGroupTotalBatteryCapacity, hwBatteryGroupAvailableBatteryCapacity, hwBatteryGroupBatteryTemperature, hwBatteryGroupBatteryRunTime,
                                       hwBatteryGroupNumberOfConnectedESMU, hwBatteryGroupChargeCurrentLimitCoefficient, hwBatteryGroupFloatChargingVolt, hwBatteryGroupEqualizedChargingVolt, hwLithiumBatteryTable, hwLithiumBatteryEntry, hwLithiumBatteryIndex, hwLithiumBatteryVolt,
                                       hwLithiumBatteryCurrent, hwLithiumBatteryDeviceAddr, hwLithiumBatteryStatus, hwLithiumBatterySOH, hwLithiumBatteryCapacity, hwLithiumBatteryCellPackageVolt, hwLithiumBatteryMaxLimitCoefficient, and modify hwIntegratedPowerEnergyWorkmode"

            REVISION     "202012080000Z"
            DESCRIPTION  "V3.67, modify hwCpuUsageTrapSlot"

            REVISION     "202011280000Z"
            DESCRIPTION  "V3.66, add hwEntityOpticalDifferentialGroupDelay, hwEntityOpticalChromaticDispersion"

            REVISION     "202011140000Z"
            DESCRIPTION  "V3.65, add hwEntitySafeId"
			
            REVISION     "202011060000Z" 
            DESCRIPTION  "V3.64, add hwEntityHigCrcErrorAlarm, hwEntityHigCrcErrorAlarmResume, hwEntityHigDown, hwEntityHigDownResume"

            REVISION     "202009190000Z"
            DESCRIPTION  "V3.63 modify hwApInfoTable, hwApInfoEntry"

            REVISION     "202009110000Z"
            DESCRIPTION  "V3.62 modify the description of hwEntityExtBootPasswordAlarm"

            REVISION     "202009080000Z"
            DESCRIPTION  "V3.61 modify the description of hwEntityPwrPower"

            REVISION     "202007270000Z"
            DESCRIPTION  "V3.60 modify hwEntitySplitAttribute"

            REVISION     "202007220000Z"
            DESCRIPTION  "V3.59 modify hwEntityOpticalHuaweiCertified"

            REVISION     "202007210000Z"
            DESCRIPTION  "V3.58 modify hwEntityOpticalType"

            REVISION     "202007160000Z"
            DESCRIPTION  "V3.57 modify threashold to threshold"

            REVISION     "202007140000Z"
            DESCRIPTION  "V3.56 modify hwEntityTemperature, hwEntityTemperatureThreshold, hwEntityVoltage, hwEntityVoltageLowThreshold, hwEntityVoltageHighThreshold, hwEntityTemperatureLowThreshold, 
hwEntityOpticalWaveLength, hwEntityOpticalBiasCurrent, hwEntityOpticalRxLowThreshold, hwEntityOpticalRxHighThreshold, hwEntityOpticalTxLowThreshold, hwEntityOpticalTxHighThreshold"

            REVISION     "202007020000Z"
            DESCRIPTION  "V3.55 modify hwEntityOpticalBandWidth"

            REVISION     "202006110000Z"
            DESCRIPTION  "V3.54 modify hwEntityExtBootPasswordAlarm"

            REVISION     "202006110000Z" 
            DESCRIPTION  "V3.53 modify hwEntityPortType"

            REVISION     "202005200000Z" 
            DESCRIPTION  "V3.52 add hwEntityExtCpuUsageNotfication, hwEntityExtCpuUsageNotficationClear"

			REVISION     "202005180000Z" 
            DESCRIPTION  "V3.51 modify hwApInfoTable, hwApInfoEntry"
			REVISION     "202005140000Z" 
            DESCRIPTION  "V3.50 modify hwEntityOpticalHuaweiCertified"
			
			REVISION     "202005140000Z"                                                                                         
            DESCRIPTION  "V3.49 modify hwBoardAcOutputState"
			
			REVISION     "202004080000Z"                                                                                   
            DESCRIPTION  "V3.48 modify hwBoardAcOutputState"  
				
			REVISION     "202004070000Z"                                                                                   
            DESCRIPTION  "V3.47 Add hwIntegratedPowerRebootPower and modify hwBoardAcOutputState"  
			
            REVISION     "202003280000Z"                                                                                   
            DESCRIPTION  "V3.46 Add hwIntegratedPower53VDCOutVoltStatus, hwIntegratedPowerACInputVoltStatus and delete hwIntegratedPowerSoftwareVersionASCII"  

            REVISION     "202003270000Z"                                                                                   
            DESCRIPTION  "V3.45, Add hwIntegratedPowerSystemTable, hwIntegratedPowerSystemEntry, hwIntegratedPowerSoftwareVersion, hwIntegratedPowerHardwareVersion, hwIntegratedPowerSoftwareVersionASCII, hwIntegratedPowerTable, hwIntegratedPowerEntry, hwIntegratedPowerEnergyWorkmode, hwIntegratedPowerTotalInputPower, hwIntegratedPower12VDCOutVoltStatus, hwIntegratedPower24VACOutVolt, hwIntegratedPower24VACOutCurrent"     

            REVISION     "202002190000Z"                                                                                   
            DESCRIPTION  "V3.44, Add denoise(11) to the list of hwEntityFanSpdAdjMode values"     
            
            REVISION     "202001020000Z" 
            DESCRIPTION  "V3.43, Add the hwEntityMemCacheUsage"

            REVISION     "201912260000Z" 
            DESCRIPTION  "V3.42, Updated the hwEntityHigStateChangeNotify, hwEntityHigStateDownNotify"

            REVISION     "201912120001Z" 
            DESCRIPTION  "V3.40, Add hwEntityTemperatureMinorThreshold,
                hwEntityVoltageFatalHighThreshold, hwEntityVoltageFatalLowThreshold"

            REVISION     "201912120000Z"                                                                                   
            DESCRIPTION  "V3.40, Add hwEntityTemperatureMinorThreshold,
                hwEntityVoltageFatalHighThreshold, hwEntityVoltageFatalLowThreshold"

            REVISION     "201909120000Z"                                                                                   
            DESCRIPTION  "V3.39, Updated the hwEntitySupportFlexCard"

            REVISION     "201908290000Z"                                                                                   
            DESCRIPTION  "V3.38, Updated the hwEntitySerdesChangeNotify, hwEntitySerdesDownNotify"

            REVISION     "201908260000Z"                                                                                   
            DESCRIPTION  "V3.37, Updated the hwBoardDcOutputState"

            REVISION     "201907130000Z"                                                                                   
            DESCRIPTION  "V3.36, Add hwEntityExtBootPasswordAlarm, hwEntityExtSmallBootPasswordAlarm"

            REVISION     "201906280000Z"                                                                                   
            DESCRIPTION  "V3.35, Add abnormal(0) to the list of hwEntityVolStatus values"
            
            REVISION     "201906150000Z"                                                                                   
            DESCRIPTION  "V3.34, Add hwApInfoTable, hwApInfoEntry, hwEntityApid, hwEntityApIndex, hwEntityApName, hwEntityApMemUsage, hwEntityApCpuUsage"

			REVISION     "201905220000Z"                                                                                   
            DESCRIPTION  "V3.33, Add hwEntityOpticalPortName"
			
            REVISION     "201903280000Z"                                                                                   
            DESCRIPTION  "V3.32, Add hwEntityExtSDCardFsErrorAlarm, hwEntityExtSDCardFsErrorResume, hwEntityExtSDCardUsageOver, hwEntityExtSDCardUsageBelow, hwEntityExtCFCardFaultAlarm, hwEntityExtCFCardFaultResume"

            REVISION     "201903070000Z"                                                                                   
            DESCRIPTION  "V3.31, Add hwEntityHigDiscardPacketNotify"

            REVISION     "201903010000Z"                                                                                   
            DESCRIPTION  "V3.30, Updated the hwEntityOpticalType"

            REVISION     "201901280000Z"
            DESCRIPTION  "V3.29, Add hwEntityOpticalSupportDDM and hwAlarmConfigTable"

            REVISION     "201901070000Z"
            DESCRIPTION  "V3.28, Add hwEntityNVRAMFaultAlarmNotification and hwEntityNVRAMFaultResumeNotification"

            REVISION     "201812200000Z"
            DESCRIPTION  "V3.27, Add hwEntityMemSizeExt "

            REVISION     "201811260000Z"
            DESCRIPTION  "V3.26, Add hwBoardAcOutputStateTable "
           
            
            REVISION     "201810110000Z"
            DESCRIPTION  "V3.25, Update hwEntityOpticalBiasLowThreshold and hwEntityOpticalBiasHighThreshold, Add  hwEntityOpticalHuaweiCertified"

            REVISION "201806050000Z"		-- June 05, 2018 at 00:00 GMT
			DESCRIPTION
				"V3.24, Add hwBoardDcOutputStateTable and hwBoardDcOutputInfoTable"	
				
            REVISION     "201805310000Z"
            DESCRIPTION  "V3.23, Add sfp28(25) to the list of hwEntityOpticalType values"
			
            REVISION     "201804260000Z"
            DESCRIPTION  "V3.22, Add cfp8(24) to the list of hwEntityOpticalType values"
            
            REVISION     "201804180000Z"
            DESCRIPTION  "V3.21, Add hwDacsStatusTable"

            REVISION     "201803230000Z"
            DESCRIPTION  "V3.20, hwPwrStatusTable Add hwEntityPwrPower"		
	
            REVISION     "201803140000Z"
            DESCRIPTION  "V3.19, hwEntityOpticalMode Add singleAndmultiMode"
			
            REVISION     "201802070000Z"
            DESCRIPTION  "V3.18, Add hwEntityMPUType"
			
            REVISION     "201801150000Z"
            DESCRIPTION  "V3.17, Modify the description"

            REVISION     "201801110000Z"
            DESCRIPTION  "V3.16, Add hwEntityOpticalTempLowThreshold, hwEntityOpticalTempHighThreshold, hwEntityOpticalVoltLowThreshold, hwEntityOpticalVoltHighThreshold, hwEntityOpticalBiasLowThreshold, hwEntityOpticalBiasHighThreshold"
			
			REVISION     "201801040000Z"
            DESCRIPTION  "V3.15, Add hwEntityOpticalManufacturedDate "
			
            REVISION     "201711300000Z"
            DESCRIPTION  "V3.14, Updated the hwEntityPwrMode, add hvdc(4) to the list of hwEntityPwrMode values "

            REVISION     "201711300000Z"
            DESCRIPTION  "V3.123 Add hwEntityDeviceStatus, hwEntityPicStatus"

            REVISION     "201711230000Z"
            DESCRIPTION  "V3.12, Add hwIfBandRateTable"

            REVISION     "201711210000Z"
            DESCRIPTION  "V3.11, Modify the description of hwHda1Error"

            REVISION     "201711170000Z"
            DESCRIPTION  "V3.10, Delete hwUploadDiagnosticsEthernetPriority, hwDownloadDiagnosticsEthernetPriority"

            REVISION     "201711020000Z"
            DESCRIPTION  "V3.09, Add hwUploadDiagnosticsTable, hwDownloadDiagnosticsTable"
			
            REVISION     "201710110000Z"
            DESCRIPTION  "V3.08, hwEntityOpticalModel Add hwEntityExtHotPatchReservedFirst, hwEntityExtHotPatchReservedSecond, hwEntityExtHotPatchReservedThird, hwEntityExtHotPatchReservedFourth, hwEntityExtHotPatchReservedFifth"	
			
            REVISION     "201708140001Z"
            DESCRIPTION  "V3.07, hwEntityOpticalModel Add copperMode"	

            REVISION     "201708140000Z"
            DESCRIPTION  "V3.06, Add hwEntityOpticalModel"	
			
            REVISION     "201707200000Z"
            DESCRIPTION  "V3.05, Modify the description of hwHda1Error"

            REVISION     "201707190000Z"
            DESCRIPTION  "V3.04, Add hwEntityFanSpdAdjMode fan workmode"

            REVISION     "201706280000Z"
            DESCRIPTION  "V3.03, Add hwEntityNPStateTable"

            REVISION    "201706090000Z"
            DESCRIPTION  "V3.02, Processing compile errors"

            REVISION    "201706070000Z"
            DESCRIPTION  "V3.01, Add gponsfp in  hwEntityOpticalType "

            REVISION     "201705020000Z"
            DESCRIPTION  "V3.00, Add hwEntityExtDevConfigurationRecovered "

            REVISION     "201703180000Z"
            DESCRIPTION  "V2.99, Add hwEntityOpticalType,
                          hwEntityOpticalType- add a new OpticalType, thoses name is sfp_sfp_plus."
            
            REVISION     "201701140000Z"
            DESCRIPTION  "V2.98, Add hwEntityModelName, hwEntityIssueNumber
                          hwEntityModelName - The model for this entity. If there is no model string in elable of this entity or this entity does not support elabel, the invalid value(zero-string) will be returned.
                          hwEntityIssueNumber - The IssueNumber for this entity. If there is no IssueNumber string in elable of this entity or this entity does not support elabel, the invalid value(zero-string) will be returned"
						  
            REVISION     "201612240000Z"
            DESCRIPTION  "V2.97, Add hwUsbConfigInfoPara"
			
            REVISION     "201612240000Z"
            DESCRIPTION  "V2.96, Add hwEntityElabelVersion"
            
            REVISION     "201612120000Z"
            DESCRIPTION  "V2.95, Updated the hwEntityOpticalType, add cfp4(20) and qsfp28(21) to the list of hwEntityOpticalType values"

            REVISION     "201612050000Z"
            DESCRIPTION  "V2.94 Modify the description of hwHda1Error "

            REVISION     "201611260000Z"
            DESCRIPTION  "V2.93, Updated the hwEntityOpticalType, add csfp(19) to the list of hwEntityOpticalType values"
			
            REVISION     "201610280000Z"
            DESCRIPTION  "V2.92, Add hwEntityModel, hwEntityExInfo"
        
            REVISION     "201610210000Z"
            DESCRIPTION  "V2.91, Add hwEntityExtCPUOverInterfaceDown"
			
            REVISION     "201610180000Z"
            DESCRIPTION  "V2.90, Updated hwEntityExtCpuUsageSuddenChangeNotification, hwEntityExtMemoryUsageSuddenChangeNotification, hwEntitySlotID, hwEntityCpuID, hwEntityPreviousValue, hwEntityCurrentValue, hwEntityChangeValue, hwEntityChangeValueThreshold"

            REVISION 	 "201610090000Z"
            DESCRIPTION  "V2.89, Add hwCfcardStateInfo, hwHda1Error"
				
            REVISION 	 "201610090000Z"
            DESCRIPTION  "V2.88, Updated the hwHardDiskStateTable, hwEntityExtHardDiskFull, hwEntityExtHardDiskFullResume, hwEntityExtHardDiskPlugIn, hwEntityExtHardDiskPlugOut, hwEntityExtHardDiskOnline, hwEntityExtHardDiskOffline, hwEntityExtLPUPlugIn, hwEntityExtLPUPlugOut"
			
            REVISION     "201609280000Z"
            DESCRIPTION  "V2.87, Add hwCpuUsageMutationNotification, hwMemoryUsageMutationNotification, hwPreValue, hwCurValue, hwChangeValue, hwChangeValueThreshold, hwSamplingInterval"
			
            REVISION 	 "201609230000Z"
            DESCRIPTION  "V2.86, Add hwHardDiskStateTable, hwEntityExtHardDiskFull, hwEntityExtHardDiskFullResume, hwEntityExtHardDiskPlugIn, hwEntityExtHardDiskPlugOut, hwEntityExtHardDiskOnline, hwEntityExtHardDiskOffline, hwEntityExtLPUPlugIn, hwEntityExtLPUPlugOut"
	    
            REVISION 	 "201608301020Z"		-- August 30, 2016 at 10:20 GMT
            DESCRIPTION  "V2.85, Add hwBoardDropRuntPacketNotify"
				
            REVISION     "201607260000Z" 
            DESCRIPTION  "V2.84, Add hwEntityOpticalWaveLengthExact"

            REVISION     "201607260000Z"
            DESCRIPTION  "V2.83, Add hwEntityExtEncryptionCardFail"
			
            REVISION     "201607160000Z"
            DESCRIPTION  "V2.82, Add hwEntityHda1Usage, hwEntityHda1UsageThreshold, hwEntityHda1UsageResumeThreshold, hwEntityExtHda1UsageThresholdNotfication, hwEntityExtHda1UsageResumeThresholdNotfication"
			
            REVISION     "201605230000Z"
            DESCRIPTION  "V2.81, Add hwDiskType"

            REVISION     "201605100000Z"
            DESCRIPTION  "V2.80, Add hwEntityExtDiskDamaged,hwEntityExtDiskFull"

            REVISION     "201605050000Z"
            DESCRIPTION  "V2.79, Add hwEntityRuntPacketCheckNotify"

            REVISION     "201604210000Z"
            DESCRIPTION  "V2.78, Add hwProcessStateInfo, hwProcessName, hwEntityExtProcessErrorNotification"

            REVISION     "201604150000Z" 			
            DESCRIPTION  "V2.77, Updated the hwEntityOpticalType, add gps(18) to the list of hwEntityOpticalType values"

            REVISION     "201604050000Z" 
            DESCRIPTION  "V2.76, Modify hwEntityHigErrorPacketThresholdAlarm"

            REVISION     "201603280000Z" 
            DESCRIPTION  "V2.75, Add hwEntityPositionMismatchNotify"
            
            REVISION     "201602010000Z" 
            DESCRIPTION  "V2.74, Delete bits from definitions"

            REVISION     "201601110000Z" 
            DESCRIPTION  "V2.73, Add hwEntityHigCrcErrorThresholdAlarm, hwEntityHigStateChangeNotify, hwEntityHigStateDownNotify"		
		
            REVISION     "201512210000Z" 
            DESCRIPTION  "V2.72, Add hwEntityOpticalBandWidth"
			
            REVISION     "201512150000Z"
            DESCRIPTION  "V2.71, Add hwEntityExtCpuUsageThresholdNotficationClear and hwEntityExtMemUsageThresholdNotificationClear"
            
            REVISION     "201511230000Z" 
            DESCRIPTION  "V2.70, Add the hwEntityOpticalTransType, hwEntityOpticalConnectType, hwEntityOpticalOrderingName, hwEntityOpticalTransferDistance"

            REVISION     "201511020000Z"
            DESCRIPTION  "V2.69, Add hwEntityStatusChange"	

            REVISION     "201509180000Z" 
            DESCRIPTION  "V2.68, Add hwEntityPbufUsage, hwEntityTMUsage"

            REVISION     "201509080000Z" 
            DESCRIPTION  "V2.67, modify hwFileGeneResourceType Description"

            REVISION     "201509010000Z" 
            DESCRIPTION  "V2.66, modify hwEntityCpuFrequency UNITS"

            REVISION     "201508070000Z" 
            DESCRIPTION  "V2.65, Add the hwEntityInputRateThresholdAlarm, hwEntityInputRateThresholdAlarmResume, hwEntityOutputRateThresholdAlarm, hwEntityOutputRateThresholdAlarmResume"

            REVISION     "201507100000Z" 
            DESCRIPTION  "V2.64, modify hwEntityCurrent UNITS"

            REVISION     "201505160000Z" 
            DESCRIPTION  "V2.63, Add hwEntityOpticalMaxRxPower,hwEntityOpticalMinRxPower,hwEntityOpticalMaxTxPower,hwEntityOpticalMinTxPower"
            
            REVISION     "201504250000Z" 
            DESCRIPTION  "V2.62, Updated the hwEntityTemperatureLowThreshold Description" 

            REVISION     "201504250000Z" 
            DESCRIPTION  "V2.61, Updated the hwEntityOpticalType, add msa100glh(17) to the list of hwEntityOpticalType values" 		
            
            REVISION     "201503250000Z"
            DESCRIPTION  "V2.60, Add hwEntityTransceiverType"
			
            REVISION     "201502120000Z" 
            DESCRIPTION  "V2.59, Add the hwEntityCpuUsageHistoryTable, hwEntityMemUsageHistoryTable" 
			
            REVISION     "201409170000Z"
            DESCRIPTION  "V2.58, Updated the hwEntityBoardClass"
            
            REVISION     "201409170000Z" 
            DESCRIPTION  "V2.57, Add the hwEntityFaultLightKeepTime" 

            REVISION     "201408100000Z"
            DESCRIPTION  "V2.56, Add CE hwPwrStatusTable and hwEntityFanDesc"
	    
            REVISION     "201406230000Z"
            DESCRIPTION  "V2.55, Add access network product's hwEntityPhysicalSpecTable"
	    
            REVISION     "201406090000Z"
            DESCRIPTION  "V2.54, Add the hwEntityOpticalVendorOUI, hwEntityOpticalVendorRev, hwEntityOpticalGponSN"
	    
            REVISION     "201406090000Z"
            DESCRIPTION  "V2.53, Add hwAdmPortTable, hwAdmPortEntry and hwAdmPortDescription."

            REVISION     "201404260000Z"                                                                                   
            DESCRIPTION  "V2.52, Updated the hwEntityOpticalType"

            REVISION     "201404180000Z"
            DESCRIPTION  "V2.51, Add hwGPSLocationInfo"

            REVISION     "201403280000Z"
            DESCRIPTION  "V2.50, Add hwBatteryState"
	    
            REVISION     "201401030000Z"
            DESCRIPTION  "V2.49, Add the  hwEntityManufacturerOUI"
	    
            REVISION     "201312280000Z"
            DESCRIPTION  "V2.48, Add hwBoardSplitPorts"
	                    
            REVISION     "201312231120Z"                                                                                          
            DESCRIPTION  "V2.47, Update the hwEntityOpticalType, hwEntityOpticalFiberType" 

            REVISION     "201311281400Z"                                                                                   
            DESCRIPTION  "V2.46, Add hwEntitySplitAttribute , hwSystemPowerReservedPower"
	    
            REVISION     "201311200000Z"                                                                                   
            DESCRIPTION  "V2.45, Add hwEntityStartMode"

            REVISION     "201308230000Z"                                                                                   
            DESCRIPTION  "V2.44, Add hwBatteryInfoTable  "

            REVISION     "201307250000Z"                                                                                   
            DESCRIPTION  "V2.43, Add hwEntityOpticalLaneBiasCurrent , hwEntityOpticalLaneRxPower  ,  hwEntityOpticalLaneTxPower  "				
				
            REVISION     "201307111307Z"                                                                                   
            DESCRIPTION  "V2.42, Updated the hwEntityOpticalTunableType  "

            REVISION     "201306270000Z"                                                                                   
            DESCRIPTION  "V2.41, Add hwDeviceServiceType  "

            REVISION     "201306070000Z"                                                                                   
            DESCRIPTION  "V2.40, Add hwOSPUnifyManageObjects ,hwEntityExtOSPTrapsPrefix ,hwEntityExtUnconnected,hwEntityExtUnconnectedResume  "

            REVISION     "201306060000Z"                                                                                   
            DESCRIPTION  "V2.39, Updated the hwEntityOpticalType, hwEntityOpticalFiberType"

            REVISION     "201304270000Z"                                                                                   
            DESCRIPTION  "V2.38, Add hwEntityOpticalWaveBand"
            
            REVISION     "201304250000Z"
            DESCRIPTION  "V2.37, Add hwEntityBoardName,hwEntityBoardDescription,hwEntity5MinCpuUsage to hwEntityStateEntry"

            REVISION     "201304230000Z"
            DESCRIPTION  "V2.36, Updated the hwEntityOpticalType enum name of value 5 and add a new hwSystemGlobalObjects  hwEntitySystemServiceType "

            REVISION     "201304080000Z"
            DESCRIPTION  "V2.35, Add hwBoardSoftwareVersionIncompatible "

            REVISION     "201304030000Z"
            DESCRIPTION  "V2.34, Add hwEntityOpticalTunableModuleChannel"

            REVISION     "201303200000Z"
            DESCRIPTION  "V2.33, Add hwAlarmPnPSequenceNo and hwAlarmPnPChangeNotification "

            REVISION     "201303130000Z"
            DESCRIPTION  "V2.32, Add hwEntityOpticalTunableType and hwEntityOpticalWaveLengthDecimal "

           REVISION     "201201250000Z"
            DESCRIPTION  "V2.20, Updated the hwSystemGlobalObjects  hwEntitySystemServiceType "  
           
            ::= { hwDatacomm 31 }



--
-- Textual conventions
--

        HwAdminState ::= TEXTUAL-CONVENTION
            STATUS current
            DESCRIPTION 
                " Represents the various possible administrative states.
                A value of locked means the resource is administratively
                prohibited from use. A value of shuttingDown means that
                usage is administratively limited to current instances of
                use. A value of unlocked means the resource is not
                administratively prohibited from use. A value of up means
                that the port is not administratively shut down and a value 
                of down is the oppsite. A value of loopback here means the
                port is working in the loopback local mode. When a port is
                both shut down and looped back, we user the vale of down."
            REFERENCE 
                "ITU Recommendation X.731, 'Information Technology - Open
                Systems Interconnection - System Management: State
                Management Function', 1992"
            SYNTAX INTEGER
                {
                notSupported(1),
                locked(2),
                shuttingDown(3),
                unlocked(4),
                up(11),
                down(12),
                loopback(13)
                }

        HwOperState ::= TEXTUAL-CONVENTION
            STATUS current
            DESCRIPTION 
                " Represents the possible values of operational states.
                A value of disabled means the resource is totally
                inoperable. A value of enabled means the resource
                is partially or fully operable. The values up(11),down(12) and
                connect(13) is used only for NE5000E BTB or it's extended system.
                A value of protocolUp means the port is available in the protocol
                lay or has already prepared for transmitting or receiving data.
                A value of linkUp means the port is only available in the physical
                lay. A value of linkDown means the port is not available physically."
            REFERENCE 
                "ITU Recommendation X.731, 'Information Technology - Open
                Systems Interconnection - System Management: State
                Management Function', 1992"
            SYNTAX INTEGER
                {
                notSupported(1),
                disabled(2),
                enabled(3),
                offline(4),
                up(11),
                down(12),
                connect(13),
                protocolUp(15),
                linkUp(16),
                linkDown(17),
                present(18),
                absent(19)
                }

        HwStandbyStatus ::= TEXTUAL-CONVENTION
            STATUS current
            DESCRIPTION 
                " Represents the possible values of standby status.
                
                A value of hotStandby means the resource is not providing
                service, but is will be immediately able to take over the
                role of the resource to be backed-up, without the need for
                initialization activity, and will contain the same
                information as the resource to be backed up. A value of
                coldStandy means that the resource is to back-up another
                resource, but will not be immediately able to take over
                the role of a resource to be backed up, and will require
                some initialization activity. A value of providingService
                means the resource is providing service."
            REFERENCE 
                "ITU Recommendation X.731, 'Information Technology - Open
                Systems Interconnection - System Management: State
                Management Function', 1992"
            SYNTAX INTEGER
                {
                notSupported(1),
                hotStandby(2),
                coldStandby(3),
                providingService(4)
                }

        HwAlarmStatus ::= TEXTUAL-CONVENTION
            STATUS current
            DESCRIPTION 
                "Represents the possible values of alarm status.
                When no bits of this attribute are set, then none of the
                status conditions described below are present. When the
                value of under repair is set, the resource is currently
                being repaired.
                
                When the value of critical is set, one or more critical
                alarms are active against the resource. When the value of
                major is set, one or more major alarms are active against
                the resource. When the value of minor is set, one or more
                minor alarms are active against the resource. When the
                value of warning is set, one or more warning alarms are
                active against the resource. When the value of
                indeterminate is set, one or more  alarms of indeterminate
                severity are active against the resource.
                
                When the value of alarm outstanding is set, one or more
                alarms is active against the resource. The fault may or may
                not be disabling. "
            REFERENCE 
                "ITU Recommendation X.731, 'Information Technology - Open
                Systems Interconnection - System Management: State
                Management Function', 1992"
            SYNTAX BITS
                {
                notSupported(0),
                underRepair(1),
                critical(2),
                major(3),
                minor(4),
                alarmOutstanding(5),
                warning(6),
                indeterminate(7)
                }

        HWLevelState ::= TEXTUAL-CONVENTION
            STATUS current
            DESCRIPTION 
                "The normal state of input line ."
            SYNTAX INTEGER
                {
                lowLevel(1),
                highLevel(2)
                }


--
-- Node definitions
--

        -- 1.3.6.1.4.1.2011.5.25.31.1
        hwEntityExtObjects OBJECT IDENTIFIER ::= { hwEntityExtentMIB 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1
        hwEntityState OBJECT IDENTIFIER ::= { hwEntityExtObjects 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1
        hwEntityStateTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwEntityStateEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table describes entity status, including the management status, operation status, backup status, alarm status, CPU usage and usage threshold, and memory usage and usage threshold."
            ::= { hwEntityState 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1
        hwEntityStateEntry OBJECT-TYPE
            SYNTAX HwEntityStateEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Information about a particular physical entity.
                Each entry provides objects (entPhysicalDescr,
                entPhysicalVendorType, and entPhysicalClass) to help an NMS
                identify and characterize the entry, and objects
                (entPhysicalContainedIn and entPhysicalParentRelPos) to help
                an NMS relate the particular entry to other entries in this
                table."
            INDEX { entPhysicalIndex }
            ::= { hwEntityStateTable 1 }


        HwEntityStateEntry ::=
            SEQUENCE { 
                hwEntityAdminStatus
                    HwAdminState,
                hwEntityOperStatus
                    HwOperState,
                hwEntityStandbyStatus
                    HwStandbyStatus,
                hwEntityAlarmLight
                    HwAlarmStatus,
                hwEntityCpuUsage
                    Integer32,
                hwEntityCpuUsageThreshold
                    Integer32,
                hwEntityMemUsage
                    Integer32,
                hwEntityMemUsageThreshold
                    Integer32,
                hwEntityMemSize
                    Integer32,
                hwEntityUpTime
                    Integer32,
                hwEntityTemperature
                    Integer32,
                hwEntityTemperatureThreshold
                    Integer32,
                hwEntityVoltage
                    Integer32,
                hwEntityVoltageLowThreshold
                    Integer32,
                hwEntityVoltageHighThreshold
                    Integer32,
                hwEntityVoltageFatalLowThreshold
                    Integer32,
                hwEntityVoltageFatalHighThreshold
                    Integer32,
                hwEntityTemperatureLowThreshold
                    Integer32,
                hwEntityTemperatureMinorThreshold
                    Integer32,
                hwEntityOpticalPower
                    Integer32,
                hwEntityCurrent
                    Integer32,
                hwEntityMemSizeMega
                    Integer32,
                hwEntityPortType
                    INTEGER,
                hwEntityDuplex
                    INTEGER,
                hwEntityOpticalPowerRx
                    Integer32,
                hwEntityCpuUsageLowThreshold
                    Integer32,
                hwEntityBoardPower
                    Integer32,
                hwEntityCpuFrequency
                    Integer32,
                hwEntitySupportFlexCard
                    INTEGER,
                hwEntityBoardClass
                    INTEGER,
                hwNseOpmStatus
                    Integer32,
                hwEntityCpuMaxUsage
                    Integer32,
                hwEntityCPUType
                    SnmpAdminString,
                hwEntityMemoryType
                    SnmpAdminString,
                hwEntityFlashSize
                    Integer32,
                hwEntityIfUpTimes
                    Integer32,
                hwEntityIfDownTimes
                    Integer32,
                hwEntityCPUAvgUsage
                    Integer32,
                hwEntityMemoryAvgUsage
                    Integer32,
                hwEntityMemUsed
                    Unsigned32,
                hwEntityTotalFanNum
                    Integer32,
                hwEntityNomalFanNum
                    Integer32,
                hwEntityTotalPwrNum
                    Integer32,
                hwEntityNomalPwrNum
                    Integer32,
                hwEntityFaultLight
                    INTEGER,
                hwEntityBoardName
                    OCTET STRING,
                hwEntityBoardDescription
                    OCTET STRING,
                hwEntity5MinCpuUsage
                     Integer32,
                hwEntityStartMode 
                    INTEGER,
                hwEntitySplitAttribute
                    OCTET STRING,
                hwEntityFaultLightKeepTime
                    Integer32,	
                hwEntityPbufUsage
					Integer32,
				hwEntityTMUsage
					Integer32,    
				hwEntityHda1Usage
					Integer32,    
				hwEntityHda1UsageThreshold
					Integer32,    
				hwEntityHda1UsageResumeThreshold
					Integer32,
				hwEntitySlotID
					Integer32,					
				hwEntityCpuID
					Integer32,					
				hwEntityPreviousValue
					Integer32,
				hwEntityCurrentValue
					Integer32,
                hwEntityChangeValue
                    Integer32,
                hwEntityChangeValueThreshold
                    Integer32,
                hwEntityModelName
                    OCTET STRING,
                hwEntityIssueNumber
                    OCTET STRING,
                hwEntityDeviceStatus
	 INTEGER,
                hwEntityPicStatus
	 INTEGER,
                hwEntityMPUType
                    OCTET STRING,
                hwEntityMemSizeExt
                    Unsigned32,
                hwEntityMemCacheUsage
                    Integer32,
                hwCpuUsageTrapType
                    Integer32,
                hwCpuUsageTrapSlot
                    OCTET STRING,
                hwCpuUsageTrapCpu
                    Integer32,
                hwCpuUsageCurrentUsage
                    Integer32,
                hwCpuUsageThreashold
                    Integer32
             }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.1
        hwEntityAdminStatus OBJECT-TYPE
            SYNTAX HwAdminState
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the entity management status."
            ::= { hwEntityStateEntry 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.2
        hwEntityOperStatus OBJECT-TYPE
            SYNTAX HwOperState
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the entity operation status."
            ::= { hwEntityStateEntry 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.3
        hwEntityStandbyStatus OBJECT-TYPE
            SYNTAX HwStandbyStatus
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the entity backup status."
            ::= { hwEntityStateEntry 3 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.4
        hwEntityAlarmLight OBJECT-TYPE
            SYNTAX HwAlarmStatus
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the entity alarm status, which is consistent with the entity alarm indicator status."
            ::= { hwEntityStateEntry 4 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.5
        hwEntityCpuUsage OBJECT-TYPE
            SYNTAX Integer32 (0..100)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the CPU usage of an entity. Generally, the overall CPU usage of the entity is calculated, without considering the number of CPUs on the entity."
            ::= { hwEntityStateEntry 5 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.6
        hwEntityCpuUsageThreshold OBJECT-TYPE
            SYNTAX Integer32 (0..100)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the CPU usage threshold. When the CPU usage exceeds the threshold, a notification is sent."
            ::= { hwEntityStateEntry 6 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.7
        hwEntityMemUsage OBJECT-TYPE
            SYNTAX Integer32 (0..100)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the memory usage of an entity, that is, the percentage of the memory that has been used."
            ::= { hwEntityStateEntry 7 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.8
        hwEntityMemUsageThreshold OBJECT-TYPE
            SYNTAX Integer32 (0..100)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the memory usage threshold. When the memory usage exceeds the threshold, a notification is sent."
            ::= { hwEntityStateEntry 8 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.9
        hwEntityMemSize OBJECT-TYPE
            SYNTAX Integer32
            UNITS "bytes"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the memory size."
            ::= { hwEntityStateEntry 9 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.10
        hwEntityUpTime OBJECT-TYPE
            SYNTAX Integer32
            UNITS "seconds"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the total duration when an entity is in the UP state."
            ::= { hwEntityStateEntry 10 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.11
        hwEntityTemperature OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the entity temperature. Unit: centigrade"
            ::= { hwEntityStateEntry 11 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.12
        hwEntityTemperatureThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the upper threshold of the entity temperature. Unit: centigrade"
            ::= { hwEntityStateEntry 12 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.13
        hwEntityVoltage OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the entity voltage. Unit: mV"
            ::= { hwEntityStateEntry 13 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.14
        hwEntityVoltageLowThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the minimum entity voltage threshold. Unit: mV"
            ::= { hwEntityStateEntry 14 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.15
        hwEntityVoltageHighThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the maximum entity voltage threshold. Unit: mV"
            ::= { hwEntityStateEntry 15 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.16
        hwEntityTemperatureLowThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the lower entity temperature threshold. Unit: centigrade"
            ::= { hwEntityStateEntry 16 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.17
        hwEntityOpticalPower OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the optical module's optical power."
            ::= { hwEntityStateEntry 17 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.18
        hwEntityCurrent OBJECT-TYPE
            SYNTAX Integer32
            UNITS "mA"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the entity current."
            ::= { hwEntityStateEntry 18 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.19
        hwEntityMemSizeMega OBJECT-TYPE
            SYNTAX Integer32
            UNITS "M bytes"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the size of the entity SDRAM."
            ::= { hwEntityStateEntry 19 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.20
        hwEntityPortType OBJECT-TYPE
            SYNTAX INTEGER
                {
                notSupported(1),
                copper(2),
                fiber100(3),
                fiber1000(4),
                fiber10000(5),
                opticalnotExist(6),
                optical(7),
                fiber25000(8),
                fiber50000(9),
                fiber100000(10),
                fiber200000(11),
                fiber400000(12),
                fiber40000(13),
                cellular(14),
                e1(15),
                serial(16)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the port type."
            ::= { hwEntityStateEntry 20 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.21
        hwEntityDuplex OBJECT-TYPE
            SYNTAX INTEGER
                {
                notSupported(1),
                full(2),
                half(3)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the duplex mode of a port."
            ::= { hwEntityStateEntry 21 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.22
        hwEntityOpticalPowerRx OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the receive power of an optical module."
            ::= { hwEntityStateEntry 22 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.23
        hwEntityCpuUsageLowThreshold OBJECT-TYPE
            SYNTAX Integer32 (0..100)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the CPU usage threshold of an entity."
            ::= { hwEntityStateEntry 23 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.24
        hwEntityBoardPower OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the board power."
            ::= { hwEntityStateEntry 24 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.25
        hwEntityCpuFrequency OBJECT-TYPE
            SYNTAX Integer32
            UNITS "Hz"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " The frequency of the entity. Unit: Hz"
            ::= { hwEntityStateEntry 25 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.26
        hwEntitySupportFlexCard OBJECT-TYPE
            SYNTAX INTEGER
                {
                notSupported(1),
                flexible(2),
                unflexible(3),
                dummy(4)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "It describes whether the whole board supports flexible cards."
            ::= { hwEntityStateEntry 26 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.27
        hwEntityBoardClass OBJECT-TYPE
            SYNTAX INTEGER
                {
                notSupported(1),
                mpu(2),
                lpu(3),
                sfu(4),
                icu(5),
                ecu(6),
                fan(7),
                power(8),
                lcd(9),
                pmu(10),
                cmu(11)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the board type."
            ::= { hwEntityStateEntry 27 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.28
        hwNseOpmStatus OBJECT-TYPE
            SYNTAX Integer32 (0..2)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "OPM status. 0: pass, 1: bypass, 2: invalid"
            ::= { hwEntityStateEntry 28 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.29
        hwEntityCpuMaxUsage OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the maximum CPU usage."
            ::= { hwEntityStateEntry 29 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.30
        hwEntityCPUType OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the CPU type."
            ::= { hwEntityStateEntry 30 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.31
        hwEntityMemoryType OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the memory type."
            ::= { hwEntityStateEntry 31 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.32
        hwEntityFlashSize OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the flash size of an entity."
            ::= { hwEntityStateEntry 32 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.33
        hwEntityIfUpTimes OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Times that the interface goes Up."
            ::= { hwEntityStateEntry 33 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.34
        hwEntityIfDownTimes OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Times that the interface goes Down."
            ::= { hwEntityStateEntry 34 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.35
        hwEntityCPUAvgUsage OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the average CPU usage."
            ::= { hwEntityStateEntry 35 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.36
        hwEntityMemoryAvgUsage OBJECT-TYPE
            SYNTAX Integer32 (0..100)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the average memory usage."
            ::= { hwEntityStateEntry 36 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.37
        hwEntityMemUsed OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the used memory size."
            ::= { hwEntityStateEntry 37 }

                    
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.38
        hwEntityTotalFanNum OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total numbers of the fans in the chassis ."
            ::= { hwEntityStateEntry 38 }
            
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.39
        hwEntityNomalFanNum OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The Nomal numbers of the fans in the chassis ."
            ::= { hwEntityStateEntry 39 }
            
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.40
        hwEntityTotalPwrNum OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The total numbers of the powers in the chassis ."
            ::= { hwEntityStateEntry 40 }
            
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.41
        hwEntityNomalPwrNum OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The nomal numbers of the powers in the chassis ."
            ::= { hwEntityStateEntry 41 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.42
        hwEntityFaultLight OBJECT-TYPE
            SYNTAX INTEGER
            {
                notSupported(1),
                normal(2),
                underRepair(3)
            }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The repair status for this entity.
                On the underrepair condition, there is a blue light on the entity."
            ::= { hwEntityStateEntry 42 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.43
        hwEntityBoardName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The board name for this entity."
            ::= { hwEntityStateEntry 43 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.44
        hwEntityBoardDescription OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The board description for this entity."
            ::= { hwEntityStateEntry 44 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.45
        hwEntity5MinCpuUsage OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Average CPU usage of the last five minutes for this entity."
            ::= { hwEntityStateEntry 45 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.46
        hwEntityStartMode OBJECT-TYPE
            SYNTAX INTEGER
            {
                notSupported(1),
                cold(2),
                warm(3),
                unknown(4)
            }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the board startup mode."
            ::= { hwEntityStateEntry 46 } 

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.47
        hwEntitySplitAttribute OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Number of the split port."
            ::= { hwEntityStateEntry 47 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.48
        hwEntityFaultLightKeepTime OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "Fault light twinkle keep time,the default is 45 seconds."
            ::= { hwEntityStateEntry 48 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.49
        hwEntityPbufUsage OBJECT-TYPE
          SYNTAX Integer32 (0..100)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " The Pbuf usage for this entity.  "
            ::= { hwEntityStateEntry 49 }		

       -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.50
       hwEntityTMUsage OBJECT-TYPE
          SYNTAX Integer32 (0..100)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " The TM usage for this entity.  "
           ::= { hwEntityStateEntry 50 }
		   
	   -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.51
       hwEntityHda1Usage OBJECT-TYPE
          SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " The Hda1 usage for this entity.  "
           ::= { hwEntityStateEntry 51 }
		   
	   -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.52
       hwEntityHda1UsageThreshold OBJECT-TYPE
          SYNTAX Integer32 (0..100)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " The hda1 usage Threshold for this entity.  "
           ::= { hwEntityStateEntry 52 }
		   
	   -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.53
       hwEntityHda1UsageResumeThreshold OBJECT-TYPE
          SYNTAX Integer32 (0..100)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " The hda1 usage resume threshold for this entity.  "
           ::= { hwEntityStateEntry 53 }		   	   
	
	   -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.54
       hwEntitySlotID OBJECT-TYPE
          SYNTAX Integer32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                " The identification of slot. "
           ::= { hwEntityStateEntry 54 }	
	
	   -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.55
       hwEntityCpuID OBJECT-TYPE
          SYNTAX Integer32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                " The identification of cpu. "
           ::= { hwEntityStateEntry 55 }
	
	   -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.56
       hwEntityPreviousValue OBJECT-TYPE
          SYNTAX Integer32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                " The previous value of the sudden change. "
           ::= { hwEntityStateEntry 56 }
	
	   -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.57
       hwEntityCurrentValue OBJECT-TYPE
          SYNTAX Integer32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                " The current value of the sudden change. "
           ::= { hwEntityStateEntry 57 }

	   -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.58
       hwEntityChangeValue OBJECT-TYPE
          SYNTAX Integer32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                " The change of the sudden change. "
           ::= { hwEntityStateEntry 58 }		   
		   
	   -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.59
       hwEntityChangeValueThreshold OBJECT-TYPE
          SYNTAX Integer32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                " The change threshold. "
           ::= { hwEntityStateEntry 59 }	
           
       -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.60
       hwEntityModelName OBJECT-TYPE
          SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The model for this entity. If there is no model string in elable of this entity or this entity does not support elabel, the invalid value(zero-string) will be returned."
           ::= { hwEntityStateEntry 60 }
           
       -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.61
       hwEntityIssueNumber OBJECT-TYPE
          SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The IssueNumber for this entity. If there is no IssueNumber string in elable of this entity or this entity does not support elabel, the invalid value(zero-string) will be returned."
           ::= { hwEntityStateEntry 61 }
  
       -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.62
       hwEntityDeviceStatus OBJECT-TYPE
          SYNTAX INTEGER
              {
              notSupported(0),
              normal(1),
              abnormal(2)
              }
          MAX-ACCESS read-only
          STATUS current
          DESCRIPTION
              "This object indicates the state of the device."
         ::= { hwEntityStateEntry 62 }
		
       -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.63
       hwEntityPicStatus OBJECT-TYPE
          SYNTAX INTEGER
              {
              notSupported(0),
              registered(1),
              online(2),
              unregistered(3),
              failed(4)
              }
          MAX-ACCESS read-only
          STATUS current
          DESCRIPTION
              "This object indicates the state of the pic."
         ::= { hwEntityStateEntry 63 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.64
        hwEntityMPUType OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
              "This object indicates the MPU type."
            ::= { hwEntityStateEntry 64 }
	    
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.65
        hwEntityMemSizeExt OBJECT-TYPE
            SYNTAX Unsigned32
            UNITS "KByte"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the memory size."
            ::= { hwEntityStateEntry 65 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.66
        hwEntityTemperatureMinorThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The minor threshold of the temperature. If the device temperature is 
                higher than the threshold, a notification is sent.
                "
            ::= { hwEntityStateEntry 66 }
        
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.67
        hwEntityVoltageFatalHighThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                " The fatal high threshold of the voltage. Generally, the voltage should 
                be greater than the fatal low threshold and lower than the fatal high threshold. 
                If the voltage is greater than the fatal high threshold, a notification is sent. "
            ::= { hwEntityStateEntry 67 }
        
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.68
        hwEntityVoltageFatalLowThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                " The fatal low threshold of the voltage. Generally, the voltage should 
                be greater than the fatal low threshold and lower than the fatal high threshold. 
                If the voltage is lower than the fatal low threshold, a notification is sent. "
            ::= { hwEntityStateEntry 68 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.69
        hwEntityMemCacheUsage OBJECT-TYPE
            SYNTAX Integer32 (0..100)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " This object indicates the memory cache usage of an entity, that is, the percentage of the memory cache that has been used."
            ::= { hwEntityStateEntry 69}	

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.70
        hwCpuUsageTrapType OBJECT-TYPE
            SYNTAX Integer32 (0..2)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " This object indicates the forwarding type of an entity."
            ::= { hwEntityStateEntry 70}	

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.71
        hwCpuUsageTrapSlot OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " This object indicates the slot id of an entity."
            ::= { hwEntityStateEntry 71}	

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.72
        hwCpuUsageTrapCpu OBJECT-TYPE
            SYNTAX Integer32 (0..100)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " This object indicates the CPU id of an entity."
            ::= { hwEntityStateEntry 72}	

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.73
        hwCpuUsageCurrentUsage OBJECT-TYPE
            SYNTAX Integer32 (0..100)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " This object indicates the cpu usage of an entity, that is, the percentage of the cpu resource that has been used."
            ::= { hwEntityStateEntry 73}		   
		
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.1.1.74
        hwCpuUsageThreashold OBJECT-TYPE
            SYNTAX Integer32 (0..100)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " This object indicates the cpu usage threshold of an entity."
            ::= { hwEntityStateEntry 74}	

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.2
        hwRUModuleInfoTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwRUModuleInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table describes production information, including the BOM ID, BOM, local description, manufacturing code, and update log. The MIB information is stored in the EEPROM of the physical entity."
            ::= { hwEntityState 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.2.1
        hwRUModuleInfoEntry OBJECT-TYPE
            SYNTAX HwRUModuleInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Information about a replaceable unit physical entity.
                Each entry provides objects of a replaceable unit to help 
                an NMS identify and characterize the entry in this table.
                "
            INDEX { entPhysicalIndex }
            ::= { hwRUModuleInfoTable 1 }


        HwRUModuleInfoEntry ::=
            SEQUENCE { 
                hwEntityBomId
                    SnmpAdminString,
                hwEntityBomEnDesc
                    SnmpAdminString,
                hwEntityBomLocalDesc
                    SnmpAdminString,
                hwEntityManufacturedDate
                    DateAndTime,
                hwEntityManufactureCode
                    Integer32,
                hwEntityCLEICode
                    SnmpAdminString,
                hwEntityUpdateLog
                    SnmpAdminString,
                hwEntityArchivesInfoVersion
                    SnmpAdminString,
                hwEntityOpenBomId
                    SnmpAdminString,
                hwEntityIssueNum
                    SnmpAdminString,
                hwEntityBoardType
                    SnmpAdminString,
                hwEntityExInfo
                    SnmpAdminString,
                hwEntityModel
                    SnmpAdminString,
                hwEntityElabelVersion
                    SnmpAdminString,
				hwEntitySafeId
                    SnmpAdminString
             }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.2.1.1
        hwEntityBomId OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the entity BOM ID, which is a unified material identifier."
            ::= { hwRUModuleInfoEntry 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.2.1.2
        hwEntityBomEnDesc OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the English description of the entity BOM."
            ::= { hwRUModuleInfoEntry 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.2.1.3
        hwEntityBomLocalDesc OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS obsolete
            DESCRIPTION
                "This object indicates the local description of the entity BOM."
            ::= { hwRUModuleInfoEntry 3 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.2.1.4
        hwEntityManufacturedDate OBJECT-TYPE
            SYNTAX DateAndTime
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the manufacturing date of an entity."
            ::= { hwRUModuleInfoEntry 4 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.2.1.5
        hwEntityManufactureCode OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS obsolete
            DESCRIPTION
                "The code of the place where this physical entity is Manufactured.
                "
            ::= { hwRUModuleInfoEntry 5 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.2.1.6
        hwEntityCLEICode OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the CLEI code of an entity."
            ::= { hwRUModuleInfoEntry 6 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.2.1.7
        hwEntityUpdateLog OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS obsolete
            DESCRIPTION
                "The maintenance log of this replaceable unit.
                "
            ::= { hwRUModuleInfoEntry 7 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.2.1.8
        hwEntityArchivesInfoVersion OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the archive information version of an entity."
            ::= { hwRUModuleInfoEntry 8 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.2.1.9
        hwEntityOpenBomId OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the sales BOM code."
            ::= { hwRUModuleInfoEntry 9 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.2.1.10
        hwEntityIssueNum OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the release code."
            ::= { hwRUModuleInfoEntry 10 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.2.1.11
        hwEntityBoardType OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the entity board type."
            ::= { hwRUModuleInfoEntry 11 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.2.1.12
        hwEntityExInfo OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Extra information, which satisfies the requirements of special components."
            ::= { hwRUModuleInfoEntry 12 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.2.1.13
        hwEntityModel OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "External type."
            ::= { hwRUModuleInfoEntry 13 }
			
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.2.1.14
        hwEntityElabelVersion OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Electronic label version."
            ::= { hwRUModuleInfoEntry 14 }
			
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.2.1.15
        hwEntitySafeId OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Main board safecard ID."
            ::= { hwRUModuleInfoEntry 15 }	

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3
        hwOpticalModuleInfoTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwOpticalModuleInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table describes optical module information, 
                including the fiber type, wavelength, transmission distance, 
                vendor information, temperature, bias current, receive optical power, 
                transmit optical power, optical module type, rate, fiber interface, 
                lower threshold of the receive power, upper threshold of the receive power, 
                lower threshold of the transmit power, upper threshold of the transmit power, 
                and whether the optical module is pluggable."
            ::= { hwEntityState 3 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1
        hwOpticalModuleInfoEntry OBJECT-TYPE
            SYNTAX HwOpticalModuleInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "An entry in the table of optical module properties for each optical module."
            INDEX { entPhysicalIndex }
            ::= { hwOpticalModuleInfoTable 1 }


        HwOpticalModuleInfoEntry ::=
            SEQUENCE { 
                hwEntityOpticalMode
                    INTEGER,
                hwEntityOpticalWaveLength
                    Integer32,
                hwEntityOpticalTransDistance
                    Integer32,
                hwEntityOpticalVendorSn
                    SnmpAdminString,
                hwEntityOpticalTemperature
                    Integer32,
                hwEntityOpticalVoltage
                    Integer32,
                hwEntityOpticalBiasCurrent
                    Integer32,
                hwEntityOpticalRxPower
                    Integer32,
                hwEntityOpticalTxPower
                    Integer32,
                hwEntityOpticalType
                    INTEGER,
                hwEntityOpticalTransBW
                    Integer32,
                hwEntityOpticalFiberType
                    INTEGER,
                hwEntityOpticalRxLowThreshold
                    Integer32,
                hwEntityOpticalRxHighThreshold
                    Integer32,
                hwEntityOpticalTxLowThreshold
                    Integer32,
                hwEntityOpticalTxHighThreshold
                    Integer32,
                hwEntityOpticalPlug
                    INTEGER,
                hwEntityOpticalDirectionType
                    INTEGER,
                hwEntityOpticalUserEeprom
                    DisplayString,
                hwEntityOpticalRxLowWarnThreshold
                    Integer32,
                hwEntityOpticalRxHighWarnThreshold
                    Integer32,
                hwEntityOpticalTxLowWarnThreshold
                    Integer32,
                hwEntityOpticalTxHighWarnThreshold
                    Integer32,
                hwEntityOpticalVenderName
                    DisplayString,
                hwEntityOpticalVenderPn
                    DisplayString,
                hwEntityOpticalAuthenticationStatus
                   INTEGER,
                hwEntityOpticalTunableType
                   INTEGER,
                hwEntityOpticalWaveLengthDecimal
                   Integer32,
               hwEntityOpticalTunableModuleChannel
                   Integer32,
               hwEntityOpticalWaveBand
                   INTEGER,
               hwEntityOpticalLaneBiasCurrent
                   SnmpAdminString,
               hwEntityOpticalLaneRxPower
                   SnmpAdminString,
               hwEntityOpticalLaneTxPower
                   SnmpAdminString,
               hwEntityOpticalVendorOUI
                    DisplayString,
               hwEntityOpticalVendorRev                    
                    DisplayString,    
               hwEntityOpticalGponSN
                    DisplayString,
              hwEntityTransceiverType
                    DisplayString,
               hwEntityOpticalMaxRxPower
                    Integer32,
               hwEntityOpticalMinRxPower
                    Integer32,
               hwEntityOpticalMaxTxPower
                    Integer32,
               hwEntityOpticalMinTxPower
                    Integer32,
	           hwEntityOpticalTransType
                    SnmpAdminString,
               hwEntityOpticalConnectType
                    SnmpAdminString,
               hwEntityOpticalOrderingName
                    SnmpAdminString,
               hwEntityOpticalTransferDistance
                    SnmpAdminString,
                hwEntityOpticalBandWidth
                    Integer32,
                hwEntityOpticalWaveLengthExact
                    DisplayString,
                hwEntityOpticalModel
                    SnmpAdminString,
		       hwEntityOpticalManufacturedDate 
                    DateAndTime,
                hwEntityOpticalTempLowThreshold 
                    Integer32,
                hwEntityOpticalTempHighThreshold 
                    Integer32,
                hwEntityOpticalVoltLowThreshold 
                    Integer32,
                hwEntityOpticalVoltHighThreshold 
                    Integer32,
                hwEntityOpticalBiasLowThreshold 
                    Integer32,
                hwEntityOpticalBiasHighThreshold 
                    Integer32,
                hwEntityOpticalHuaweiCertified
	Integer32,
                hwEntityOpticalSupportDDM
	INTEGER,
                hwEntityOpticalPortName
                    DisplayString,
	         hwEntityOpticalDifferentialGroupDelay
                    Unsigned32,
                hwEntityOpticalChromaticDispersion
                    Integer32
     }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.1
        hwEntityOpticalMode OBJECT-TYPE
            SYNTAX INTEGER
                {
                notSupported(1),
                singleMode(2),
                multiMode5(3),
                multiMode6(4),
                noValue(5),
                gpsMode(6),
                copperMode(7),
                singleAndmultiMode(8)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the fiber type."
            DEFVAL { notSupported }
            ::= { hwOpticalModuleInfoEntry 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.2
        hwEntityOpticalWaveLength OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the wavelength of an optical module. Unit: nm"
            ::= { hwOpticalModuleInfoEntry 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.3
        hwEntityOpticalTransDistance OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the transmission distance of an optical module."
            ::= { hwOpticalModuleInfoEntry 3 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.4
        hwEntityOpticalVendorSn OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the vendor information of an optical module."
            ::= { hwOpticalModuleInfoEntry 4 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.5
        hwEntityOpticalTemperature OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the temperature of an optical module. 2147483647 is an invalid value. Unit: C."
            ::= { hwOpticalModuleInfoEntry 5 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.6
        hwEntityOpticalVoltage OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the voltage of an optical module. 2147483647 is an invalid value. Unit: mV."
            ::= { hwOpticalModuleInfoEntry 6 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.7
        hwEntityOpticalBiasCurrent OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the bias current of an optical module. 2147483647 is an invalid value. Unit: uA"
            ::= { hwOpticalModuleInfoEntry 7 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.8
        hwEntityOpticalRxPower OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the receive optical power of an optical module. Unit: dBm. the value is expanded 100 times, so the real value should be reduced 100 times."
            ::= { hwOpticalModuleInfoEntry 8 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.9
        hwEntityOpticalTxPower OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the transmit optical power of an optical module. Unit: dBm. the value is expanded 100 times, so the real value should be reduced 100 times."
            ::= { hwOpticalModuleInfoEntry 9 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.10
        hwEntityOpticalType OBJECT-TYPE
            SYNTAX INTEGER
                {
                unknown(0),
                sc(1),
                gbic(2),
                sfp(3),
                esfp(4),
                rj45(5),
                xfp(6),
                xenpak(7),
                transponder(8),
                cfp(9),
                smb(10),
                sfpplus(11),
                cxp(12),
                qsfp(13),
                qsfpplus(14),
                cfp2(15),
                dwdmsfp(16),
                msa100glh(17),
                gps(18),
                csfp(19),
                cfp4(20),
                qsfp28(21),
                sfpsfpplus(22),
                gponsfp(23),
                cfp8(24),
                sfp28(25),
                qsfpdd(26),
                cfp2dco(27),
                sfp56(28),
                qsfp56(29),
                oa(30),
                micro(31)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the optical module type."
            ::= { hwOpticalModuleInfoEntry 10 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.11
        hwEntityOpticalTransBW OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the transmission bandwidth of an optical module."
            ::= { hwOpticalModuleInfoEntry 11 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.12
        hwEntityOpticalFiberType OBJECT-TYPE
            SYNTAX INTEGER
                {
                unknown(0),
                sc(1),
                style1CopperConnector(2),
                style2CopperConnector(3),
                bncTnc(4),
                coaxialHeaders(5),
                fiberJack(6),
                lc(7),
                mtRj(8),
                mu(9),
                sg(10),
                opticalPigtail(11),
                mpo(12),
                mpo1x12(13),
                mpo2x16(14),
                rj45(15),
                noSeparable(16),
                mxc2x16(17),
                csOptical(18),
                snOptical(19),
                hssdcII(20),
                copperPigtail(21),
                mpo2x12(22),
                mpo1x16(23),
                angledLc(24)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the fiber type."
            ::= { hwOpticalModuleInfoEntry 12 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.13
        hwEntityOpticalRxLowThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the lower threshold of the receive power of an optical module. Unit: dBm. the value is expanded 100 times, so the real value should be reduced 100 times."
            ::= { hwOpticalModuleInfoEntry 13 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.14
        hwEntityOpticalRxHighThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the upper threshold of the receive power of an optical module. Unit: dBm. the value is expanded 100 times, so the real value should be reduced 100 times."
            ::= { hwOpticalModuleInfoEntry 14 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.15
        hwEntityOpticalTxLowThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the lower threshold of the transmit power of an optical module. Unit: dBm. the value is expanded 100 times, so the real value should be reduced 100 times."
            ::= { hwOpticalModuleInfoEntry 15 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.16
        hwEntityOpticalTxHighThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the upper threshold of the transmit power of an optical module. Unit: dBm. the value is expanded 100 times, so the real value should be reduced 100 times."
            ::= { hwOpticalModuleInfoEntry 16 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.17
        hwEntityOpticalPlug OBJECT-TYPE
            SYNTAX INTEGER
                {
                notSupported(0),
                true(1),
                false(2)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates whether an optical module is pluggable."
            ::= { hwOpticalModuleInfoEntry 17 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.18
        hwEntityOpticalDirectionType OBJECT-TYPE
            SYNTAX INTEGER
                {
                notSupported(1),
                twoFiberBidirection(2),
                oneFiberBidirection(3),
                twoFiberTwoPortBidirection(4)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the direction type of an optical module."
            ::= { hwOpticalModuleInfoEntry 18 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.19
        hwEntityOpticalUserEeprom OBJECT-TYPE
            SYNTAX DisplayString (SIZE (0..120))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the EEPROM of an optical module."
            ::= { hwOpticalModuleInfoEntry 19 }
        
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.20
        hwEntityOpticalRxLowWarnThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the lower warning threshold for the optical power of an optical module in the receive direction."
            ::= { hwOpticalModuleInfoEntry 20 }

        
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.21
        hwEntityOpticalRxHighWarnThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the upper warning threshold for the optical power of an optical module in the receive direction."
            ::= { hwOpticalModuleInfoEntry 21 }

        
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.22
        hwEntityOpticalTxLowWarnThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the lower warning threshold for the optical power of an optical module in the transmit direction."
            ::= { hwOpticalModuleInfoEntry 22 }

        
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.23
        hwEntityOpticalTxHighWarnThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the upper warning threshold for the optical power of an optical module in the transmit direction."
            ::= { hwOpticalModuleInfoEntry 23 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.24
        hwEntityOpticalVenderName OBJECT-TYPE
            SYNTAX DisplayString (SIZE (0..120))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the vendor name of an optical module."
            ::= { hwOpticalModuleInfoEntry 24 }
            
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.25
        hwEntityOpticalVenderPn OBJECT-TYPE
            SYNTAX DisplayString (SIZE (0..120))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the PN of an optical module."
            ::= { hwOpticalModuleInfoEntry 25 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.26
        hwEntityOpticalAuthenticationStatus OBJECT-TYPE
            SYNTAX INTEGER
                {
                unknown(0),
                authenticated(1),
                unauthenticated(2)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The authentication status of optical module."
            ::= { hwOpticalModuleInfoEntry 26 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.27
        hwEntityOpticalTunableType OBJECT-TYPE
            SYNTAX INTEGER
                {
                notSupported(1),
                notTunable(2), 
                tunable(3),
                supportTunableType(4)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The tunable type of the optical module."
            ::= { hwOpticalModuleInfoEntry 27 }

       
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.28
        hwEntityOpticalWaveLengthDecimal OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the wavelength of an optical module."
            ::= { hwOpticalModuleInfoEntry 28 }
    
       -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.29
        hwEntityOpticalTunableModuleChannel OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The current configuration of tunable optical module channel."
            ::= { hwOpticalModuleInfoEntry 29 }
            
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.30
        hwEntityOpticalWaveBand OBJECT-TYPE
            SYNTAX INTEGER
                {
                unknown(0),
                clBand(1),
                cBand(2),
                lBand(3),
                c32Band(4),
                ramancBand(5),
                ramanlBand(6),
                cwdmBand(7),
                smcBand(8),
                c96bBand(9),
                c192bBand(10)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The wave band of the optical module."
            ::= { hwOpticalModuleInfoEntry 30 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.31
        hwEntityOpticalLaneBiasCurrent OBJECT-TYPE
            SYNTAX SnmpAdminString (SIZE (0..255))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The bias current of the QSFP or CFP optical module. Unit: mA.(e.g.,
 	37.88,39.15,39.84,37.82)"
            ::= { hwOpticalModuleInfoEntry 31 }
			
			
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.32
        hwEntityOpticalLaneRxPower OBJECT-TYPE
            SYNTAX SnmpAdminString (SIZE (0..255))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the receive power of a QSFP or CFP optical module. Unit: dBm"
            ::= { hwOpticalModuleInfoEntry 32 }
			
			
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.33
        hwEntityOpticalLaneTxPower OBJECT-TYPE
            SYNTAX SnmpAdminString (SIZE (0..255))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the transmission power of a QSFP or CFP optical module. Unit: dBm"
            ::= { hwOpticalModuleInfoEntry 33 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.34
        hwEntityOpticalVendorOUI OBJECT-TYPE
            SYNTAX DisplayString (SIZE (0..8))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Vendor ID of the optical module assigned by IEEE."
            ::= { hwOpticalModuleInfoEntry 34 } 
            
       -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.35
        hwEntityOpticalVendorRev OBJECT-TYPE
            SYNTAX DisplayString (SIZE (0..8))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The Vender Version of the optical module."
            ::= { hwOpticalModuleInfoEntry 35 } 
            
       -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.36
        hwEntityOpticalGponSN OBJECT-TYPE
            SYNTAX DisplayString (SIZE (0..20))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The SN of the optical module provided by the vendor."
            ::= { hwOpticalModuleInfoEntry 36 }

       -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.37
        hwEntityTransceiverType OBJECT-TYPE
            SYNTAX DisplayString (SIZE (0..80))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The transceiver type of the optical module provided by the vendor."
            ::= { hwOpticalModuleInfoEntry 37 }
            
       -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.38
        hwEntityOpticalMaxRxPower OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The maximum receive power of the optical module. Unit: dBm. the value is expanded 100 times,so the real value should be reduced 100 times."
            ::= { hwOpticalModuleInfoEntry 38 }
            
       -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.39
        hwEntityOpticalMinRxPower OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The minimum receive power of the optical module. Unit: dBm. the value is expanded 100 times,so the real value should be reduced 100 times."
            ::= { hwOpticalModuleInfoEntry 39 }
            
       -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.40
        hwEntityOpticalMaxTxPower OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The maximum transmit power of the optical module. Unit: dBm. the value is expanded 100 times,so the real value should be reduced 100 times."
            ::= { hwOpticalModuleInfoEntry 40 }
            
       -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.41
        hwEntityOpticalMinTxPower OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The minimum transmit power of the optical module. Unit: dBm. the value is expanded 100 times,so the real value should be reduced 100 times."
            ::= { hwOpticalModuleInfoEntry 41 }
			
	   -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.42
        hwEntityOpticalTransType OBJECT-TYPE
            SYNTAX SnmpAdminString (SIZE (0..50))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The Transceiver Type of the optical module."
            ::= { hwOpticalModuleInfoEntry 42 }
		
       -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.43
        hwEntityOpticalConnectType OBJECT-TYPE
            SYNTAX SnmpAdminString (SIZE (0..50))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The Connector Type of the optical module."
            ::= { hwOpticalModuleInfoEntry 43 }		
			
	   -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.44
        hwEntityOpticalOrderingName OBJECT-TYPE
            SYNTAX SnmpAdminString (SIZE (0..50))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The Ordering Name of the optical module."
            ::= { hwOpticalModuleInfoEntry 44 }	
	    
	    -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.45
        hwEntityOpticalTransferDistance OBJECT-TYPE
            SYNTAX SnmpAdminString (SIZE (0..100))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The Transfer Distance of the optical module."
            ::= { hwOpticalModuleInfoEntry 45 }	
			
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.46
        hwEntityOpticalBandWidth OBJECT-TYPE
            SYNTAX Integer32 (0..400000)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Maximum bandwidth for an optical module, in Mbps. The value is 0 if the optical module is not present."
            ::= { hwOpticalModuleInfoEntry 46 }
	    
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.47
        hwEntityOpticalWaveLengthExact OBJECT-TYPE
            SYNTAX DisplayString (SIZE (0..64))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The wave length of the optical module. Unit: nm."
            ::= { hwOpticalModuleInfoEntry 47 }
			
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.48
        hwEntityOpticalModel OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The model of the optical module."
            ::= { hwOpticalModuleInfoEntry 48 }	
	    
	-- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.49
        hwEntityOpticalManufacturedDate OBJECT-TYPE
            SYNTAX DateAndTime
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The Manufactured Date of the optical module."
            ::= { hwOpticalModuleInfoEntry 49 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.50
        hwEntityOpticalTempLowThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The temperature low threshold of the optical module. Unit: C."
            ::= { hwOpticalModuleInfoEntry 50 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.51
        hwEntityOpticalTempHighThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The temperature high threshold of the optical module. Unit: C."
            ::= { hwOpticalModuleInfoEntry 51 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.52
        hwEntityOpticalVoltLowThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The voltage low threshold of the optical module. Unit: mV."
            ::= { hwOpticalModuleInfoEntry 52 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.53
        hwEntityOpticalVoltHighThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The voltage high threshold of the optical module. Unit: mV."
            ::= { hwOpticalModuleInfoEntry 53 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.54
        hwEntityOpticalBiasLowThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The Bias Low Threshold of the optical module. Unit: uA."
            ::= { hwOpticalModuleInfoEntry 54 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.55
        hwEntityOpticalBiasHighThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The Bias High Threshold of the optical module. Unit: uA."
            ::= { hwOpticalModuleInfoEntry 55 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.56
        hwEntityOpticalHuaweiCertified OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The Huawei Certification of the optical module. 0 represents yes and 1 represents no.
                 After disabling non-Huawei-certified alarm. This node can not get information about non-Huawei-certified optical module."
            ::= { hwOpticalModuleInfoEntry 56 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.57
        hwEntityOpticalSupportDDM OBJECT-TYPE
            SYNTAX INTEGER
                 {
                     support(0),
                     notSupport(1)
                 }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Judge Optical Support DDM or not."
            ::= { hwOpticalModuleInfoEntry 57 }			

		-- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.58
        hwEntityOpticalPortName OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The ShowName of the port."
            ::= { hwOpticalModuleInfoEntry 58 }

		-- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.59
        hwEntityOpticalDifferentialGroupDelay OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the optical module differential group delay. Unit: ps."
            ::= { hwOpticalModuleInfoEntry 59 }

		-- 1.3.6.1.4.1.2011.5.25.31.1.1.3.1.60
        hwEntityOpticalChromaticDispersion OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Indicates the optical module chromatic dispersion. Unit: ps/nm."
            ::= { hwOpticalModuleInfoEntry 60 }
			
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.4
        hwMonitorInputTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwMonitorInputEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table contains one row per replaceable unit physical entity.
                This table is used to set the status of monitor port."
            ::= { hwEntityState 4 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.4.1
        hwMonitorInputEntry OBJECT-TYPE
            SYNTAX HwMonitorInputEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This is a replaceable unit physical entity."
            INDEX { hwMonitorInputIndex }
            ::= { hwMonitorInputTable 1 }


        HwMonitorInputEntry ::=
            SEQUENCE { 
                hwMonitorInputIndex
                    Integer32,
                hwMonitorInputName
                    DisplayString,
                hwMonitorInputState
                    HWLevelState,
                hwMonitorInputStateEnable
                    EnabledStatus,
                hwMonitorInputRowStatus
                    RowStatus
             }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.4.1.1
        hwMonitorInputIndex OBJECT-TYPE
            SYNTAX Integer32 (1..4)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Monitor port index.
                This is a number of input line,ranging from 1 to 4.
                "
            ::= { hwMonitorInputEntry 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.4.1.2
        hwMonitorInputName OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Monitor line name.
                "
            ::= { hwMonitorInputEntry 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.4.1.3
        hwMonitorInputState OBJECT-TYPE
            SYNTAX HWLevelState
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Monitor line status.  
                The value is high or low.
                "
            ::= { hwMonitorInputEntry 3 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.4.1.4
        hwMonitorInputStateEnable OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Enable monitor line. 
                "
            ::= { hwMonitorInputEntry 4 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.4.1.5
        hwMonitorInputRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Status of monitor input row.
                "
            ::= { hwMonitorInputEntry 5 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.5
        hwMonitorOutputTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwMonitorOutputEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table contains one row per replaceable unit physical entity.
                This table is used to create a output view."
            ::= { hwEntityState 5 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.5.1
        hwMonitorOutputEntry OBJECT-TYPE
            SYNTAX HwMonitorOutputEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This is a replaceable unit physical entity."
            INDEX { hwMonitorOutputIndex, hwMonitorOutputRuleIndex }
            ::= { hwMonitorOutputTable 1 }


        HwMonitorOutputEntry ::=
            SEQUENCE { 
                hwMonitorOutputIndex
                    Integer32,
                hwMonitorOutputRuleIndex
                    Integer32,
                hwMonitorOutputMask
                    DisplayString,
                hwMonitorOutputKey
                    DisplayString,
                hwMonitorOutputRowStatus
                    RowStatus
             }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.5.1.1
        hwMonitorOutputIndex OBJECT-TYPE
            SYNTAX Integer32 (1..3)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Monitor output view index. 
                Through this index ,you can turn into the output view.
                "
            ::= { hwMonitorOutputEntry 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.5.1.2
        hwMonitorOutputRuleIndex OBJECT-TYPE
            SYNTAX Integer32 (1..16)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Monitor output rule index. 
                This is used to set the rules about all of the input line.
                "
            ::= { hwMonitorOutputEntry 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.5.1.3
        hwMonitorOutputMask OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Monitor output mask . 
                This is used to matching the level of monitor input line.
                "
            ::= { hwMonitorOutputEntry 3 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.5.1.4
        hwMonitorOutputKey OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Normal level value of this output line.
                "
            ::= { hwMonitorOutputEntry 4 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.5.1.5
        hwMonitorOutputRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "Status of monitor input row
                "
            ::= { hwMonitorOutputEntry 5 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.6
        hwEntPowerUsedInfoTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwEntPowerUsedInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "A table of information that displays the power use of entity ."
            ::= { hwEntityState 6 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.6.1
        hwEntPowerUsedInfoEntry OBJECT-TYPE
            SYNTAX HwEntPowerUsedInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Entry of the table of information that displays the power use of entity."
            INDEX { entPhysicalIndex }
            ::= { hwEntPowerUsedInfoTable 1 }


        HwEntPowerUsedInfoEntry ::=
            SEQUENCE { 
                hwEntPowerUsedInfoBoardName
                    OCTET STRING,
                hwEntPowerUsedInfoBoardType
                    OCTET STRING,
                hwEntPowerUsedInfoBoardSlot
                    Integer32,
                hwEntPowerUsedInfoPower
                    Integer32
             }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.6.1.1
        hwEntPowerUsedInfoBoardName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Board name."
            ::= { hwEntPowerUsedInfoEntry 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.6.1.2
        hwEntPowerUsedInfoBoardType OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Board type."
            ::= { hwEntPowerUsedInfoEntry 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.6.1.3
        hwEntPowerUsedInfoBoardSlot OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Board's slot number."
            ::= { hwEntPowerUsedInfoEntry 3 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.6.1.4
        hwEntPowerUsedInfoPower OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Used power of board."
            ::= { hwEntPowerUsedInfoEntry 4 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.7
        hwVirtualCableTestTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwVirtualCableTestEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table contains one row per replaceable unit physical entity.
                This table is used to display VCT result."
            ::= { hwEntityState 7 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.7.1
        hwVirtualCableTestEntry OBJECT-TYPE
            SYNTAX HwVirtualCableTestEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This is a replaceable unit physical entity."
            INDEX { hwVirtualCableTestIfIndex }
            ::= { hwVirtualCableTestTable 1 }


        HwVirtualCableTestEntry ::=
            SEQUENCE { 
                hwVirtualCableTestIfIndex
                    InterfaceIndex,
                hwVirtualCableTestPairStatus
                    INTEGER,
                hwVirtualCableTestPairLength
                    Integer32,
                hwVirtualCableTestOperation
                    INTEGER,
                hwVirtualCableTestLastTime
                    Integer32,
                hwVirtualCableTestPairAStatus
                    INTEGER,
                hwVirtualCableTestPairBStatus
                    INTEGER,
                hwVirtualCableTestPairCStatus
                    INTEGER,
                hwVirtualCableTestPairDStatus
                    INTEGER,
                hwVirtualCableTestPairALength
                    Integer32,
                hwVirtualCableTestPairBLength
                    Integer32,
                hwVirtualCableTestPairCLength
                    Integer32,
                hwVirtualCableTestPairDLength
                    Integer32
             }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.7.1.1
        hwVirtualCableTestIfIndex OBJECT-TYPE
            SYNTAX InterfaceIndex
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "IfIndex of port that you want to test cable."
            ::= { hwVirtualCableTestEntry 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.7.1.2
        hwVirtualCableTestPairStatus OBJECT-TYPE
            SYNTAX INTEGER
                {
                normal(1),
                abnormalOpen(2),
                abnormalShort(3),
                abnormalOpenShort(4),
                abnormalCrossTalk(5),
                unknown(6),
                notSupport(7)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Pair status. 
                This indicate the status of cable.
                "
            ::= { hwVirtualCableTestEntry 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.7.1.3
        hwVirtualCableTestPairLength OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Pair Length.
                This indicate the length of cable.
                "
            ::= { hwVirtualCableTestEntry 3 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.7.1.4
        hwVirtualCableTestOperation OBJECT-TYPE
            SYNTAX INTEGER
                {
                startTest(1),
                resetTestValue(2),
                readyStartTest(3)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "VirtualCableTestOperation. 
                This Operation of VirtualCableTest."
            ::= { hwVirtualCableTestEntry 4 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.7.1.5
        hwVirtualCableTestLastTime OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The last test time for the entity. The mean of last time is 
                when the entity is tested, and the value of the object 
                will add one per seconds until now."
            ::= { hwVirtualCableTestEntry 5 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.7.1.6
        hwVirtualCableTestPairAStatus OBJECT-TYPE
            SYNTAX INTEGER
                {
                normal(1),
                abnormalOpen(2),     
                abnormalShort(3),
                abnormalOpenShort(4),    
                abnormalCrossTalk(5),
                unknown(6),
                notSupport(7)
            }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Pair A status. 
                 This indicate the status of cable.
                 "
            ::= { hwVirtualCableTestEntry 6 }



        -- 1.3.6.1.4.1.2011.5.25.31.1.1.7.1.7
        hwVirtualCableTestPairBStatus OBJECT-TYPE
            SYNTAX INTEGER
            {
                normal(1),
                abnormalOpen(2),
                abnormalShort(3),
                abnormalOpenShort(4),
                abnormalCrossTalk(5),
                unknown(6),
                notSupport(7)
            }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Pair B status. 
                 This indicate the status of cable.
                 "
            ::= { hwVirtualCableTestEntry 7 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.7.1.8
        hwVirtualCableTestPairCStatus OBJECT-TYPE
            SYNTAX INTEGER
                {
                normal(1),
                abnormalOpen(2),     
                abnormalShort(3),
                abnormalOpenShort(4),    
                abnormalCrossTalk(5),
                unknown(6),
                notSupport(7)
            }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Pair C status. 
                 This indicate the status of cable.
                 "
            ::= { hwVirtualCableTestEntry 8 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.7.1.9
        hwVirtualCableTestPairDStatus OBJECT-TYPE
            SYNTAX INTEGER
                {
                normal(1),
                abnormalOpen(2),     
                abnormalShort(3),
                abnormalOpenShort(4),    
                abnormalCrossTalk(5),
                unknown(6),
                notSupport(7)
            }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Pair D status. 
                 This indicate the status of cable.
                 "
            ::= { hwVirtualCableTestEntry 9 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.7.1.10 
        hwVirtualCableTestPairALength OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Pair A Length.
                 This indicate the length of cable.
                "
            ::= { hwVirtualCableTestEntry 10 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.7.1.11
        hwVirtualCableTestPairBLength OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Pair B Length.
                 This indicate the length of cable.
                "
            ::= { hwVirtualCableTestEntry 11 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.7.1.12
        hwVirtualCableTestPairCLength OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Pair C Length.
                 This indicate the length of cable.
                "
            ::= { hwVirtualCableTestEntry 12 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.7.1.13
        hwVirtualCableTestPairDLength OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Pair D Length.
                 This indicate the length of cable.
                "
            ::= { hwVirtualCableTestEntry 13 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.8
        hwTemperatureThresholdTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwTemperatureThresholdEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table describes Huawei device temperature objects."
            ::= { hwEntityState 8 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.8.1
        hwTemperatureThresholdEntry OBJECT-TYPE
            SYNTAX HwTemperatureThresholdEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Defines an entry in the hwTemperatureThresholdTable."
            INDEX { hwEntityTempSlotId, hwEntityTempI2CId, hwEntityTempAddr, hwEntityTempChannel }
            ::= { hwTemperatureThresholdTable 1 }


        HwTemperatureThresholdEntry ::=
            SEQUENCE { 
                hwEntityTempSlotId
                    Integer32,
                hwEntityTempI2CId
                    Integer32,
                hwEntityTempAddr
                    Integer32,
                hwEntityTempChannel
                    Integer32,
                hwEntityTempStatus
                    INTEGER,
                hwEntityTempValue
                    Integer32,
                hwEntityTempMinorAlmThreshold
                    Integer32,
                hwEntityTempMajorAlmThreshold
                    Integer32,
                hwEntityTempFatalAlmThreshold
                    Integer32
             }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.8.1.1
        hwEntityTempSlotId OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the entity slot."
            ::= { hwTemperatureThresholdEntry 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.8.1.2
        hwEntityTempI2CId OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the I2C of the entity temperature."
            ::= { hwTemperatureThresholdEntry 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.8.1.3
        hwEntityTempAddr OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the address of the entity temperature."
            ::= { hwTemperatureThresholdEntry 3 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.8.1.4
        hwEntityTempChannel OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the channel of the entity temperature."
            ::= { hwTemperatureThresholdEntry 4 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.8.1.5
        hwEntityTempStatus OBJECT-TYPE
            SYNTAX INTEGER
                {
                normal(1),
                minor(2),
                major(3),
                fatal(4)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the status of the entity temperature."
            ::= { hwTemperatureThresholdEntry 5 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.8.1.6
        hwEntityTempValue OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the current value of the entity temperature."
            ::= { hwTemperatureThresholdEntry 6 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.8.1.7
        hwEntityTempMinorAlmThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the minor alarm threshold of the entity temperature."
            ::= { hwTemperatureThresholdEntry 7 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.8.1.8
        hwEntityTempMajorAlmThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the major alarm threshold of the entity temperature."
            ::= { hwTemperatureThresholdEntry 8 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.8.1.9
        hwEntityTempFatalAlmThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the fatal alarm threshold of the entity temperature."
            ::= { hwTemperatureThresholdEntry 9 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.9
        hwVoltageInfoTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwVoltageInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table describes Huawei device voltage objects."
            ::= { hwEntityState 9 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.9.1
        hwVoltageInfoEntry OBJECT-TYPE
            SYNTAX HwVoltageInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Defines an entry in the hwVoltageInfoTable."
            INDEX { hwEntityVolSlot, hwEntityVolI2CId, hwEntityVolAddr, hwEntityVolChannel }
            ::= { hwVoltageInfoTable 1 }


        HwVoltageInfoEntry ::=
            SEQUENCE { 
                hwEntityVolSlot
                    Integer32,
                hwEntityVolI2CId
                    Integer32,
                hwEntityVolAddr
                    Integer32,
                hwEntityVolChannel
                    Integer32,
                hwEntityVolStatus
                    INTEGER,
                hwEntityVolRequired
                    Integer32,
                hwEntityVolCurValue
                    Integer32,
                hwEntityVolRatio
                    Integer32,
                hwEntityVolLowAlmMajor
                    Integer32,
                hwEntityVolLowAlmFatal
                    Integer32,
                hwEntityVolHighAlmMajor
                    Integer32,
                hwEntityVolHighAlmFatal
                    Integer32
             }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.9.1.1
        hwEntityVolSlot OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the slot ID of an entity."
            ::= { hwVoltageInfoEntry 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.9.1.2
        hwEntityVolI2CId OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the I2C of the entity voltage."
            ::= { hwVoltageInfoEntry 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.9.1.3
        hwEntityVolAddr OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the address of the entity voltage."
            ::= { hwVoltageInfoEntry 3 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.9.1.4
        hwEntityVolChannel OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the channel of the entity voltage."
            ::= { hwVoltageInfoEntry 4 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.9.1.5
        hwEntityVolStatus OBJECT-TYPE
            SYNTAX INTEGER
                {
                abnormal(0),
                normal(1),
                major(2),
                fatal(3)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the status of the entity voltage."
            ::= { hwVoltageInfoEntry 5 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.9.1.6
        hwEntityVolRequired OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the required value of the entity voltage."
            ::= { hwVoltageInfoEntry 6 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.9.1.7
        hwEntityVolCurValue OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the current value of the entity voltage."
            ::= { hwVoltageInfoEntry 7 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.9.1.8
        hwEntityVolRatio OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the voltage split ratio of the entity voltage."
            ::= { hwVoltageInfoEntry 8 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.9.1.9
        hwEntityVolLowAlmMajor OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the entity low-voltage alarm threshold."
            ::= { hwVoltageInfoEntry 9 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.9.1.10
        hwEntityVolLowAlmFatal OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the entity low-voltage fatal alarm threshold."
            ::= { hwVoltageInfoEntry 10 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.9.1.11
        hwEntityVolHighAlmMajor OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the entity high-voltage alarm threshold."
            ::= { hwVoltageInfoEntry 11 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.9.1.12
        hwEntityVolHighAlmFatal OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the entity high-voltage fatal alarm threshold."
            ::= { hwVoltageInfoEntry 12 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.10
        hwFanStatusTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwFanStatusEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table describes fan information on a device."
            ::= { hwEntityState 10 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.10.1
        hwFanStatusEntry OBJECT-TYPE
            SYNTAX HwFanStatusEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Defines an entry in the hwFanStatusTable."
            INDEX { hwEntityFanSlot, hwEntityFanSn }
            ::= { hwFanStatusTable 1 }


        HwFanStatusEntry ::=
            SEQUENCE { 
                hwEntityFanSlot
                    Integer32,
                hwEntityFanSn
                    Integer32,
                hwEntityFanReg
                    INTEGER,
                hwEntityFanSpdAdjMode
                    INTEGER,
                hwEntityFanSpeed
                    Integer32,
                hwEntityFanPresent
                    INTEGER,
                hwEntityFanState
                    INTEGER,
                hwEntityFanDesc
                    OCTET STRING,
                hwEntityFanName
                    INTEGER     
             }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.10.1.1
        hwEntityFanSlot OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the slot of a fan."
            ::= { hwFanStatusEntry 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.10.1.2
        hwEntityFanSn OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the number of the fan in the same slot."
            ::= { hwFanStatusEntry 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.10.1.3
        hwEntityFanReg OBJECT-TYPE
            SYNTAX INTEGER
                {
                yes(1),
                no(2)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the fan registration status."
            ::= { hwFanStatusEntry 3 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.10.1.4
        hwEntityFanSpdAdjMode OBJECT-TYPE
            SYNTAX INTEGER
                {
                auto(1),
                manual(2),
                unknown(3),
                silent(4),
                denoise(11)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the fan speed adjustment mode."
            ::= { hwFanStatusEntry 4 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.10.1.5
        hwEntityFanSpeed OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the fan speed."
            ::= { hwFanStatusEntry 5 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.10.1.6
        hwEntityFanPresent OBJECT-TYPE
            SYNTAX INTEGER 
                {
                present(1),
                absent(2)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the fan in-position status."
            ::= { hwFanStatusEntry 6 }  

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.10.1.7
        hwEntityFanState OBJECT-TYPE
            SYNTAX INTEGER 
            {
                normal(1),
                abnormal(2)
            }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the fan status."
            ::= { hwFanStatusEntry 7 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.10.1.8
        hwEntityFanDesc OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the description of the fan."
            ::= { hwFanStatusEntry 8 }
            
            -- 1.3.6.1.4.1.2011.5.25.31.1.1.10.1.9
			hwEntityFanName OBJECT-TYPE
            SYNTAX INTEGER 
            {
                fan023ab(1),
                fan031ab(2),
                fan031af(3),
                internalFan(4),
                none(5)
            }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the fan name."
            ::= { hwFanStatusEntry 9 }
			
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.11
        hwEntityGlobalPara OBJECT IDENTIFIER ::= { hwEntityState 11 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.11.1
        hwEntityServiceType OBJECT-TYPE
            SYNTAX INTEGER
                {
                sslvpn(1),
                firewall(2),
                loadBalance(3),
                ipsec(4),
                netstream(5),
                wlan(6)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " It describes the service-type of spu board ."
            ::= { hwEntityGlobalPara 1 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.11.2	
        hwDeviceServiceType OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " It describes the service-type of the device. bit0 is WLAN, bit1 is SSLVPN, bit2 is ipsec,other bits temporarily without easy back extension. Each bit 0 is disable, 1 is enable."
            ::= { hwEntityGlobalPara 2 }
            
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.11.3	
        hwEntityManufacturerOUI OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " It describes the Manufacturer of the device."
            ::= { hwEntityGlobalPara 3 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.12
        hwPortBip8StatisticsTable OBJECT-TYPE
            SYNTAX      SEQUENCE OF HwPortBip8StatisticsEntry
            MAX-ACCESS  not-accessible
            STATUS      current
            DESCRIPTION
                "This table describes port BIP8 statistics."
            ::= { hwEntityState 12 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.12.1
        hwPortBip8StatisticsEntry OBJECT-TYPE
            SYNTAX HwPortBip8StatisticsEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the BIP8 statistics.
                This table lists the various BIP8 statistics."
            INDEX  { entPhysicalIndex }    
            ::= { hwPortBip8StatisticsTable 1 }


        HwPortBip8StatisticsEntry  ::= 
            SEQUENCE{
                hwPhysicalPortBip8StatisticsEB                    Counter64,
                hwPhysicalPortBip8StatisticsES                    Counter64,
                hwPhysicalPortBip8StatisticsSES                   Counter64,
                hwPhysicalPortBip8StatisticsUAS                   Counter64,
                hwPhysicalPortBip8StatisticsBBE                   Counter64,
                hwPhysicalPortSpeed                               Unsigned32
                }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.12.1.1
        hwPhysicalPortBip8StatisticsEB OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
              "This object indicates the bit error block."
            ::= { hwPortBip8StatisticsEntry 1 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.12.1.2
        hwPhysicalPortBip8StatisticsES OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
              "This object indicates the errored second."
            ::= { hwPortBip8StatisticsEntry 2 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.12.1.3
        hwPhysicalPortBip8StatisticsSES OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
              "This object indicates the severely errored second."
            ::= { hwPortBip8StatisticsEntry 3 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.12.1.4
        hwPhysicalPortBip8StatisticsUAS OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
              "This object indicates the unavailable second."
            ::= { hwPortBip8StatisticsEntry 4 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.12.1.5
        hwPhysicalPortBip8StatisticsBBE OBJECT-TYPE
            SYNTAX Counter64
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
              "This object indicates the background block error."
            ::= { hwPortBip8StatisticsEntry 5 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.12.1.6
        hwPhysicalPortSpeed OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
              "This object indicates the port rate, in Mbit/s."
            ::= { hwPortBip8StatisticsEntry 6 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.13
        hwStorageEntTable OBJECT-TYPE
            SYNTAX      SEQUENCE OF HwStorageEntEntry
            MAX-ACCESS  not-accessible
            STATUS      current
            DESCRIPTION
                "This table describes CF card information about the local chassis."
            ::= { hwEntityState 13 }
            
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.13.1
        hwStorageEntEntry OBJECT-TYPE
            SYNTAX HwStorageEntEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Indicates the Storage statistics.
                This table lists the Entity Storage statistics."
            INDEX  { entPhysicalIndex }    
            ::= { hwStorageEntTable 1 }

	HwStorageEntEntry  ::= 
            SEQUENCE{
                hwStorageEntIndex                   Integer32,
                hwStorageEntType                    Integer32,
                hwStorageEntSpace                   Integer32,
                hwStorageEntSpaceFree               Integer32,
                hwStorageEntName                    SnmpAdminString,
                hwStorageEntDescr                   SnmpAdminString
                }

	-- 1.3.6.1.4.1.2011.5.25.31.1.1.13.1.1
        hwStorageEntIndex OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
              "This object indicates the index."
            ::= { hwStorageEntEntry 1 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.13.1.2
        hwStorageEntType OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
              "This object indicates the storage component type."
            ::= { hwStorageEntEntry 2 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.13.1.3
        hwStorageEntSpace OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
              "This object indicates the storage space."
            ::= { hwStorageEntEntry 3 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.13.1.4
        hwStorageEntSpaceFree OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
              "This object indicates the available space."
            ::= { hwStorageEntEntry 4 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.13.1.5
        hwStorageEntName OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
              "This object indicates the component name."
            ::= { hwStorageEntEntry 5 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.13.1.6
        hwStorageEntDescr OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
              "This object indicates the component description."
            ::= { hwStorageEntEntry 6 }

		
	-- 1.3.6.1.4.1.2011.5.25.31.1.1.14
	hwSystemPowerTable OBJECT-TYPE
	SYNTAX SEQUENCE OF HwSystemPowerEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"System power information table."
	::= { hwEntityState 14 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.14.1
		hwSystemPowerEntry OBJECT-TYPE
			SYNTAX HwSystemPowerEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"System power information entry."
			INDEX { hwSystemPowerDeviceID }
			::= { hwSystemPowerTable 1 }

		
	HwSystemPowerEntry ::=
			SEQUENCE { 
				hwSystemPowerDeviceID
					Integer32,
				hwSystemPowerTotalPower
					Integer32,
				hwSystemPowerUsedPower
					Integer32,
				hwSystemPowerRemainPower
					Integer32,
                                hwSystemPowerReservedPower
                                        Integer32
			 }

		-- 1.3.6.1.4.1.2011.5.25.31.1.1.14.1.1
		hwSystemPowerDeviceID OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"System power information device ID."
			::= { hwSystemPowerEntry 1 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.14.1.2
		hwSystemPowerTotalPower OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"System power information total power."
			::= { hwSystemPowerEntry 2 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.14.1.3
		hwSystemPowerUsedPower OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"System power information used power."
			::= { hwSystemPowerEntry 3 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.14.1.4
		hwSystemPowerRemainPower OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"System power information remain power."
			::= { hwSystemPowerEntry 4 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.14.1.5
		hwSystemPowerReservedPower OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"System power information reserved power."
			::= { hwSystemPowerEntry 5 }

		
--  1.3.6.1.4.1.2011.5.25.31.1.1.15
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.15
		hwBatteryInfoTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwBatteryInfoEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description.Battery information table"
			::= { hwEntityState 15 }

		
--  1.3.6.1.4.1.2011.5.25.31.1.1.15.1
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.15.1
		hwBatteryInfoEntry OBJECT-TYPE
			SYNTAX HwBatteryInfoEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description.Battery information entry"
			INDEX { entPhysicalIndex }
			::= { hwBatteryInfoTable 1 }

		
		HwBatteryInfoEntry ::=
			SEQUENCE { 
				hwBatteryState
					INTEGER,
				hwBatteryTemperatureLow
					Integer32,
			    hwBatteryTemperatureHigh
					Integer32,
				hwBatteryRemainPercent
					Integer32,
			    hwBatteryRemainTime
					Integer32,
				hwBatteryElecTimes
					Integer32,
				hwBatteryLifeThreshold
					Integer32
			 }

		-- 1.3.6.1.4.1.2011.5.25.31.1.1.15.1.1
		hwBatteryState OBJECT-TYPE
			SYNTAX INTEGER
			{
			charge(1),
			discharge(2),
			full(3),
			abnormal(4)
			}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description.The state of lithium battery."
			::= { hwBatteryInfoEntry 1 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.15.1.2
		hwBatteryTemperatureLow OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description.The lowest temperature of lithium battery."
			::= { hwBatteryInfoEntry 2 }    
			
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.15.1.3
		hwBatteryTemperatureHigh OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description.The highest temperature of lithium battery."
			::= { hwBatteryInfoEntry 3 }


		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.15.1.4
		hwBatteryRemainPercent OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description. The remained electricity quantity percent of lithium battery,unit in minute."
			::= { hwBatteryInfoEntry 4 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.15.1.5
		hwBatteryRemainTime OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description. The remained time of lithium battery."
			::= { hwBatteryInfoEntry 5 }


		-- 1.3.6.1.4.1.2011.5.25.31.1.1.15.1.6
		hwBatteryElecTimes OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description.The charge and discharge times of lithium battery."
			::= { hwBatteryInfoEntry 6 }
         
         
                                            -- 1.3.6.1.4.1.2011.5.25.31.1.1.15.1.7
		hwBatteryLifeThreshold OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description.The warning threshold of lithium battery's lifetime.(unit in minute,the default value is 20)"
			::= { hwBatteryInfoEntry 7 }

			
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.16
		hwGPSLocationInfo OBJECT IDENTIFIER ::= { hwEntityState 16 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.16.1
		hwGPSLongitude OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				" Description.The longitude of the device location."
			::= { hwGPSLocationInfo 1 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.16.2
		hwGPSLatitude OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				" Description.The latidude of the device location."
			::= { hwGPSLocationInfo 2 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.16.3
		hwGPSVelocity OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				" Description.The velocity of the device."
			::= { hwGPSLocationInfo 3 }
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.17
        hwAdmPortTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwAdmPortEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The table of ADM(Add/Drop Multiplexer) port properties."
            ::= { hwEntityState 17 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.17.1
        hwAdmPortEntry OBJECT-TYPE
            SYNTAX HwAdmPortEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The entry of ADM(Add/Drop Multiplexer) port properties table."
            INDEX { entPhysicalIndex }
            ::= { hwAdmPortTable 1 }


        HwAdmPortEntry ::=
            SEQUENCE {
                hwAdmPortDescription
                    OCTET STRING
             }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.17.1.1
        hwAdmPortDescription OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The description of ADM(Add/Drop Multiplexer) port."
            ::= { hwAdmPortEntry 1 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.18
        hwPwrStatusTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwPwrStatusEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table lists the status of powers. You can read the status of the powers on the device."
            ::= { hwEntityState 18 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.18.1
        hwPwrStatusEntry OBJECT-TYPE
            SYNTAX HwPwrStatusEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Defines an entry in the hwPwrStatusTable."
            INDEX { hwEntityPwrSlot, hwEntityPwrSn }
            ::= { hwPwrStatusTable 1 }


        HwPwrStatusEntry ::=
            SEQUENCE { 
                hwEntityPwrSlot
                    Integer32,
                hwEntityPwrSn
                    Integer32,
                hwEntityPwrReg
                    INTEGER,
                hwEntityPwrMode
                    INTEGER,
                hwEntityPwrPresent
                    INTEGER,
                hwEntityPwrState
                    INTEGER,
                hwEntityPwrCurrent
                    Integer32,
                hwEntityPwrVoltage
                    Integer32,
                hwEntityPwrDesc
                    OCTET STRING,
                hwEntityPwrPower
                    Integer32
             }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.18.1.1
        hwEntityPwrSlot OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the slot ID of a power."
            ::= { hwPwrStatusEntry 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.18.1.2
        hwEntityPwrSn OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the serial number of the power in a certain slot."
            ::= { hwPwrStatusEntry 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.18.1.3
        hwEntityPwrReg OBJECT-TYPE
            SYNTAX INTEGER
                {
                yes(1),
                no(2)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates whether the power is registered."
            ::= { hwPwrStatusEntry 3 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.18.1.4
        hwEntityPwrMode OBJECT-TYPE
            SYNTAX INTEGER
                {
                unknown(1),
                dc(2),
                ac(3),
                hvdc(4)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the mode of the power."
            ::= { hwPwrStatusEntry 4 }
			

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.18.1.5
        hwEntityPwrPresent OBJECT-TYPE
            SYNTAX INTEGER 
                {
                present(1),
                absent(2)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the present information of the power."
            ::= { hwPwrStatusEntry 5 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.18.1.6
        hwEntityPwrState OBJECT-TYPE
            SYNTAX INTEGER 
            {
                supply(1),
                notSupply(2),
                sleep(3),
                unknown(4)
            }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the state of the power."
            ::= { hwPwrStatusEntry 6 }	

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.18.1.7
        hwEntityPwrCurrent OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the current of the power. Unit: mA "
            ::= { hwPwrStatusEntry 7 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.18.1.8
        hwEntityPwrVoltage OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the voltage of the power. Unit: mV "
            ::= { hwPwrStatusEntry 8 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.18.1.9
        hwEntityPwrDesc OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the description of the power."
            ::= { hwPwrStatusEntry 9 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.18.1.10
        hwEntityPwrPower OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the rated power of the power. Unit: W"
            ::= { hwPwrStatusEntry 10 }
        
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.19     
        hwEntityCpuUsageHistoryTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwEntityCpuUsageHistoryEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table lists the CPU usage history."
            ::= { hwEntityState 19 }            
            
         -- 1.3.6.1.4.1.2011.5.25.31.1.1.19.1     
           hwEntityCpuUsageHistoryEntry OBJECT-TYPE
            SYNTAX HwEntityCpuUsageHistoryEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Defines an entry in the hwEntityCpuUsageHistoryTable."
            INDEX { hwCpuUsageHistoryIndex }
            ::= { hwEntityCpuUsageHistoryTable 1 }
         
          HwEntityCpuUsageHistoryEntry ::=
            SEQUENCE { 
                hwCpuUsageHistoryIndex
                    Integer32,
                hwCpuUsageHistoryTime
                    DateAndTime,
                hwCpuUsageHistoryRate
                    Integer32
             }                             
             
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.19.1.1                     
        hwCpuUsageHistoryIndex OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the index of the CPU usage."
            ::= { hwEntityCpuUsageHistoryEntry 1 }    
            
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.19.1.2 
        hwCpuUsageHistoryTime OBJECT-TYPE
            SYNTAX DateAndTime
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the time of the CPU usage"
            ::= { hwEntityCpuUsageHistoryEntry 2 }
            
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.19.1.3
        hwCpuUsageHistoryRate OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the the CPU usage"
            ::= { hwEntityCpuUsageHistoryEntry 3 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.20
          hwEntityMemUsageHistoryTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwEntityMemUsageHistoryEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table lists the MemUsageHistory."
            ::= { hwEntityState 20 }   

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.20.1                                   
        hwEntityMemUsageHistoryEntry OBJECT-TYPE
            SYNTAX HwEntityMemUsageHistoryEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Defines an entry in the hwEntityMemUsageHistoryTable."
            INDEX { hwMemUsageHistoryIndex }
            ::= { hwEntityMemUsageHistoryTable 1 }  
                                               
          HwEntityMemUsageHistoryEntry ::=
            SEQUENCE { 
                hwMemUsageHistoryIndex
                    Integer32,
                hwMemUsageHistoryTime
                    DateAndTime,
                hwMemUsageHistoryRate
                    Integer32
             }
                      
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.20.1.1
        hwMemUsageHistoryIndex OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the the index of memory usage history."
            ::= { hwEntityMemUsageHistoryEntry 1 }
            
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.20.1.2
           hwMemUsageHistoryTime OBJECT-TYPE
            SYNTAX DateAndTime
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the the index of memory usage history."
            ::= { hwEntityMemUsageHistoryEntry 2 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.20.1.3
           hwMemUsageHistoryRate OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the the index of memory usage history."
            ::= { hwEntityMemUsageHistoryEntry 3 }    

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.21
            hwProcessStateInfo OBJECT IDENTIFIER ::= { hwEntityState 21 }

		
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.21.1
        hwProcessName OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (1..100))
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "This object indicates the process name."
        ::= { hwProcessStateInfo 1 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.22
            hwDiskStateInfo OBJECT IDENTIFIER ::= { hwEntityState 22 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.22.1
        hwDiskType OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (1..100))
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "This object indicates the disk type."
        ::= { hwDiskStateInfo 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.22.2
        hwDiskSN OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (1..100))
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "This object indicates the disk SN."
        ::= { hwDiskStateInfo 2 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.22.3
        hwDiskUsage OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "This object indicates the disk usage rate."
        ::= { hwDiskStateInfo 3 }

		-- 1.3.6.1.4.1.2011.5.25.31.1.1.22.4
        hwDiskUsageThreshold OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "This object indicates the disk usage rate alarm threshold."
        ::= { hwDiskStateInfo 4 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.22.5
        hwDiskSlot OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "This object indicates the disk slot."
        ::= { hwDiskStateInfo 5 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.23
            hwLpuStateInfo OBJECT IDENTIFIER ::= { hwEntityState 23 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.23.1
        hwLPUType OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (1..100))
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "This object indicates the lpu type."
        ::= { hwLpuStateInfo 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.23.2
        hwLPUSlot OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "This object indicates the lpu slot."
        ::= { hwLpuStateInfo 2 }
		
		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.24
        hwHardDiskStateTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwHardDiskStateEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table lists the status of hard disks. You can read the status of the hard disks on the device."
            ::= { hwEntityState 24 }
		
		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.24.1
        hwHardDiskStateEntry OBJECT-TYPE
            SYNTAX HwHardDiskStateEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Defines an entry in the hwHardDiskStateTable."
            INDEX { hwHardDiskIndex }
            ::= { hwHardDiskStateTable 1 }


        HwHardDiskStateEntry ::=
            SEQUENCE { 
                hwHardDiskIndex
                    Integer32,
                hwHardDiskSN
                    OCTET STRING,
                hwHardDiskType
                    OCTET STRING,
                hwHardDiskCapacity
                    Integer32,
                hwHardDiskUsage
                    Integer32,
                hwHardDiskUsageThreshold
                    Integer32,
                hwEntitySDCardUsage
                    Integer32, 
                hwEntitySDCardUsageThreshold
                    Integer32                
             }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.24.1.1
        hwHardDiskIndex OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object indicates the index of a hard disk."
            ::= { hwHardDiskStateEntry 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.24.1.2
        hwHardDiskSN OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the serial number of the hard disk with a specified index."
            ::= { hwHardDiskStateEntry 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.24.1.3
        hwHardDiskType OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the type of the hard disk with a specified index."
            ::= { hwHardDiskStateEntry 3 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.24.1.4
        hwHardDiskCapacity OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the capacity of the hard disk with a specified index."
            ::= { hwHardDiskStateEntry 4 }

			

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.24.1.5
        hwHardDiskUsage OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the usage of the hard disk with a specified index."
            ::= { hwHardDiskStateEntry 5 }

			
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.24.1.6
        hwHardDiskUsageThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the usage threshold of the hard disk with a specified index."
            ::= { hwHardDiskStateEntry 6 } 
		
	     -- 1.3.6.1.4.1.2011.5.25.31.1.1.24.1.7
        hwEntitySDCardUsage OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the usage of the SDCard with a specified index."
            ::= { hwHardDiskStateEntry 7 } 
         -- 1.3.6.1.4.1.2011.5.25.31.1.1.24.1.8
        hwEntitySDCardUsageThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the usage threshold of the SDCard with a specified index."
            ::= { hwHardDiskStateEntry 8 } 
            
        -- 1.3.6.1.4.1.2011.5.25.31.1.2
        hwEntityPhysicalSpecTable OBJECT IDENTIFIER ::= { hwEntityExtObjects 2 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.2.1
		hwEntityPhysicalSpecRack OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The rack coefficient used for calculating the index of the physical entity. "
			::= { hwEntityPhysicalSpecTable 1 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.2.2
		hwEntityPhysicalSpecFrame OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The frame coefficient used for calculating the index of the physical entity. "
			::= { hwEntityPhysicalSpecTable 2 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.2.3
		hwEntityPhysicalSpecSlot OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The slot coefficient used for calculating the index of the physical entity. "
			::= { hwEntityPhysicalSpecTable 3 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.2.4
		hwEntityPhysicalSpecBoard OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The board coefficient used for calculating the index of the physical entity. "
			::= { hwEntityPhysicalSpecTable 4 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.2.5
		hwEntityPhysicalSpecSubSlot OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The sub slot coefficient used for calculating the index of the physical entity. "
			::= { hwEntityPhysicalSpecTable 5 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.2.6
		hwEntityPhysicalSpecSubBoard OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The sub board coefficient used for calculating the index of the physical entity. "
			::= { hwEntityPhysicalSpecTable 6 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.2.7
		hwEntityPhysicalSpecPort OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The port coefficient used for calculating the index of the physical entity.  "
			::= { hwEntityPhysicalSpecTable 7 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.2.8
		hwEntityPhysicalSpecEmu OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The EMU(Environment monitoring unit) coefficient used for calculating the index of the physical entity.  "
			::= { hwEntityPhysicalSpecTable 8 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.2.9
		hwEntityPhysicalSpecPowerframe OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The power frame coefficient used for calculating the index of the physical entity.  "
			::= { hwEntityPhysicalSpecTable 9 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.2.10
		hwEntityPhysicalSpecPowermodule OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The power module coefficient used for calculating the index of the physical entity.  "
			::= { hwEntityPhysicalSpecTable 10 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.2.11
		hwEntityPhysicalSpecBattery OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"The battery coefficient used for calculating the index of the physical entity.  "
			::= { hwEntityPhysicalSpecTable 11 }

		-- 1.3.6.1.4.1.2011.5.25.31.2
		hwEntityExtTraps OBJECT IDENTIFIER ::= { hwEntityExtentMIB 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.2.0
        hwEntityExtTrapsPrefix OBJECT IDENTIFIER ::= { hwEntityExtTraps 0 }


        -- 1.3.6.1.4.1.2011.5.25.31.2.0.1
        hwEntityExtTemperatureThresholdNotification NOTIFICATION-TYPE
            OBJECTS { hwEntityTemperature, hwEntityTemperatureThreshold, hwEntityAdminStatus, hwEntityAlarmLight }
            STATUS current
            DESCRIPTION 
                " The hwEntityEnvTemperatureThresholdNotification
                indicates the temperature have been exceed the threshold.
                In the condition, user should check the hardware and the 
                environment of the entity, sometimes it happened because
                of the failture of air-condition. Anyway, the threshold
                should lower than the value that most service work fine. "
            ::= { hwEntityExtTrapsPrefix 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.2.0.2
        hwEntityExtVoltageLowThresholdNotification NOTIFICATION-TYPE
            OBJECTS { hwEntityVoltage, hwEntityVoltageLowThreshold, hwEntityAdminStatus, hwEntityAlarmLight }
            STATUS current
            DESCRIPTION 
                " The hwEntityExtVoltageLowThresholdNotification indicates
                the voltage is lower than the threshold. This may decrease
                the usability of the entity. If the voltage is lower too much 
                than the hardware needed, the entity will stop working. 
                Anyway, the threshold should higher than the value that 
                most service work fine. "
            ::= { hwEntityExtTrapsPrefix 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.2.0.3
        hwEntityExtVoltageHighThresholdNotification NOTIFICATION-TYPE
            OBJECTS { hwEntityVoltage, hwEntityVoltageHighThreshold, hwEntityAdminStatus, hwEntityAlarmLight }
            STATUS current
            DESCRIPTION 
                " The hwEntityExtVoltageHighThresholdNotification indicates
                the voltage is higher than the threshold. This may decrease
                the usability of the entity. If the voltage is higher too much 
                than the hardware needed, the entity may be destroyed by the high
                voltage. Anyway, the threshold should lower than the value 
                that most service work fine. "
            ::= { hwEntityExtTrapsPrefix 3 }


        -- 1.3.6.1.4.1.2011.5.25.31.2.0.4
        hwEntityExtCpuUsageThresholdNotfication NOTIFICATION-TYPE
            OBJECTS { hwEntityCpuUsage, hwEntityCpuUsageThreshold, hwEntityTemperature, hwEntityTemperatureThreshold, hwEntityAdminStatus, 
                hwEntityAlarmLight }
            STATUS current
            DESCRIPTION 
                " The hwEntityExtCpuUsageThresholdNotfication indicates
                the entity is overload, and the service running in the entity
                will not get the performance it should because of CPU's 
                performance. Anyway, the threshold should lower than the 
                value that most service work fine. "
            ::= { hwEntityExtTrapsPrefix 4 }


        -- 1.3.6.1.4.1.2011.5.25.31.2.0.5
        hwEntityExtMemUsageThresholdNotification NOTIFICATION-TYPE
            OBJECTS { hwEntityMemUsage, hwEntityMemUsageThreshold, hwEntityMemSize, hwEntityAdminStatus, hwEntityAlarmLight
                 }
            STATUS current
            DESCRIPTION 
                " The hwEntityExtMemUsageThresholdNotification indicates
                the entity is overload, and the service running in the entity
                will not get the performance it should because of lower 
                memory. Anyway, the threshold should lower than the 
                value that most service work fine. "
            ::= { hwEntityExtTrapsPrefix 5 }


        -- 1.3.6.1.4.1.2011.5.25.31.2.0.6
        hwEntityExtOperEnabled NOTIFICATION-TYPE
            OBJECTS { hwEntityAdminStatus, hwEntityAlarmLight }
            STATUS current
            DESCRIPTION 
                "The entity is operational. The entity this
                notification refers can be identified by
                extracting the entPhysicalIndex from one of the
                variable bindings."
            ::= { hwEntityExtTrapsPrefix 6 }


        -- 1.3.6.1.4.1.2011.5.25.31.2.0.7
        hwEntityExtOperDisabled NOTIFICATION-TYPE
            OBJECTS { hwEntityAdminStatus, hwEntityAlarmLight }
            STATUS current
            DESCRIPTION 
                "The entity is operational. The entity this
                notification refers can be identified by
                extracting the entPhysicalIndex from one of the
                variable bindings."
            ::= { hwEntityExtTrapsPrefix 7 }


        -- 1.3.6.1.4.1.2011.5.25.31.2.0.8
        hwEntityExtMonitorBoardAbnormalNotification NOTIFICATION-TYPE
            STATUS current
            DESCRIPTION 
                "The monitor board turns normal to abnormal."
            ::= { hwEntityExtTrapsPrefix 8 }


        -- 1.3.6.1.4.1.2011.5.25.31.2.0.9
        hwEntityExtMonitorBoardNormalNotification NOTIFICATION-TYPE
            STATUS current
            DESCRIPTION 
                "The monitor board turns abnormal to normal."
            ::= { hwEntityExtTrapsPrefix 9 }


        -- 1.3.6.1.4.1.2011.5.25.31.2.0.10
        hwEntityExtMonitorPortAbnormalNotification NOTIFICATION-TYPE
            OBJECTS { hwMonitorInputState, hwMonitorInputName }
            STATUS current
            DESCRIPTION 
                "The monitor port turns normal to abnormal."
            ::= { hwEntityExtTrapsPrefix 10 }


        -- 1.3.6.1.4.1.2011.5.25.31.2.0.11
        hwEntityExtMonitorPortNormalNotification NOTIFICATION-TYPE
            OBJECTS { hwMonitorInputState, hwMonitorInputName }
            STATUS current
            DESCRIPTION 
                "The monitor port turns abnormal to normal."
            ::= { hwEntityExtTrapsPrefix 11 }


        -- 1.3.6.1.4.1.2011.5.25.31.2.0.12
        hwEntityExtCpuUsageLowThresholdNotfication NOTIFICATION-TYPE
            OBJECTS { hwEntityCpuUsage, hwEntityCpuUsageThreshold, hwEntityTemperature, hwEntityTemperatureThreshold, hwEntityAdminStatus, 
                hwEntityAlarmLight }
            STATUS current
            DESCRIPTION 
                " The hwEntityExtCpuUsageThresholdNotfication indicates
                the entity is overload, and the service running in the entity
                will not get the performance it should because of CPU's 
                performance. Anyway, the threshold should lower than the 
                value that most service work fine. "
            ::= { hwEntityExtTrapsPrefix 12 }

        -- 1.3.6.1.4.1.2011.5.25.31.2.0.13
        hwEntityExtCpuUsageThresholdNotficationClear NOTIFICATION-TYPE
            OBJECTS { hwEntityCpuUsage, hwEntityCpuUsageThreshold, hwEntityTemperature, hwEntityTemperatureThreshold, hwEntityAdminStatus, 
                hwEntityAlarmLight }
            STATUS current
            DESCRIPTION 
                " The hwEntityExtCpuUsageThresholdNotficationClear indicates
                  the entity CPU usage fell below the threshold. "
            ::= { hwEntityExtTrapsPrefix 13 }


        -- 1.3.6.1.4.1.2011.5.25.31.2.0.14
        hwEntityExtMemUsageThresholdNotificationClear NOTIFICATION-TYPE
            OBJECTS { hwEntityMemUsage, hwEntityMemUsageThreshold, hwEntityMemSize, hwEntityAdminStatus, hwEntityAlarmLight
                 }
            STATUS current
            DESCRIPTION 
                " The hwEntityExtMemUsageThresholdNotificationClear indicates
                  the memory usage fell below the threshold. "
            ::= { hwEntityExtTrapsPrefix 14 }

        -- 1.3.6.1.4.1.2011.5.25.31.2.0.15
	hwEntityExtProcessErrorNotification NOTIFICATION-TYPE
	    OBJECTS { hwProcessName }
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtProcessErrorNotification indicates
		  some important process had exception. "
	    ::= { hwEntityExtTrapsPrefix 15 }

        -- 1.3.6.1.4.1.2011.5.25.31.2.0.16
	hwEntityExtDiskDamaged NOTIFICATION-TYPE
	    OBJECTS { hwDiskType }
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtDiskDamaged indicates
		  disk was damaged. "
	    ::= { hwEntityExtTrapsPrefix 16 }

        -- 1.3.6.1.4.1.2011.5.25.31.2.0.17
	hwEntityExtDiskFull NOTIFICATION-TYPE
	    OBJECTS { hwDiskType }
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtDiskFull indicates
		  disk was full. "
	    ::= { hwEntityExtTrapsPrefix 17 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.2.0.18
	hwEntityExtHda1UsageThresholdNotfication NOTIFICATION-TYPE
	    OBJECTS { hwEntityHda1Usage,hwEntityHda1UsageThreshold }
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtHda1UsageThresholdNotfication indicates
		  the hda1 usage is overload. "
	    ::= { hwEntityExtTrapsPrefix 18 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.2.0.19
	hwEntityExtHda1UsageResumeThresholdNotfication NOTIFICATION-TYPE
	    OBJECTS { hwEntityHda1Usage,hwEntityHda1UsageResumeThreshold }
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtHda1UsageResumeThresholdNotfication indicates
		  the hda1 usage fell below the resume threshold. "
	    ::= { hwEntityExtTrapsPrefix 19 }
            
		-- 1.3.6.1.4.1.2011.5.25.31.2.0.20
	hwEntityExtEncryptionCardFail NOTIFICATION-TYPE
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtEncryptionCardFail indicates
		  the encryption card is faulty. "
	    ::= { hwEntityExtTrapsPrefix 20 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.2.0.21
		hwEntityExtHardDiskFull NOTIFICATION-TYPE
		OBJECTS { hwDiskType, hwDiskSN, hwDiskUsage, hwDiskUsageThreshold }
	    STATUS current
	    DESCRIPTION 
	        " hwEntityExtHardDiskFull indicates
			that the hard disk's spare space is insufficient. "
	    ::= { hwEntityExtTrapsPrefix 21 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.2.0.22
		hwEntityExtHardDiskFullResume NOTIFICATION-TYPE
		OBJECTS { hwDiskType, hwDiskSN, hwDiskUsage, hwDiskUsageThreshold }
	    STATUS current
	    DESCRIPTION 
	        " hwEntityExtHardDiskFullResume indicates
			that the hard disk's usage fell below the alarm clearing threshold. "
	    ::= { hwEntityExtTrapsPrefix 22 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.2.0.23
		hwEntityExtHardDiskPlugIn NOTIFICATION-TYPE
		OBJECTS { hwDiskType, hwDiskSN, hwDiskSlot }
	    STATUS current
	    DESCRIPTION 
	        " hwEntityExtHardDiskPlugIn indicates
		    that the hard disk was plugged in. "
	    ::= { hwEntityExtTrapsPrefix 23 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.2.0.24
		hwEntityExtHardDiskPlugOut NOTIFICATION-TYPE
		OBJECTS { hwDiskType, hwDiskSN, hwDiskSlot }
	    STATUS current
	    DESCRIPTION 
	        " hwEntityExtHardDiskPlugOut indicates
		    that the hard disk was pulled out. "
	    ::= { hwEntityExtTrapsPrefix 24 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.2.0.25
		hwEntityExtHardDiskOnline NOTIFICATION-TYPE
		OBJECTS { hwDiskType, hwDiskSN, hwDiskSlot }
	    STATUS current
	    DESCRIPTION 
	        " hwEntityExtHardDiskOnline indicates
			that the hard disk went online successfully."
	    ::= { hwEntityExtTrapsPrefix 25 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.2.0.26
		hwEntityExtHardDiskOffline NOTIFICATION-TYPE
		OBJECTS { hwDiskType, hwDiskSN, hwDiskSlot }
	    STATUS current
	    DESCRIPTION 
	        " hwEntityExtHardDiskOffline indicates
			that the hard disk went offline. "
	    ::= { hwEntityExtTrapsPrefix 26 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.2.0.27
		hwEntityExtLPUPlugIn NOTIFICATION-TYPE
		OBJECTS { hwLPUSlot }
	    STATUS current
	    DESCRIPTION 
	        " hwEntityExtLPUPlugIn indicates
			that the LPU was plugged in. "
	    ::= { hwEntityExtTrapsPrefix 27 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.2.0.28
		hwEntityExtLPUPlugOut NOTIFICATION-TYPE
		OBJECTS { hwLPUSlot }
	    STATUS current
	    DESCRIPTION 
	        " hwEntityExtLPUPlugOut indicates
			that the LPU was pulled out. "
	    ::= { hwEntityExtTrapsPrefix 28 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.2.0.29
		hwEntityExtCpuUsageSuddenChangeNotification NOTIFICATION-TYPE
		OBJECTS { hwEntitySlotID, hwEntityCpuID, hwEntityPreviousValue, hwEntityCurrentValue,hwEntityChangeValue, hwEntityChangeValueThreshold }
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtCpuUsageSuddenChangeNotification indicates that the CPU usage suddenly changed. "
	    ::= { hwEntityExtTrapsPrefix 29 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.2.0.30
		hwEntityExtMemoryUsageSuddenChangeNotification NOTIFICATION-TYPE
		OBJECTS { hwEntitySlotID, hwEntityCpuID, hwEntityPreviousValue, hwEntityCurrentValue, hwEntityChangeValue, hwEntityChangeValueThreshold }
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtMemoryUsageSuddenChangeNotification indicates that the memory usage suddenly changed. "
	    ::= { hwEntityExtTrapsPrefix 30 }
	    
	  -- 1.3.6.1.4.1.2011.5.25.31.2.0.31
		hwEntityExtCPUOverInterfaceDown NOTIFICATION-TYPE
		OBJECTS { hwEntitySlotID, hwEntityCpuID }		
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtCPUOverInterfaceDown indicates that the cpu usage reached the threshold for interface management ,and the interface was shutdown. "
	    ::= { hwEntityExtTrapsPrefix 31 }

	-- 1.3.6.1.4.1.2011.5.25.31.2.0.32
	    hwEntityExtDevConfigurationRecovered NOTIFICATION-TYPE
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtDevConfigurationRecovered indicates
		  the device configuration was recovered."
	    ::= { hwEntityExtTrapsPrefix 32 }

	-- 1.3.6.1.4.1.2011.5.25.31.2.0.33
	    hwEntityExtHotPatchReservedFirst NOTIFICATION-TYPE
                       OBJECTS { hwProcessName}
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtHotPatchReservedFirst indicates
		  the first reserved information of hot patch."
	    ::= { hwEntityExtTrapsPrefix 33 }
		
	-- 1.3.6.1.4.1.2011.5.25.31.2.0.34
	    hwEntityExtHotPatchReservedSecond NOTIFICATION-TYPE
                       OBJECTS { hwProcessName}
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtHotPatchReservedSecond indicates
		  the second reserved information of hot patch."
	    ::= { hwEntityExtTrapsPrefix 34 }
		
	-- 1.3.6.1.4.1.2011.5.25.31.2.0.35
	    hwEntityExtHotPatchReservedThird NOTIFICATION-TYPE
                       OBJECTS { hwProcessName}
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtHotPatchReservedThird indicates
		  the third reserved information of hot patch."
	    ::= { hwEntityExtTrapsPrefix 35 }
		
	-- 1.3.6.1.4.1.2011.5.25.31.2.0.36
	    hwEntityExtHotPatchReservedFourth NOTIFICATION-TYPE
                       OBJECTS { hwProcessName}
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtHotPatchReservedFourth indicates
		  the fourth reserved information of hot patch."
	    ::= { hwEntityExtTrapsPrefix 36 }
		
	-- 1.3.6.1.4.1.2011.5.25.31.2.0.37
	    hwEntityExtHotPatchReservedFifth NOTIFICATION-TYPE
                       OBJECTS { hwProcessName}
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtHotPatchReservedFifth indicates
		  the fifth reserved information of hot patch."
	    ::= { hwEntityExtTrapsPrefix 37 } 
	
	-- 1.3.6.1.4.1.2011.5.25.31.2.0.38
	    hwEntityExtSDCardFsErrorAlarm NOTIFICATION-TYPE 	   
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtSDCardFsErrorAlarm indicates
		  the SDCard was damaged."
	    ::= { hwEntityExtTrapsPrefix 38 }
	    
	    
	-- 1.3.6.1.4.1.2011.5.25.31.2.0.39 
	    hwEntityExtSDCardFsErrorResume NOTIFICATION-TYPE   
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtSDCardFsErrorResume indicates
		  the SDCard was restored."
	    ::= { hwEntityExtTrapsPrefix 39 }
	    
	    
	-- 1.3.6.1.4.1.2011.5.25.31.2.0.40 
	    hwEntityExtSDCardUsageOver NOTIFICATION-TYPE
	    OBJECTS {hwEntitySDCardUsage,hwEntitySDCardUsageThreshold} 
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtSDCardUsageOver indicates
		  the SDCard usage is overload."
	    ::= { hwEntityExtTrapsPrefix 40 }
	    
	    
	-- 1.3.6.1.4.1.2011.5.25.31.2.0.41 
	    hwEntityExtSDCardUsageBelow NOTIFICATION-TYPE
	    OBJECTS {hwEntitySDCardUsage,hwEntitySDCardUsageThreshold} 
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtSDCardUsageBelow indicates
		  the SDCard usage fell below the resume threshold."
	    ::= { hwEntityExtTrapsPrefix 41 }
	    
	     
	-- 1.3.6.1.4.1.2011.5.25.31.2.0.42 
	    hwEntityExtCFCardFaultAlarm NOTIFICATION-TYPE  	      
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtCFCardFaultAlarm indicates
		  the CFCard was damaged."
	    ::= { hwEntityExtTrapsPrefix 42 }
	    
	    
	-- 1.3.6.1.4.1.2011.5.25.31.2.0.43  
	    hwEntityExtCFCardFaultResume NOTIFICATION-TYPE     
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtCFCardFaultResume indicates
		  the CFCard was restored."
	    ::= { hwEntityExtTrapsPrefix 43 }
	    
	    
	-- 1.3.6.1.4.1.2011.5.25.31.2.0.44
	   hwEntityNVRAMFaultAlarmNotification NOTIFICATION-TYPE
                       OBJECTS { hwProcessName}
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityNVRAMFaultAlarmNotification indicates
		  the main NVRAM was damaged."
	    ::= { hwEntityExtTrapsPrefix 44 }
		
	-- 1.3.6.1.4.1.2011.5.25.31.2.0.45
	    hwEntityNVRAMFaultResumeNotification NOTIFICATION-TYPE
                       OBJECTS { hwProcessName}
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityNVRAMFaultResumeNotification indicates
		  that it was successful to switch main NVRAM to backup NVRAM ."
	    ::= { hwEntityExtTrapsPrefix 45 }

	-- 1.3.6.1.4.1.2011.5.25.31.2.0.46
	    hwEntityExtBootPasswordAlarm NOTIFICATION-TYPE
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityNVRAMFaultResume indicates
		  that the BootLoader password is not set, which poses security risks. You are advised to change the password."
	    ::= { hwEntityExtTrapsPrefix 46 }      

	-- 1.3.6.1.4.1.2011.5.25.31.2.0.47
	    hwEntityExtSmallBootPasswordAlarm NOTIFICATION-TYPE
	    STATUS current
	    DESCRIPTION 
	        " The hwEntityExtSmallBootPasswordAlarm indicates
		  that the small boot password was initial password and needed to change."
	    ::= { hwEntityExtTrapsPrefix 47 }

        -- 1.3.6.1.4.1.2011.5.25.31.2.0.48
        hwEntityExtCpuUsageNotfication NOTIFICATION-TYPE
            OBJECTS { hwCpuUsageTrapType, hwCpuUsageTrapSlot, hwCpuUsageTrapCpu, hwCpuUsageCurrentUsage, hwCpuUsageThreashold }
            STATUS current
            DESCRIPTION 
                " The hwEntityExtCpuUsageNotfication indicates the entity is overload, and the service running in the entity will not get the performance it should because of CPU's performance. Anyway, the threshold should lower than the value that most service work fine. "
            ::= { hwEntityExtTrapsPrefix 48 }
        
         -- 1.3.6.1.4.1.2011.5.25.31.2.0.49
        hwEntityExtCpuUsageNotficationClear NOTIFICATION-TYPE
            OBJECTS { hwCpuUsageTrapType, hwCpuUsageTrapSlot, hwCpuUsageTrapCpu, hwCpuUsageCurrentUsage, hwCpuUsageThreashold }
            STATUS current
            DESCRIPTION 
                " The hwEntityExtCpuUsageNotficationClear indicates the entity CPU usage fell below the threshold. "
            ::= { hwEntityExtTrapsPrefix 49 }

		-- 1.3.6.1.4.1.2011.5.25.31.2.0.50
		hwEntityExtHardDiskOnlineFail NOTIFICATION-TYPE
		OBJECTS { hwDiskType, hwDiskSN, hwDiskSlot }
	    STATUS current
	    DESCRIPTION 
	        " The object indicates
			that the hard disk went online fail."
	    ::= { hwEntityExtTrapsPrefix 50 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.2.0.51
		hwEntityExtHardDiskOfflineFail NOTIFICATION-TYPE
		OBJECTS { hwDiskType, hwDiskSN, hwDiskSlot }
	    STATUS current
	    DESCRIPTION 
	        " The object indicates
			that the hard disk went offline fail. "
	    ::= { hwEntityExtTrapsPrefix 51 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.2.1
        hwEntityExtTrapObject OBJECT IDENTIFIER ::= { hwEntityExtTraps 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.2.1.1
        hwEntityExtTrapBaseSoftwareVersion OBJECT-TYPE
			SYNTAX OCTET STRING
	MAX-ACCESS accessible-for-notify
	STATUS current
	DESCRIPTION
	        "System bassic software version."
	::= { hwEntityExtTrapObject 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.2.1.2
		hwEntityExtTrapBoardSoftwareVersion OBJECT-TYPE
			SYNTAX OCTET STRING
	MAX-ACCESS accessible-for-notify
	STATUS current
	DESCRIPTION
	        "Board software version compare to basic software version."
	::= { hwEntityExtTrapObject 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.2.1.3
		hwPhysicalName OBJECT-TYPE
			SYNTAX OCTET STRING
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
            "The textual name of the physical entity.  The value of this
            object should be the name of the component as assigned by
            the local device and should be suitable for use in commands
            entered at the device's `console'.  This might be a text
            name, such as `console' or a simple component number (e.g.,
            port or module number), such as `1', depending on the
            physical component naming syntax of the device.

            If there is no local name, or this object is otherwise not
            applicable, then this object contains a zero-length string.

            Note that the value of entPhysicalName for two physical
            entities will be the same in the event that the console
            interface does not distinguish between them, e.g., slot-1
            and the card in slot-1."
	          ::= { hwEntityExtTrapObject 3 }

		    hwEntityExtTrapBoardSlotID OBJECT-TYPE
			      SYNTAX OCTET STRING
	          MAX-ACCESS accessible-for-notify
				    STATUS current
			      DESCRIPTION
	          "Slot ID of board."
	          ::= { hwEntityExtTrapObject 4 }

		    hwEntityExtTrapUnitID OBJECT-TYPE
			      SYNTAX Integer32
	          MAX-ACCESS accessible-for-notify
				    STATUS current
			      DESCRIPTION
	          "ID of chip."
	          ::= { hwEntityExtTrapObject 5 }

		    hwEntityExtTrapHigPortID OBJECT-TYPE
			      SYNTAX OCTET STRING
	          MAX-ACCESS accessible-for-notify
				    STATUS current
			      DESCRIPTION
	          "HIG port ID of chip."
	          ::= { hwEntityExtTrapObject 6 }

		    hwEntityExtTrapChannelCurUsage OBJECT-TYPE
			      SYNTAX Integer32
	          MAX-ACCESS accessible-for-notify
				    STATUS current
			      DESCRIPTION
	          "The currently usage of channel."
	          ::= { hwEntityExtTrapObject 7 }

		    hwEntityExtTrapChannelThreshold OBJECT-TYPE
			      SYNTAX Integer32
	          MAX-ACCESS accessible-for-notify
				    STATUS current
			      DESCRIPTION
	          "The usage threshold of channel."
	          ::= { hwEntityExtTrapObject 8 }

		    hwEntityExtTrapPeerBoardSlotID OBJECT-TYPE
			      SYNTAX OCTET STRING
	          MAX-ACCESS accessible-for-notify
				    STATUS current
			      DESCRIPTION
	          "Slot ID of peer board."
	          ::= { hwEntityExtTrapObject 9 }

		    hwEntityExtTrapErrorPacketStatistics OBJECT-TYPE
			      SYNTAX OCTET STRING
	          MAX-ACCESS accessible-for-notify
				    STATUS current
			      DESCRIPTION
	          "The statistics of CRC."
	          ::= { hwEntityExtTrapObject 10 }

		    hwEntityExtTrapErrorPacketThreshold OBJECT-TYPE
			      SYNTAX OCTET STRING
	          MAX-ACCESS accessible-for-notify
				    STATUS current
			      DESCRIPTION
	          "The threshold of CRC."
	          ::= { hwEntityExtTrapObject 11 }

		    hwEntityExtTrapHigStateChangeTimes OBJECT-TYPE
			      SYNTAX OCTET STRING
	          MAX-ACCESS accessible-for-notify
				    STATUS current
			      DESCRIPTION
	          "The state change times of HIG port."
	          ::= { hwEntityExtTrapObject 12 }

		    hwEntityExtTrapMonitorInterval OBJECT-TYPE
			      SYNTAX OCTET STRING
	          MAX-ACCESS accessible-for-notify
				    STATUS current
			      DESCRIPTION
	          "The monitor interval."
	          ::= { hwEntityExtTrapObject 13 }

	
		-- 1.3.6.1.4.1.2011.5.25.31.2.1.14
		hwEntityExtTrapBoardDropRuntPktStatistics OBJECT-TYPE
			SYNTAX Counter64
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The statistic of dropped runt packets on the board."
			::= { hwEntityExtTrapObject 14 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.2.1.15
		hwEntityExtTrapBoardDropRuntPktTimeInterval OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The time interval."
			::= { hwEntityExtTrapObject 15 }

		-- 1.3.6.1.4.1.2011.5.25.31.2.1.16
		hwEntityExtTrapDiscardNumber OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The statistics of drop."
			::= { hwEntityExtTrapObject 16 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.2.1.17
		hwEntityExtTrapThreshold OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The threshold of drop."
			::= { hwEntityExtTrapObject 17 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.2.1.18
		hwEntityExtTrapInterval OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The time interval."
			::= { hwEntityExtTrapObject 18 }

		-- 1.3.6.1.4.1.2011.5.25.31.2.2
        hwEntityExtTrap OBJECT IDENTIFIER ::= { hwEntityExtTraps 2 }		
				
		-- 1.3.6.1.4.1.2011.5.25.31.2.2.1
        hwBoardSoftwareVersionIncompatible NOTIFICATION-TYPE
                   OBJECTS { entPhysicalName, hwEntityExtTrapBaseSoftwareVersion, hwEntityExtTrapBoardSoftwareVersion }
                   STATUS current
                   DESCRIPTION 
	        "Board software version incompatible with basic software version."
					::= { hwEntityExtTrap 1 }
		-- 1.3.6.1.4.1.2011.5.25.31.2.2.2
	    hwBoardSplitPorts NOTIFICATION-TYPE
                   OBJECTS { hwPhysicalName }
                   STATUS current
                   DESCRIPTION 
	        "When the split ports exist on the board, send a SNMP trap to network manager."
					::= { hwEntityExtTrap 2 }

	    hwEntityInputRateThresholdAlarm NOTIFICATION-TYPE
          OBJECTS { hwEntityExtTrapBoardSlotID, hwEntityExtTrapUnitID, hwEntityExtTrapHigPortID, hwEntityExtTrapPeerBoardSlotID, hwEntityExtTrapChannelCurUsage, hwEntityExtTrapChannelThreshold }
          STATUS current
          DESCRIPTION 
	        "When the input usage of channel is more than the threshold of alarm, send a SNMP trap to network manager."
					::= { hwEntityExtTrap 3 }

	    hwEntityInputRateThresholdAlarmResume NOTIFICATION-TYPE
          OBJECTS { hwEntityExtTrapBoardSlotID, hwEntityExtTrapUnitID, hwEntityExtTrapHigPortID, hwEntityExtTrapPeerBoardSlotID, hwEntityExtTrapChannelCurUsage, hwEntityExtTrapChannelThreshold }
          STATUS current
          DESCRIPTION 
	        "When the input usage of channel is less than the threshold of resume, send a SNMP trap to network manager."
					::= { hwEntityExtTrap 4 }

	    hwEntityOutputRateThresholdAlarm NOTIFICATION-TYPE
          OBJECTS { hwEntityExtTrapBoardSlotID, hwEntityExtTrapUnitID, hwEntityExtTrapHigPortID, hwEntityExtTrapPeerBoardSlotID, hwEntityExtTrapChannelCurUsage, hwEntityExtTrapChannelThreshold }
          STATUS current
          DESCRIPTION 
	        "When the output usage of channel is more than the threshold of alarm, send a SNMP trap to network manager."
					::= { hwEntityExtTrap 5 }

	    hwEntityOutputRateThresholdAlarmResume NOTIFICATION-TYPE
          OBJECTS { hwEntityExtTrapBoardSlotID, hwEntityExtTrapUnitID, hwEntityExtTrapHigPortID, hwEntityExtTrapPeerBoardSlotID, hwEntityExtTrapChannelCurUsage, hwEntityExtTrapChannelThreshold }
          STATUS current
          DESCRIPTION 
	        "When the output usage of channel is less than the threshold of resume, send a SNMP trap to network manager."
					::= { hwEntityExtTrap 6 }

	    hwEntityStatusChange NOTIFICATION-TYPE
          OBJECTS { entPhysicalIndex , entPhysicalName, entPhysicalClass, hwEntityOperStatus }
          STATUS current
          DESCRIPTION 
	        "The entity status was changed."
					::= { hwEntityExtTrap 7 }

	    hwEntityHigErrorPacketThresholdAlarm NOTIFICATION-TYPE
          OBJECTS { hwEntityExtTrapBoardSlotID, hwEntityExtTrapUnitID, hwEntityExtTrapHigPortID, hwEntityExtTrapPeerBoardSlotID, hwEntityExtTrapErrorPacketStatistics, hwEntityExtTrapErrorPacketThreshold, hwEntityExtTrapMonitorInterval }
          STATUS current
          DESCRIPTION 
	        "When the CRC errors of HIG port are more than the threshold, send a SNMP trap to network manager."
					::= { hwEntityExtTrap 8 }

	    hwEntityHigStateChangeNotify NOTIFICATION-TYPE
          OBJECTS { hwEntityExtTrapBoardSlotID, hwEntityExtTrapUnitID, hwEntityExtTrapHigPortID, hwEntityExtTrapPeerBoardSlotID, hwEntityExtTrapHigStateChangeTimes }
          STATUS current
          DESCRIPTION 
	        "When the CRC errors of Serdes channel are more than the threshold, send a SNMP trap to network manager."
					::= { hwEntityExtTrap 9 }

	    hwEntityHigStateDownNotify NOTIFICATION-TYPE
          OBJECTS { hwEntityExtTrapBoardSlotID, hwEntityExtTrapUnitID, hwEntityExtTrapHigPortID, hwEntityExtTrapPeerBoardSlotID, hwEntityExtTrapMonitorInterval }
          STATUS current
          DESCRIPTION 
	        "When the state of Serdes channel is always down, send a SNMP trap to network manager."
					::= { hwEntityExtTrap 10 }

      hwEntityPositionMismatchNotify NOTIFICATION-TYPE
          OBJECTS { hwEntityExtTrapBoardSlotID }
          STATUS current
          DESCRIPTION 
	        "When the board type and slotID is mismatch,send a SNMP notify to network manager."
					::= { hwEntityExtTrap 11 }

	    hwEntityRuntPacketCheckNotify NOTIFICATION-TYPE
          OBJECTS { hwEntityExtTrapBoardSlotID, hwEntityExtTrapUnitID, hwEntityExtTrapHigPortID }
          STATUS current
          DESCRIPTION 
	        "When the statistics of runt packets is more than the threshold, send a SNMP trap to network manager."
					::= { hwEntityExtTrap 12 }

	    hwEntityHigCrcErrorAlarm NOTIFICATION-TYPE
          OBJECTS { hwEntityExtTrapBoardSlotID, hwEntityExtTrapUnitID, hwEntityExtTrapHigPortID, hwEntityExtTrapPeerBoardSlotID, hwEntityExtTrapErrorPacketStatistics, hwEntityExtTrapErrorPacketThreshold, hwEntityExtTrapMonitorInterval }
          STATUS current
          DESCRIPTION 
	        "When the CRC errors of HIG port are more than the threshold, send a SNMP alarm trap to network manager."
					::= { hwEntityExtTrap 17}

	    hwEntityHigCrcErrorAlarmResume NOTIFICATION-TYPE
          OBJECTS { hwEntityExtTrapBoardSlotID, hwEntityExtTrapUnitID, hwEntityExtTrapHigPortID, hwEntityExtTrapPeerBoardSlotID, hwEntityExtTrapErrorPacketStatistics, hwEntityExtTrapErrorPacketThreshold, hwEntityExtTrapMonitorInterval }
          STATUS current
          DESCRIPTION 
	        "When the number of CRC errors on the HIG port falls below the threshold, an SNMP trap is sent to the network manager."
					::= { hwEntityExtTrap 18}

	    hwEntityHigDown NOTIFICATION-TYPE
          OBJECTS { hwEntityExtTrapBoardSlotID, hwEntityExtTrapUnitID, hwEntityExtTrapHigPortID, hwEntityExtTrapPeerBoardSlotID, hwEntityExtTrapMonitorInterval }
          STATUS current
          DESCRIPTION 
	        "When the state of Serdes channel is always down, send a SNMP trap to network manager."
					::= { hwEntityExtTrap 19}

	    hwEntityHigDownResume NOTIFICATION-TYPE
          OBJECTS { hwEntityExtTrapBoardSlotID, hwEntityExtTrapUnitID, hwEntityExtTrapHigPortID, hwEntityExtTrapPeerBoardSlotID, hwEntityExtTrapMonitorInterval }
          STATUS current
          DESCRIPTION 
	        "When the Serdes channel goes Up, an SNMP trap is sent to the network manager."
					::= { hwEntityExtTrap 20}

	  -- 1.3.6.1.4.1.2011.5.25.31.2.2.13
	  hwBoardDropRuntPacketNotify NOTIFICATION-TYPE
	  	OBJECTS { entPhysicalName, hwEntityExtTrapBoardDropRuntPktStatistics, hwEntityExtTrapBoardDropRuntPktTimeInterval }
	  	STATUS current
	  	DESCRIPTION 
	  	"When the statistics of dropped runt packets on the board is more than the threshold, send a SNMP trap to network manager."
	  	::= { hwEntityExtTrap 13 }

	  -- 1.3.6.1.4.1.2011.5.25.31.2.2.14
	  hwEntityHigDiscardPacketNotify NOTIFICATION-TYPE
	  	OBJECTS { hwEntityExtTrapBoardSlotID, hwEntityExtTrapUnitID, hwEntityExtTrapHigPortID, hwEntityExtTrapPeerBoardSlotID, hwEntityExtTrapDiscardNumber, hwEntityExtTrapThreshold, hwEntityExtTrapInterval }
	  	STATUS current
	  	DESCRIPTION 
	  	"When the congistion drop packets of HIG port are more than the threshold, send a SNMP trap to network manager."
	  	::= { hwEntityExtTrap 14 }

	-- 1.3.6.1.4.1.2011.5.25.31.2.2.15
		hwEntitySerdesChangeNotify NOTIFICATION-TYPE
			OBJECTS { hwEntityExtTrapBoardSlotID, hwEntityExtTrapUnitID, hwEntityExtTrapHigPortID, hwEntityExtTrapPeerBoardSlotID, hwEntityExtTrapHigStateChangeTimes
				 }
			STATUS current
			DESCRIPTION 
				"When the CRC errors of Fic port are more than the threshold, send a SNMP trap to network manager."
			::= { hwEntityExtTrap 15 }
		
	-- 1.3.6.1.4.1.2011.5.25.31.2.2.16
		hwEntitySerdesDownNotify NOTIFICATION-TYPE
			OBJECTS { hwEntityExtTrapBoardSlotID, hwEntityExtTrapUnitID, hwEntityExtTrapHigPortID, hwEntityExtTrapPeerBoardSlotID, hwEntityExtTrapMonitorInterval
				 }
			STATUS current
			DESCRIPTION 
				"When the state of Fic port is always down, send a SNMP trap to network manager."
			::= { hwEntityExtTrap 16 }

        -- 1.3.6.1.4.1.2011.5.25.31.3
        hwDevicePowerInfoObjects OBJECT IDENTIFIER ::= { hwEntityExtentMIB 3 }


        -- 1.3.6.1.4.1.2011.5.25.31.3.1
        hwDevicePowerInfoTotalPower OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the total power of the device."
            ::= { hwDevicePowerInfoObjects 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.3.2
        hwDevicePowerInfoUsedPower OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the current power of the device."
            ::= { hwDevicePowerInfoObjects 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.4
        hwEntityExtConformance OBJECT IDENTIFIER ::= { hwEntityExtentMIB 4 }


        -- 1.3.6.1.4.1.2011.5.25.31.4.1
        hwEntityExtCompliances OBJECT IDENTIFIER ::= { hwEntityExtConformance 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.4.1.1
        hwEntityExtCompliance MODULE-COMPLIANCE
            STATUS current
            DESCRIPTION 
                "The compliance statement for systems supporting
                the HUAWEI Entity extent MIB."
            MODULE -- this module
                MANDATORY-GROUPS { hwEntityExtGroup }
                OBJECT hwEntityAdminStatus
                    MIN-ACCESS read-only
                    DESCRIPTION 
                        "Write access is not required."
                OBJECT hwEntityCpuUsageThreshold
                    MIN-ACCESS read-only
                    DESCRIPTION 
                        "Write access is not required."
                OBJECT hwEntityMemUsageThreshold
                    MIN-ACCESS read-only
                    DESCRIPTION 
                        "Write access is not required."
                OBJECT hwEntityTemperatureThreshold
                    MIN-ACCESS read-only
                    DESCRIPTION 
                        "Write access is not required."
                OBJECT hwEntityVoltageLowThreshold
                    MIN-ACCESS read-only
                    DESCRIPTION 
                        "Write access is not required."
                OBJECT hwEntityVoltageHighThreshold
                    MIN-ACCESS read-only
                    DESCRIPTION 
                        "Write access is not required."
            ::= { hwEntityExtCompliances 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.4.2
        hwEntityExtGroups OBJECT IDENTIFIER ::= { hwEntityExtConformance 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.4.2.1
        hwEntityExtGroup OBJECT-GROUP
            OBJECTS { hwEntityAdminStatus, hwEntityOperStatus, hwEntityStandbyStatus, hwEntityAlarmLight, hwEntityCpuUsage, 
                hwEntityCpuUsageThreshold, hwEntityMemUsage, hwEntityMemUsageThreshold, hwEntityMemSize, hwEntityUpTime, 
                hwEntityTemperature, hwEntityTemperatureThreshold, hwEntityVoltage, hwEntityVoltageLowThreshold, hwEntityVoltageHighThreshold, 
                hwEntityTemperatureLowThreshold, hwEntityOpticalPower, hwEntityCurrent, hwEntityMemSizeMega, hwEntityPortType, 
                hwEntityDuplex, hwEntityOpticalPowerRx, hwEntityCpuUsageLowThreshold, hwEntityBoardPower, hwEntityCpuFrequency, 
                hwEntitySupportFlexCard, hwEntityBoardClass, hwNseOpmStatus, hwEntityCpuMaxUsage, hwEntityServiceType, hwDeviceServiceType, 
                hwEntityCPUType, hwEntityMemoryType, hwEntityFlashSize, hwEntityIfUpTimes, hwEntityIfDownTimes,
                hwEntity5MinCpuUsage,hwEntityBoardDescription,hwEntityBoardName,  hwEntityStartMode , hwEntitySplitAttribute,
                hwEntityCPUAvgUsage, hwEntityMemoryAvgUsage, hwEntityExtTrapBaseSoftwareVersion, hwEntityExtTrapBoardSoftwareVersion, 
                hwProcessName, hwPhysicalName, hwGPSLongitude, hwGPSLatitude, hwGPSVelocity, hwEntityExtTrapBoardSlotID, hwEntityExtTrapUnitID, hwEntityExtTrapHigPortID,
                hwEntityExtTrapChannelCurUsage, hwEntityExtTrapChannelThreshold, hwEntityExtTrapPeerBoardSlotID, hwEntityExtTrapErrorPacketStatistics,
                hwEntityExtTrapErrorPacketThreshold, hwEntityExtTrapHigStateChangeTimes, hwEntityExtTrapMonitorInterval,
				hwEntitySlotID, hwEntityCpuID, hwEntityPreviousValue, hwEntityCurrentValue, hwEntityChangeValue, hwEntityChangeValueThreshold,hwDownloadDiagnosticsStatus, hwDownloadDiagnosticsRowStatus,
				hwDownloadDiagnosticsSpeed, hwDownloadDiagnosticsDSCP, hwDownloadDiagnosticsTransports, hwDownloadDiagnosticsURL, hwDownloadDiagnosticsProgress,
				hwUploadDiagnosticsProgress, hwUploadDiagnosticsStatus, hwUploadDiagnosticsRowStatus,hwUploadDiagnosticsSpeed,  hwUploadDiagnosticsTestFileSize, hwUploadDiagnosticsDSCP, 
				hwUploadDiagnosticsTransports, hwUploadDiagnosticsURL, hwEntityDeviceStatus, hwEntityPicStatus, hwEntityTemperatureMinorThreshold,
                hwEntityVoltageFatalHighThreshold, hwEntityVoltageFatalLowThreshold}
            STATUS current
            DESCRIPTION 
                "Standard HUAWEI Entity Extent group."
            ::= { hwEntityExtGroups 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.4.2.2
        hwEntityExtNotificationGroup NOTIFICATION-GROUP
            NOTIFICATIONS { hwEntityExtTemperatureThresholdNotification, hwEntityExtVoltageLowThresholdNotification, hwEntityExtVoltageHighThresholdNotification, hwEntityExtCpuUsageThresholdNotfication, hwEntityExtMemUsageThresholdNotification, 
                hwEntityExtOperEnabled, hwEntityExtOperDisabled, hwEntityExtMonitorBoardAbnormalNotification, hwEntityExtMonitorBoardNormalNotification, hwEntityExtMonitorPortAbnormalNotification, 
                hwEntityExtMonitorPortNormalNotification, hwEntityExtCpuUsageLowThresholdNotfication,hwInsertDiffFromPreDisposed,hwPreDisposedChangeNotification,hwEntityHeartbeatTrap,
                hwHardwareCapaChangeNotification, hwEntityExtProcessErrorNotification, hwAlarmPnPChangeNotification, hwBoardSoftwareVersionIncompatible, hwBoardSplitPorts,
                hwEntityInputRateThresholdAlarm, hwEntityInputRateThresholdAlarmResume, hwEntityOutputRateThresholdAlarm, hwEntityOutputRateThresholdAlarmResume, hwEntityStatusChange, hwEntityHigCrcErrorAlarm, hwEntityHigCrcErrorAlarmResume, hwEntityHigDown, hwEntityHigDownResume,
                hwEntityHigErrorPacketThresholdAlarm, hwEntityHigStateChangeNotify, hwEntityHigStateDownNotify,hwEntityPositionMismatchNotify,hwEntityRuntPacketCheckNotify,hwHda1Error,hwEntityExtCpuUsageSuddenChangeNotification,
                hwEntityExtMemoryUsageSuddenChangeNotification,hwEntityExtCPUOverInterfaceDown,hwEntityExtDevConfigurationRecovered,hwEntityExtHotPatchReservedFirst,hwEntityExtHotPatchReservedSecond,hwEntityExtHotPatchReservedThird,
                hwEntityExtHotPatchReservedFourth,hwEntityExtHotPatchReservedFifth,hwEntityExtSDCardFsErrorAlarm,hwEntityExtSDCardFsErrorResume,hwEntityExtSDCardUsageOver,hwEntityExtSDCardUsageBelow,hwEntityExtCFCardFaultAlarm,
                hwEntityExtCFCardFaultResume,hwEntityNVRAMFaultAlarmNotification,hwEntityNVRAMFaultResumeNotification,hwEntityExtBootPasswordAlarm,hwEntityExtSmallBootPasswordAlarm}
            STATUS current
            DESCRIPTION 
                "Standard HUAWEI Entity Extent Notification group."
            ::= { hwEntityExtGroups 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.4.2.3
        hwRUModuleInfoGroup OBJECT-GROUP
            OBJECTS { hwEntityBomId, hwEntityBomEnDesc, hwEntityManufacturedDate, hwEntityCLEICode, hwEntityArchivesInfoVersion, 
                hwEntityOpenBomId, hwEntityIssueNum, hwEntityBoardType, hwEntityExInfo, hwEntityModel, hwEntityElabelVersion, hwEntitySafeId }
            STATUS current
            DESCRIPTION 
                "Standard HUAWEI Entity Extent group."
            ::= { hwEntityExtGroups 3 }


        -- 1.3.6.1.4.1.2011.5.25.31.4.2.4
        hwEntityExtOldObjectsGroup OBJECT-GROUP
            OBJECTS { hwEntityBomLocalDesc, hwEntityManufactureCode, hwEntityUpdateLog }
            STATUS obsolete
            DESCRIPTION 
                "Group for old objects that may be obsoleted."
            ::= { hwEntityExtGroups 4 }


        -- 1.3.6.1.4.1.2011.5.25.31.4.2.5
        hwOpticalModuleInfoGroup OBJECT-GROUP
            OBJECTS { hwEntityOpticalMode, hwEntityOpticalWaveLength, hwEntityOpticalTransDistance, hwEntityOpticalVendorSn, hwEntityOpticalTemperature, 
                hwEntityOpticalVoltage, hwEntityOpticalBiasCurrent, hwEntityOpticalRxPower, hwEntityOpticalTxPower, hwEntityOpticalType, 
                hwEntityOpticalTransBW, hwEntityOpticalFiberType, hwEntityOpticalRxLowThreshold, hwEntityOpticalRxHighThreshold, hwEntityOpticalTxLowThreshold, 
                hwEntityOpticalTxHighThreshold, hwEntityOpticalPlug, hwEntityOpticalDirectionType, hwEntityOpticalUserEeprom, hwEntityOpticalLaneBiasCurrent, 
				hwEntityOpticalLaneRxPower, hwEntityOpticalLaneTxPower, hwEntityOpticalVendorOUI, hwEntityOpticalVendorRev, hwEntityOpticalGponSN,
                hwEntityOpticalTransType,hwEntityOpticalConnectType,hwEntityOpticalOrderingName,hwEntityOpticalTransferDistance,hwEntityOpticalBandWidth,
				hwEntityOpticalWaveLengthExact,hwEntityOpticalModel,hwEntityOpticalManufacturedDate,hwEntityOpticalBiasLowThreshold,hwEntityOpticalBiasHighThreshold,hwEntityOpticalHuaweiCertified,
				hwEntityOpticalPortName,hwEntityOpticalDifferentialGroupDelay,hwEntityOpticalChromaticDispersion}
            STATUS current
            DESCRIPTION 
                "Collection of objects that display the fiber module working information."
            ::= { hwEntityExtGroups 5 }


        -- 1.3.6.1.4.1.2011.5.25.31.4.2.6
        hwMonitorInputGroup OBJECT-GROUP
            OBJECTS { hwMonitorInputName, hwMonitorInputState, hwMonitorInputStateEnable, hwMonitorInputRowStatus }
            STATUS current
            DESCRIPTION 
                "Standard HUAWEI Entity Extent group."
            ::= { hwEntityExtGroups 6 }


        -- 1.3.6.1.4.1.2011.5.25.31.4.2.7
        hwMonitorOutputGroup OBJECT-GROUP
            OBJECTS { hwMonitorOutputMask, hwMonitorOutputKey, hwMonitorOutputRowStatus }
            STATUS current
            DESCRIPTION 
                "Standard HUAWEI Entity Extent group."
            ::= { hwEntityExtGroups 7 }


        -- 1.3.6.1.4.1.2011.5.25.31.4.2.8
        hwEntPowerUsedInfoGroup OBJECT-GROUP
            OBJECTS { hwEntPowerUsedInfoBoardName, hwEntPowerUsedInfoBoardType, hwEntPowerUsedInfoBoardSlot, hwEntPowerUsedInfoPower }
            STATUS current
            DESCRIPTION 
                "Collection of objects that display the power informations of entity."
            ::= { hwEntityExtGroups 8 }


        -- 1.3.6.1.4.1.2011.5.25.31.4.2.9
        hwDevicePowerInfoGroup OBJECT-GROUP
            OBJECTS { hwDevicePowerInfoTotalPower, hwDevicePowerInfoUsedPower }
            STATUS current
            DESCRIPTION 
                "Collection of objects that display the power informations of device."
            ::= { hwEntityExtGroups 9 }


        -- 1.3.6.1.4.1.2011.5.25.31.4.2.10
        hwVirtualCableTestGroup OBJECT-GROUP
            OBJECTS { hwVirtualCableTestPairStatus, hwVirtualCableTestPairLength, hwVirtualCableTestOperation, hwVirtualCableTestLastTime,
                          hwVirtualCableTestPairAStatus,hwVirtualCableTestPairBStatus,hwVirtualCableTestPairCStatus,hwVirtualCableTestPairDStatus,
                          hwVirtualCableTestPairALength,hwVirtualCableTestPairBLength,hwVirtualCableTestPairCLength,hwVirtualCableTestPairDLength}
            STATUS current
            DESCRIPTION 
                "Collection of objects that display the status of cable."
            ::= { hwEntityExtGroups 10 }


        -- 1.3.6.1.4.1.2011.5.25.31.4.2.11
        hwTemperatureThresholdGroup OBJECT-GROUP
            OBJECTS { hwEntityTempSlotId, hwEntityTempI2CId, hwEntityTempAddr, hwEntityTempChannel, hwEntityTempStatus, 
                hwEntityTempValue, hwEntityTempMinorAlmThreshold, hwEntityTempMajorAlmThreshold, hwEntityTempFatalAlmThreshold }
            STATUS current
            DESCRIPTION 
                "Temperature threshold group."
            ::= { hwEntityExtGroups 11 }


        -- 1.3.6.1.4.1.2011.5.25.31.4.2.12
        hwVoltageInfoGroup OBJECT-GROUP
            OBJECTS { hwEntityVolSlot, hwEntityVolI2CId, hwEntityVolAddr, hwEntityVolChannel, hwEntityVolStatus, 
                hwEntityVolRequired, hwEntityVolLowAlmMajor, hwEntityVolLowAlmFatal, hwEntityVolHighAlmMajor, hwEntityVolHighAlmFatal, 
                hwEntityVolCurValue, hwEntityVolRatio }
            STATUS current
            DESCRIPTION 
                "Voltage info group."
            ::= { hwEntityExtGroups 12 }


        -- 1.3.6.1.4.1.2011.5.25.31.4.2.13
        hwFanStatusGroup OBJECT-GROUP
            OBJECTS { hwEntityFanSlot, hwEntityFanSn, hwEntityFanReg, hwEntityFanSpdAdjMode, hwEntityFanSpeed,hwEntityFanPresent,hwEntityFanState,hwEntityFanDesc,hwEntityFanName
                 }
            STATUS current
            DESCRIPTION 
                "fan state group."
            ::= { hwEntityExtGroups 13 }


        -- 1.3.6.1.4.1.2011.5.25.31.4.2.14
        hwPnpGroup OBJECT-GROUP
            OBJECTS { hwAlarmPnPSequenceNo, hwHardwareCapaSequenceNo, hwFileGeneIndex, hwFileGeneResourceType, hwFileGeneResourceID, hwFileGeneDestinationFile, 
                hwFileGeneOperState, hwFileGeneRowStatus, hwHardwareCapaChangeNotification, hwAlarmPnPChangeNotification }
            STATUS current
            DESCRIPTION 
                "Pnp group."
            ::= { hwEntityExtGroups 14 }


        -- 1.3.6.1.4.1.2011.5.25.31.4.2.15
        hwSystemGlobalGroup OBJECT-GROUP
            OBJECTS { hwEntitySystemNetID, hwEntitySoftwareName, hwEntitySoftwareVersion, hwEntitySoftwareVendor, hwEntitySystemModel, 
                hwEntitySystemTime, hwEntitySystemMacAddress, hwEntitySystemReset, hwEntitySystemHealthInterval, hwEntitySystemNEId, hwEntitySystemServiceType }
            STATUS current
            DESCRIPTION 
                "System global group."
            ::= { hwEntityExtGroups 15 }


        -- 1.3.6.1.4.1.2011.5.25.31.4.2.16
        hwHeartbeatGroup OBJECT-GROUP
            OBJECTS { hwEntityHeartbeatOnOff, hwEntityHeartbeatPeriod, hwEntityHeartbeatTrap }
            STATUS current
            DESCRIPTION 
                "Heart beat group."
            ::= { hwEntityExtGroups 16 }

        -- 1.3.6.1.4.1.2011.5.25.31.4.2.17
        hwPortBip8StatisticsObjectGroup OBJECT-GROUP
            OBJECTS{ hwPhysicalPortBip8StatisticsEB, hwPhysicalPortBip8StatisticsES, hwPhysicalPortBip8StatisticsSES,
                     hwPhysicalPortBip8StatisticsUAS, hwPhysicalPortBip8StatisticsBBE }
            STATUS current
            DESCRIPTION 
                "The BIP8 statistics group."
            ::= { hwEntityExtGroups 17 }

        -- 1.3.6.1.4.1.2011.5.25.31.4.2.18
        hwPredisposeGroup OBJECT-GROUP
            OBJECTS { hwPreDisposeSequenceNo, hwDisposeSlot, hwDisposeCardId, hwDisposeSbom,  
                hwDisposeRowStatus, hwDisposeOperState, hwDisposeEntPhysicalIndex, hwDisposeEntPhysicalDescr, hwDisposeEntPhysicalVendorType, 
                hwDisposeEntPhysicalContainedIn, hwDisposeEntPhysicalClass, hwDisposeEntPhysicalParentRelPos, hwDisposeEntPhysicalName, hwInsertDiffFromPreDisposed,
                hwPreDisposedChangeNotification }
            STATUS current
            DESCRIPTION 
                "Pnp group."
            ::= { hwEntityExtGroups 18 }

-- 1.3.6.1.4.1.2011.5.25.31.4.2.19
      hwSystemPowerGroup OBJECT-GROUP
           OBJECTS { hwSystemPowerDeviceID, hwSystemPowerTotalPower, hwSystemPowerUsedPower, hwSystemPowerRemainPower, hwSystemPowerReservedPower }
           STATUS current
          DESCRIPTION 
               "Description."
          ::= { hwEntityExtGroups 19 }

-- 1.3.6.1.4.1.2011.5.25.31.4.2.20
        hwX86BoardGroup NOTIFICATION-GROUP
            NOTIFICATIONS {hwEntityExtUnconnected , hwEntityExtUnconnectedResume  }
            STATUS current
            DESCRIPTION 
                "X86 group."
            ::= { hwEntityExtGroups 20 }

        -- 1.3.6.1.4.1.2011.5.25.31.4.2.21
        hwPwrStatusGroup OBJECT-GROUP
            OBJECTS { hwEntityPwrSlot, hwEntityPwrSn, hwEntityPwrReg, hwEntityPwrMode, hwEntityPwrPresent,hwEntityPwrState,hwEntityPwrCurrent,hwEntityPwrVoltage,hwEntityPwrDesc,hwEntityPwrPower
                 }
            STATUS current
            DESCRIPTION 
                "pwr state group."
            ::= { hwEntityExtGroups 21 } 
         
         -- 1.3.6.1.4.1.2011.5.25.31.4.2.22
        hwEntityCpuUsageHistoryGroup OBJECT-GROUP
            OBJECTS { hwCpuUsageHistoryIndex, hwCpuUsageHistoryTime, hwCpuUsageHistoryRate }
            STATUS current
            DESCRIPTION 
                "CPU usage histroy group."
            ::= { hwEntityExtGroups 22 }   
            
        -- 1.3.6.1.4.1.2011.5.25.31.4.2.23
        hwEntityMemUsageHistoryGroup OBJECT-GROUP
            OBJECTS { hwMemUsageHistoryIndex, hwMemUsageHistoryTime, hwMemUsageHistoryRate }
            STATUS current
            DESCRIPTION 
                "Memery usage histroy group."
            ::= { hwEntityExtGroups 23 }
            
            
        
        -- 1.3.6.1.4.1.2011.5.25.31.5
        hwPnpObjects OBJECT IDENTIFIER ::= { hwEntityExtentMIB 5 }


        -- 1.3.6.1.4.1.2011.5.25.31.5.1
        hwPnpInfo OBJECT IDENTIFIER ::= { hwPnpObjects 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.5.1.1
        hwHardwareCapaSequenceNo OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the sequence number of the 'hardware capability file'.The value consists of the file version number and CRC code."
            ::= { hwPnpInfo 1 }
			
		-- 1.3.6.1.4.1.2011.5.25.31.5.1.2
        hwAlarmPnPSequenceNo OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the sequence number of the 'alarm capability file'.The value consists of the file version number and CRC code."
            ::= { hwPnpInfo 2 }	


        -- 1.3.6.1.4.1.2011.5.25.31.5.2
        hwPnpTraps OBJECT IDENTIFIER ::= { hwPnpObjects 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.5.2.1
        hwHardwareCapaChangeNotification NOTIFICATION-TYPE
            OBJECTS { hwHardwareCapaSequenceNo }
            STATUS current
            DESCRIPTION 
                "This object indicates the change of the 'hardware capability file'. An alarm is generated if the sequence number of the 'hardware capability file' in the current startup file is different from that in the last startup file."
            ::= { hwPnpTraps 1 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.5.2.2
        hwAlarmPnPChangeNotification NOTIFICATION-TYPE
            OBJECTS { hwAlarmPnPSequenceNo }
            STATUS current
            DESCRIPTION 
                "This object indicates the change of the 'alarm capability file'. An alarm is generated if the sequence number of the 'alarm capability file' in the current startup file is different from that in the last startup file."
            ::= { hwPnpTraps 2 }
		

        -- 1.3.6.1.4.1.2011.5.25.31.5.3
        hwPnpOperateTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwPnpOperateEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table describes the hardware functions. Using this table, you can obtain the specified 'hardware description file' or 'hardware capability file'."
            ::= { hwPnpObjects 3 }


        -- 1.3.6.1.4.1.2011.5.25.31.5.3.1
        hwPnpOperateEntry OBJECT-TYPE
            SYNTAX HwPnpOperateEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION            " "
            INDEX { hwFileGeneIndex }
            ::= { hwPnpOperateTable 1 }


        HwPnpOperateEntry ::=
            SEQUENCE { 
                hwFileGeneIndex
                    Integer32,
                hwFileGeneOperState
                    INTEGER,
                hwFileGeneResourceType
                    INTEGER,
                hwFileGeneResourceID
                    SnmpAdminString,
                hwFileGeneDestinationFile
                    SnmpAdminString,
                hwFileGeneRowStatus
                    RowStatus
             }

        -- 1.3.6.1.4.1.2011.5.25.31.5.3.1.1
        hwFileGeneIndex OBJECT-TYPE
            SYNTAX Integer32 (1..2147483647)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the operation index, which can be specified by the user. 
                The value ranges from 1 to 2147483647."
            ::= { hwPnpOperateEntry 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.5.3.1.2
        hwFileGeneOperState OBJECT-TYPE
            SYNTAX INTEGER
                {
                opInProgress(1),
                opSuccess(2),
                opGetFileError(3),
                opInvalidDestName(4),
                opNoFlashSpace(5),
                opWriteFileError(6),
                opDestoryError(7)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the operation status.
                opInProgress(1): The operation is ongoing. 
                opSuccess(2): The operation succeeds. 
                opGetFileError(3): Obtaining the file fails. 
                opInvalidDestName(4): The specified storage path is invalid. 
                opNoFlashSpace(5): The space in the flash memory is insufficient. 
                opWriteFileError(6): Writing the file fails. 
                opDestoryError(7): Deleting the file fails."
            ::= { hwPnpOperateEntry 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.5.3.1.3
        hwFileGeneResourceType OBJECT-TYPE
            SYNTAX INTEGER
                {
                pnpcard(1),
                pnpsubcard(2),
                pnphardcapability(3),
                pnpPreDisposeCapability(4),
                pnpframe(5),
                pnpdevtype(6),
                pnpalarm(7) 
               }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the type of the file to be obtained.
                pnpcard(1): board description file
                pnpsubcard(2): subcard description file
                pnphardcapability(3): hardware capability file
                pnpPreDisposeCapability(4): predispose capability file
                pnpframe(5):frame description file
                pnpdevtype(6):device description file
                pnpalarm(7):alarm description file"
            ::= { hwPnpOperateEntry 3 }


        -- 1.3.6.1.4.1.2011.5.25.31.5.3.1.4
        hwFileGeneResourceID OBJECT-TYPE
            SYNTAX SnmpAdminString (SIZE (0..255))
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the ID of the 'hardware capability file' to be obtained."
            ::= { hwPnpOperateEntry 4 }


        -- 1.3.6.1.4.1.2011.5.25.31.5.3.1.5
        hwFileGeneDestinationFile OBJECT-TYPE
            SYNTAX SnmpAdminString (SIZE (0..255))
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the target path storing the file, which does not need to be specified."
            ::= { hwPnpOperateEntry 5 }


        -- 1.3.6.1.4.1.2011.5.25.31.5.3.1.6
        hwFileGeneRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the row status.
                active(1) 
                notInService(2) 
                notReady(3) 
                createAndGo(4) 
                createAndWait(5) 
                destroy(6)"
            ::= { hwPnpOperateEntry 6 }


        -- 1.3.6.1.4.1.2011.5.25.31.6
        hwSystemGlobalObjects OBJECT IDENTIFIER ::= { hwEntityExtentMIB 6 }


        -- 1.3.6.1.4.1.2011.5.25.31.6.1
        hwEntitySystemNetID OBJECT-TYPE
            SYNTAX OCTET STRING 
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "Network element ID."
            ::= { hwSystemGlobalObjects 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.6.2
        hwEntitySoftwareName OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "System software name."
            ::= { hwSystemGlobalObjects 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.6.3
        hwEntitySoftwareVersion OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Software version number. "
            ::= { hwSystemGlobalObjects 3 }


        -- 1.3.6.1.4.1.2011.5.25.31.6.4
        hwEntitySoftwareVendor OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Software vendor."
            ::= { hwSystemGlobalObjects 4 }


        -- 1.3.6.1.4.1.2011.5.25.31.6.5
        hwEntitySystemModel OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "Device model."
            ::= { hwSystemGlobalObjects 5 }


        -- 1.3.6.1.4.1.2011.5.25.31.6.6
        hwEntitySystemTime OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "System time displayed on the device."
            ::= { hwSystemGlobalObjects 6 }


        -- 1.3.6.1.4.1.2011.5.25.31.6.7
        hwEntitySystemMacAddress OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "MAC address of the device."
            ::= { hwSystemGlobalObjects 7 }


        -- 1.3.6.1.4.1.2011.5.25.31.6.8
        hwEntitySystemReset OBJECT-TYPE
            SYNTAX INTEGER
                {
                normal(1),
                restart(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "System reset."
            ::= { hwSystemGlobalObjects 8 }


        -- 1.3.6.1.4.1.2011.5.25.31.6.9
        hwEntitySystemHealthInterval OBJECT-TYPE
            SYNTAX Integer32 (5..900)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "Statistical interval for average CPU and memory usage, in seconds (By default, the value is 300) ."
            ::= { hwSystemGlobalObjects 9 }

        -- 1.3.6.1.4.1.2011.5.25.31.6.10
        hwEntitySystemNEId OBJECT-TYPE
            SYNTAX Integer32 (0..16777215)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the system NE ID."
            ::= { hwSystemGlobalObjects 10 }

        -- 1.3.6.1.4.1.2011.5.25.31.6.11
        hwEntitySystemServiceType OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the system service type."
            ::= { hwSystemGlobalObjects 11 }



        -- 1.3.6.1.4.1.2011.5.25.31.7
        hwHeartbeatObjects OBJECT IDENTIFIER ::= { hwEntityExtentMIB 7 }


        -- 1.3.6.1.4.1.2011.5.25.31.7.1
        hwHeartbeatConfig OBJECT IDENTIFIER ::= { hwHeartbeatObjects 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.7.1.1
        hwEntityHeartbeatOnOff OBJECT-TYPE
            SYNTAX INTEGER
                {
                on(1),
                off(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "Whether Heartbeat sending periodically enabled."
            ::= { hwHeartbeatConfig 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.7.1.2
        hwEntityHeartbeatPeriod OBJECT-TYPE
            SYNTAX Integer32 (60..86400)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "Heartbeat sending period detected in the trap reporting channel, with the minimum value of 60 seconds."
            ::= { hwHeartbeatConfig 2 }


        -- 1.3.6.1.4.1.2011.5.25.31.7.2
        hwHeartbeatTrapPrefix OBJECT IDENTIFIER ::= { hwHeartbeatObjects 2 }
       
        --1.3.6.1.4.1.2011.5.25.31.1.1.25
        hwCfcardStateInfo OBJECT IDENTIFIER ::= { hwEntityState 25 }

        -- 1.3.6.1.4.1.2011.5.25.31.7.2.1
        hwEntityHeartbeatTrap NOTIFICATION-TYPE
            STATUS current
            DESCRIPTION 
                "Heartbeat trap."
            ::= { hwHeartbeatTrapPrefix 1 }
 
       --1.3.6.1.4.1.2011.5.25.31.1.1.25.1
       hwHda1Error NOTIFICATION-TYPE
            STATUS current
            DESCRIPTION 
                "The file system in the hda1 directory has errors."
            ::= { hwCfcardStateInfo 1 }             

			
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.26
        hwLedConfigInfoPara OBJECT IDENTIFIER ::= { hwEntityState 26 }

		
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.26.1
        hwLedConfigStatus OBJECT-TYPE
                SYNTAX Integer32
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "Whether Led Off config enabled."
                ::= { hwLedConfigInfoPara 1 }

		
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.26.2
        hwLedTimeRangeName OBJECT-TYPE
                SYNTAX OCTET STRING (SIZE (0..32))
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "Led off time range name, if Led Off Time Range config enabled."
                ::= { hwLedConfigInfoPara 2 }

		
        --  1.3.6.1.4.1.2011.5.25.31.1.1.27
        hwUsbConfigInfoPara OBJECT IDENTIFIER ::= { hwEntityState 27 }

		
        --  1.3.6.1.4.1.2011.5.25.31.1.1.27.1
        hwUsbConfigStatus OBJECT-TYPE
                SYNTAX Integer32
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "Whether Usb Enable config enabled."
                ::= { hwUsbConfigInfoPara 1 }

        
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.28
        hwEntityNPStateTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwEntityNPStateEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                " A table of information that displays the forward performance usage       of entity ."
            ::= { hwEntityState 28 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.28.1
       hwEntityNPStateEntry OBJECT-TYPE
            SYNTAX HwEntityNPStateEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                " Entry of the table of information that displays the forward performance usage of entity."
            INDEX { entPhysicalIndex }
            ::= { hwEntityNPStateTable 1 }

        HwEntityNPStateEntry::=
            SEQUENCE { 
                hwEntityForwardPerformanceUsage
                    Integer32
             }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.28.1.1
        hwEntityForwardPerformanceUsage OBJECT-TYPE
            SYNTAX Integer32 (0..100)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                " The forward performance usage for this entity. "
            ::= { hwEntityNPStateEntry 1 }


		-- 1.3.6.1.4.1.2011.5.25.31.1.1.29
		hwUploadDiagnosticsTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwUploadDiagnosticsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table lists the info of upload diagnostics. You can read the info of the upload diagnostics on the device."
			::= { hwEntityState 29 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.29.1
		hwUploadDiagnosticsEntry OBJECT-TYPE
			SYNTAX HwUploadDiagnosticsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Defines an entry in the hwUploadDiagnosticsTable."
			INDEX { hwUploadDiagnosticsIndex }
			::= { hwUploadDiagnosticsTable 1 }

		
		HwUploadDiagnosticsEntry ::=
			SEQUENCE { 
				hwUploadDiagnosticsIndex
					Integer32,
				hwUploadDiagnosticsURL
					OCTET STRING,
				hwUploadDiagnosticsTransports
					Integer32,
				hwUploadDiagnosticsDSCP
					Integer32,
				hwUploadDiagnosticsTestFileSize
					Integer32,
				hwUploadDiagnosticsProgress
					Integer32,
				hwUploadDiagnosticsSpeed
					OCTET STRING,
				hwUploadDiagnosticsStatus
					OCTET STRING,
				hwUploadDiagnosticsRowStatus
					RowStatus
			 }

			 
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.29.1.1
		hwUploadDiagnosticsIndex OBJECT-TYPE
			SYNTAX Integer32 (1..2147483647)
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This object indicates the index of the upload diagnostics."
			::= { hwUploadDiagnosticsEntry 1 }


		-- 1.3.6.1.4.1.2011.5.25.31.1.1.29.1.2
		hwUploadDiagnosticsURL OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the URL of the upload diagnostics."
			::= { hwUploadDiagnosticsEntry 2 }


		-- 1.3.6.1.4.1.2011.5.25.31.1.1.29.1.3
		hwUploadDiagnosticsTransports OBJECT-TYPE
			SYNTAX Integer32 (0..65535)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the transports of the upload diagnostics."
			::= { hwUploadDiagnosticsEntry 3 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.29.1.4
		hwUploadDiagnosticsDSCP OBJECT-TYPE
			SYNTAX Integer32 (0..63)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the DSCP of the upload diagnostics."
			::= { hwUploadDiagnosticsEntry 4 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.29.1.5
		hwUploadDiagnosticsTestFileSize OBJECT-TYPE
			SYNTAX Integer32 (0..2147483647)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the test file size of the upload diagnostics."
			::= { hwUploadDiagnosticsEntry 5}

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.29.1.6
		hwUploadDiagnosticsProgress OBJECT-TYPE
			SYNTAX Integer32 (0..100)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the progress of the upload diagnostics."
			::= { hwUploadDiagnosticsEntry 6 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.29.1.7
		hwUploadDiagnosticsSpeed OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the speed of the upload diagnostics."
			::= { hwUploadDiagnosticsEntry 7 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.29.1.8
		hwUploadDiagnosticsStatus OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the status of the upload diagnostics."
			::= { hwUploadDiagnosticsEntry 8 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.29.1.9
		hwUploadDiagnosticsRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-create
			STATUS current
			DESCRIPTION
				"This object indicates the row status of the upload diagnostics."
			::= { hwUploadDiagnosticsEntry 9 }


		-- 1.3.6.1.4.1.2011.5.25.31.1.1.30
		hwDownloadDiagnosticsTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwDownloadDiagnosticsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table lists the info of download diagnostics. You can read the info of the download diagnostics on the device."
			::= { hwEntityState 30 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.30.1
		hwDownloadDiagnosticsEntry OBJECT-TYPE
			SYNTAX HwDownloadDiagnosticsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Defines an entry in the hwdownloadDiagnosticsTable."
			INDEX { hwDownloadDiagnosticsIndex }
			::= { hwDownloadDiagnosticsTable 1 }

		
		HwDownloadDiagnosticsEntry ::=
			SEQUENCE { 
				hwDownloadDiagnosticsIndex
					Integer32,
				hwDownloadDiagnosticsURL
					OCTET STRING,
				hwDownloadDiagnosticsTransports
					Integer32,
				hwDownloadDiagnosticsDSCP
					Integer32,
				hwDownloadDiagnosticsProgress
					Integer32,
				hwDownloadDiagnosticsSpeed
					OCTET STRING,
				hwDownloadDiagnosticsStatus
					OCTET STRING,
				hwDownloadDiagnosticsRowStatus
					RowStatus
			 }

			 
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.30.1.1
		hwDownloadDiagnosticsIndex OBJECT-TYPE
			SYNTAX Integer32 (1..2147483647)
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This object indicates the index of the download diagnostics."
			::= { hwDownloadDiagnosticsEntry 1 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.30.1.2
		hwDownloadDiagnosticsURL OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the URL of the download diagnostics."
			::= { hwDownloadDiagnosticsEntry 2 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.30.1.3
		hwDownloadDiagnosticsTransports OBJECT-TYPE
			SYNTAX Integer32 (0..65535)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the transports of the download diagnostics."
			::= { hwDownloadDiagnosticsEntry 3 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.30.1.4
		hwDownloadDiagnosticsDSCP OBJECT-TYPE
			SYNTAX Integer32 (0..63)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the DSCP of the download diagnostics."
			::= { hwDownloadDiagnosticsEntry 4 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.30.1.5
		hwDownloadDiagnosticsProgress OBJECT-TYPE
			SYNTAX Integer32 (0..100)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the progress of the download diagnostics."
			::= { hwDownloadDiagnosticsEntry 5 }


		-- 1.3.6.1.4.1.2011.5.25.31.1.1.30.1.6
		hwDownloadDiagnosticsSpeed OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the speed of the download diagnostics."
			::= { hwDownloadDiagnosticsEntry 6 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.30.1.7
		hwDownloadDiagnosticsStatus OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the status of the download diagnostics."
			::= { hwDownloadDiagnosticsEntry 7 }

		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.30.1.8
		hwDownloadDiagnosticsRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-create
			STATUS current
			DESCRIPTION
				"This object indicates the row status of the download diagnostics."
			::= { hwDownloadDiagnosticsEntry 8 }

		-- 1.3.6.1.4.1.2011.5.25.31.1.1.31
		hwIfBandRateTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwIfBandRateEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table lists the info of download diagnostics. You can read the info of the download diagnostics on the device."
			::= { hwEntityState 31 }

		-- 1.3.6.1.4.1.2011.5.25.31.1.1.31.1
		hwIfBandRateEntry OBJECT-TYPE
			SYNTAX HwIfBandRateEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Defines an entry in the hwdownloadDiagnosticsTable."
			INDEX { hwIfBandRateIndex }
			::= { hwIfBandRateTable 1 }

		HwIfBandRateEntry ::=
			SEQUENCE { 
				hwIfBandRateIndex
					Integer32,
				hwIfBandRateName
					OCTET STRING,
				hwIfBandRateInput
					Integer32,
				hwIfBandRateOutput
					Integer32
			 }

		-- 1.3.6.1.4.1.2011.5.25.31.1.1.31.1.1
		hwIfBandRateIndex OBJECT-TYPE
			SYNTAX Integer32 (1..2147483647)
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This object indicates the index of the interface."
			::= { hwIfBandRateEntry 1 }

		-- 1.3.6.1.4.1.2011.5.25.31.1.1.31.1.2
		hwIfBandRateName OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the name of the interface."
			::= { hwIfBandRateEntry 2 }

		-- 1.3.6.1.4.1.2011.5.25.31.1.1.31.1.3
		hwIfBandRateInput OBJECT-TYPE
			SYNTAX Integer32 (0..100)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the input bandwidth utilization of the interface."
			::= { hwIfBandRateEntry 3 }

		-- 1.3.6.1.4.1.2011.5.25.31.1.1.31.1.4
		hwIfBandRateOutput OBJECT-TYPE
			SYNTAX Integer32 (0..100)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the output bandwidth utilization of the interface."
			::= { hwIfBandRateEntry 4 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.32
        hwDacsStatusTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwDacsStatusEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table lists the status of DACS. You can read the status of the DACS on the device."
            ::= { hwEntityState 32 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.32.1
        hwDacsStatusEntry OBJECT-TYPE
            SYNTAX HwDacsStatusEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Defines an entry in the hwDacsStatusTable."
            INDEX { hwEntityDacsIndex }
            ::= { hwDacsStatusTable 1 }


        HwDacsStatusEntry ::=
            SEQUENCE { 
                hwEntityDacsIndex
                    Integer32,
                hwEntityDacsPresent
                    INTEGER,
                hwEntityDacsStatus
                    INTEGER,
                hwEntityDacsInSource
                    OCTET STRING,
                hwEntityDacsInVolA
                    Integer32,
                hwEntityDacsInVolB
                    Integer32,
                hwEntityDacsOutVol
                    Integer32,
                hwEntityDacsOutCur
                    Integer32,
                hwEntityDacsOutStatus
                    INTEGER,
                hwEntityDacsDesc
                    OCTET STRING
             }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.32.1.1
        hwEntityDacsIndex OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the index of a DACS."
            ::= { hwDacsStatusEntry 1 }


        -- 1.3.6.1.4.1.2011.5.25.31.1.1.32.1.2
        hwEntityDacsPresent OBJECT-TYPE
            SYNTAX INTEGER 
                {
                present(1),
                absent(2)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the present information of the DACS."
            ::= { hwDacsStatusEntry 2 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.32.1.3
        hwEntityDacsStatus OBJECT-TYPE
            SYNTAX INTEGER 
            {
                normal(1),
                abnormal(2)
            }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the status of the DACS."
            ::= { hwDacsStatusEntry 3 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.32.1.4
        hwEntityDacsInSource OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the input source of the DACS."
            ::= { hwDacsStatusEntry 4 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.32.1.5
        hwEntityDacsInVolA OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the input voltage from input source A. Unit: mV"
            ::= { hwDacsStatusEntry 5 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.32.1.6
        hwEntityDacsInVolB OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the input voltage from input source B. Unit: mV"
            ::= { hwDacsStatusEntry 6 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.32.1.7
        hwEntityDacsOutVol OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the output voltage of the DACS. Unit: mV"
            ::= { hwDacsStatusEntry 7 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.32.1.8
        hwEntityDacsOutCur OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the output current of the DACS. Unit: mA"
            ::= { hwDacsStatusEntry 8 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.32.1.9
        hwEntityDacsOutStatus OBJECT-TYPE
            SYNTAX INTEGER 
                {
                on(1),
                off(2)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the output status of the DACS."
            ::= { hwDacsStatusEntry 9 }

        -- 1.3.6.1.4.1.2011.5.25.31.1.1.32.1.10
        hwEntityDacsDesc OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the description of the DACS."
            ::= { hwDacsStatusEntry 10 }
			
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.33
		hwBoardDcOutputStateTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwBoardDcOutputStateEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { hwEntityState 33 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.33.1
		hwBoardDcOutputStateEntry OBJECT-TYPE
			SYNTAX HwBoardDcOutputStateEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { hwBoardDcOutputLineIndex }
			::= { hwBoardDcOutputStateTable 1 }
		
		HwBoardDcOutputStateEntry ::=
			SEQUENCE { 
				hwBoardDcOutputLineIndex
					Integer32,
				hwBoardDcOutputState
					EnabledStatus
			 }

--  1.3.6.1.4.1.2011.5.25.31.1.1.33.1.1
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.33.1.1
		hwBoardDcOutputLineIndex OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the index of device dc-output line. 
				0 indicates 12V-line1 dc-output line.
				1 indicates 12V-line2 dc-output line.
				2 indicates 24V dc-output line."
			::= { hwBoardDcOutputStateEntry 1 }
		
--  1.3.6.1.4.1.2011.5.25.31.1.1.33.1.2
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.33.1.2
		hwBoardDcOutputState OBJECT-TYPE
			SYNTAX EnabledStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the device dc-output line state."
			::= { hwBoardDcOutputStateEntry 2 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.34
		hwBoardDcOutputInfoTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwBoardDcOutputInfoEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { hwEntityState 34 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.34.1
		hwBoardDcOutputInfoEntry OBJECT-TYPE
			SYNTAX HwBoardDcOutputInfoEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { hwBoardDcOutputTypeIndex }
			::= { hwBoardDcOutputInfoTable 1 }
		
		HwBoardDcOutputInfoEntry ::=
			SEQUENCE { 
				hwBoardDcOutputTypeIndex
					Integer32,
				hwBoardDcOutputVoltage
					Integer32,
				hwBoardDcOutputCurrent
					Integer32,
				hwBoardDcOutputPower
					Integer32
			 }

--  1.3.6.1.4.1.2011.5.25.31.1.1.34.1.1
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.34.1.1
		hwBoardDcOutputTypeIndex OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the index of device dc-output information. 
				0 indicates 12V dc-output line information.
				1 indicates 24V dc-output line information."
			::= { hwBoardDcOutputInfoEntry 1 }
		
--  1.3.6.1.4.1.2011.5.25.31.1.1.34.1.2
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.34.1.2
		hwBoardDcOutputVoltage OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the device dc-output voltage. Unit: V"
			::= { hwBoardDcOutputInfoEntry 2 }
		
--  1.3.6.1.4.1.2011.5.25.31.1.1.34.1.3
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.34.1.3
		hwBoardDcOutputCurrent OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the device dc-output current. Unit: mA"
			::= { hwBoardDcOutputInfoEntry 3 }
		
--  1.3.6.1.4.1.2011.5.25.31.1.1.34.1.4
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.34.1.4
		hwBoardDcOutputPower OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the device dc-output power. Unit: mW"
			::= { hwBoardDcOutputInfoEntry 4 }
		

                                       -- 1.3.6.1.4.1.2011.5.25.31.1.1.35
		hwBoardAcOutputStateTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwBoardAcOutputStateEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { hwEntityState 35 }
		

		-- 1.3.6.1.4.1.2011.5.25.31.1.1.35.1
		hwBoardAcOutputStateEntry OBJECT-TYPE
			SYNTAX HwBoardAcOutputStateEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { hwBoardAcOutputLineIndex }
			::= { hwBoardAcOutputStateTable 1 }
		
		HwBoardAcOutputStateEntry ::=
			SEQUENCE { 
				hwBoardAcOutputLineIndex
					Integer32,
				hwBoardAcOutputState
					OCTET STRING
			 }

--  1.3.6.1.4.1.2011.5.25.31.1.1.35.1.1
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.35.1.1
		hwBoardAcOutputLineIndex OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description."
			::= { hwBoardAcOutputStateEntry 1 }
		
--  1.3.6.1.4.1.2011.5.25.31.1.1.35.1.2
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.35.1.2
		hwBoardAcOutputState OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the device ac-output line state. 
				1 indicates ac-output 24V enable.
				2 indicates ac-output 24V disable."
			::= { hwBoardAcOutputStateEntry 2 }
			
-- 1.3.6.1.4.1.2011.5.25.31.1.1.36
		hwAlarmConfigTable OBJECT IDENTIFIER ::= { hwEntityState 36 }
		
		-- 1.3.6.1.4.1.2011.5.25.31.1.1.36.1
		hwAlarmResendInterval OBJECT-TYPE
			SYNTAX Integer32 (0..65535)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				" set alarm  resend interval,the defult is 10 minutes."
			::= { hwAlarmConfigTable 1 }

    -- 1.3.6.1.4.1.2011.5.25.31.1.1.37
        hwApInfoTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwApInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table describes virtual-access AP device information."
            ::= { hwEntityState 37 }
    
        -- 1.3.6.1.4.1.2011.5.25.31.1.1.37.1
        hwApInfoEntry OBJECT-TYPE
            SYNTAX HwApInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Information about an AP device. Each entry provides objects of an AP device to help an NMS identify and characterize the entry in this table."
            INDEX { hwEntityApid, hwEntityApIndex }
            ::= { hwApInfoTable 1 }
            
        HwApInfoEntry ::=
            SEQUENCE { 
                hwEntityApid
                    Integer32,
                hwEntityApIndex
                    PhysicalIndex,
                hwEntityApName
                    SnmpAdminString,
                hwEntityApMemUsage
                    Integer32,
                hwEntityApCpuUsage
                    Integer32
             }

        --  1.3.6.1.4.1.2011.5.25.31.1.1.37.1.1
        hwEntityApid OBJECT-TYPE
                SYNTAX Integer32 (1024..8191)
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                    "Ap-id of the virtual-access AP."
                ::= { hwApInfoEntry 1 }
                
        --  1.3.6.1.4.1.2011.5.25.31.1.1.37.1.2
        hwEntityApIndex OBJECT-TYPE
                SYNTAX PhysicalIndex
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                    "The index for this entry."
                ::= { hwApInfoEntry 2 }
                
        --  1.3.6.1.4.1.2011.5.25.31.1.1.37.1.3
        hwEntityApName OBJECT-TYPE
                SYNTAX SnmpAdminString
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                    "The textual name of the physical entity."
                ::= { hwApInfoEntry 3 }
                
        --  1.3.6.1.4.1.2011.5.25.31.1.1.37.1.4
        hwEntityApMemUsage OBJECT-TYPE
                SYNTAX Integer32 (0..100)
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                    "This object indicates the memory usage of an entity, that is, the percentage of the memory that has been used."
                ::= { hwApInfoEntry 4 }

        --  1.3.6.1.4.1.2011.5.25.31.1.1.37.1.5
        hwEntityApCpuUsage OBJECT-TYPE
                SYNTAX Integer32 (0..100)
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                    "This object indicates the CPU usage of an entity. Generally, the overall CPU usage of the entity is calculated, without considering the number of CPUs on the entity."
                ::= { hwApInfoEntry 5 }

-- 1.3.6.1.4.1.2011.5.25.31.1.1.38
        hwIntegratedPowerSystemTable OBJECT-TYPE
                SYNTAX SEQUENCE OF HwIntegratedPowerSystemEntry
                MAX-ACCESS not-accessible
                STATUS current
                DESCRIPTION
                    "This table describes information about the integrated power supply system."
                ::= { hwEntityState 38 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.38.1
        hwIntegratedPowerSystemEntry OBJECT-TYPE
                SYNTAX HwIntegratedPowerSystemEntry
                MAX-ACCESS not-accessible
                STATUS current
                DESCRIPTION
	"This entry describes information about the integrated power supply system."
                INDEX { entPhysicalIndex }
                ::= { hwIntegratedPowerSystemTable 1 }
		
                HwIntegratedPowerSystemEntry ::=
                SEQUENCE { 
                    hwIntegratedPowerSoftwareVersion
	     OCTET STRING,
	 hwIntegratedPowerHardwareVersion
	     OCTET STRING,
         hwIntegratedPowerSoftwareVersionASCII
		OCTET STRING
	 }

-- 1.3.6.1.4.1.2011.5.25.31.1.1.38.1.1
        hwIntegratedPowerSoftwareVersion OBJECT-TYPE
                SYNTAX OCTET STRING
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                    "This object indicates the software version."
                ::= { hwIntegratedPowerSystemEntry 1 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.38.1.2
        hwIntegratedPowerHardwareVersion OBJECT-TYPE
                SYNTAX OCTET STRING
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                    "This object indicates the hardware version."
                ::= { hwIntegratedPowerSystemEntry 2 }

-- 1.3.6.1.4.1.2011.5.25.31.1.1.38.1.3
		hwIntegratedPowerSoftwareVersionASCII OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the software version (ASCII)."
			::= { hwIntegratedPowerSystemEntry 3 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.39
        hwIntegratedPowerTable OBJECT-TYPE
                SYNTAX SEQUENCE OF HwIntegratedPowerEntry
                MAX-ACCESS not-accessible
                STATUS current
                DESCRIPTION
                    "This table describes information about the integrated power supply."
                ::= { hwEntityState 39 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1
        hwIntegratedPowerEntry OBJECT-TYPE
                SYNTAX HwIntegratedPowerEntry
                MAX-ACCESS not-accessible
                STATUS current
                DESCRIPTION
                    "This entry describes information about the integrated power supply."
                INDEX { entPhysicalIndex }
                ::= { hwIntegratedPowerTable 1 }
		
                HwIntegratedPowerEntry ::=
                        SEQUENCE { 
	         hwIntegratedPowerEnergyWorkmode
                                    INTEGER,
	         hwIntegratedPowerTotalInputPower
	                 Integer32,
	         hwIntegratedPower12VDCOutVoltStatus
	                 INTEGER,
	         hwIntegratedPower24VACOutVolt
	                 Integer32,
	         hwIntegratedPower24VACOutCurrent
	                 Integer32,
	         hwIntegratedPower53VDCOutVoltStatus
	                 INTEGER,
	         hwIntegratedPowerACInputVoltStatus
	                 INTEGER,
			 hwIntegratedPowerRebootPower
	                 INTEGER,
                hwIntegratedPowerCurrentMode
			INTEGER,
		hwIntegratedPowerBusbarVolt
			Integer32,
		hwIntegratedPowerACVolt
			Integer32,
		hwIntegratedPowerSolarInputVolt
			Integer32,
		hwIntegratedPowerSolarInputCurrent
			Integer32,
		hwIntegratedPower53VDCOutVolt
			Integer32,
		hwIntegratedPowerTotalLoadPower
			Integer32,
		hwIntegratedPowerDCOverVoltThreshold
			Integer32,
		hwIntegratedPowerDCUnderVoltThreshold
			Integer32,
		hwIntegratedPowerLowLoadVoltPowerOffThreshold
			Integer32,
		hwIntegratedPower53VDCOutVoltLowerThreshold
			Integer32,
		hwIntegratedPowerACCurrent
			Integer32,
		hwIntegratedPower53VDCOutCurrent
	        Integer32,
		hwIntegratedPwrChip1UpgrageStatus
	        INTEGER,
		hwIntegratedPwrChip2UpgrageStatus
	        INTEGER,
		hwIntegratedPwrChip3UpgrageStatus
	        INTEGER,
		hwIntegratedPwrChip4UpgrageStatus
	        INTEGER,
	    hwIntegratedPowerResetOutput
	        INTEGER
                        }

-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.1
        hwIntegratedPowerEnergyWorkmode OBJECT-TYPE
                SYNTAX INTEGER
                {
                    hybridPower500(0),
	            mainsPower500(1),
                    hybridPower500B(2)
                }
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                    "This object indicates the power supply mode."
                ::= { hwIntegratedPowerEntry 1 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.2
        hwIntegratedPowerTotalInputPower OBJECT-TYPE
                SYNTAX Integer32
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                    "This object indicates the total input power, in mW."
                ::= { hwIntegratedPowerEntry 2 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.3
        hwIntegratedPower12VDCOutVoltStatus OBJECT-TYPE
                SYNTAX INTEGER
                {
                    normal(0),
	 abnormal(1)
                }
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                    "This object indicates the 12 V DC output voltage status."
                ::= { hwIntegratedPowerEntry 3 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.4
        hwIntegratedPower24VACOutVolt OBJECT-TYPE
                SYNTAX Integer32
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                    "This object indicates the 24 V AC output voltage, in mV."
                ::= { hwIntegratedPowerEntry 4 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.5
        hwIntegratedPower24VACOutCurrent OBJECT-TYPE
                SYNTAX Integer32
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                    "This object indicates the 24 V AC output current, in mA."
                ::= { hwIntegratedPowerEntry 5 }

-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.6
        hwIntegratedPower53VDCOutVoltStatus OBJECT-TYPE
                SYNTAX INTEGER
                {
                    normal(0),
	 abnormal(1)
                }
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                    "This object indicates the 53 V DC output voltage status."
                ::= { hwIntegratedPowerEntry 6 }

-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.7
        hwIntegratedPowerACInputVoltStatus OBJECT-TYPE
                SYNTAX INTEGER
                {
                    normal(0),
	 abnormal(1)
                }
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                    "This object indicates the AC input voltage status."
                ::= { hwIntegratedPowerEntry 7 }

-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.8
        hwIntegratedPowerRebootPower OBJECT-TYPE
                SYNTAX INTEGER
                {
                    reset(1)
                }
                MAX-ACCESS read-write
                STATUS current
                DESCRIPTION
                    "This object is used to reset a switch remotely."
                ::= { hwIntegratedPowerEntry 8 }

-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.9
		hwIntegratedPowerCurrentMode OBJECT-TYPE
			SYNTAX INTEGER
				{
				solar(0),
				solarAndMains(1),
				solarAndBattery(2),
				mains(3),
				battery(4)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the current power supply mode."
			::= { hwIntegratedPowerEntry 9 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.10
		hwIntegratedPowerBusbarVolt OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the busbar voltage, in mV."
			::= { hwIntegratedPowerEntry 10 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.11
		hwIntegratedPowerACVolt OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the AC voltage, in mV."
			::= { hwIntegratedPowerEntry 11 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.12
		hwIntegratedPowerSolarInputVolt OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the input voltage of solar power, in mV."
			::= { hwIntegratedPowerEntry 12 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.13
		hwIntegratedPowerSolarInputCurrent OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the input current of solar power, in mA."
			::= { hwIntegratedPowerEntry 13 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.14
		hwIntegratedPower53VDCOutVolt OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the 53 V DC output voltage, in mV."
			::= { hwIntegratedPowerEntry 14 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.15
		hwIntegratedPowerTotalLoadPower OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the total load power, in mW."
			::= { hwIntegratedPowerEntry 15 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.16
		hwIntegratedPowerDCOverVoltThreshold OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the DC overvoltage alarm threshold, in mV."
			::= { hwIntegratedPowerEntry 16 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.17
		hwIntegratedPowerDCUnderVoltThreshold OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the DC undervoltage alarm threshold, in mV."
			::= { hwIntegratedPowerEntry 17 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.18
		hwIntegratedPowerLowLoadVoltPowerOffThreshold OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the voltage lower than which the device is powered off, in mV."
			::= { hwIntegratedPowerEntry 18 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.19
		hwIntegratedPower53VDCOutVoltLowerThreshold OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the lower voltage threshold for the 53 V DC output, in mV."
			::= { hwIntegratedPowerEntry 19 }
			
-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.20
		hwIntegratedPowerACCurrent OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the AC current, in mA."
			::= { hwIntegratedPowerEntry 20 }
			
-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.21
		hwIntegratedPower53VDCOutCurrent OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the lower current threshold for the 53 V DC output, in mA."
			::= { hwIntegratedPowerEntry 21 }
			
-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.22
        hwIntegratedPwrChip1UpgrageStatus OBJECT-TYPE
                SYNTAX INTEGER
                {
                    normal(0),
	 abnormal(1)
                }
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                    "This object indicates the power chip 1 upgrage status."
                ::= { hwIntegratedPowerEntry 22 }

-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.23
        hwIntegratedPwrChip2UpgrageStatus OBJECT-TYPE
                SYNTAX INTEGER
                {
                    normal(0),
	 abnormalpsu(1),
	 abnormalcur(2)
                }
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                    "This object indicates the power chip 2 upgrage status."
                ::= { hwIntegratedPowerEntry 23 }

-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.24
        hwIntegratedPwrChip3UpgrageStatus OBJECT-TYPE
                SYNTAX INTEGER
                {
                    normal(0),
	 abnormal(1)
                }
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                    "This object indicates the power chip 3 upgrage status."
                ::= { hwIntegratedPowerEntry 24 }

-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.25
        hwIntegratedPwrChip4UpgrageStatus OBJECT-TYPE
                SYNTAX INTEGER
                {
                    normal(0),
	 abnormal(1)
                }
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                    "This object indicates the power chip 4 upgrage status."
                ::= { hwIntegratedPowerEntry 25 }

-- 1.3.6.1.4.1.2011.5.25.31.1.1.39.1.26
        hwIntegratedPowerResetOutput OBJECT-TYPE
                SYNTAX INTEGER
                {
                    normal(0),
                    reset(1)
                }
                MAX-ACCESS read-write
                STATUS current
                DESCRIPTION
                    "This object is used to reset power output."
                ::= { hwIntegratedPowerEntry 26 }
				
-- 1.3.6.1.4.1.2011.5.25.31.1.1.40
		hwLithiumBatteryGroupTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwLithiumBatteryGroupEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table describes information about lithium battery groups."
			::= { hwEntityState 40 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.40.1
		hwLithiumBatteryGroupEntry OBJECT-TYPE
			SYNTAX HwLithiumBatteryGroupEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This entry describes information about lithium battery groups."
			INDEX { entPhysicalIndex }
			::= { hwLithiumBatteryGroupTable 1 }
		
		HwLithiumBatteryGroupEntry ::=
			SEQUENCE { 
				hwBatteryGroupBatteryStatus
					INTEGER,
				hwBatteryGroupBatteryVolt
					Integer32,
				hwBatteryGroupBatteryCurrent
					Integer32,
				hwBatteryGroupTotalBatteryCapacity
					Integer32,
				hwBatteryGroupAvailableBatteryCapacity
					OCTET STRING,
				hwBatteryGroupBatteryTemperature
					OCTET STRING,
				hwBatteryGroupBatteryRunTime
					OCTET STRING,
				hwBatteryGroupNumberOfConnectedESMU 
					Integer32,
				hwBatteryGroupChargeCurrentLimitCoefficient
					OCTET STRING,
				hwBatteryGroupFloatChargingVolt
					Integer32,
				hwBatteryGroupEqualizedChargingVolt
	                                Integer32,
				hwBatteryGroupInstallTimeYear
					Integer32,
				hwBatteryGroupInstallTimeMonth
					Integer32,
				hwBatteryGroupInstallTimeDay
					Integer32
			 }

-- 1.3.6.1.4.1.2011.5.25.31.1.1.40.1.1
		hwBatteryGroupBatteryStatus OBJECT-TYPE
			SYNTAX INTEGER
				{
				firstPowerOn(0),
				powerOff(1),
				floatCharging(2),
				equalizedCharging(3),
				discharging(4)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the battery status."
			::= { hwLithiumBatteryGroupEntry 1 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.40.1.2
		hwBatteryGroupBatteryVolt OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the battery voltage, in mV."
			::= { hwLithiumBatteryGroupEntry 2 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.40.1.3
		hwBatteryGroupBatteryCurrent OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the battery current, in mA."
			::= { hwLithiumBatteryGroupEntry 3 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.40.1.4
		hwBatteryGroupTotalBatteryCapacity OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the total battery capacity, in Ah."
			::= { hwLithiumBatteryGroupEntry 4 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.40.1.5
		hwBatteryGroupAvailableBatteryCapacity OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the available battery capacity, in percentage."
			::= { hwLithiumBatteryGroupEntry 5 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.40.1.6
		hwBatteryGroupBatteryTemperature OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the battery temperature, in degC."
			::= { hwLithiumBatteryGroupEntry 6 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.40.1.7
		hwBatteryGroupBatteryRunTime OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the battery run time, in hours."
			::= { hwLithiumBatteryGroupEntry 7 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.40.1.8
		hwBatteryGroupNumberOfConnectedESMU  OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the number of connected ESMUs."
			::= { hwLithiumBatteryGroupEntry 8 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.40.1.9
		hwBatteryGroupChargeCurrentLimitCoefficient OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the charge current limit coefficient, in C10."
			::= { hwLithiumBatteryGroupEntry 9 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.40.1.10
		hwBatteryGroupFloatChargingVolt OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the float charging voltage, in mV."
			::= { hwLithiumBatteryGroupEntry 10 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.40.1.11
		hwBatteryGroupEqualizedChargingVolt OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the equalized charging voltage, in mV."
			::= { hwLithiumBatteryGroupEntry 11 }

-- 1.3.6.1.4.1.2011.5.25.31.1.1.40.1.12
		hwBatteryGroupInstallTimeYear OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the battery install time year."
			::= { hwLithiumBatteryGroupEntry 12 }
			
-- 1.3.6.1.4.1.2011.5.25.31.1.1.40.1.13
		hwBatteryGroupInstallTimeMonth OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the battery install time month."
			::= { hwLithiumBatteryGroupEntry 13 }
			
-- 1.3.6.1.4.1.2011.5.25.31.1.1.40.1.14
		hwBatteryGroupInstallTimeDay OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"This object indicates the battery install time day."
			::= { hwLithiumBatteryGroupEntry 14 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.41
		hwLithiumBatteryTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwLithiumBatteryEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table describes information about a single lithium battery."
			::= { hwEntityState 41 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.41.1
		hwLithiumBatteryEntry OBJECT-TYPE
			SYNTAX HwLithiumBatteryEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This entry describes information about a single lithium battery."
			INDEX { entPhysicalIndex }
			::= { hwLithiumBatteryTable 1 }
		
		HwLithiumBatteryEntry ::=
			SEQUENCE { 
				hwLithiumBatteryIndex
					Integer32,
				hwLithiumBatteryVolt
					Integer32,
				hwLithiumBatteryCurrent
					Integer32,
				hwLithiumBatteryDeviceAddr
					Integer32,
				hwLithiumBatteryStatus
					INTEGER,
				hwLithiumBatterySOH
					OCTET STRING,
				hwLithiumBatteryCapacity
					Integer32,
				hwLithiumBatteryCellPackageVolt
					Integer32,
				hwLithiumBatteryMaxLimitCoefficient
					OCTET STRING,
				hwLithiumBatteryVersion
					OCTET STRING
			 }

-- 1.3.6.1.4.1.2011.5.25.31.1.1.41.1.1
		hwLithiumBatteryIndex OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the battery index."
			::= { hwLithiumBatteryEntry 1 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.41.1.2
		hwLithiumBatteryVolt OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the battery voltage, in mV."
			::= { hwLithiumBatteryEntry 2 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.41.1.3
		hwLithiumBatteryCurrent OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the battery current, in mA."
			::= { hwLithiumBatteryEntry 3 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.41.1.4
		hwLithiumBatteryDeviceAddr OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the device address."
			::= { hwLithiumBatteryEntry 4 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.41.1.5
		hwLithiumBatteryStatus OBJECT-TYPE
			SYNTAX INTEGER
				{
				offline(0),
				online(1),
				hibernation(2),
				disconnected(3),
				charge(4),
				discharging(5)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the battery status."
			::= { hwLithiumBatteryEntry 5 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.41.1.6
		hwLithiumBatterySOH OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the battery SOH, in percentage."
			::= { hwLithiumBatteryEntry 6 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.41.1.7
		hwLithiumBatteryCapacity OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the battery capacity, in Ah."
			::= { hwLithiumBatteryEntry 7 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.41.1.8
		hwLithiumBatteryCellPackageVolt OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the electrochemical cell package voltage, in mV."
			::= { hwLithiumBatteryEntry 8 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.41.1.9
		hwLithiumBatteryMaxLimitCoefficient OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the maximum allowable current limiting coefficient, in C10."
			::= { hwLithiumBatteryEntry 9 }

-- 1.3.6.1.4.1.2011.5.25.31.1.1.41.1.10
		hwLithiumBatteryVersion OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the battery version."
			::= { hwLithiumBatteryEntry 10}
			
-- 1.3.6.1.4.1.2011.5.25.31.1.1.42
		hwBatteryChipTable OBJECT-TYPE
			SYNTAX SEQUENCE OF HwBatteryChipEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This table describes information about a single battery chip."
			::= { hwEntityState 42 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.42.1
		hwBatteryChipEntry OBJECT-TYPE
			SYNTAX HwBatteryChipEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"This entry describes information about a single battery chip."
			INDEX { entPhysicalIndex }
			::= { hwBatteryChipTable 1 }
		
		HwBatteryChipEntry ::=
			SEQUENCE { 
				hwBatteryChipVolt
					Integer32,
				hwBatteryChipTemp
					OCTET STRING
			 }

-- 1.3.6.1.4.1.2011.5.25.31.1.1.42.1.1
		hwBatteryChipVolt OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the battery chip voltage, in mv."
			::= { hwBatteryChipEntry 1 }
		
-- 1.3.6.1.4.1.2011.5.25.31.1.1.42.1.2
		hwBatteryChipTemp OBJECT-TYPE
			SYNTAX OCTET STRING
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"This object indicates the battery chip temperature, in degC."
			::= { hwBatteryChipEntry 2 }
	
        -- 1.3.6.1.4.1.2011.5.25.31.8

        hwPreDisposeObjects OBJECT IDENTIFIER ::= { hwEntityExtentMIB 8 }

        -- 1.3.6.1.4.1.2011.5.25.31.8.1
        hwPreDisposeInfo OBJECT IDENTIFIER ::= { hwPreDisposeObjects 1 }
        
        -- 1.3.6.1.4.1.2011.5.25.31.8.1.1
        hwPreDisposeSequenceNo OBJECT-TYPE
            SYNTAX SnmpAdminString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the sequence number of the 'predispose capability file'.The value consists of the file version number and CRC code."
            ::= { hwPreDisposeInfo 1 }
        
        -- 1.3.6.1.4.1.2011.5.25.31.8.2
        hwPreDisposedTraps OBJECT IDENTIFIER ::= { hwPreDisposeObjects 2 }
        
        -- 1.3.6.1.4.1.2011.5.25.31.8.2.1
        hwInsertDiffFromPreDisposed NOTIFICATION-TYPE
            OBJECTS { hwDisposeEntPhysicalIndex, hwDisposeEntPhysicalVendorType, entPhysicalVendorType }
            STATUS current
            DESCRIPTION 
                "This object indicates the type of the inserted entity is different from that of pre-disposed entity on the slot."
            ::= { hwPreDisposedTraps 1 } 
            
        -- 1.3.6.1.4.1.2011.5.25.31.8.2.2
        hwPreDisposedChangeNotification NOTIFICATION-TYPE
            OBJECTS { hwPreDisposeSequenceNo }
            STATUS current
            DESCRIPTION 
                "This object indicates the change of the 'predispose capability file'. An alarm is generated if the sequence number of the 'predispose capability file' in the current startup file is different from that in the last startup file."
            ::= { hwPreDisposedTraps 2 }     

    -- 1.3.6.1.4.1.2011.5.25.31.8.3
        hwPreDisposeConfigTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwPreDisposeConfigEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Table of predisposing boards or flexible subcards."
            ::= { hwPreDisposeObjects 3 }
            
        -- 1.3.6.1.4.1.2011.5.25.31.8.3.1
        hwPreDisposeConfigEntry OBJECT-TYPE
            SYNTAX HwPreDisposeConfigEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Entry of the table to predispose boards or flexible subcards."                
            INDEX { hwDisposeSlot, hwDisposeCardId }
            ::= { hwPreDisposeConfigTable 1 } 
            
    HwPreDisposeConfigEntry ::=
            SEQUENCE { 
                hwDisposeSlot
                    Integer32,
                hwDisposeCardId
                    Integer32,
                hwDisposeSbom
                    OCTET STRING,
                hwDisposeRowStatus
                    RowStatus,
                hwDisposeOperState
                    INTEGER                                    
             }                  
        
        -- 1.3.6.1.4.1.2011.5.25.31.8.3.1.1
        hwDisposeSlot OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the slot ID of predisposed board. "
            ::= { hwPreDisposeConfigEntry 1 }           
            
        -- 1.3.6.1.4.1.2011.5.25.31.8.3.1.2
        hwDisposeCardId OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the card ID of predisposed subcard. "
            ::= { hwPreDisposeConfigEntry 2 }
            
        -- 1.3.6.1.4.1.2011.5.25.31.8.3.1.3
        hwDisposeSbom OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object indicates the sbom information of predisposed board or subcard. "
            ::= { hwPreDisposeConfigEntry 3 }
            
        -- 1.3.6.1.4.1.2011.5.25.31.8.3.1.4
        hwDisposeRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the row status when config predispose.
                active(1) 
                notInService(2) 
                notReady(3) 
                createAndGo(4) 
                createAndWait(5) 
                destroy(6)"
            ::= { hwPreDisposeConfigEntry 4 }  
            
        -- 1.3.6.1.4.1.2011.5.25.31.8.3.1.5
        hwDisposeOperState OBJECT-TYPE
            SYNTAX INTEGER
                {
                opSuccess(1),
                opInProgress(2),
                opDevNotSupportPredispose(3),
                opCardNotSupportPredispose(4),
                opAlreadyPredispose(5),
                opCardConflict(6),
                opDevOperationError(7)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of this object identifies the operation status.
                opSuccess(1): The operation succeeds.
                opInProgress(2): The operation is ongoing.  
                opDevNotSupportPredispose(3): The device does not support predispose. 
                opCardNotSupportPredispose(4): The type of card or subcard is not supported to be predisposed on this device. 
                opAlreadyPredispose(5): The slot or subslot has already been predisposed. 
                opCardConflict(6): The slot or subslot to be predisposed conflict with others. 
                opDevOperationError(7): Other error occurs on the device."
            ::= { hwPreDisposeConfigEntry 5 }     
            
        -- 1.3.6.1.4.1.2011.5.25.31.8.4
        hwPreDisposeEntInfoTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwPreDisposeEntInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This table is used to get the information of predisposed entitys."
            ::= { hwPreDisposeObjects 4 }
            
        -- 1.3.6.1.4.1.2011.5.25.31.8.4.1
        hwPreDisposeEntInfoEntry OBJECT-TYPE
            SYNTAX HwPreDisposeEntInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Entry of the table to get the information of predisposed entitys."                
            INDEX { hwDisposeEntPhysicalIndex }
            ::= { hwPreDisposeEntInfoTable 1 } 
            
    HwPreDisposeEntInfoEntry ::=
            SEQUENCE { 
                hwDisposeEntPhysicalIndex            PhysicalIndex,
                hwDisposeEntPhysicalDescr            SnmpAdminString,
                hwDisposeEntPhysicalVendorType       AutonomousType,
                hwDisposeEntPhysicalContainedIn      Integer32,
                hwDisposeEntPhysicalClass            PhysicalClass,
                hwDisposeEntPhysicalParentRelPos     Integer32,
                hwDisposeEntPhysicalName             SnmpAdminString                
             }
        
        -- 1.3.6.1.4.1.2011.5.25.31.8.4.1.1     
        hwDisposeEntPhysicalIndex    OBJECT-TYPE
           SYNTAX      PhysicalIndex
           MAX-ACCESS  accessible-for-notify
           STATUS      current
           DESCRIPTION
               "The index for this entry."
           ::= { hwPreDisposeEntInfoEntry 1 }
        
        -- 1.3.6.1.4.1.2011.5.25.31.8.4.1.2
        hwDisposeEntPhysicalDescr OBJECT-TYPE
           SYNTAX      SnmpAdminString
           MAX-ACCESS  read-only
           STATUS      current
           DESCRIPTION
               "A textual description of predisposed physical entity.This object
               should contain a string which identifies the manufacturer's
               name for the physical entity. "
           ::= { hwPreDisposeEntInfoEntry 2 }
        
        -- 1.3.6.1.4.1.2011.5.25.31.8.4.1.3
        hwDisposeEntPhysicalVendorType OBJECT-TYPE
           SYNTAX      AutonomousType
           MAX-ACCESS  read-only
           STATUS      current
           DESCRIPTION
               "An indication of the vendor-specific hardware type of the
               predisposed physical entity.       
               "
           ::= { hwPreDisposeEntInfoEntry 3 }
        
        -- 1.3.6.1.4.1.2011.5.25.31.8.4.1.4
        hwDisposeEntPhysicalContainedIn OBJECT-TYPE
           SYNTAX      Integer32 (0..2147483647)
           MAX-ACCESS  read-only
           STATUS      current
           DESCRIPTION
               "The value of 'entPhysicalContainedIn' for the predisposed physical entity."
           ::= { hwPreDisposeEntInfoEntry 4 }
        
        -- 1.3.6.1.4.1.2011.5.25.31.8.4.1.5
        hwDisposeEntPhysicalClass OBJECT-TYPE
           SYNTAX      PhysicalClass
           MAX-ACCESS  read-only
           STATUS      current
           DESCRIPTION
               "An indication of the general hardware type of the predisposed physical entity."
           ::= { hwPreDisposeEntInfoEntry 5 }
        
        -- 1.3.6.1.4.1.2011.5.25.31.8.4.1.6
        hwDisposeEntPhysicalParentRelPos OBJECT-TYPE
           SYNTAX      Integer32 (-1..2147483647)
           MAX-ACCESS  read-only
           STATUS      current
           DESCRIPTION
               "An indication of the relative position of this 'child' component among all its 'sibling' components."
           ::= { hwPreDisposeEntInfoEntry 6 }
        
        -- 1.3.6.1.4.1.2011.5.25.31.8.4.1.7
        hwDisposeEntPhysicalName OBJECT-TYPE
           SYNTAX      SnmpAdminString
           MAX-ACCESS  read-only
           STATUS      current
           DESCRIPTION
               "The textual name of the predisposed physical entity."
           ::= { hwPreDisposeEntInfoEntry 7 }

        -- 1.3.6.1.4.1.2011.5.25.31.9
        hwOSPUnifyManageObjects OBJECT IDENTIFIER ::= { hwEntityExtentMIB 9 }

        -- 1.3.6.1.4.1.2011.5.25.31.9.1
        hwEntityExtOSPTrapsPrefix OBJECT IDENTIFIER ::= { hwOSPUnifyManageObjects 1 }

        -- 1.3.6.1.4.1.2011.5.25.31.9.1.1
        hwEntityExtUnconnected NOTIFICATION-TYPE
        	OBJECTS { entPhysicalIndex, entPhysicalName }
            	STATUS current
            	DESCRIPTION
                "Board become unconnected for some reason."
            ::= { hwEntityExtOSPTrapsPrefix 1 }
            
        -- 1.3.6.1.4.1.2011.5.25.31.9.1.2
        hwEntityExtUnconnectedResume NOTIFICATION-TYPE
        	OBJECTS { entPhysicalIndex, entPhysicalName }
            	STATUS current
            	DESCRIPTION
                "Board resume from unconnected"
            ::= { hwEntityExtOSPTrapsPrefix 2 }

     END

--
-- HUAWEI-ENTITY-EXTENT-MIB.mib
--














