-- =================================================================

-- Description: DIFFSERV-DSCP-TC
-- Reference:   This mib was extracted from RFC 3289
-- =================================================================
DIFFSERV-DSCP-TC DEFINITIONS ::= BEGIN

    IMPORTS
    Integer32, MODULE-IDENTITY, mib-2
         FROM SNMPv2-SMI
    TEXTUAL-CONVENTION
         FROM SNMPv2-TC;

    diffServDSCPTC MODULE-IDENTITY
        LAST-UPDATED "200205090000Z"
        ORGANIZATION "IETF Differentiated Services WG"
        CONTACT-INFO
           "       Fred Baker
                   Cisco Systems
                   1121 Via Del Rey
                   Santa Barbara, CA 93117, USA
                   E-mail: fred@cisco.com
    
                   Kwok Ho Chan
                   Nortel Networks
                   600 Technology Park Drive
                   Billerica, MA 01821, USA
                   E-mail: khchan@nortelnetworks.com
    
                   Andrew Smith
                   Harbour Networks
                   Jiuling Building
                   21 North Xisanhuan Ave.
                   Beijing, 100089, PRC
                   E-mail: ah_smith@acm.org
    
                     Differentiated Services Working Group:
                     diffserv@ietf.org"
        DESCRIPTION
           "The Textual Conventions defined in this module should be used
           whenever a Differentiated Services Code Point is used in a MIB."
        REVISION "200205090000Z"
        DESCRIPTION
           "Initial version, published as RFC 3289."
        ::= { mib-2 96 }
    
    Dscp ::= TEXTUAL-CONVENTION
        DISPLAY-HINT "d"
        STATUS   current
        DESCRIPTION
           "A Differentiated Services Code-Point that may be used for
           marking a traffic stream."
        REFERENCE
            "RFC 2474, RFC 2780"
        SYNTAX   Integer32 (0..63)
    
    DscpOrAny ::= TEXTUAL-CONVENTION
        DISPLAY-HINT "d"
        STATUS   current
        DESCRIPTION
           "The IP header Differentiated Services Code-Point that may be
           used for discriminating among traffic streams. The value -1 is
           used to indicate a wild card i.e. any value."
        REFERENCE
            "RFC 2474, RFC 2780"
        SYNTAX   Integer32 (-1 | 0..63)

END

