# Action Groups

When configuring policy based routing (PBR), action groups specify the route that you want the packet to take. You specify the “action” for the route by defining the next interface, the next-hop, or both.

The Action Group List table lists the following information:

- Seq No, the sequence number

- Next Interface or Next Hop, this is the action you want the traffic to take

- Configure, which is a mechanism to remove the action group entry

To permanently remove an entry, click Remove in the Configure column.