# Wireless Association Details

The Association Details page displays additional information about the selected wireless client. It displays the following status information:

MAC Address: The MAC address of the wireless client that is associated with the interface on the device.

State: Displays the status of the connection between the wireless client and the device. The status can be one of the following:

AUTH: The wireless client was authenticated but is not associated with the device.

ASSOC: The wireless client was authenticated and is associated with the device.

WLAN Mode: Operational mode of the wireless client — 802.11a (includes 802.11a turbo if applicable), 802.11b, 802.11g, or 108g (802.11g turbo).

Encryption: Indicates whether encryption is enabled.

Ciphers: Specifies the encryption used between the device and the wireless client. The values are: None, WEP, AES, or TKIP.

Power Save Mode: Indicates whether the wireless client has enabled power save mode.

Rx Data Rate: Rate, in Mbps, of the last frame the device received from the wireless client.

Rx Signal Strength: Strength of the last frame received from the wireless client.

The table displays the statistics of the following types of frames which AP received and transmitted from/to the client. Rx indicates traffic from the client. Tx indicates traffic to the client.

- MSDU: MAC Service Data Units (MSDUs)

- DATA: Good data packets

- Mcast: Multicast data

The table also displays the number of frames that were dropped and contained errors.