The specific phase or state of the connection establishment process between the two BGP speakers. The states can be Idle, Connect, Active, OpenSent, OpenConnect, Establish. The Idle state is the beginning state. The Connect and Active states are the intermediate states. OpenSent and OpenConnect are prefinal states. Establish is a final state where the connection has been established. The default state is Idle.