# Controllers - Infranet Controller Settings

This page lists the Infranet Controller settings that the security device (Infranet Enforcer) uses.

Infranet Controller Settings

- Contact Interval: Specify how often the security device should ping the Infranet Controller for connectivity. The default value is 10 seconds and the range is 3 to 300 seconds.

- Timeout Action: Specify what action to take when the Infranet Controller times out:

- close removes existing sessions and dynamic configuration and blocks further traffic.

- open allows existing and new session traffic as allowed by infranet policies.

- no-change preserves existing connections and dynamic configuration, such as tunnels, but new sessions require authentication.

Infranet Enforcer Settings

Mode: Select Regular (default) or Test only.

- Test only places the security device in test mode, where traffic is always allowed and policies are not enforced. However, the permit or deny decision associated with the infranet-auth policies is logged.

- Regular turns off the “test” mode. The infranet-auth policy decisions are enforced and not only logged. In this default mode, the infranet-auth policies are applied and logged based on the auth table entries.