# Syslog Report Settings

Syslog is a facility that enables the logging of system events to a single file for later review. A NetScreen device can generate syslog messages for system events at predefined severity levels and optionally for traffic that policies permit across a firewall. It sends these messages via UDP (port 514) to up to four designated syslog hosts running on UNIX/Linux systems. The severity level of an event determines whether the event is communicated in a syslog message (see Log Settings).

### To Enable Syslog

1. Select Enable syslog messages.

2. On the Source interface drop-down list, select the interface from which syslog packets are sent.

3. Enter the necessary information for each syslog server you are adding:

Enable: Select this option to enable the syslog server.

IP/ Hostname: The IP address of the syslog host.

Port: The port to which the NetScreen device sends syslog messages.

Security Facility: The security facility, which classifies and sends emergency and alert level messages to the syslog host.

Facility: The regular facility, which classifies and sends all other messages for events unrelated to security.

Event Log: Select this option to send event log entries to the syslog host.

Traffic Log: Select this option to send traffic log entries to the syslog host.

TCP: Select this option to use TCP as the transport protocol.

2. Click Apply or Apply and Reset Connections.

Note: When you enable Syslog on a NetScreen device running in Transparent mode, you must set up a static route on the Route Table.