# Enabling Track IP

To enable track IP for the device or for a VSD group:

1. Enter the necessary information:

Enable Track IP: Click to enable the Track IP feature.

Failover Threshold: The cumulative total weight of all the failed attempts required to cause a VSD group master to step down. You can set the device failover threshold at any value between 1 and 255. The default is 255.

2. Click Apply to save your settings.