# Interface Weights

The Interface Weights page lists the physical Ethernet interfaces on the device. To assign a weight to an interface, select the check box for the interface, enter a number in the appropriate box in the Weight column, and then click Apply to save your settings.

You can set the object failure weight at any value between 1 and 255. The default failure weight for a monitored interface is 255.