# VLAN Group List Edit (Basic)

You can assign (import) or delete a range of VLAN IDs to and from a VLAN group.

Start indicates where the beginning of the VLAN group, End indicates the end point of the VLAN group.

You can assign a VLAN to one vsys only. You can assign VLAN IDs from 2 to 4094, with VLAN ID 1 identifying the root system. Traffic entering the secuirty device is classified to a vsys based on the VLAN tag. Assigning the VLANs to an aggregate interface provides 2 Gbps in each direction, but cannot exceed 4 Gbps for bi-direction traffic per Application-Specific Integrated Circuit (ASIC). The securitydevice can manage a maximum of 500 virtual systems.

### To Add a VLAN Group

To add a VLAN group, select the VLAN ID to start from and the VLAN ID to end at, and then click Add.