# Manual Key VPN Tunnel List

The table on this page lists the Manual Key VPN tunnels that are configured on the security device and provides the following information about each one:

Name: Indicates the name of the VPN tunnel.

Gateway: Indicates the IP address of the gateway the VPN tunnel uses.

Local SPI and Remote SPI: A security index number that uniquely distinguishes a particular encrypted tunnel from the others being used at the same time. The Local Security Index serves as the other end's Remote Security Index and vice versa. If you enter "Value_A Value_B", the other end of the tunnel must switch the order of the two components, as in "Value_B Value_A".

Configure: Click Edit to modify the entry, or Remove to delete the entry. Remove is only available if the entry is not already in use in a policy.

## Viewing the VPN Tunnel List

You can sort the list by Name or Gateway by clicking on the appropriate column title.

You can select how many entries per page you want to view from the List_per page drop-down list.

You can jump to another page by selecting it from the Go to Page drop-down list.

## Configuring a Manual Key VPN Tunnel

To configure a manual key VPN tunnel, click New. For more information, see Manual Key VPN Tunnel Configuration.