# VLAN Retagging List

This page displays a table listing all the VLAN Retagging pairs configured on the security device, and includes the following information:

Retagging-Pair-Name: Name of the VLAN retagging pair.

From: The beginning VLAN ID (the range is 2 to 4095).

To: The ending VLAN ID (the range is 2 to 4095).

Note that From and To do not indicate the direction of traffic flow, VLAN retagging pairs are bidirectional.

Port: The port the VLAN retagging pair is bound to.

Egress/Ingress: This field is not used.

Configuration: Click Edit to modify an existing VLAN retagging pair. Click Remove to delete a VLAN retagging pair from the system.

Click New to create a VLAN retagging pair.