# VLAN Group List Edit (Basic)

You can assign (import) or delete a range of VLAN IDs to and from a VLAN group.

Start specifies the beginning of the Vlan group, End specifies the end point of the Vlan group.

You can assign a VLAN to one vsys only. You can assign VLAN IDs from 2 to 4094, with VLAN ID 1 identifying the root system. Traffic entering the security device is classified to a vsys based on the VLAN tag. Assigning VLANs to an aggregate interface provides 2 Gbps of bandwidth in each direction; however, total bandwidth per Application-Specific Integrated Circuit (ASIC) cannot exceed 4 Gbps for bi-directional traffic. The security device can manage a maximum of 500 virtual systems.

### To Add a VLAN Group

To add a VLAN group enter a VLAN Group Name, select a Start and End VLAN ID, and click Add.