ea#-02-I.01
-
The system remains in layout mode until instructed
to exit. Choose EDIT from the main menu.
Choose option
-
Choose the TRM/EXT option.
  
Choose option
- 
Choose FIRST.
    
Choose option   
-
Select the highlighted portion of the line to trim. This
is the portion of the line to remain after trimming.   
Select entity to trim
line
-
Select the highlighted line as the trimming entity.
The trimming entity cuts this line to a shorter length.   
Select trimming entity   (position near intersection)
line
-
The view 7 instance is now completely modified to show
a correct hidden line representation.
Select entity to trim 
-
Press ESCAPE to return to the main menu.
    
Select entity to trim
-
ea#-02-I.02
-
Work on the isometric instance is complete. Autoscale
the display to view the layout. Press ALT-A
Choose option
ALT-A
-
ALT-V changes the active instance in layout mode.
Press ALT-V to change the active instance.
Choose option
ALT-V
-
Cursor-indicate in the highlighted region to select
the top view instance.
-
Press ALT-W to window-in on the top instance.
     
Choose Option
ALT-W
-
Cursor-indicate in the highlighted box for the first
corner of the window.
Indicate 1st corner of window
-   
Cursor-indicate in the highlighted box for the second
corner of the window.
Indicate 2nd corner of window
-
Choose the DETAIL option.
  
Choose option     
-
Choose the LAYOUT option.
  
Choose option   
-
Choose the MODELIZE option.
  
Choose option   
-       
Choose INSTANCE.
   
Choose modelize option 
-
Cursor-indicate in the highlighted region to select
the top view instance.
-
Choose YES to accept the selections to be
modelized. 
Okay to modelize selections? (NO)
-
The border disappeared to show that the instance
is now layout geometry.
Choose modelize option
-
Press ESCAPE to return to the main menu.
    
Choose modelize option
-
Choose the EDIT option.
   
Choose option
-
Choose the BREAK option.
  
Choose option 
-
Choose DOUBLE
   
Choose option   
-
ea#-02-I.03
-
Use the immediate mode command ALT-T to change the line
type to dashed.
Select entity to break
ALT-T
-
Choose the second line type: dashed
     
-
Select the highlighted portion of the ellipse.
   
Select entity to break
ellipse
-
Select the highlighted portion of the circle.
     
Select breaking entity.
circle
-
Select the highlighted portion of the circle.
     
Select breaking entity.
circle
- 
The ellipse was selected on the right, keeping a solid
line. The new entity on the left is dashed.
Select entity to break
-
Use the immediate mode command ALT-T to change the line
type back to solid.
Select entity to break
ALT-T
-
Select the top line type: solid
    
-
Press ESCAPE to return to the main menu.
    
Select entity to break
-
The change in line type back to solid insures that any
new geometry has this normal solid line type.
Select entity to break
-
Use the immediate mode command CTRL-Q to delete the line
joining the circle to the ellipse
Choose Option
CTRL-Q
-
Select the highlighted line for deletion.
    
Select entity 1   (press RETURN when done)
line
-
Press ENTER to accept the selection.
    
Select entity 2   (press RETURN when done)
-
Press ALT-A to autoscale the display.
   
Choose Option
ALT-A
-
Changes to geometry are complete. The next steps bring
in border geometry from a pattern file.
Choose Option
-
Choose the FILES option.
   
Choose option   
-
Choose the PATTERN option.
 
Choose option
-
Choose the RETRIEVE option.
 
Choose option
-
Enter BORDB (bordb) as pattern file to load.
 
Enter pattern file name (): 
bordb
-
Choose the NO option to not group the entities.
 
Group pattern entities (YES) ?
-
Choose the CUR-LEV option to have the file placed on 
level 1, the current level. 
Choose level option (CUR-LEV)
-
Enter 1 as scale factor.
 
Enter scale factor (1) => 
scale factor
-
Enter 0 as rotation angle.
 
Enter rotation angle (0) => 
rotation angle
-
Choose the KEY-IN option.
 
Enter pattern base position  / Cursor-indicate position
-
The base position of the border is its lower left
corner. To position this corner, enter 0.0 for XV.
Enter pattern base position  / XV = 
XV
-
Enter 0.0 for YV.
 
Enter pattern base position  / YV = 
YV
-
Enter 0.0 for ZV.
 
Enter pattern base position  / ZV = 
ZV
-
The geometry added is specific to this layout.
It does not change the model.
Enter pattern base position
-
Press ESCAPE to exit this function.
   
Enter pattern base position  / XV = 
-
ea#-02-I.04
-
ea#-02-r.05
-
That's all folks
-




