de#-01-i.01
- 
This is an illustration of the Finger Guide when this 
section is completed.
Choose option
-
de#-01-i.02
-
The highlighted circle will be created in this step.
 
Choose option 
- 
Use the Immediate Mode command ALT-K to define a 
construction plane. 
Choose option
ALT-K
-
Choose the 3 PTS option. 
  
Choose option 
- 
Choose the ENDENT option. 
  
Choose option 
- 
Select the highlighted portion of the line to indicate the
first point on the X axis. 
Indicate 1st point on X axis  / Select entity
line 
- 
Select the highlighted portion of the line to indicate
the second point on the X axis.  
Indicate 2nd point on X axis  / Select entity
line 
- 
Select the highlighted portion of the line to indicate
the direction for the Y axis.  
Indicate direction for Y axis  / Select entity
line 
- 
The next step is to create the circle on the newly defined
construction plane. Choose the CREATE option.  
Choose option 
- 
Choose the CIRCLE option. 
  
Choose option 
- 
Choose the CTR+RAD option. 
  
Choose option 
- 
Enter a radius of 0.375
  
Enter radius (0.5) => 
radius
- 
Choose the DELTA option. 
  
Choose option 
- 
Choose the ENDENT option. 
  
Choose option 
- 
Select the highlighted portion of the line to indicate the 
delta reference position.  
Indicate delta reference position  / Select entity
line 
- 
Enter -0.625 for the X axis distance (dXV).
  
dXV = 
dXV
- 
Enter -1.25 for the Y axis distance (dYV).
  
dXV =-0.625             dYV = 
dYV
- 
Enter 0 for the z axis distance (dZV).
  
dXV =-0.625             dYV =  -1.25            dZV = 
dZV
- 
Now change the construction plane back to the display view
using the Immediate Mode command ALT-K.
Choose option
ALT-K
-
Choose the CP = DV option to make the construction plane
equal to the display view.  
Choose option 
- 
Press ESCAPE to exit from this function. 
  
Choose option
- 
de#-01-r.03
-

