menu
1
;Main Menu
 1) Set graphics options
 2) Set input device options
 3) Set plotter options
 4) Set printer options
 5) Set program options
 6) Set default pathnames for data files
 7) Set automatic file loading options

 8) Exit without saving changes
 9) Exit and save changes
menu
10
;Main Menu
 1) Set graphics options
 2) Set input device options
 3) Set plotter options
 4) Set printer options
 5) Set program options
 6) Set default pathnames for data files

 7) Exit without saving changes
 8) Exit and save changes
menu
11
;Set Graphics Options
 1) Select graphics device
 2) Set color options
 3) Set viewport options
 4) Set graphics CDE option
 5) Return to Main Menu
menu
111
;Set Graphics Options
 1) Select graphics device
 2) Set color options
 3) Return to Main Menu
menu
1111
;Menu Cursor Type
 1) Inverse video
 2) Arrow
menu
1112
;Monitor Configuration
 1) One monitor
 2) Two monitors with CADKEY graphics device as primary
 3) Two monitors with CADKEY graphics device as secondary
menu
112
;Set Color Options
 1) Menu options window
 2) System mode indicator
 3) Break window
 4) Status window
 5) History line
 6) Prompt line
 7) Cursor tracking window
 8) Pop Up menus
 9) Viewport area
10) Cursor and marker
11) Return to Set Graphics Options Menu
menu
1121
;The CADKEY color graphics table is:
   0-Black        4-Yellow       8-Blue        12-Lt.Red
   1-Green        5-Cyan         9-Lt.Blue     13-Lt.Magenta
   2-Red          6-Magenta     10-Lt.Green    14-White 
   3-Amber        7-Grey        11-Lt.Cyan     15-High White
menu
113
;Set Default Viewport Configuration
 1) Single
 2) Two vertical
 3) Two horizontal
 4) Two left, one right
 5) One left, two right    
 6) One top, two bottom
 7) Two top, one bottom
 8) Four
menu
1131
;Display Construction View Axes Options
 1) Off
 2) Primary Viewport
 3) All Viewports
menu
12
;Set Input Device Options
 1) CADKEY input device
 2) CADL input device
 3) Return to main menu
menu
123
;Tablet/Mouse Serial Ports
1) COM1
2) COM2
menu
13
;Plotting Devices
 1) Hewlett Packard HPGL lower left origin plotters
 2) Hewlett Packard HPGL center origin plotters
 3) Houston Instruments DMPL plotters, 1 MIL res
 4) Houston Instruments DMPL plotters, 2.5 MIL res
 5) Houston Instruments DMPL plotters, 4 MIL res
 6) Houston Instruments DMPL plotters, 5 MIL res
 7) Calcomp pen plotters
 8) Calcomp electrostatic plotters
 9) RS-274 driven devices
10) Benson BGL plotters
11) Western Graphtec GP-GL
12) IP Mutoh
13) none
menu
131
;Plot Paper Sizes
 1) A size drawing (8.5 x 11.0 in)
 2) B size drawing (11.0 x 17.0 in)
 3) C size drawing (17.0 x 22.0 in)
 4) D size drawing (22.0 x 34.0 in)
 5) E size drawing (34.0 x 44.0 in)
 6) A4 size drawing (210 x 297 mm or 8.27 x 11.69 in)
 7) A3 size drawing (297 x 420 mm or 11.69 x 16.54 in)
 8) A2 size drawing (420 x 594 mm or 16.54 x 23.39 in)
 9) A1 size drawing (594 x 841 mm or 23.39 x 33.11 in)
10) A0 size drawing (841 x 1189 mm or 33.11 x 46.81 in)
11) Enter paper size
menu
134
;Pen Sorting Options
1) No sort
2) Sort pens in low to high order
3) Sort pens in order found
menu
138
;Plotter Baud Rates
1) 300
2) 600
3) 1200
4) 2400
5) 4800
6) 9600
7) 19200
8) 38400
menu
141
;Printing Resolutions
1) low
2) medium
3) high
menu
144
;Printer Baud Rates
1) 110
2) 150
3) 300
4) 600
5) 1200
6) 2400
7) 4800
8) 9600
menu
15114
;Units Modes For CADKEY
1) Inches
2) Millimeters
3) Feet
4) Centimeters
5) Yards
6) Meters
menu
15127
;Entity Selection Highlighting Styles
1) Drawn markers
2) Flashing markers
3) Drawn, highlighted entities (selected viewport)
4) Flashing, highlighted entities (selected viewport)
5) Drawn, highlighted entities (all viewports)
6) Flashing, highlighted entities (all viewports)
menu
15128
;Part File Auto-Save
1) Disable
2) Enable
menu
15129
;Dimensioning Standard For CADKEY
1) ANSI
2) DIN
3) ISO
4) JIS
menu
99999
dummy
