da#-01-i.01
- 
This illustration shows the transformations that are made 
to the front and back of the Finger Guide.      
Choose option 
- 
da#-01-i.02
-
The highlighted section of the 2-D part will be projected 
to create the dashed yellow lines.   
Choose option 
- 
da#-01-i.03
- 
Choose the DISPLAY option. 
  
Choose option 
- 
Choose the VIEW option. 
  
Choose option 
- 
Enter 7 to change to the Isometeric view (View 7). 
  
Enter view number or choose menu option (1-8) => 
- 
Notice that your part does not fit in the entire  
viewport.                                          
Choose option 
- 
da#-01-i.04
- 
Choose the BACK-UP option to return to the DISPLAY menu. 
  
Choose option 
- 
Choose the ZOOM option. 
  
Choose option 
- 
Choose the AUTO option. 
  
Choose option 
- 
The display of the part was expanded to fit the viewport. 
Press ESCAPE to exit this function.
Choose option 
- 
da#-01-i.05
- 
Choose the CONTROL option.
 
Choose option
- 
Choose the COORDS option.
 
Choose option
- 
Choose the WORLD option.
 
Choose option
- 
Look at the COORD: option in the Status Window. It reads 
COORD: WLD because you just toggled CADKEY to the world 
coordinate system. Now press ESCAPE to exit the function.
Choose option 
- 
da#-01-r.06
-
