Instructions for MicroTN.exe  - TSR version of Tn3270.

1. Use a minimal config.tel file, take out any host you will not be connecting
   to, all options that don't apply to 3270 emulation, nameserver info, etc.

2. You must place the name and hostip of your destination in the config.tel file.

3. You must use a packet driver.

4. Usage:
	microtn [-h config.fil] [-r] [ hostname ]

5. The -r switch is required to make it resident, otherwise it will not be
   resident.

6. hostname is optional.

7. In resident mode:
	ALT-RIGHT_SHIFT 	pops up tn3270
	ALT-B			pops back to DOS
	ALT-X			closes current connection
	ALT-P			sets the capture file name.
	ALT-M			displays free memory.
	ALT-U			unloads program, if at the Enter Host prompt

8. In non resident mode:
	ALT-X			closes current connection, exits program
	ALT-P			sets the capture file name.
	ALT-M			displays free memory.
	ALT-U			exits program, if at the Enter Host prompt
	<ESC>			exits program, if at the Enter host prompt

Note:
	Video page 4 is used by the program to store the 3720 screen, this
	may interfere w/ your DOS software if run in resident mode.  
	Also, if you pop up over a screen that has no cursor, then no cursor
	will appear in tn3270.

	Finally, you can not run other TCP programs if you have microtn loaded
	as a TSR, use ALT-X and ALT-U to unload the program.





