****************************************************************************
            SiS PCI Fast Ethernet Adapter Installation
                   for Windows NT 4.0 Driver
****************************************************************************

driver file:  .\sisnic.sys
INF file:     .\oemsetup.inf

To install the SiS PCI Fast Ethernet adapter and driver for use with
Windows NT 4.0, please do the following:

1.  Power off your PC and install the adapter in a PCI slot in your PC.

2.  Reboot the computer using the Windows NT operating system.

3.  Double click the Network icon in the Control Panel.

4.  Select the "Adapter" tab and click "Add..."

5.  Select Have Disk. Insert the "SiS PCI Fast Ethernet Adapter Drivers Disk"
    in your floppy drive and specify the correct path.

6.  Select one of the following models:

    "SiS 900 PCI Fast Ethernet Adapter"

    then click OK.

7.  In the dialog box that appears, select the Media Type and enter the
    Network address for the adapter if necessary(You can click Help for more
    detailed information about these settings).
    Click OK to complete this dialog box (or Cancel to terminate the
    configuration without completing it).

8.  Exit the Network control panel window. Windows NT asks if you wish to
    reboot. You must reboot before the adapter will function properly.

