### Scan Destination

The Scan to function of VistaScan allows you to send the scanned images to a preconfigured file, printer, fax, mail and other applications. To do so, you have to setup your scan destination first.

### File

Select File Directory, Filename and File Format for your scan image.

Filename
When you use Batch Scan to scan multiple images, the driver will add two digits (starting from 00) at the end of the filename for each image as default filename. In other words, the filename will go like: filename+00, 01,02 etc.

Please take note that filenames longer than 8 bytes will be truncated to 6 bytes.

File Format
The supported file formats include: BMP, TIF, PCX, PSD, TGA and JPG.

### Printer

Printer dialogue box will display the default printer driver for VistaScan. You may change the printer by clicking the Setup button for configuration.

### Mail

Both Microsoft Exchange and Lotus cc:Mail are supported in Mail function. The former, however, will be disabled in Windows3.1 environments.

You may also setup the image format for the file to be mailed. The supported formats include: BMP, TIF, PCX, PSD, TGA, JPG.

### Fax

Click the Fax button to display the Fax dialogue box.

To change the default fax driver, click the Setup button to select your fax driver.

Most fax drivers share the same printer port that the printer driver uses for output. Thus, any changes to the fax driver will change the default printer driver as well, vice versa.

### Application

Setup the Application's name, directory path, filename and file format to which the VistaScan will send the scanned images.

[Back][General][Scanner Information]