## OCR Configuration
Optical Character Recognition(OCR) Destination:Select a text editing application from the pull-down list. (VistaScan will show the avaliable text editing software applications that have been installed in your system.) After scanning, the scanned image will be translated into text format through OCR engine and send to the designated text editing application for further editing. Note:If you do not see the OCR icon on the Push Button Configuration page, click the Custom icon to bring out the function. Resolution:The Resolution setting determines the amount of information the scanner will capture in a resulting scanned image and is measured in dots per inch (dpi). The resolution for OCR processing is fixed to 400 dpi. You can not change it. Brightness:This function is fixed by program. You can not change it. Original:
Reflective | Choose this option for paper originals (non-transparencies) which do not consist of a "see through" type of material, such as photographs, flyers, newspapers and so on.
Transmissive | Choose this option for transparent objects (through which light can pass, e.g. overhead projector slides) if a Transparency Adapter is installed and turned on.
Scan Size:The scan size is fixed by program. You can not change it. |
##### Push Button Setup Scan Mode Copy Mode Mail Mode OCR Mode