These are the Sound Blaster 2.0 CT-1350B Install disks from 1994 (version 2)

This is the second (1994 version) install set for the Sound Blaster 2.0, the original 
install set was released in 1993.

The files are in thier own directories, you need to copy the the files from
the directories to floppy to install. The install program expects a seperate 
disk for each directory and you will need to follow that procedure to get it installed.

To start the install you need to run install.exe from disk1

You can use either 720k or 1.44MB floppy disks, or even seperate CD's if your computer has a CD drive.