SUPPORT.LST
                        Tape Mate II Archiving Software
                                Version 1.20
                          Device Support Information

------------------------------------------------------------------------------
                               Supported Devices
------------------------------------------------------------------------------

        Archive
        -------
        Python DDS DAT Drive
        Viper 2060S Tape Drive
        Viper 2125S Tape Drive
        Viper 2150S Tape Drive
        Viper 2525S Tape Drive
        QIC-02/QIC-36 Tape Devices
        Archive Anaconda 2750 Tape Drive
        Archive Anaconda 2800 Tape Drive

        CMS
        ---
        CMS Enhancements T250/150

	Emerald
	-------
        TDC 3600 Series Tape Drives
        TDC 3800 Series Tape Drives
        TDC 4100 Series Tape Drives

        Everex
        ------
        Excel 1G, DC 2000 Tape Drive

        Exabyte
        -------
        EXB-2501 ¬ inch Tape Drive
        EXB-4200 4mm DAT Drive
        EXB-4200c 4mm DAT Drive
        EXB-8200 8mm Cartridge Drive
        EXB-8200SX 8mm Cart Drive
        EXB-8205 8mm Cartridge Drive
        EXB-8500 8mm Cartridge Drive
        EXB-8500c Cartridge Drive
        EXB-8505 8mm Cartridge Drive

        Gigatrend
        ---------
        Gigatape DDS DAT Drive

        Hewlett Packard
        ---------------
        35450A 4mm 5¬" DAT Storage Drive
        35470A 4mm 3«" DAT Storage Drive
        35480A 4mm 3«" DAT Storage Drive

        SONY
        ----
        SDT-1000 5¬" DAT Storage Drive
        SDT-2000 3«" DAT Storage Drive
        SDT-4000 3«" DAT Storage Drive

        JVC
        ---
        4mm Data/DAT Drive

        R-Byte
        ------
        RB100 DDS DAT Drive

        Sankyo
        ------
        CP150SE SCSI Streaming Tape
        CP525SE SCSI Streaming Tape
        CP1000SE SCSI Streaming Tape

        Shinwa
        ------
        Shinwa SDX-81 100MB SCSI QIC Tape
        Shinwa SDX-85 250MB SCSI QIC Tape

        Tandberg
        --------
          SCSI-1
          ------
          TDC 3600 Series Tape Drives
          TDC 3800 Series Tape Drives
          TDC 4100 Series Tape Drives

          SCSI-2
          ------
          TDC 3600 Series Tape Drives
          TDC 3800 Series Tape Drives
          TDC 4100 Series Tape Drives
          TDC 4200 Series Tape Drives

        Teac
        ----
        MT-01N Mini Data Cartridge Tape
        MT-2ST/20S/45S Cassette Tape
        MT-2ST/F50 Streaming Cassette
        MT-2ST/N50 Streaming Cassette

        WangDAT
        -------
        Model 1300 5¬" DDS DAT Drive
        Model 2600 5¬" DDS DAT Drive
        Model 3100 3«" DDS DAT Drive
        Model 3200 3«" DDS DAT Drive

        Wangtek
        -------
        QIC-02/QIC-36 Tape Devices
        Model 6130HS DDS DAT
        Model 6200HS DDS DAT

        YE-DATA
        -------
        YD-7101 Series Streaming Cassette
        YD-7106 Series Streaming Cassette
        YD-7201 Series SCSI QIC Tape

------------------------------------------------------------------------------
                  Supported Device Configuration Parameters
------------------------------------------------------------------------------

                8mm Helical Scan Drives
        ---------------------------------------------------

        Exabyte EXB-8200 8mm Cartridge Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Block Size:     512 Bytes, 1024 Bytes

        Exabyte EXB-8200SX 8mm Cart Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Block Size:     512 Bytes, 1024 Bytes

        Exabyte EXB-8205 8mm Cartridge Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Density:        Default, EXB-8200, EXB-8200c
                Block Size:     512 Bytes, 1024 Bytes

        Exabyte EXB-8500 8mm Cartridge Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Density:        Default, EXB-8200, EXB-8500
                Block Size:     512 Bytes, 1024 Bytes

        Exabyte EXB-8500c Cartridge Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Density:        Default, EXB-8500, EXB-8200, EXB-8200c,
                                EXB-8500c
                Block Size:     512 Bytes, 1024 Bytes

        Exabyte EXB-8505 8mm Cartridge Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Density:        Default, EXB-8500, EXB-8200, EXB-8200c,
                                EXB-8500c
                Block Size:     512 Bytes, 1024 Bytes


                4mm Helical Scan Drives (DAT)
        ---------------------------------------------------

        Archive Python DDS DAT Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Compression:    Disabled, Enabled

        Exabyte EXB-4200 4mm DAT Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6

        Exabyte EXB-4200c 4mm DAT Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Compression:    Disabled, Enabled

        Gigatrend Gigatape DDS DAT Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6

        HP 35450A 4mm 5¬" DAT Storage Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6

        HP 35470A 4mm 3«" DAT Storage Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6

        HP 35480A 4mm 3«" DAT Storage Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Compression:    Disabled, Enabled

        SONY SDT-1000 5¬" DAT Storage Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6

        SONY SDT-2000 3«" DAT Storage Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6

        SONY SDT-4000 3«" DAT Storage Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Compression:    Disabled, Enabled

        JVC 4mm Data/DAT Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6

        R-BYTE RB100 DDS DAT Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6

        WangDAT Model 1300 5¬" DDS DAT Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6

        WangDAT Model 2600 5¬" DDS DAT Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Compression:    Disabled, Enabled

        WangDAT Model 3100 3«" DDS DAT Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6

        WangDAT Model 3200 3«" DDS DAT Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Compression:    Disabled, Enabled

        Wangtek Model 6130HS DDS DAT
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6

        Wangtek Model 6200HS DDS DAT
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6



                SCSI QIC Drives
        ---------------------------------------------------

        Archive Viper 2060S Tape Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6

        Archive Viper 2125S Tape Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6

        Archive Viper 2150S Tape Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Format:    Default, QIC-24, QIC-120, QIC-150

        Archive Viper 2525 Tape Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Format:    Default, QIC-24, QIC-120, QIC-150, QIC-525

        Archive Anaconda 2750 Tape Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Format:    Default, QIC-120, QIC-150, QIC-525, QIC-1350
                                QIC-1000, QIC-2100

        Archive Anaconda 2800 Tape Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Format:    Default, QIC-120, QIC-150, QIC-525, QIC-1350
                                QIC-1000, QIC-2100

        Exabyte EXB-2501 ¬ inch Tape Drive
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6

        Excel 1G, DC 2000 Tape Drive (Everex)
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6

        Sankyo CP150SE SCSI Streaming Tape
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                
        Sankyo CP525SE SCSI Streaming Tape
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                
        Sankyo CP1000SE SCSI Streaming Tape
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
        
        Shinwa SDX-81 100MB SCSI QIC Tape
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6

        Shinwa SDX-85 250MB SCSI QIC Tape
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Format:    Default, QIC-24, QIC-120, QIC-150

        Emerald TDC 3600 SCSI-1 Series Tape
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Format:    Default, QIC-11, QIC-24, QIC-120, QIC-150
                Preference:     Save Time, Save Tape

        Emerald TDC 3800 SCSI-1 Series Tape
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Format:    Default, QIC-120, QIC-150, QIC-525
                Preference:     Save Time, Save Tape

        Emerald TDC 4100 SCSI-1 Series Tape
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Format:    Default, QIC-120, QIC-150, QIC-525, QIC-1000
                Preference:     Save Tape, Save Time

        Tandberg TDC 3600 SCSI-1 Series Tape
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Format:    Default, QIC-11, QIC-24, QIC-120, QIC-150
                Preference:     Save Time, Save Tape

        Tandberg TDC 3800 SCSI-1 Series Tape
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Format:    Default, QIC-120, QIC-150, QIC-525
                Preference:     Save Time, Save Tape

        Tandberg TDC 3600 SCSI-2 Series Tape
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Format:    Default, QIC-11, QIC-24, QIC-120, QIC-150
                Preference:     Save Time, Save Tape

        Tandberg TDC 3800 SCSI-2 Series Tape
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Format:    Default, QIC-120, QIC-150, QIC-525
                Preference:     Save Time, Save Tape

        Tandberg TDC 4100 SCSI-2 Series Tape
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Format:    Default, QIC-120, QIC-150, QIC-525, QIC-1000
                Preference:     Save Time, Save Tape

        Tandberg TDC 4200 SCSI-2 Series Tape
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Format:    Default, QIC-120, QIC-150, QIC-525, QIC-1000
                                QIC-2000
                Preference:     Save Time, Save Tape

        Wangtek SCSI Streaming Tape
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Format:    Default, QIC-24, QIC-120, QIC-150

        YD-7201 Series Streaming Tape
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Format:    Default, QIC-24, QIC-120, QIC-150



                SCSI Cassette Cartridge Tapes
        ---------------------------------------------------

        TEAC MT-01N Mini Data Cartridge Tape
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Speed:     122.5 KB/Sec, 99.5 KB/Sec,
                                84.2 KB/Sec, 61.3 KB/Sec

        TEAC MT-2ST/20S/45S Cassette Tape
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6

        TEAC MT-2ST/F50 Streaming Cassette
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Speed:     242.3 KB/Sec, 196.9 KB/Sec, 
                                166.6 KB/Sec, 121.2 KB/Sec

        TEAC MT-2ST/N50 Streaming Cassette
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Speed:     122.5 KB/Sec, 99.5 KB/Sec,
                                84.2 KB/Sec, 61.3 KB/Sec

        YD-7101 Series Streaming Cassette (YEDATA)
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Speed:     122.5 KB/Sec, 99.5 KB/Sec,
                                84.2 KB/Sec, 61.3 KB/Sec

        YD-7106 Series Streaming Cassette (YEDATA)
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6
                Tape Speed:     242.3 KB/Sec, 196.9 KB/Sec, 
                                166.6 KB/Sec, 121.2 KB/Sec


                Generic SCSI Device Driver (General Purpose) 
        ---------------------------------------------------

        GENERIC Tape Device Driver
                SCSI ID:        Auto, 0, 1, 2, 3, 4, 5, 6


                QIC-02/QIC-36 Controllers/Devices
        ---------------------------------------------------

        CMS Enhancements T250/150 QIC02
                Port:           370, 300, 200, 280, 2AC, 338, 3F6
                IRQ:            3, 2, 4, 5, 7
                DMA:            1, 2, 3
                Format:         Default, QIC-24, QIC-120, QIC-150

        Archive QIC-02/QIC-36 Tape Adapter
                Port:           200h, 280h, 2ACh, 300h, 338h, 3F6h
                IRQ:            5, 2, 3, 4, 7
                DMA:            1, 2, 3

        Wangtek QIC-02/QIC-36 Tape Adapter
                Port:           300h, 200h , 280h, 2ACh, 338h, 3F6h
                IRQ:            3, 2, 4, 5, 7
                DMA:            1, 2, 3
                Format:         Default, QIC-24, QIC-120, QIC-150

