READ.ME    Trantor Systems, Ltd.   November 1993

SCSIworks! Version 1.2

Install Note:
If you have an Adaptec 154x series adapter in your computer, do NOT use
the Automatic Search for Host Adapter option in the Install menu.  It
will usually 'lock up' your computer and require a reboot.  Use the
arrow keys to select the Trantor SCSI adapter you want to install.

IBM ThinkPad 720 note:
New ASPI Managers for the T348 and T358 are included... MAxxxIBM.SYS.
These drivers will need to be manually included in place of the standard
ASPI Manager when installed on the ThinkPad 720.  They force the i/o to
slow down, since the 720 parallel port i/o is too fast for the signals
to latch normally.

IBM ThinkPad 750 note:
Use the /M04 option with the T358 to force it to bi-directional mode.
Using the T348 and also an APA-460 PCMCIA SCSI adapter on the same 750,
you will need to load the T348 ASPI Manager before the Card & Socket
Services and use the /M2 command line option with the T348 ASPI Manager.


TSCSI.SYS 4.58
now has full INT13 support.  You can use the DOS FDISK and FORMAT
programs on all re-writeable media with even the MiniSCSI series
adapters.  Drives >1G are now supported on all Trantor SCSI adapters and
can be formatted with the FDISK/FORMAT combination.

ASPI for Windows is now supported by the T130, T160, APA-460, T348 and
T358 Trantor ASPI Managers.  The T338 does not support ASPI for Windows.
Since Adaptec's ASPI for Windows requires an IRQ of 9 or higher, we need
to 'trick' it for the T130 and the T348 MiniSCSI Plus, since they only
have the 8 bit IRQs available.  To do that, add the command line option
/IPx, where x is the free IRQ on your system that you want to use for
the ASPI for Windows emulation.  If you are using an IRQ higher than 9
(like with the T160), you don't need to use this trick... ASPI for
Windows will work automatically with your selected IRQ.


TFORMAT 2.02 fixes a bug related to formatting IOMEGA floptical disks
and also fixes a problem with larger drives and the Custom Partitioning.


TSLCDR.SYS  version 3.09
Support added for NEC CDR-210, CDR-400, CDR-500, CDR-600; Hitachi 6750;
Philips CM-215; Apple PowerCD

Apple PowerCD must be the only CD-ROM drive on the chain.  It won't
daisy-chain with other CD-ROM devices properly.

Work-around for the Teac CD-50 1.06 firmware and Mayo Clinic audio test.

Audio quirkiness on some drives with MusicBox fixed.

Tape Mate II
Version 1.2 now included.  Supports many more drives and includes a
GENERIC tape driver for tapes that are not specifically supported.  The
GENERIC driver may work better with some host adapters, like the
MediaVision PAS series.


**************************************************************************
READ.ME    Trantor Systems, Ltd.   August 1993

SCSIworks! version 1.1

TSCSI.SYS 4.56 adds support for larger hard drives >1G
  More IOMEGA floptical fixes added.

TFORMAT 2.01 now supports >1G hard drives.  Low level format will be
  bypassed unless the command line switch /L is added to the TFORMAT
  command line.  This will eliminate unnecessary low level formats for
  most media.
  If your drive is larger than 1G, TFORMAT will exit after performing a
  low-level format.  To partition and use the drive, you will need to
  use a Trantor SCSI adapter with a ROM BIOS.  Turn the ROM BIOS on and
  boot up your system.  Use the DOS program FDISK to partition the
  drive, then the DOS FORMAT command to format it.
  NOTE: drives greater than 1G can NOT be partitioned with FDISK on any
  of the MiniSCSI series adapters.  The MiniSCSI adapters will support
  the >1G drive if it is partitioned and formatted on another SCSI
  adapter that does contain a ROM BIOS.

TSJII.SYS scanner driver updated to support more non-Trantor ASPI
 versions.

TSLCDR.SYS 3.07 adds support for:
 (all support multi-session Photo CD unless noted)
 Apple   CD-300
 Chinon  CDX-535
 Philips CM425A
 Sony    8012 (Sun version) (single session Photo CD only)
 Teac    CD-50
 Texel   DM3028
         DM5028

Provided a work around for Xtree Gold and for the LOOM CD game.

TSLCDR.SYS now defaults to a SCSI-2 command set if it doesn't know the
CD-ROM drive at boot time.  Photo CD multisession is supported with the
same default mode as Windows NT uses.  This should allow any new drive
following these standards to work without any future driver changes.

NEC Versa note:
With the T358 MiniSCSI EPP, you MUST add a command line option of /M2 to
the MA358.SYS ASPI Manager to allow it to work correctly and find the
T358 SCSI adapter.  eg: device=c:\tscsi\ma358.sys /m2

IBM ThinkPad 720C note:
With the 720C, you will need to slow the computer down with the IBM
Reference Disk.  The 50MHz speed will not work correctly with the T348
or T358.

Added ASPI2DOS for use with Adaptec 1510, 1520, and 1522 SCSI adapters.
The Trantor Install program will automatically find them.

Updated OS/2 drivers and moved them and Windows NT drivers to the Tape
Mate II disk.  Windows NT ships with drivers for the T130 and T128 on
disc, but the T160 and MiniSCSI series drivers are here.  The updated
T130 and T128 drivers on this disk can be manually installed in NT after
the drivers on the NT disc are running, but NT won't install them if it
already has a driver on the distribution disc.

Added Magic Lantern - a Windows viewer program for Photo CD images.
Full documentation for Magic Lantern is available on line through the
Windows help system.  Magic Lantern is on the second SCSIworks! disk
along with Tape Mate II.

TSLCDR.SYS version 3 and higher supports multi-session Kodak Photo CD on
hardware that is compatible.
