Some older SCSI hardware has limitations that newer hardware does not.
We have provided older versions of our drivers for devices that do not
work correctly with newer drivers because of these hardware limitations.

To use one of the older drivers, copy the file to your TSCSI directory
and rename it as appropriate.  For example, if you want to use CD-ROM
driver TSLCDR.140, rename it to TSLCDR.SYS.

CD-ROM Drives
NEC CDR-35
    CDR-77
    CDR-80
Panasonic CR-501
                Use TSLCDR.140 or earlier.  These drives are unable to
                deal with the code in later drivers added for PhotoCD
                compatibility.

