Windows 95 Installation Procedure

The SoundPiper 16 is supported under Windows 95 using the drivers located
on this diskette

Installation Procedure
======================

Place the Windows Supoort Disk 2 Revision 2.0 into your A: drive.
Select My Computer.
Select Control Panel.
Select Add New Hardware.
Select Next.
Select No to Automatic Hardware search.
Select Sound, Video, and Game Controllers.
Select Have Disk...
Copy manufacturer's files from: A:\
Select OK.
Select ESS ESS688 AudioDrive.
Select OK.
Let Windows 95 add drivers.
Restart the system.

You can use the Sound Recorder to record and playback with the microphone.
You can use the Media Player to play MIDI and WAVE files.
You can use the Volume Control to adjust the input and output levels.

Piper Research, Inc.
303 21st Street - Suite 241
P.O. Box 241
Newport, MN 55055

Office: 612 459 2770
FAX:    612 458 1978
BBS:    612 459 1566
E-Mail: 73672.560@compuserve.com
