
    o  See also T-R Recommended Solutions, T-R "Positioning" Chart
    o  HelpFax 1-800-465-3299 - ask for doc# 35052 (Network Card Summary Matrix, 2 pages)
    o  HelpFax 1-800-465-3299 - ask for doc# 35062 (T-Ring Adapter Summary, 25 pages)
    o  HelpFax 1-800-465-3299 - ask for doc# 35058 (T-R 16/4 Adapters, Glossy Brochure, 2 pages)

       ÚÄÄÄÄÄÄÄÂÄÄÄÄÄÄÄÄÄÄÄÂÄÄÄÄÂÄÄÄÄÄÄÂÄÄÄÄÄÄÄÂÄÄÄÄÄÄÄÄÄÄÄÄÂÄÄÄÄÂÄÄÄÄÄÂÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ¿
       ³Single ³bulk p/nos ³Bus ³Speed ³Databus³Architecture³Warr³Conn-³Other                     ³
       ³p/no   ³           ³Type³(Mbps)³Addrbus³            ³anty³ector³                          ³
       ÃÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÄÅÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ´
       ³25F9858³92G9011(5) ³ISA ³4     ³8 bit/ ³shared RAM  ³1 yr³DB9  ³RIPL via 83X7839. UTP/RJ45³
       ³       ³92F9049(30)³    ³      ³20 bit ³            ³    ³     ³via 92F2973               ³
       ÃÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÄÅÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ´
       ³25F7367³60G0987(30)³ISA ³16/4  ³8 bit/ ³shared RAM  ³1 yr³DB9  ³RIPL via 25F8887. UTP/RJ45³
       ³       ³           ³    ³      ³20 bit ³            ³    ³     ³via 92F2973               ³
       ÃÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÄÅÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ´
       ³73G2032³92G9023(5) ³ISA ³16/4  ³16 bit/³shared RAM  ³5 yr³DB9  ³RIPL/UTP filters incl.    ³
       ³       ³73G2079(30)³    ³      ³24 bit ³            ³    ³RJ45 ³LSP-light included        ³
       ÃÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÄÅÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ´
       ³03F0215³60G0989(30)³ISA ³16/4  ³16 bit/³BusMaster   ³5 yr³DB9  ³RIPL/UTP filters included ³
       ³       ³           ³    ³      ³24 bit ³DMA         ³    ³RJ45 ³                          ³
       ÃÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÄÅÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ´
       ³73G8308³N/A        ³ISA ³16/4  ³8 bit/ ³shared RAM  ³1 yr³DB9  ³Trace&Perf (DatagLANce)   ³
       ³       ³           ³    ³      ³20 bit ³            ³    ³     ³UTP/RJ45 via 92F2973      ³
       ÃÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÄÅÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ´
       ³69X8138³N/A        ³MC  ³4     ³16 bit/³shared RAM  ³1 yr³DB9  ³RIPL via 25F8887. UTP/RJ45³
       ³       ³           ³    ³      ³24 bit ³            ³    ³     ³via 92F2973               ³
       ÃÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÄÅÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ´
       ³74F9410³92G9013(5) ³MC  ³16/4  ³16 bit/³shared RAM  ³1 yr³DB9  ³RIPL included. UTP/RJ45   ³
       ³       ³60G0985(30)³    ³      ³24 bit ³            ³    ³     ³via 92F2973               ³
       ÃÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÄÅÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ´
       ³74F4140³n/a        ³MC  ³16/4  ³16 bit ³BusMaster   ³1yr ³DB9  ³STP/UTP RIPL included     ³
       ÃÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÄÅÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ´
       ³74G0801³92G9016(5) ³MC  ³16/4  ³16 bit/³pipeline    ³5 yr³DB9  ³RIPL/UTP filters included ³
       ³       ³74G0813(30)³    ³      ³24 bit ³(streamer)  ³    ³RJ45 ³                          ³
       ÃÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÄÅÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ´
       ³74G0103³92G9015(5) ³MC  ³16/4  ³32 bit/³pipeline    ³5 yr³DB9  ³RIPL/UTP filters included ³
       ³       ³74G0102(30)³    ³      ³32 bit ³(streamer)  ³    ³RJ45 ³                          ³
       ÃÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÄÅÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ´
       ³73G8309³N/A        ³MC  ³16/4  ³16 bit/³shared RAM  ³1 yr³DB9  ³Trace&Perf (DatagLANce).  ³
       ³       ³           ³    ³      ³24 bit ³            ³    ³     ³UTP/RJ45 via 92F2973      ³
       ÃÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÄÅÄÄÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÅÄÄÄÄÅÄÄÄÄÄÅÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ´
       ³63F0412³54G2327    ³EISA³16/4  ³32 bit/³BusMaster   ³5 yr³DB9  ³UTP filters incl. No RIPL ³
       ³       ³           ³    ³      ³32 bit ³DMA         ³    ³RJ45 ³support                   ³
       ÀÄÄÄÄÄÄÄÁÄÄÄÄÄÄÄÄÄÄÄÁÄÄÄÄÁÄÄÄÄÄÄÁÄÄÄÄÄÄÄÁÄÄÄÄÄÄÄÄÄÄÄÄÁÄÄÄÄÁÄÄÄÄÄÁÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÙ


       STP: Shielded Twisted Pair
       UTP: Unshielded Twisted Pair
       RIPL: Remote Initial Program Load




    o  HelpFax 1-800-465-3299 - ask for doc# 35061 (Token Ring ISA Adapter Positioning, 3 pages)
    o  Token Ring Adapter Cross-Reference

    o  Single Part Number  25F9858
    o  Service Part Number  16F0463
    o  Feature Code 9858

    o  30-pack Part Number  60G0987
    o  Feature Code 0987
    o  Bus Master  Yes

       The IBM Token-Ring Network PC Adapter II provides for the attachment of Personal Computers 5160, 5162,
       5170, and PS/2 8525 and 8530 to the IBM Token-Ring Network.  Attachment is provided for rings operating
       at 4M bps.  It requires a single short or standard length feature slot in the PCs and PS/2s.



    o  Token Ring Adapter Cross-Reference
    o  Mktg Part Number  83X7839
    o  Service Part Number  83X7839
    o  Feature Code 7839

       The IBM Token-Ring Network Remote Program Load feature makes it possible for an IBM Personal
       Computer or IBM PS/2 to gain access to the Token-Ring Network and request that it be loaded with
       programs, even though it may not have a disk or diskette drive.  It is required for each of the devices on
       the network that are required to be loaded from a controlling station.  The Remote Program Load (RPL)
       feature is a module designed to be plugged into an available socket on the IBM Token-Ring Network
       Adapters (#3391, #5063, or #9858.)



    o  HelpFax 1-800-465-3299 - ask for doc# 35058 (T-R 16/4 Adapters, Glossy Brochure, 2 pages)
    o  HelpFax 1-800-465-3299 - ask for doc# 35061 (T-R ISA Adapter Positioning, 3 pages)
    o  Token Ring Adapter Cross-Reference
    o  16/4 Token Ring Adapter Positioning

    o  Single Mktg Part Number  25F7367
    o  Service Part Number  93F0334
    o  Feature Code 7367

    o  30-pack Part Number  60G0987
    o  Feature Code 0987

       The IBM Token-Ring Network 16/4 Adapter provides for the attachment of Personal Computers 5160, 5162,
       5170, and PS/2 8525 and 8530 to the IBM Token-Ring Network.  Attachment is provided for rings operating
       at either 4 or 16M bps.  It requires a single standard length (approximately eight inches) feature slot in the
       PCs and PS/2s.



    o  Token Ring Adapter Cross-Reference
    o  Mktg Part Number  25F8887
    o  Service Part Number  83X9180
    o  Feature Code 8881

       Token-Ring Network Adapter/A - Remote Program Load (RPL) is an EPROM designed to be plugged into an
       available socket on the Token-Ring Network Adapter/A (#4790) card.  It is required for each of the
       devices on the network which are to be loaded from a loading device.  The RPL feature will automatically
       issue a request to be loaded any time the device is reset and if the device has no system disk available.
       (Example: Power-on, CTRL-ALT-DEL).  The loading device program is the responsibility of the user and is
       not provided with this feature.

       Each RPL Feature Kit contains one 8K EPROM module with micro code, a 3‡ inch diskette containing a
       sample program for the loading device, and a publication.  The publication contains the following:
       Introduction, Installing the Remote Program Load module, and Programming Requirements.

  .


    o  HelpFax 1-800-465-3299 - ask for doc# 30689 (Announcement letter detail, 8 pages)
    o  HelpFax 1-800-465-3299 - ask for doc# 35058 (T-R 16/4 Adapters, Glossy Brochure, 2 pages)
    o  HelpFax 1-800-465-3299 - ask for doc# 35059 (LAN Product Planning, 13 pages)
    o  HelpFax 1-800-465-3299 - ask for doc# 35061 (T-Ring ISA Adapter Positioning, 3 pages)
    o  Token Ring Adapter Cross-Reference
    o  Token Ring Recommended Solutions

    o  Single Part Number 73G2032 (16-bit adapter)
    o  Service Part Number  73G2048
    o  Feature Code 7462

    o  30-pack Part Number  73G2079
    o  Feature Code 7470

       HIGHLIGHTS

         -  16-bit data path for improved data throughput
         -  Onboard Unshielded Twisted Pair (UTP) filters
         -  ISA bus connection to 16/4 Token-Ring Networks
         -  Remote Program Load (RPL) included
         -  Device drivers included

              o  DOS, OS/2, Novell Netware(R)
              o  Reduced memory DOS transport modules for DOS 802.2 and NETBIOS applications



    o  HelpFax 1-800-465-3299 - ask for doc# 20773 (Announcement letter detail, 8 pages)
    o  HelpFax 1-800-465-3299 - ask for doc# 35058 (T-R 16/4 Adapters, Glossy Brochure, 2 pages)
    o  HelpFax 1-800-465-3299 - ask for doc# 35059 (LAN Product Planning, 13 pages)
    o  HelpFax 1-800-465-3299 - ask for doc# 35061 (T-Ring ISA Adapter Positioning, 3 pages)
    o  Token Ring Adapter Cross-Reference
    o  16/4 Token Ring Adapter Positioning
    o  Token Ring Recommended Solutions

    o  Single Part Number 03F0215 (16-bit adapter)
    o  Service Part Number  03F0212
    o  Feature Code 5120

    o  30-pack Part Number  60G0989
    o  Feature Code 0989

       HIGHLIGHTS

         -  The additional throughput provided by the IBM Token-Ring Network 16/4 Adapter II extends the time
            before additional hardware is required as LAN activity increases.  It supports improved user response
            time as application demands increase.
         -  UTP support allows the option of using telephone twisted-pair media or IBM Cabling System media for
            network wiring.
         -  Device drivers included with the adapter provide the capability to operate with many of today's
            leading network operating systems including OS/2 LAN Server and NetWare(1).
         -  RPL included  with the adapter provides the capability for improved security and simplified Initial
            Program Load content control for workstations without purchasing additional software. (1) Registered
          trade-mark of Novell Corporation.

          PROGRAMMING REQUIREMENTS:

          The IBM Token-Ring Network 16/4 Adapter II is designed to operate with the following programs:

         -  IBM DOS (DOS LAN Requester or workstation environment)

              o  IBM DOS 3.3, 4.0 or 5.0

              o  IBM LAN Support Program 1.3

                 Note:  The PC LAN Program 1.3 using the LAN Support Program and the NDIS driver is only
                 supported as a Requester.

         -  OS/2 (server or workstation environment)

              o  IBM LAN Server Version 2.0 and Version 3.0

              o  IBM Extended Services for OS/2 Version 1.0 including the Communications Manager

          Note:  IBM Extended Services for OS/2 Version 1.0 and Communications Manager run on OS/2 (SE)
          Version 1.30.1 and OS/2 Version 2. IBM LAN Server Version 2.0 runs on OS/2 (SE) Version 1.30.2 and OS/2
          Version 2.

          RPL

         -  NetWare from IBM Version 2.2 and Novell NetWare 2.2 Server Driver

         -  NetWare from IBM Version 3.11 and Novell NetWare 3.11 Server Driver

          Software Support Supplied with 16/4 Adapter II Option Diskette

         -  IBM DOS Network Device Interface Specification (NDIS) Driver

         -  IBM OS/2 NDIS Driver

         -  NetWare from IBM Version 2.2 and Novell NetWare 2.2 Server Driver

         -  NetWare from IBM Version 3.11 and Novell NetWare 3.11 Server Driver

         -  Novell DOS Open Data-Link Interface (ODI) Workstation Driver

         -  Novell OS/2 ODI Workstation Driver

         -  Ring Diagnostic program to assist in problem determination for the token-ring the machine resides on.

         -  Adapter Diagnostic program to assist in problem determination for the adapter.

          Note:  Both 5¥ double-sided, 1.2-MB and 3‡, 720-KB, inch diskettes are provided.

          COMPATIBILITY:

          The following products have been tested and operate properly with the IBM Token-Ring Network 16/4
          Adapter II, P/N 03F0215, F/C 5120:

         -  IBM OS/2 LAN Server Version 2.0 and Version 3.0

         -  IBM Extended Services (ES) Version 1.0 including the Communications Manager

         -  IBM Personal Communications/3270 Version 2.0

          The following Novell device drivers have been certified by Novell through their Independent Manufacture
          Support Program (IMSP):

         -  Novell NetWare 2.2 Server Driver

         -  Novell NetWare 3.11 Server Driver

         -  Novell DOS ODI Workstation Driver

         -  Novell OS/2 ODI Workstation Driver

          LIMITATIONS:

         -  A maximum of three IBM Token-Ring Network 16/4 Adapter IIs may be installed in a machine.  If using
            the LAN Support Program with 2 or more actively running IBM Token-Ring Network 16/4 Adapter IIs in
            the same machine, the LAN Support Program PTF UR37464 is required.  Planned availability for this
            PTF is December 29, 1992.

         -  The IBM Token-Ring Network 16/4 Adapter II will not work in an 8-bit data slot.

         -  On a bridge machine, IBM Token-Ring Network 16/4 Adapter II is not supported by the IBM Token-Ring
            Network Bridge Program.

         -  The IBM Token-Ring Network 16/4 Adapter II can not be used by the LAN Network Manager for
            managing the network at this time.  However  this adapter when installed on other machines in the
            Token-Ring network can be managed by the LAN Network Manager.

          Cable Orders:

          A customer-supplied attachment cable is required by this feature to attach to the IBM Token-Ring
          Network.  The IBM Token-Ring Network PC Adapter Cable (part 6339098), is available from IBM for
          customers desiring shielded twisted pair wiring.  Customers desiring unshielded  twisted pair wiring for
          attachment to the IBM Token-Ring Network, must use a UTP cable with a RJ-45 connector on one end
          for the adapter.  The other end of the cable should have the appropriate connector for attachment to
          the customer's wall outlet.

          Accessories and/or workstation elements can be ordered individually as required by calling IBM Direct via
          the toll-free number 1-800-465-7999.



    o  Token Ring Adapter Cross-Reference
    o  HelpFax 1-800-465-3299 - ask for doc# 31146 (Annc. letter, 5 pages)

    o  Mktg Part Number  73G8308 (ISA)
    o  Service Part Number  73G8308
    o  Feature Code 8308

    o  Mktg Part Number  73G8309 (MC)
    o  Service Part Number  73G8309
    o  Feature Code 8309

    o  Mktg Part Number  73G8310 (PCMCIA)
    o  Service Part Number  73G8310
    o  Feature Code 8310

       The IBM DatagLANce (tm) Token-Ring Adapters ensure that the LAN Network Manager does not remove
       them from the ring and provide maximum performance for the DatagLANce Network Analyzer Software.
       These adapters should only be used with the DatagLANce Network Analyzer Software, reference Product
       Announcement A93-1147, dated November 12, 1993.

       The DatagLANce Network Analyzer for Ethernet and Token-Ring Software provides network managers and
       support personnel the ability to fine-tune and trouble-shoot an Ethernet or Token-Ring Network.
       DatagLANce displays real-time statistics about the network as well as providing frame capture and 7-layer
       protocol decode functions. It uses an OS/2 graphical user interface to present information with complete
       full on-line help and references . This information is a useful aid for debugging application software,
       capacity planning, network reconfigurations, as well as trouble-shooting inter-networking protocols.



    o  Token Ring Adapter Cross-Reference
    o  Mktg Part Number  69X8138
    o  Service Part Number  25F7540
    o  Feature Code 4790
    o  POS ID: E000

       Token-Ring Network attachment for the PS/2 Micro Channel is available through this option.  The adapter
       transmits and receives at a speed of four million bpi using protocols conforming to IEEE 802.5 and ECMA 89
       standards.  The adapter provides logical link control functions conforming with the IEEE 802.2 standard.
       The adapter is compatible with International Standard ISO - 8802/5.  The adapter provides 16K bytes of
       Random Access Memory (RAM) for increased message segment size and/or increasing the number of link
       stations supported by the adapter.

       The Token-Ring Network Adapter/A is a feature card for the PS/2 Micro Channel systems.  The adapter
       contains a microprocessor operating under control of adapter resident microcode.  This adapter requires
       one slot. A diskette is included with the adapter which contains an adapter description file, adapter
       diagnostic and a single ring network diagnostic.  The adapter diagnostic program is used to verify the
       correct operation of the adapter.

       The ring diagnostic program is used as an aid in network problem determination.  Permanent and
       recoverable error conditions are detected, and information on the probable source of the error is
       presented.  The Token-Ring Network Problem Determination Guide, SX27-3710, should be obtained for
       instructions on how to use the ring diagnostic.

       An Installation and Testing Instructions document is included with the adapter to assist the customer with
       the adapter set up. Pre-requisites:  A customer supplied attachment cable is required for connecting the
       adapter to the network cabling system.  The Token-Ring Network PC Adapter Cable (FC 3390, P/N
       6339098) for the Cabling System available from IBM or the Type 3 Media Filter for the Type 3 cable
       available from Authorized Referenced IBM Distributors.  Customer Setup (CSU):  Yes.

  HIGHLIGHTS:

    o  Transmits and receives at 4 million bits-per-second
    o  Provides 16KB of random access memory (RAM)

       Designed specifically for the PS/2 Micro Channel advanced I/O channel to take advantage of the greater
       80286 and 80386 processing speeds.
    o  Provides for Remote Program Load (RPL) as an optional feature

  .


    o  Token Ring Adapter Cross-Reference
    o  16/4 Token Ring Adapter Positioning
    o  Token Ring Recommended Solutions
    o  HelpFax 1-800-465-3299 - ask for doc# 35058 (T-R 16/4 Adapters, Glossy Brochure, 2 pages)

    o  Mktg Part Number  74F9410
    o  Service Part Number  93F0331
    o  Feature Code 0149

    o  30-pack Part Number  60G0985
    o  Feature Code 0985
    o  POS ID: E001

       The IBM Token-Ring Network 16/4 Adapter/A is used to attach an IBM PS/2 (PS/2) to an IBM Token-Ring
       Network operating at either 16 million or 4 million bits per second.  It requires one feature slot in the PS/2.
       Limitations:  Maximum:  Two.  Pre-requisites:  None.  Co-requisites:  None. Compatibility Conflicts:  None.
       Customer Setup:  Yes.  Field Installable: Yes.  Cable Order:  IBM Token-Ring PC Adapter Cable, P/N 6339098,
       FC 3390, may be ordered for attachment to the network.  If the IBM Token-Ring Network 16/4 Adapter/A is
       installed in an 8573 short slot, IBM Token-Ring L-Shaped Connector Cable, P/N 79F3229, FC 3229, must be
       ordered in addition to the IBM Token-Ring Adapter Cable.

  .


    o  Token Ring Adapter Cross-Reference
    o  16/4 Token Ring Adapter Positioning
    o  Token Ring Recommended Solutions
    o  HelpFax 1-800-465-3299 - ask for doc# 35058 (T-R 16/4 Adapters, Glossy Brochure, 2 pages)

    o  Mktg Part Number  74F9410
    o  Service Part Number  93F0331
    o  Feature Code 0149

    o  30-pack Part Number  60G0985
    o  Feature Code 0985
    o  POS ID: E001

       The IBM Token-Ring Network 16/4 Adapter/A is used to attach an IBM PS/2 (PS/2) to an IBM Token-Ring
       Network operating at either 16 million or 4 million bits per second.  It requires one feature slot in the PS/2.
       Limitations:  Maximum:  Two.  Pre-requisites:  None.  Co-requisites:  None. Compatibility Conflicts:  None.
       Customer Setup:  Yes.  Field Installable: Yes.  Cable Order:  IBM Token-Ring PC Adapter Cable, P/N 6339098,
       FC 3390, may be ordered for attachment to the network.  If the IBM Token-Ring Network 16/4 Adapter/A is
       installed in an 8573 short slot, IBM Token-Ring L-Shaped Connector Cable, P/N 79F3229, FC 3229, must be
       ordered in addition to the IBM Token-Ring Adapter Cable.

  .


    o  HelpFax 1-800-465-3299 - ask for doc# 95002 (Trade-in promotion detail - to 74G0103 LANStreamer 32
       Adapter/A)
    o  Token Ring Adapter Cross-Reference
    o  HelpFax 1-800-465-3299 - ask for doc# 35058 (T-R 16/4 Adapters, Glossy Brochure, 2 pages)

    o  Mktg Part Number 74F4140
    o  Service Part Number  74F4149
    o  Feature Code 4041
    o  POS ID: 8FC8
    o  Bus Master  Yes
    o  Withdrawn 30 June/93 (replacement 74G0103)

       Used to attach a PS/2 computer with the Micro Channel bus, configured as a server, to an IBM Token-Ring
       Network operating at either 16 million or 4 million bits per second. Provides high throughput capability
       while requiring less host- processor involvement than previous IBM Token-Ring adapters. This reduction in
       host-processor involvement is enabled through the bus master capability of the adapter which allows
       adapter-to-system-memory transfer of data independent of the host-processor.  The server's processor is
       available for other tasks.



    o  HelpFax 1-800-465-3299 - ask for doc# 35055 (Glossy brochure, MC-32 and MC-16 versions, 3 pages)
    o  HelpFax 1-800-465-3299 - ask for doc# 95002 (Trade-in promotion detail - from 74F4140 Token Ring 16/4
       Busmaster Server Adapter/A)
    o  Token Ring Adapter Cross-Reference
    o  16/4 Token Ring Adapter Positioning
    o  Token Ring Recommended Solutions

    o  Marketing Single MC-32 Part Number 60G1592
    o  p/no changed from 92F8942, 74G0103
    o  Service MC-32 Part Number 74G0098
    o  Feature Code 8942
    o  Bus Master  Yes
    o  Warranty    5 years

    o  5-pack MC-32 Part Number 92G9015
    o  30-pack MC-32 Part Number 74G0102
    o  p/no changed from 60G1100
    o  Feature Code 1100


    o  Marketing Single MC-16 Part Number 74G0801
    o  p/no changed from 59G8998
    o  Service MC-16 Part Number 74G0800
    o  Feature Code 8998

    o  5-pack MC-16 Part Number 92G9016
    o  30-pack MC-16 Part Number 74G0813
    o  Feature Code 1515


    o  Marketing Single EISA Part Number 63F0412
    o  Service EISA Part Number 63F0417
    o  Feature Code 0412
    o  Bus Master  Yes

    o  30-pack EISA Part Number 54G2327
    o  Feature Code 2327

    o  Bus Master  Yes
    o  Warranty    5 years

       HIGHLIGHTS

         -  Improved performance for servers provided by the IBM LANStreamer MC 32 and MC 16 Adapters extend
            the time before additional hardware is required as local area network (LAN) activity increases. With
            the adapters providing media speed on a 16 Mbps token ring, user response time is improved as
            application demands increase.
         -  Unshielded Twisted Pair (UTP) support provides the user with greater flexibility and improved usability
            without requiring an external filter and allows easy movement of the adapter in the customer's
            environment to adapt to either UTP or Shielded Twisted Pair (STP) wiring schemes.

          DESCRIPTION Increased Performance

          The new enhanced Token-Ring technology incorporated on the IBM LANStreamer MC 32 and MC 16
          Adapters provides significant performance improvements. These include frame processing capacity of
          over 30,000 frames per second and very low latency (under 50 microseconds).

          Both UTP and STP connectors are offered on the IBM LANStreamer MC 32 Adapter, providing greater
          flexibility in meeting customer's wiring plans. The dual connections provide portability in the growing
          Token-Ring Network without requiring customers to rewire existing buildings.

          DEVICE DRIVERS PROVIDED WITH ADAPTER

          The device drivers shipped with each adapter include both OS/2 and NetWare 3.1 and 4.0 (when
          available) server drivers. DOS NDIS server and workstation drivers, OS/2 workstation NDIS driver and ODI
          workstation driver will be available April 30, 1993.
          *NetWare is a registered trade-mark of Novell, INC.

          USER PRODUCTIVITY

          Because of the IBM LANStreamer Adapters' increased throughput capacity, more clients can be supported
          using a single adapter without degrading customer response time. In addition, the adapters' faster file
          transfer performance can result in reduction of 20% to 30% in the time It takes customers to download
          files from their servers in a NetWare(R) 3.11 environment. Similar improvements can be expected in a
          LAN server environment.

          * NetWare is a registered trade-mark of Novell, INC.

          CONNECTIVITY SOLUTIONS.

          The IBM LANStreamer MC 32 and MC 16 Adapters offer both UTP and STP connections at 16Mbps or 4
          Mbps without the use of external filters. The dual connectivity makes the adapter very portable and
          easy to adapt to either media installation.

          Many applications require access to random access memory (RAM) above the 16MB range. The IBM
          LANStreamer MC 32 and MC 16 Adapter and associated software provide this capability to applications,
          thus freeing the memory ranges below 16MB.

          ENHANCED ADAPTER TECHNOLOGY

          New priority transmit and receive channels have also been included in the new technology providing an
          easy migration to the multimedia applications without the addition of new hardware.

          POSITIONING

          The current Token-Ring 16/4 Adapter/A should be used in:  memory constrained DOS environments;
          where the adapter is dedicated to 3270 emulation; and with the IBM Token-Ring Bridge Program.

          The Token-Ring 16/4 Busmaster adapter may be used interim to the availability of the IBM LANStreamer
          MC 32 Adapter

          TECHNICAL INFORMATION

           Width:  8.827cm (3.476 inches)
           Length: 20.32cm (8 inches)
           Depth:  2.667cm (1 inch)
           Weight: 5.33 oz.

          OPERATING ENVIRONMENT

          This product meets DOC equivalent of FCC Class A criteria (up to 6 adapters per machine) when
          configured with shielded cabling which meets the IBM specifications.

          This product meets DOC equivalent of FCC Class A criteria (up to 6 adapters per machine) when
          configured with unshielded cabling (UTP) which meets the IBM specifications.



    o  HelpFax 1-800-465-3299 - ask for doc# 35055 (Glossy brochure, MC-32 and MC-16 versions, 3 pages)
    o  HelpFax 1-800-465-3299 - ask for doc# 95002 (Trade-in promotion detail - from 74F4140 Token Ring 16/4
       Busmaster Server Adapter/A)
    o  Token Ring Adapter Cross-Reference
    o  16/4 Token Ring Adapter Positioning
    o  Token Ring Recommended Solutions

    o  Marketing Single MC-32 Part Number 60G1592
    o  p/no changed from 92F8942, 74G0103
    o  Service MC-32 Part Number 74G0098
    o  Feature Code 8942
    o  Bus Master  Yes
    o  Warranty    5 years

    o  5-pack MC-32 Part Number 92G9015
    o  30-pack MC-32 Part Number 74G0102
    o  p/no changed from 60G1100
    o  Feature Code 1100


    o  Marketing Single MC-16 Part Number 74G0801
    o  p/no changed from 59G8998
    o  Service MC-16 Part Number 74G0800
    o  Feature Code 8998

    o  5-pack MC-16 Part Number 92G9016
    o  30-pack MC-16 Part Number 74G0813
    o  Feature Code 1515


    o  Marketing Single EISA Part Number 63F0412
    o  Service EISA Part Number 63F0417
    o  Feature Code 0412
    o  Bus Master  Yes

    o  30-pack EISA Part Number 54G2327
    o  Feature Code 2327

    o  Bus Master  Yes
    o  Warranty    5 years

       HIGHLIGHTS

         -  Improved performance for servers provided by the IBM LANStreamer MC 32 and MC 16 Adapters extend
            the time before additional hardware is required as local area network (LAN) activity increases. With
            the adapters providing media speed on a 16 Mbps token ring, user response time is improved as
            application demands increase.
         -  Unshielded Twisted Pair (UTP) support provides the user with greater flexibility and improved usability
            without requiring an external filter and allows easy movement of the adapter in the customer's
            environment to adapt to either UTP or Shielded Twisted Pair (STP) wiring schemes.

          DESCRIPTION Increased Performance

          The new enhanced Token-Ring technology incorporated on the IBM LANStreamer MC 32 and MC 16
          Adapters provides significant performance improvements. These include frame processing capacity of
          over 30,000 frames per second and very low latency (under 50 microseconds).

          Both UTP and STP connectors are offered on the IBM LANStreamer MC 32 Adapter, providing greater
          flexibility in meeting customer's wiring plans. The dual connections provide portability in the growing
          Token-Ring Network without requiring customers to rewire existing buildings.

          DEVICE DRIVERS PROVIDED WITH ADAPTER

          The device drivers shipped with each adapter include both OS/2 and NetWare 3.1 and 4.0 (when
          available) server drivers. DOS NDIS server and workstation drivers, OS/2 workstation NDIS driver and ODI
          workstation driver will be available April 30, 1993.
          *NetWare is a registered trade-mark of Novell, INC.

          USER PRODUCTIVITY

          Because of the IBM LANStreamer Adapters' increased throughput capacity, more clients can be supported
          using a single adapter without degrading customer response time. In addition, the adapters' faster file
          transfer performance can result in reduction of 20% to 30% in the time It takes customers to download
          files from their servers in a NetWare(R) 3.11 environment. Similar improvements can be expected in a
          LAN server environment.

          * NetWare is a registered trade-mark of Novell, INC.

          CONNECTIVITY SOLUTIONS.

          The IBM LANStreamer MC 32 and MC 16 Adapters offer both UTP and STP connections at 16Mbps or 4
          Mbps without the use of external filters. The dual connectivity makes the adapter very portable and
          easy to adapt to either media installation.

          Many applications require access to random access memory (RAM) above the 16MB range. The IBM
          LANStreamer MC 32 and MC 16 Adapter and associated software provide this capability to applications,
          thus freeing the memory ranges below 16MB.

          ENHANCED ADAPTER TECHNOLOGY

          New priority transmit and receive channels have also been included in the new technology providing an
          easy migration to the multimedia applications without the addition of new hardware.

          POSITIONING

          The current Token-Ring 16/4 Adapter/A should be used in:  memory constrained DOS environments;
          where the adapter is dedicated to 3270 emulation; and with the IBM Token-Ring Bridge Program.

          The Token-Ring 16/4 Busmaster adapter may be used interim to the availability of the IBM LANStreamer
          MC 32 Adapter

          TECHNICAL INFORMATION

           Width:  8.827cm (3.476 inches)
           Length: 20.32cm (8 inches)
           Depth:  2.667cm (1 inch)
           Weight: 5.33 oz.

          OPERATING ENVIRONMENT

          This product meets DOC equivalent of FCC Class A criteria (up to 6 adapters per machine) when
          configured with shielded cabling which meets the IBM specifications.

          This product meets DOC equivalent of FCC Class A criteria (up to 6 adapters per machine) when
          configured with unshielded cabling (UTP) which meets the IBM specifications.



    o  Token Ring Adapter Cross-Reference
    o  HelpFax 1-800-465-3299 - ask for doc# 31146 (Annc. letter, 5 pages)

    o  Mktg Part Number  73G8308 (ISA)
    o  Service Part Number  73G8308
    o  Feature Code 8308

    o  Mktg Part Number  73G8309 (MC)
    o  Service Part Number  73G8309
    o  Feature Code 8309

    o  Mktg Part Number  73G8310 (PCMCIA)
    o  Service Part Number  73G8310
    o  Feature Code 8310

       The IBM DatagLANce (tm) Token-Ring Adapters ensure that the LAN Network Manager does not remove
       them from the ring and provide maximum performance for the DatagLANce Network Analyzer Software.
       These adapters should only be used with the DatagLANce Network Analyzer Software, reference Product
       Announcement A93-1147, dated November 12, 1993.

       The DatagLANce Network Analyzer for Ethernet and Token-Ring Software provides network managers and
       support personnel the ability to fine-tune and trouble-shoot an Ethernet or Token-Ring Network.
       DatagLANce displays real-time statistics about the network as well as providing frame capture and 7-layer
       protocol decode functions. It uses an OS/2 graphical user interface to present information with complete
       full on-line help and references . This information is a useful aid for debugging application software,
       capacity planning, network reconfigurations, as well as trouble-shooting inter-networking protocols.



    o  HelpFax 1-800-465-3299 - ask for doc# 35055 (Glossy brochure, MC-32 and MC-16 versions, 3 pages)
    o  HelpFax 1-800-465-3299 - ask for doc# 95002 (Trade-in promotion detail - from 74F4140 Token Ring 16/4
       Busmaster Server Adapter/A)
    o  Token Ring Adapter Cross-Reference
    o  16/4 Token Ring Adapter Positioning
    o  Token Ring Recommended Solutions

    o  Marketing Single MC-32 Part Number 60G1592
    o  p/no changed from 92F8942, 74G0103
    o  Service MC-32 Part Number 74G0098
    o  Feature Code 8942
    o  Bus Master  Yes
    o  Warranty    5 years

    o  5-pack MC-32 Part Number 92G9015
    o  30-pack MC-32 Part Number 74G0102
    o  p/no changed from 60G1100
    o  Feature Code 1100


    o  Marketing Single MC-16 Part Number 74G0801
    o  p/no changed from 59G8998
    o  Service MC-16 Part Number 74G0800
    o  Feature Code 8998

    o  5-pack MC-16 Part Number 92G9016
    o  30-pack MC-16 Part Number 74G0813
    o  Feature Code 1515


    o  Marketing Single EISA Part Number 63F0412
    o  Service EISA Part Number 63F0417
    o  Feature Code 0412
    o  Bus Master  Yes

    o  30-pack EISA Part Number 54G2327
    o  Feature Code 2327

    o  Bus Master  Yes
    o  Warranty    5 years

       HIGHLIGHTS

         -  Improved performance for servers provided by the IBM LANStreamer MC 32 and MC 16 Adapters extend
            the time before additional hardware is required as local area network (LAN) activity increases. With
            the adapters providing media speed on a 16 Mbps token ring, user response time is improved as
            application demands increase.
         -  Unshielded Twisted Pair (UTP) support provides the user with greater flexibility and improved usability
            without requiring an external filter and allows easy movement of the adapter in the customer's
            environment to adapt to either UTP or Shielded Twisted Pair (STP) wiring schemes.

          DESCRIPTION Increased Performance

          The new enhanced Token-Ring technology incorporated on the IBM LANStreamer MC 32 and MC 16
          Adapters provides significant performance improvements. These include frame processing capacity of
          over 30,000 frames per second and very low latency (under 50 microseconds).

          Both UTP and STP connectors are offered on the IBM LANStreamer MC 32 Adapter, providing greater
          flexibility in meeting customer's wiring plans. The dual connections provide portability in the growing
          Token-Ring Network without requiring customers to rewire existing buildings.

          DEVICE DRIVERS PROVIDED WITH ADAPTER

          The device drivers shipped with each adapter include both OS/2 and NetWare 3.1 and 4.0 (when
          available) server drivers. DOS NDIS server and workstation drivers, OS/2 workstation NDIS driver and ODI
          workstation driver will be available April 30, 1993.
          *NetWare is a registered trade-mark of Novell, INC.

          USER PRODUCTIVITY

          Because of the IBM LANStreamer Adapters' increased throughput capacity, more clients can be supported
          using a single adapter without degrading customer response time. In addition, the adapters' faster file
          transfer performance can result in reduction of 20% to 30% in the time It takes customers to download
          files from their servers in a NetWare(R) 3.11 environment. Similar improvements can be expected in a
          LAN server environment.

          * NetWare is a registered trade-mark of Novell, INC.

          CONNECTIVITY SOLUTIONS.

          The IBM LANStreamer MC 32 and MC 16 Adapters offer both UTP and STP connections at 16Mbps or 4
          Mbps without the use of external filters. The dual connectivity makes the adapter very portable and
          easy to adapt to either media installation.

          Many applications require access to random access memory (RAM) above the 16MB range. The IBM
          LANStreamer MC 32 and MC 16 Adapter and associated software provide this capability to applications,
          thus freeing the memory ranges below 16MB.

          ENHANCED ADAPTER TECHNOLOGY

          New priority transmit and receive channels have also been included in the new technology providing an
          easy migration to the multimedia applications without the addition of new hardware.

          POSITIONING

          The current Token-Ring 16/4 Adapter/A should be used in:  memory constrained DOS environments;
          where the adapter is dedicated to 3270 emulation; and with the IBM Token-Ring Bridge Program.

          The Token-Ring 16/4 Busmaster adapter may be used interim to the availability of the IBM LANStreamer
          MC 32 Adapter

          TECHNICAL INFORMATION

           Width:  8.827cm (3.476 inches)
           Length: 20.32cm (8 inches)
           Depth:  2.667cm (1 inch)
           Weight: 5.33 oz.

          OPERATING ENVIRONMENT

          This product meets DOC equivalent of FCC Class A criteria (up to 6 adapters per machine) when
          configured with shielded cabling which meets the IBM specifications.

          This product meets DOC equivalent of FCC Class A criteria (up to 6 adapters per machine) when
          configured with unshielded cabling (UTP) which meets the IBM specifications.


