	 GENOA GVGA 6000 SERIES BOARDS DRIVER INSTALLATION
		  FOR MICROSOFT WINDOWS 3.0 & 3.1

The following instructions are applicable to users of Microsoft Windows 3.X.
Note: to use 800x600 or higher resolution modes, a multisync ANALOG
monitor capable of synchronizing with these modes is required.

Follow the instructions listed below carefully to install the drivers.

Instructions:

1. Follow Windows 3.0 or 3.1 setup procedures to install Windows. Run an
   application program to make sure you have successfully installed Windows.

2. Exit to DOS and put the "GENOA SuperVGA Utility Programs, DISK #2"
   into floppy drive A. And then change directory to "a:\WIN3X".

3. Run "INSTALL.EXE" and follow the program instructions.

4. From the Windows 3.0 or 3.1 driectory, run "SETUP.EXE".

5. Scroll through the display options until you find the Genoa GVGA display
   options.  Select the appropriate display resolution.

6. Restart Windows.


NOTE:

1. The drivers support the following video modes:
    Resolution         Minimum display     Driver name         Windows Font
		       memory required

    640x480x16              256kb          VGA.DRV      **     VGA
    800x600x16              256kb          GVGA86.DRV          VGA
    640x480x256             512kb          G640256.DRV         VGA
    800x600x256             512kb          G800256.DRV         VGA
   1024x768x16              512kb          GVGA1k.DRV          8514

   ** uses the VGA drivers come with Windows 3.0 or 3.1 

2. If you wish to change the display type after completing the installation,
   click on the Windows Setup icon found in the Main desktop window or run 
   the "SETUP.EXE" program.
