
      *****                                                         *****
      ***** GENOA SuperVGA 6000 Series Utilities & Drivers Diskette *****
      *****                                                         *****

>> DISK #1
         \UTIL\
              RAM resident video bios driver
                                                 rambios .sys
              Extended ANSI driver
                                                 gansi   .sys
              Smooth/jump scrolling utility
                                                 smooth  .com
                                                 jump    .com
              Setmode & diagnostic utility
                                                 gvga    .exe
              Manual performance tuning utility
                                                 tune    .exe
              Automatic performance tuning utility
                                                 atune   .exe
              Extended clear screen utility
                                                 clear   .com
              Video Passthrough utility
                                                 vpass   .exe
         \AUTOCAD\
              Autodesk AutoCAD 2.5 drivers
                  1024x768x16 colors             ds5f    .exe
                  1024x768x4 colors              ds7f    .exe
                  800x600x16 colors              ds86    .exe
              Autodesk AutoCAD 9.0 & 10.0 drivers
                  1024x768x16 colors             ds1k16  .exe
                  1024x768x4 colors              ds1k4   .exe
                  800x600x16 colors              ds800   .exe
                  color selection program
                    (for four colors mode only)  color4  .exe
                  800x600x256 colors             ds8256  .exe
                  640x480x256 colors             ds6256  .exe
              Autodesk AutoCAD 9.0 & 10.0 display list drivers
                  1024x768x16 colors             dsdl1k  .exe
                  800x600x16 colors              dsdl800 .exe
         \AUTOSHAD\
              Autodesk AutoShade 1.1 Display & Rendering drivers
                  800x600x256 colors             rd800   .com
                  640x480x256 colors             rd640   .com
                  512x512x256 colors             rd512   .com
         \ACAD386\
              Autodesk AutoCAD 10, 386 version drivers
                  1024x768x16 colors             dsp1024 .exp
                  800x600x16 colors              dsp800  .exp
         \GEMVEN\
              Xerox Ventura Publisher 3.0, 2.0 & 1.1 drivers
                  1024x768x16 colors             sd1k16  .vga
                  1024x768x2 colors              sd1k2c  .vga
                  800x600x16 colors              sd800600.vga
         \GEMVEN\
              Digital Research GEM/3 3.11, 3.01 driver
                  1024x768x16 colors             sd1k16  .vga
                  1024x768x2 colors              sd1k2c  .vga
                  800x600x16 colors              sd800600.vga
         \LOTUS\
              Lotus-123 2.01, 2.20 & Symphony 2.0 text driver
                  132 x 25/29/32/44/60           132xall .drv
         \WP51\
              WordPerfect 5.1 graphics driver
                  1024x768x16 colors             gna1k16 .vrs
         \WP50\
              WordPerfect 5.0 graphics driver
                  1024x768x16 colors             wp1k16  .wpd
                  800x600x16 colors              wp800   .wpd
>> DISK #2
         \PM\
              Microsoft OS/2 Presentation Manager 1.1 drivers
                  800x600x16 colors              gvga800 .dll
                  640x480x16 colors              gvga640 .dll
         \WIN30\
              Microsoft Windows 3.0 drivers
                  640x480x256 colors
                  800x600x16  colors
                  1024x768x16 colors

         \WIN386\
              Microsoft Windows/386 2.10 & 2.03 drivers
                  800x600x8 colors
                  1024x768x8 colors
         \WIN286\
              Microsoft Windows/286 2.10 & 2.03 drivers
                  800x600x8 colors
                  1024x768x8 colors

         *****    1024x768 16 colors mode only works on GENOA SuperVGA
                  6400 and 6600 Microchannel graphics board.
         *****    800x600 256 colors and 640x480 256 colors modes only
                  work on GENOA SuperVGA 6400 and 6600 Microchannel
                  graphics board.

*****************************************************************************
>>>  DISK   # 1
********************************************************************************
RAMBIOS device driver.              (in directory  \UTIL)

   - RAMBIOS  SYS  ...a program to speed up video read and write operation.

     Put DEVICE=RAMBIOS.SYS as the first device driver command in CONFIG.SYS
     file. It should be installed before any other device driver in order to be
     compatible with most application programs.

********************************************************************************
GANSI device driver.                (in directory  \UTIL)

   - GANSI    SYS  ...an enhanced standard input and standard output
                      device driver

     Include DEVICE=GANSI.SYS in CONFIG.SYS file. This command causes DOS
     to replace the standard input and output support by the extended
     SuperVGA features.

********************************************************************************
SMOOTH/JUMP scrolling utility.      (in directory  \UTIL)

   - SMOOTH   COM  ...smooth scrolling
   - JUMP     COM  ...jump scrolling

     To obtain a better result, system speed should be 8 MHz or up. Type
     "smooth" at DOS prompt, the display will be changed to smooth scrolling
     screen, or type "jump" at the DOS prompt, display will be toggled to
     jump scroll when speed is preferred.

****************************************************************************
Set mode and Diagnostic utility.    (in directory  \UTIL)

   - GVGA     EXE ...a menu driven mode switching utility

     This set mode and diagnostic program allows you to select and preview
     any mode that is available to your configuration. You may run this
     program either directly from the DOS prompt or from a menu.

     USAGE  ::

         1)  GVGA   <enter>
             Type this command at the DOS prompt, you are entering a menu-
             driven set mode  program. There are six menus, and you will be
             entering one of  these menus depending on the monitor and the
             switch setting of the SuperVGA adapter.

         2)  GVGA   KEYWORD    <enter>
             For instance GVGA V13 <enter>, you are entering the 320x200
             256-color graphics mode.
             To return to the default mode use: GVGA V3 <enter>

         3)  GVGA   [MDA, CGA, HCD]     <enter>
             GVGA   {AON, AOFF}         <enter>
             All the backward compatibility support, including MDA/Hercules,
             CGA and CDOS (Chinese applications based on Hercules), are listed
             in each GVGA menu. These features can be enabled by either using
             the syntax mentioned above or simply enter AON (AutoDisplay ON)
             or AOFF (AutoDisplay OFF) to enable or disable all backward
             support.

         4)  GVGA   [60, 70]            <enter>
             The Flicker-Free feature in the GVGA increases the vertical
             refresh rate of 640x480 mode from 60 Hz to 70 Hz for all
             SuperVGA 6000 series product.
             For models 6600A and 6400A, this may increase the vertical
             refresh rates to 70 Hz for all the 640x480, 800x600, and
             1024x768 modes. After entering the above command, you will be
             provided with a list of 70Hz modes.

         5)  GVGA   [256,512]           <enter>
             This toggle function allows you to override the video RAM size
             if your system failed to detect it correctly.
             For example, model 6300 only has 256K memory, and model 6400,
             6400A or 6600 have 512K memory.

         NOTE :  Press 'W' under 640x480, 800x600, or 1024x768 modes, a
                 white rectangle will show on the screen. You may press '6'
                 to change the refresh rate to 60 Hz or press '7' to 70 Hz.
                 This white rectangle can show you the flicking difference
                 between 60 Hz and 70Hz. 'W' is a toggle hardkey, press 'W'
                 again, it switches you back to GVGA display screen.

****************************************************************************
Manual performance tuning utility.           (in directory  \UTIL)

   - TUNE     EXE ...a manual tuning program to set graphics speed ratio

     This utility can tune the system and graphics configuration to its
     best performance. By typing

          TUNE   <enter>
     at the DOS prompt and choosing the ratio that you prefer. You can
     manually tune the parameters as your requirement, or you may type

          TUNE   RATIO VALUE    <enter>
     to perform the same function. The valid ratio value are 2, 3, and 4.
     The default value is 4.

****************************************************************************
Automatic performance tuning utility.        (in directory  \UTIL)

   - ATUNE    EXE ...an automatic tuning program to set graphics speed ratio

     This utility automatically gives you the best performance ratio when
     you type ATUNE at the DOS prompt.

****************************************************************************
Extended clear screen utility.               (in directory  \UTIL)

   - CLEAR    COM ...clear screen function for GENOA extended mode

     The DOS 4.0 clear screen command, CLS only clears a portion of the screen
     under extended modes. For DOS 4.0 users, please use CLEAR.COM instead of
     CLS to clear the whole screen.

     Copy this file, CLEAR.COM, to the root directory of your boot drive,
     and set a PATH to root. Therefore, you can use CLEAR.COM wherever
     you want to.

*****************************************************************************
Video Passthrough utility:                   (in directory  \UTIL)

   - VPASS    EXE ...enable/disable the Video Passthrough function

     Vpass.exe is used to enable or disable the Video Passthrough function.
     The command syntax is shown below :

     DOS-PROMPT>  VPASS   BasicVGA (or VPASS B)    <enter>

                  Enable BasicVGA capability.
                  This means that only the system board VGA capability is
                  available to you through Genoa's SuperVGA connector.

     DOS-PROMPT>  VPASS   SuperVGA (or VPASS S)    <enter>

                  Enable SuperVGA capability.
                  This means that the system board VGA is disabled and the
                  SuperVGA capability is available to you.

     DOS-PROMPT>  VPASS   <enter>

                  Display current video status.

*****************************************************************************
AutoCAD 9.0 & 10.0 driver.                   (in directory  \AUTOCAD)

     - DS1K4    EXE ...1024x768x4  colors driver
     - DS1K16   EXE ...1024x768x16 colors driver
     - DS800    EXE ...800x600x16 colors driver
     - COLOR4   EXE ...An interactive color selection program for 4 colors mode
     - DS8256   EXE ...800x600x256 colors driver
     - DS6256   EXE ...640x480x256 colors driver

       Installation Procedures,
          (1)  Install AutoCAD 9.0/10.0 follows normal AutoCAD procedures.
          (2)  Invoke AutoCAD by typing ACAD at the DOS prompt.

               >>   ACAD    <enter>

          (3)  From the AutoCAD main Menu, select option number 5,
               "Configure AutoCAD".

               Enter selection : 5     <enter>
               Press RETURN to continue:   <enter>

          (4)  From the AutoCAD Configuration menu, select option number 3,
               "Configure video display".

               Enter selection <0> :  3     <enter>
               Type "Yes" to select a new display.

          (5)  From the Available video displays, select number 1 for
               "ADI display".

               Select device number ......:   1   <enter>
               Hexadecimal interrupt code (INT 0XXh) <7A> :   <enter>

               Answer your preference options Yes, No or accept the default
               by pressing <enter>.

          (6)  From the Configuration menu, select number 0,
               "Exit to Main Menu".

               Enter selection <0>  :     <enter>
               Keep Configuration changes? <Y>    <enter>

          (7)  From AutoCAD Main Menu, select number 0,
               "Exit to AutoCAD".

               Enter selection  :  0    <enter>

          (8)  Copy "DS1K16.EXE", "DS800.EXE", "DS1K4.EXE", "COLOR4.EXE",
               "DS8256.EXE", and "DS6256.EXE" to AutoCAD 9 or 10 directory.

          (9)  Execute "DS1K16.EXE" or "DS1K4.EXE" for the 1024x768x16/4
               color resolution mode or "DS800.EXE" for the 800x600x16
               resolution mode.
               Execute "DS8256.EXE" for the 800x600x256 color resolution mode.
               Execute "DS6256.EXE" for the 640x480x256 color resolution mode.
               Before running DS1K4.EXE you may execute COLOR4.EXE to select
               the desired color option for this four colors mode. (see note 2)

               >>  DSxxx [?] [i] [xx]     <enter>

               Example:
                         DSxxx ?  <enter>
               The following will be displayed:

                   Usage : DSxxx [?] [i] [xx]
                   i       Black Background
                   xx      Installation Vector in HEX
                   ?       This message

               *** DRIVER NOT INSTALLED ***

               The i option (inverse video) installs a Black Background instead
               of the default White Background.
               The xx option is two hexadecimal digits specifying an interrupt
               vector other than the default 7Ah.  On a NOVELL network
               specifying 7Bh here, and in the Autocad ADI selection, will
               remove the interrupt conflict.

               You need to install this driver once at every power up.

         (10)  Type "ACAD" to run AutoCAD.
               To run AutoCAD with two monitors, type "Mode Mono" to switch to
               the secondary monitor, and then type "ACAD".

               >>  MODE MONO   <enter>
               >>  ACAD        <enter>


     NOTE.1. ::  GENOA.RGB will be created/modified when you run ds1k16.exe,
                 ds800.exe, ds8256.exe, or ds6256.exe. GENOA.RGB contains the
                 color attribute to supply individual color for parts of the
                 AutoCAD graphics screen. You may change the screen color by
                 editing GENOA.RGB file or updating color attributes when
                 executing those driver files.
                 If you want to reset the screen to default color after you
                 modified GENOA.RGB. Delete GENOA.RGB and run the driver file
                 to set the default color.

     NOTE.2. :::::::::  Color Selection for 4 colors mode  ::::::::::::::::

       RGB4.TXT is a file with color selection for GENOA GVGA 6400/6300/6100
       AUTOCAD 9.0 and 10.0 four colors mode driver. Color4.exe is an
       interactive program to help you to create your RGB4.TXT file. The driver,
       DS1K4.EXE (1024x768x4 colors driver), reads the values in RGB4.TXT to
       set the screen color.

       You may use the default colors from the driver, or you may execute
       color4.exe to set the colors you like on the screen.

       Once the driver (ds1k4.exe) resides in the memory, you may execute
       color4.exe to change the values in RGB4.TXT. Then, the driver reads
       the RGB4.TXT values to set the colors when you execute AutoCAD.

                     -----------------------------
                     Format for the file: RGB4.TXT
                     ----------------------------

       RBG4.TXT is a text file with 16 lines.  Each line has 5 characters on it:
       3 digits separated by 2 spaces.
       The digits represent color intensities and can be values of: 0,1,2 or 3
       for 16 colors modes and values of 0 or 1 for the 4 color mode.
       The first digit is the intensity of Red,
       the second digit is the intensity for Green and
       the third digit is the intensity for Blue.
       Each line represents a color index.  The first line represents index 0.
       The 16th line represents index 15. In the 4 color mode, index 0 to index
       3 are the only available colors.  Index 5 and index 7 are the border and
       background in this mode, and can be any of the first 4 colors.
       Each line (including line 16) ends with a carriage return.
       R G BΔΩ
       The file size should not be over 127 bytes.  The file should be on the
       directory where you execute Autocad.  If the file is not there, the
       driver will use the default values.

     NOTE.3. ::  As the Genoa 6100/6300 PCBs are populated with 256K RAM, the
                 following modes are unavailable: DS1K16.EXE, DS8256.EXE and
                 DS6256.EXE.  The Genoa 6400 and 6600 have the 512K necessary
                 for these modes.

*****************************************************************************
AutoCAD 9.0 & 10.0 display list driver.      (in directory  \AUTOCAD)

     - DSDL1K   EXE ...1024x768x16 colors driver
     - DSDL800  EXE ...800X600X16 colors driver

       Installation Procedures,
          (1)  Copy DSDL1K.EXE and DSDL800.EXE to your AutoCAD Directory.

          (2)  Execute DSDL1K.EXE for 1024x768 16 colors mode driver.
               Execute DSDL800.EXE for 800x600 16 colors mode driver.

               EXAMPLE :   DSDLxxx  fyyy

                        xxx  ::   1k/800
                        yyy  ::   Free bytes (memory space) on EMS board for
                                  AutoCAD. Others will be left for display list.

                              ex.  Suppose there are 2048k on EMS board
                                   as expanded memory.

                                   dsdl1k f500  =>    1552k for display list
                                                       496k free

                                   dsdl1k f400  =>    1648k for display list
                                                      400k free

                                   dsdl1k f300  =>    1760k for display list
                                                      288k free


     NOTE ::  Before using these drivers, you should have Intel EMS board
              on your system.  Set the EMS board as expanded memory for
              your system.  These drivers can not work if there is no EMS
              board detected on the system.  Other expanded memory boards
              must adhere to the LIM 4.0 specification.

******************************************************************************
AutoCAD 2.5 driver.                 (in directory  \AUTOCAD)

     - DS5F     EXE ...1024x768x16 colors driver
     - DS7F     EXE ...1024x768x4  colors driver
     - DS86     EXE ...800x600x16 colors driver

       Installation Procedures,
          (1)  -  (7)  Follows step (1) to (7) in AutoCAD 9.0/10.0 setup
                       procedure to install your AutoCAD.

          (8)  Copy "DS5F.EXE", "DS7F.EXE", and "DS86.EXE" to AutoCAD 2.5
               directory.

          (9)  Execute "DS5F.EXE" or "DS7F.EXE" to install the 1024x768x16/4
               colors resolution driver.
               Execute "DS86.EXE" to install the 800x600x16 colors resolution
               driver.

               DSxx    [i]      <enter>

               Argument i changes the background color to black.
               You need to install this driver once at every power up.

         (10)  Type "ACAD" to run AutoCAD.

     NOTE ::  DS5F.EXE, the 1024x768x16 colors mode driver, does not work on
              GENOA GVGA 6300/6100 boards. Those two boards don't support
              1024x768x16 colors mode.

******************************************************************************
AutoShade 1.1 driver.               (in directory  \AUTOSHAD)

     - RD800    COM ...800x600x16 Display & 800x600x256 Rendering driver
     - RD640    COM ...800x600x16 Display & 640x480x256 Rendering driver
     - RD512    COM ...800x600x16 Display & 512x512x256 Rendering driver

     From AutoShade's Installation & Performance Guide p.8 -- "We do not
     recommend that you run AutoCAD and AutoShade at the same time under DOS".
     We recommend that you may create your .FLM file under AutoCAD use AutoCAD
     driver. Reboot the system, install one of these two AutoShade drivers to
     display picture on the screen.

       Installation Procedures,
          (1)  Install the AutoShade program.

          (2)  Copy "RD800.COM","RD640.COM", and "RD512.COM" to AutoShade 1.1
               directory.

          (3)  Execute "RD800.COM" to install 800x600x16 colors display driver
               and 800x600x256 colors rendering driver.
               Execute "RD640.COM" to install 800x600x16 colors display driver
               and 640x480x256 colors rendering driver.
               Execute "RD512.COM" to install 800x600x16 colors display driver
               and 512x512x256 colors rendering driver.

          (4)  Type SHADE or SHADE -R to configure or reconfigure AutoShade.

               >>   SHADE   <enter>        or
               >>   SHADE   -R    <enter>

          (5)  a) From the Select display device, select option number 1,
                  "AutoDesk Device Interface display driver".

                  Display selection :  1    <enter>

               b) From the Select rendering display device, select option 1,
                  "AutoDesk Device Interface Rendering driver".

                  Rendering Selection :  1    <enter>

               c) Do the display and rendering devices share a single
                  screen (default = NO): Y   <enter>

                  Does FLIPSCREEN require a redraw (default = NO): Y    <enter>

          (6)  Now, you may enter AutoShade display screen.

     NOTE ::  RD800.COM and RD640.COM doesn't work on GENOA GVGA 6300/6100
              boards. Those two boards don't support those two resolutions.

*****************************************************************************
AutoCAD 10, 386 version driver.                   (in directory  \ACAD386)

     - DSP1024  EXP ...1024x768x16 colors driver
     - DSP800   EXP ...800x600x16 colors driver

       Install AutoCAD release 10, ver. 386 :

       1. Copy DSP1024.EXP and DSP800.EXP to your AutoCAD directory.
          Assume it is 'C:\ACAD'.

       2. In C:\AUTOEXEC.BAT or your batch file, add the following line

          "SET DSPADI=C:\ACAD\DSP1024.EXP"    or
          "SET DSPADI=C:\ACAD\DSP800.EXP"

          depending on which resolution you want to run AutoCAD.

       3. Reboot your system.

       4. Follow AutoCAD menu to install AutoCAD 386, and run it.
          When do "Configure video display", select item
              1. ADI P386 display


* If you want to change screen resolution, go back to step 2, 3 and 4.

* You need to load mouse driver before running AutoCAD.


*****************************************************************************
VENTURA 3.0, 2.0, 1.1 drivers.           (in directory  \GEMVEN)

   - SD1K16   VGA  ...1024x768x16 colors driver
   - SD1K2C   VGA  ...1024x768x2 colors driver
   - SD800600 VGA  ...800x600x16 colors driver


     How to install the high resolution driver :

     A. If you have not previously installed Ventura Publisher application:

        (1)  Install Ventura Publisher application according to the Ventura
             Publisher manual.  Select "IBM VGA .." or "GENOA SuperVGA HiRes
             (800x600) 16 colors" if it exists  as the display driver

        (2)  Follow step (1) through (5) below.

     B. If you have previously installed Ventura Publisher application:

        (1)  Insert GENOA SuperVGA 6000 series Utility & Driver Diskette in
             drive A, change directory to A:\GEMVEN\.

        (3)  Run RES800.BAT for the 800x600x16 colors driver.
             Run RES1K2.BAT for the 1024x768x2 colors driver.
             Run RES1K16.BAT for the 1024x768x16 colors driver.
             Follow the instructions to install your high resolution driver.

             a) From the GEM/Ventura Driver Installation menu, use arrow key
                to select 2 or 3 and then press ENTER.

             b) Enter the drive name that Ventura is installed and then press
                ENTER. Press ENTER if you have installed Ventura on C drive.

             c) From the TYPE OF LOCATOR menu, use the arrow key to select
                locator that you have installed for Ventura and then press
                ENTER.

             d) From the LOCATOR PORT menu, use arrow key to select an
                appropriate locator port and then press ENTER.

             e) Press ENTER to accept the setting.

             f) From the GEM/Ventura Driver Installation menu, select
                "Exit to DOS" and then press ENTER.

        (4)  Log on to the root directory of the drive where you installed
             your Ventura application.

        (5)  Run VP.BAT to start Ventura Publisher.

****************************************************************************
GEM/3 3.11 drivers.       (in directory  \GEMVEN)

   - SD1K16    VGA ...1024x768x16 colors driver
   - SD1K2C    VGA ...1024x768x2 colors driver
   - SD800600  VGA ...800x600x16 colors driver

     Installation Procedures
        (1)  Install GEM/3 according to the GEM/3 manual.

        (2)  Insert GENOA SuperVGA 6000 series Utility & Driver Diskette in
             drive A, change directory to A:\GEMVEN\.

        (3)  Run RES800.BAT for the 800x600x16 colors driver.
             Run RES1K2.BAT for the 1024x768x2 colors driver.
             Run RES1K16.BAT for the 1024x768x16 colors driver.
             Follow the instructions to install your high resolution driver.

             a) From the GEM/Ventura Driver Installation menu, use arrow key
                to select GEM/3 and then press ENTER.

             b) Enter the drive name that GEM is installed and then press
                ENTER. Press ENTER if you have installed GEM in C drive.

             c) From the TYPE OF LOCATOR menu, use the arrow key to select
                locator that you have installed for GEM and then press ENTER.

             d) From the LOCATOR PORT menu, use arrow key to select an
                appropriate locator port and then press ENTER.

             e) Press ENTER to accept the setting.

             f) From the GEM/Ventura Driver Installation menu, select
                "Exit to DOS" and then press ENTER.

        (4)  Log on to the root directory of the drive where you installed
             your GEM/3 application.

        (5)  Run GEM.BAT to start GEM/3 application.


        *   The 1024x768x16 colors driver, SD1K16.VGA, does not support
            GEM Graph version 1.01.

********************************************************************************
LOTUS 1-2-3 2.01, 2.20 & SYMPHONY 2.0 text drivers.     (in directory  \LOTUS)

   - 132xALL  DRV  ...all resolutions text driver
                      (include 132x25/29/32/44/60 and 80x25)

     Installation Procedures,
        (1) Install your Lotus 123 or Symphony program.

        (2) Copy driver file, 132xALL.DRV, to Lotus 123 or Symphony directory.
            Delete SINGLE.LBR, if it exists.

        (3) Run Lotus installation program to change text display driver
            to Genoa's 132 columns driver.

            Follow the simplified instructions as below:
               a.  From the Main Menu, select "Advanced Option".

               b.  Select "Add New Driver to Library" Option.

               c.  Go back to the Main Menu.

               d.  Select "Advanced Options" again

               e.  Select "Modify Current Driver" Option.

               f.  Select "Text Display" Option.
                   Select "GENOA SuperVGA Bd (132x25/29/32/44/60)".

               g.  Go back to the Main Menu, Save changes and Exit.

     This completes the installation of your LOTUS drivers.

     When you enter "123", "LOTUS" or "SYMPHONY" use "Ctl-A" and follow the
     instructions on the pop-up menus to switch text mode.


********************************************************************************
WordPerfect  5.0 graphics drivers.   (in directory  \WP50)

   - WP1K16   WPD  ...1024x768x16 graphics driver.
   - WP800    WPD  ...800x600x16 graphics driver.

     Use the following steps to install the driver :

        (1)  Copy WP1K16.WPD and WP800.WPD to the WordPerfect directory.

        (2)  Type "WP" to start WordPerfect.

        (3)  Within the Document screen, press Shift-F1 to enter to
             SETUP screen.

        (4)  From SETUP screen, select Display option.

             Selection :  [3, D]

        (5)  From Display menu, select Graphics Screen Type

             Selection :  [5, G]

        (6)  Use Up-Down arrow key to select
             "GENOA 6000 series 800x600 16 colors" for
                         800x600x16 colors graphics mode, or
             "GENOA 6000 series 1Kx768 16-color" for
                         1024x768x16 colors graphics mode.

        (7)  Press ENTER to ensure your selection.

        (8)  Press EXIT (F7) to return to the Document.

        You may (1) Press Print (Shift-F7) to display the Print menu,
        then (2) Select View Document (press "6" or "v") to show the document,
        which is based on the graphics mode you set, on the screen.

     NOTE ::  WP1K16.WPD, the 1024x768x16 colors mode driver, does not work on
              GENOA GVGA 6300/6100 boards. Those two boards don't support
              1024x768x16 colors mode.

*****************************************************************************
WordPerfect  5.1 graphics drivers.   (in directory  \WP51)

   - GNA1K16  VRS  ...1024x768x16 graphics driver.

     Use the following steps to install the driver :

        (1)  Copy GNA1K16.VRS to the WordPerfect 5.1 directory.

        (2)  Type "WP" to start WordPerfect.

        (3)  Within the Document screen, press Shift-F1 to enter to
             SETUP screen.

        (4)  From SETUP screen, select Display option.

             Selection :  [2, D]

        (5)  From Setup:Display menu, select Graphics Screen Type

             Selection :  [2, G]

        (6)  From Setup:Graphic Screen Driver screen, use Up-Down arrow key
             to select
                     GENOA 6000/512 series

        (7)  Select "GVGA 1kx768 16 color" as the display driver

        (8)  Press ENTER to ensure your selection.

        (9)  Press EXIT (F7) to return to the Document.

        Now, you may (1) Press Print (Shift-F7) to display the Print menu,
        then (2) Select View Document (press "6" or "v") to show the document,
        which is based on the graphics mode you set, on the screen.

     NOTE ::  GNA1K16.VRS, the 1024x768x16 colors driver, does not work on
              GENOA GVGA 6300/6100 boards. Those two boards don't support
              1024x768x16 colors mode.


*****************************************************************************
>>>  DISK   # 2
*****************************************************************************
Microsoft OS/2 Presentation Manager 1.1 drivers. (in directory   \PM)

   - GVGA800  DLL  ...800x600x16 colors driver
   - GVGA640  DLL  ...640x480x16 colors driver

     To install Genoa's high resolution display driver:

        (1)  Install OS/2 on your hard disk.

        (2)  Use MS-DOS start up diskette (Version 4.01 or above) to boot up
             the system.

             * save the original .DLL file before step (2).

               COPY C:\OS2\DLL\DISPLAY.DLL   C:\OS2\DLL\DISPLAY.OLD

        (3)  Use the MS-DOS COPY command to copy one of the display driver
             over the original display driver - "DISPLAY.DLL" in the OS2\DLL
             directory.

             * to copy the new display driver.

             COPY A:\PM\GVGA640.DLL  C:\OS2\DLL\DISPLAY.DLL  (for 640x480 70Hz)
               or
             COPY A:\PM\GVGA800.DLL  C:\OS2\DLL\DISPLAY.DLL  (for 800X600 70Hz)

        (4)  Reboot your system by pressing Ctrl-Alt-Del.


        NOTE :: These two drivers, "GVGA640.DLL" and "GVGA800.DLL", are used
                ON Genoa 6000 series FlickerFree display card running 640x480
                and 800x600 16-color 70Hz instead of IBM standard 60Hz under
                Microsoft OS/2 Presentation Manager.  With these two drivers
                you will see less screen flicker on your monitor. However, due
                to the spec. of the monitor, some models may not fully utilize
                the 70Hz advantage.  The following list is for your reference:

                  switch           reference     ver. ref. rate w/ PM driver
                  1   2   3   4    monitor            640x480    800x600
                  ---------------  ---------          --------   --------
                  OFF OFF OFF OFF  IBM 85xx             60(Hz)     --
                  ON  ON  ON  OFF  SONY 1302            70         60(Hz)
                  OFF ON  ON  OFF  SONY 1304            70         70
                  OFF OFF ON  OFF  NANAO 9070           70         70
                  ON  ON  OFF OFF  NEC 2A               70         60
                  ON  OFF OFF OFF  NEC 3D               70         60
                  OFF ON  OFF OFF  NEC XL               70         70
                  OFF ON  ON  ON   NEC 4D,5D,           70         70
                                   Mitsu.6605TK,6615,
                                   NANAO 9500

                Please reference the USER'S MANUAL for detail.


*****************************************************************************
Microsoft Windows 3.0 drivers.       (in directory \WIN30)

   - G640256  DRV  ...640x480x256 colors driver
   - GVGA1K   DRV  ...1024x768x16 colors driver
   - GVGA86   DRV  ...800x600x16 colors driver


     How to install GENOA VGA Windows Version 3.0 drivers

     A.  If you have previously installed Windows 3.0:

         1.  Copy "SETUP.INF" from the Genoa VGA Utility Diskette to the
             C:"WINDOWS\SYSTEM" sub-directory.  This will overwrite the old
             "SETUP.INF" file.

         2.  Follow step 5 through 6 below.

     B.  If you have not previously installed Windows 3.0:

         1.  Make a "diskcopy" of all of the Windows application program
             diskettes.  Put the original diskettes in a safe place.

         2.  Copy the file "SETUP.INF" on the Genoa VGA Utility diskette to
             the copy of the Windows Disk 1. This will overwrite the SETUP.INF
             file on the application diskette.

         3.  Insert the modified Disk 1 into drive A and run setup.

         4.  Follow Windows 3.0 setup procedures.  At the end of install
             procedure you will be asked to "Restart Windows" or "Return
             to Dos".  Restart Windows.

         5.  Windows 3.0 Main Menu will be on the screen.
             Select the "Windows Setup" icon.
             At the next Window select "Options"
             At the next Window select "Display"

         6.  Scroll through the options and you will see four Genoa VGA
             display options near the top of the option box.  Select the
             appropriate display resolution.

         7.  Insert the Genoa VGA Utility diskette when requested by Windows
             setup.  Select the appropriate drive and path.  Restart Windows
             and the Genoa driver will be loaded.

         8.  After the installation procedure is finished, if you want to
             change display resolution, you only need to open Windows and
             follow steps 5 through 6.



     C:  To change the Display Resolution after Installing a Genoa Driver.

         1.  Follow steps 5 through 6 above.

     Once you install a resolution driver the proper file is copied to the
     "WINDOWS\SYSTEM" subdirectory and you will not be prompted for a diskette.

********************************************************************************
WINDOWS/386 2.10 & 2.03 drivers.             (in directory  \WIN386)

   - 800X600  DRV  ...800x600x8 driver
   - 800X600  LGO  ...Windows logo driver
   - 800X600  GRB  ...Grabber file
   - 800x600  3EX  ...Display dependent file
   - 800x600  386  ...Display dependent file

   - 1024x768 DRV  ...1024x768x8 driver
   - 1024x768 LGO  ...Windows logo driver
   - 1024x768 GRB  ...Grabber file
   - 1024x768 3EX  ...Display dependent file
   - 1024x768 386  ...Display dependent file

     Installation Procedures,
        (1)  Run the Microsoft Windows/386 Setup program.

        (2)  When you get to the display adapter selection menu, moves
             the cursor to "Other (requires disk provided by a hardware
             manufacturer)". Press <enter> key.

        (3)  Following the prompt, insert GENOA SuperVGA 6000 series Utility
             & Drivers Disk into the A: drive and change path to A:\WIN386.
             Press <enter> key.

        (4)  Select the appropriate screen resolution you prefer.

        (5)  Continue the subsequent installation procedure and choose the
             system and terminal fonts you prefer.

     This completes the installation of your Windows/386 2.10 or 2.03 drivers.

   NOTES:
       *   Before you run Windows, please delete device=mouse.sys from
           config.sys, because Windows will load its own mouse driver.

       *   1024x768 mode driver does not work on Genoa SuperVGA 6100 and
           6300 boards. These two boards do not support this resolution.

********************************************************************************
WINDOWS/286 2.1 & 2.03 drivers:              (in directory  \WIN286)

   - 800X600  DRV  ...800x600x8 driver
   - 800X600  LGO  ...Windows logo driver
   - 800X600  GRB  ...Grabber file

   - 1024x768 DRV  ...1024x768x8 driver
   - 1024x768 LGO  ...Windows logo driver
   - 1024x768 GRB  ...Grabber file

     Installation Procedures,
        (1)  Run the Microsoft Windows/286 Setup program.

        (2)  When you get to the display adapter selection menu, moves
             the cursor to "Other (requires disk provided by a hardware
             manufacturer)". Press <enter> key.

        (3)  Following the prompt, insert GENOA SuperVGA 6000 series Utility
             & Drivers Disk into the A: drive and change path to A:\WIN286.
             Press <enter> key.

        (4)  Select the appropriate screen resolution you prefer.

        (5)  Continue the subsequent installation procedure and choose the
             system and terminal fonts you prefer.

     This completes the installation of your Windows/286 2.1 or 2.03 drivers.

   NOTES:
       *   Before you run Windows, please delete device=mouse.sys from
           config.sys, because Windows will load its own mouse driver.

       *   1024x768 mode driver does not work on Genoa SuperVGA 6100 and
           6300 boards. These two boards do not support this resolution.

*****************************************************************************


