

    **  Installation of the OS/2 2.1 256-Color Video Drivers  **
	----------------------------------------------------


1)  Insert Video Drivers Diskette #1 into Diskette Drive A:.

2)  Invoke an OS/2 Window Session or an OS/2 Full-Screen Session.

3)  Change to Diskette Drive A:.

4)  Run CLINST21.CMD from Diskette Drive A:, by entering CLINST21 x
    where x is the Drive Letter for the files to be copied to.

    For example:  CLINST21 C copies the files to Drive C:.

5)  Check the 'Primary Display' Check Box from the DISPLAY DRIVER INSTALL
    Dialog Box.

6)  Select 'Cirrus Logic Blitter Driver' from the PRIMARY DISPLAY ADAPTER 
    TYPE Dialog Box.

7)  Click 'OK' in the MONITOR CONFIGURATION/SELECTION UTILITY Dialog Box.

8)  Select the Display Resolution of choice from the SELECT DISPLAY 
    RESOLUTION List Box.

9)  Click the 'Install' Button in the SOURCE DIRECTORY Dialog Box and
    follow the prompts.


NOTE:  During installation, the Target File may have a newer date than the
       Source File, select the 'Yes' button when the Installation Program 
       displays a Dialog Box to notify the user of this situation.

       Subsequent installation of the OS/2 2.1 256-Color Video Drivers and
       Resolutions can be performed by entering DSPINSTL in an OS/2 Window
       Session and follow the prompts.



            Using the CLMODE Utility to Select Monitor Types:
            -------------------------------------------------

    The CLMODE Utility allows the user to define the type of monitor
    attached and to set the video modes supported by the on-board SVGA.

    To run CLMODE:

1)  Invoke an OS/2 Window Session or an OS/2 Full-Screen Session.

2)  Copy CLMODEVD.EXE (Video Drivers Diskette #2) onto your hard drive
    and enter CLMODEVD to self-extract the utility.
          
3)  Insert Video Drivers Diskette #1 into Diskette Drive A:.

4)  Change to Diskette Drive A:.

5)  Run CLINST21.CMD from Diskette Drive A:, by entering CLINST21 x
    where x is the Drive Letter for the files to be copied to.

    For example:  CLINST21 C copies the files to Drive C:.

6)  Check the 'Primary Display' Check Box from the DISPLAY DRIVER INSTALL
    Dialog Box.

7)  Select 'Cirrus Logic Blitter Driver' from the PRIMARY DISPLAY ADAPTER 
    TYPE Dialog Box.

8)  Select 'Install Using Display Adapter Utility Programs' from the 
    MONITOR CONFIGURATION/SELECTION UTILITY Dialog Box and enter the path 
    of the CLMODE Utility as well as CLMODE.EXE.  

    For example:  C:\CLMODEVD\CLMODE.EXE for path C:\CLMODEVD

9)  Follow the CLMODE Utility prompts (reference READ_MON.TXT on Video 
    Drivers Diskette #2).

10) After exiting CLMODE, select the Display Resolution of choice from 
    the SELECT DISPLAY RESOLUTION List Box.

11) Click the 'Install' Button in the SOURCE DIRECTORY Dialog Box and
    follow the prompts.


