Instructions for creating the OS/2 2.11 and Warp 3.0 driver diskettes

ImageAccel OS/2 2.11 and Warp 3.0 Display Driver Release 1.03

This file includes disk one and disk two of ImageAccel driver disks.  
To create the install and driver disk use an unzipping utility such as Pkunzip.  
This file is on our BBS. 

For example use:
PKUNZIP DISK1 A: FOR DISK1 OF THE INSTALLATION DISKS
PKUNZIP DISK2 A: FOR DISK2 OF THE INSTALLATION DISKS

The driver disks must be labled before they will work properly.  
The lable names IA-DISP-1 (DISK1) and IA-DISP-2 (DISK2).  
To lable the disks use the following command at the dos prompt.

lable a:ia-disp-1 (lable disk as disk 1)
lable a:ia-disp-2 (lable disk as disk 2)

Please review the README file on disk 1 and 2.  The file name is iareadme.txt.  
This file includes the most resent information about installation and troubleshooting.

If you have any problems please contact our support deparment.

