# Integrated RAID controller object

Use this object to work with integrated RAID controllers and their subobjects or to display their properties.

The integrated RAID controller is displayed in the ServeRAID Manager tree as two controller objects. However, you can configure only one array and RAID level-1 logical drive on an integrated RAID controller. The controller information in the right pane lists the controller type as LSI 1030.

Notes:
  1. The integrated RAID controller provides limited function compared to ServeRAID controllers.
  2. The ServeRAID Manager can display a maximum of four LSI 1030 controller objects in a system.

## Possible subobject

- (Arrays)
- (Logical drives)
- (Physical drives)
- (Hot-spare drives)

## Warning and error conditions

- (warning) is displayed for the following conditions:
  - Any subobject of the controller has any warning or error conditions.
- (error) is displayed for the following conditions:
  - The controller has failed.
  - The controller has a bad configuration.

## Actions

- Identify all physical drives

The following actions are available only in startable-CD mode:

- Configure RAID
- Delete all arrays
- Enable or disable unattended mode

Glossary | Contents

x-0220-SRM-00-02-EN