This README file contains the latest information about the  
IBM TotalStorage™ FAStT Storage Manager version 8.3 storage
controller firmware.

Refer to the IBM TotalStorage™ Support Web Site or CD for the
installation and support guide.

For other related publications (refer to Related Publications in the 
installation and support guide) and the latest information and 
updated readme file.

Last Update:  04/09/2003

Products Supported: 

      ---------------------------------------------------
     |           | Machine Type |     Model              | 
     |-----------|--------------|------------------------|
     | FAStT 900 |     1742     | 90X , 90U              |
     |-----------|--------------|------------------------|
     | FAStT 600 |     1722     | 60U , 60X              |
     |-----------|--------------|------------------------|
     | FAStT 700 |     1742     | 1RX , 1RU              |
     |-----------|--------------|------------------------|
     | FAStT 500 |     3552     | 1RX , 1RU              |
     |-----------|--------------|------------------------|
     | FAStT 200 |     3542     | 1RX , 1RU ,2RX and 2RU |
      ---------------------------------------------------


CONTENTS
--------
1.0  Overview
2.0  Change History
3.0  Installation and Setup Instructions
4.0  Configuration Information
5.0  Unattended Mode
6.0  Web Sites and Support Phone Number
7.0  Trademarks and Notices
8.0  Disclaimer

=======================================================================
1.0   Overview
--------------

   This IBM Storage Manager release includes the IBM FAStT Storage 
   Manager version 8.3 storage controller Firmware and NVSRAM files for 
   upgrading IBM machine types 1742 (models 1RX and 1RU) and 3552 (all 
   models ) at firmware version 05.00.0x.xx or higher and IBM machine 
   type 3542 (all models) at firmware version 05.20.xx.xx or higher.
   This is the first release of the firmware for IBM machine types 1742
   (models 90X and 90U) and 1722 (models 60X and 60U). 
   
   The IBM FAStT Storage Manager version 8.3 Installation and Support 
   Guides are available on IBM's Support Web Site as a downloadable 
   Portable Document Format (PDF) file. 

   Please see IBM Marketing representatives if you want to upgrade 
   machine type 3552 and 3542 at firmware version 04.xx.xx.xx to 
   firmware version 05.3x.xx.xx or higher because it is a purchased option.
   In addition, IBM FAStT FlashCopy and IBM FAStT Remote Mirror premium 
   feature options are purchased separate from the Storage Manager 8.3 
   Upgrade option. The IBM FlashCopy option requires firmware version 
   05.00.04.xx or higher and the IBM Remote Mirror option requires 
   firmware version 05.20.0x.xx or higher. 
   
   The FAStT storage partitioning premium feature is standard on all 
   IBM FAStT storage subsystems with the exception of the IBM FAStT600
   (machine type 1722) storage subsystem. Please contact IBM
   Marketing representatives or IBM resellers if you want to purchase
   the IBM FAStT storage partitioning premium feature option for it. 

   Refer to the IBM Support Web Site for the latest Firmware and 
   NVSRAM files for the IBM FAStT Storage Subsystems.

=======================================================================
1.1  Limitations
---------------------

1. Upgrading FAStT500 with 512MB Cache. If you are upgrading controller 
   firmware on a FAStT500 (machine type 3552) with 512MB of cache, you 
   will need to stop I/O and reboot the controller before upgrading 
   firmware followed by NVSRAM.

   To determine Storage Controller cache level, perform the following:

   a. On a storage management station start the client software and 
      select a storage subsystem.
   b. Select Tools -> Manage Device to open the Subsystem Management 
      Window.
   c. Highlight the Storage Subsystem that you are upgrading and then 
      select Storage Subsystem -> Profile. It may take a little time for 
      it to create the Storage Subsystem profile.   
   d. Under the Controllers heading is an entry that displays 
      information similar to the following example:

      Cache/processor size (MB):  256/32

   If this setting is listed as 512/32 you will need to arrange to 
   perform this upgrade procedure at a time that you can stop I/O to the 
   Storage Subsystem in order to ensure a successful firmware download 
   and installation.

2. Storage Manager prompts you for a password if all hard disk 
   drives are removed from the storage subsystem.

   After removing all drives from a storage subsystem (or not powering 
   on drives and only the  controller), the IBM FAStT Storage Manager 
   software will prompt you for a password when trying to start the 
   software or trying to perform protected operations. Any password 
   entered will fail.

   Password information is stored on a reserved area of each hard disk 
   drive on the storage subsystem.  Each drive stores a mirrored copy of 
   the password data.  When there are no drives in the storage 
   subsystem, the storage management software does not find the password 
   data when you attempt password protected operations. Add one drive to 
   the storage subsystem and retry the operation.
   
   Since the RAID controller unit should not be powered on until the 
   expansion units are attached and powered on, this should be done by 
   powering off the RAID controller unit, properly attaching all 
   expansion units (with drives installed), to the RAID controller unit 
   and powering them on, and then powering the RAID controller unit back 
   on.  At this point the storage subsystems can be re-discovered and 
   managed using the IBM FAStT Storage Manager 8.2 software.

3. Auto LUN/Array Transfer is not enable for Microsoft Windows, IBM AIX 
   and SUN Solaris OS's. If a controller fails over arrays to the alternate
   controller and the failed controller is replaced and brought back online,
   the arrays do not automatically transfer to the preferred controller. 
   This must be done manually by selecting the redistributing arrays menu
   option in the storage subsystem window of the IBM FAStT storage manager 
   client program.

4. Display issues when using 256 color settings. A brownish hash 
   pattern is displayed on the windows and in online help when running 
   in 256 color mode.  Run the Storage Manager 8 application in a higher 
   display mode.

5. The FAStT Storage Management dialog windows may be displayed 
   cropped without the vertical and horizontal scroll bars. Just move 
   the mouse pointer over the edge of the window until the mouse pointer 
   change to window resize pointer, left click and hold to grip the 
   window edge to resize it. 

6. If you get "Error 21 - The Operation cannot complete because a 
   ...  is in progress" error when you issue a Subsystem Management 
   command from the IBM FAStT Storage Manager Client, the command may be 
   cached. If the command is cached, the IBM FAStT Storage Manager 
   Client will run the command as soon as the controller resources are 
   available. Wait for at least ten minutes and check to see whether the 
   command has been run. If not, re-attempt the command. 

7. If the controller in the IBM FAStT Storage Server with firmware 
   05.3x.xx.xx is connected to a SAN with more than 64 host connections
   per controller port that can log into the controllers, one must 
   either use the switch zoning function or rearrange the SAN 
   connections so that only the maximum number of host connections can
   be seen and log into the controller. The FAStT Storage Subsystem 
   FAStT900, FAStT700 and FAStT500 (IBM machine type 1742 and 3552)
   have two ports per controller - one per minihub slot. The FAStT 
   Storage FAStT600 (IBM machine type 1722) has two ports per
   controller. The FAStT storage Subsystem FAStT200 (IBM machine type
   3542) has only one port per controller.
 
8. The IBM FAStT Storage Server hardware and software is designed to 
   have redundant paths from the host system to ensure the availability 
   of storage. However, it is possible to connect a single host adapter 
   from the host system to one of the controller minihubs and then 
   connect this minihub to the minihub of the other controller. This 
   configuration will create a FC-AL loop between the host adapter and 
   the two IBM FAStT Storage Server controllers and no redundant path to 
   the host system. When you connect the two minihubs together, always 
   connect the "IN" port of one minihub to the "OUT" port of the other 
   minihub or vice versa. Do not connect the "IN" port of one to the 
   "IN" port of the other minihub or the "OUT" port of one minihub to 
   the "OUT" port of the other minihub.
                     
9. When creating a Remote Mirror of a base volume the following 
   restriction applies. First, you have created a snapshot of a base 
   volume and the base volume is receiving I/O. Second, you decide to 
   create a mirror relationship, using the base volume as the primary 
   volume in the mirrored pair. As you create the mirror relationship, 
   the snapshot volume is failed. The work around is to stop I/O to 
   the base volume while you are creating the mirror relationship. 
   Alternatively, if the mirror relationship is created before creating 
   the snapshot volume, this will not happen.
   
        
=======================================================================
                
1.2  Enhancements
-----------------
     N/A

=======================================================================
            
1.3  Prerequisites
------------------
    
    "Direct connection of the FAStT600 to a host system running 
    Microsoft Windows, Novell NetWare or x86 Linux is only supported 
    using the IBM FAStT FC2-133 Host Bus Adapter (HBA), IBM option part 
    number 24P0960 or feature code 2104 with the last 6 digits of the 13 
    digit serial number of the HBA is H21160 or higher. For example, if 
    the serial number is FFC0308H21161, the last 6 digits will be 
    H21161, which indicates that this HBA meets the FAStT600 direct 
    connect prerequisite.  

    In addition, direct connect to the NAS 300G (Machine Type 5196) 
    Model G27 or Model G02 containing Feature Code 3706 is only 
    supported if the last 6 digits of the 13 digit serial number of the 
    HBA is above H21160.

=======================================================================
            
1.4  Dependencies
-----------------


   IBM FAStT Storage Manager version 8.3 provides full management support
   IBM machine types 3552 and 3542 storage subsystems that have at least
   firmware version 04.00.02.xx, IBM machine type 1742 (models 1RX, 1RU)
   storage subsystem that have at least firmware version 05.00.04.xx or
   IBM machine types 1742 (models 90X, 90U) and 1722 storage subsystems
   that have at least firmware version 05.3x.xx.xx.
    
   The only IBM FAStT Storage Manager 8.3 supported management function 
   on controllers with firmware version 04.xx.xx.xx to 04.xx.01.xx is 
   controller firmware and NVSRAM download. 
   
=======================================================================

2.0   Change History
-----------------------------

======================================================================

2.1 Key Features added to IBM FAStT Storage Manager 8.3 with controller 
    firmware version 05.3x.xx.xx.
     
    - Support for IBM TotalStorage FAStT600 Fibre Channel Storage Server.
      The machine type and models of the FAStT 600 storage server is 1722
      and 60X and 60U, respectively.
    - Support for IBM TotalStorage FAStT900 Fibre Channel Storage Server.
      The machine type and models of the FAStT 900 storage server is 1742
      and 90X and 90U, respectively.
    - Support for online Environmental Services Monitor (ESM) card firmware
      downloads. The ESM cards are customer replaceable unit (CRU) components
      in the IBM FAStT storage expansion units. The ESM firmware can be 
      updated while the storage subsystem receives I/Os from the servers.
    - Support for offline Fibre Channel hard drive firmware and mode page 
      downloads. The I/O from the servers must be suspended during the 
      duration of the hard drive firmware and mode page download.
    - Support for Media Scan without Parity repairs
    - Support for forcibly disabling Fibre Channel drive-level write caching
    - Support the controller state dump function for diagnostics
       
=======================================================================
        
2.2 Code levels at time of release are as follows
-------------------------------------------------

     1. Storage Controller Firmware versions:
         
       a. Upgrade CD
          FAStT 900:  FW_05300900_05300000
          FAStT 700:  FW_05300900_05300000
          FAStT 600:  SNAP_05330500
          FAStT 500:  FW_05300900_05300000
          FAStT 200:  SNAP_05300900
       
       b. Web download 
          FAStT 900:  FW_05300901_05300000
          FAStT 700:  FW_05300901_05300000
          FAStT 600:  SNAP_05330500
          FAStT 500:  FW_05300901_05300000
          FAStT 200:  SNAP_05300901
          
          NOTE:  The web download firmware will only install on a FAStT Storage Server that 
                 is currently running Storage Manager 8.0 or higher firmware. 
                        
     2. Storage Controller NVSRAM versions:
       a.  FAStT 900:  N1742F900R830V04
       b.  FAStT 700:  N1742F700R830V03
       d.  FAStT 600:  N1722F600R833V02
       c.  FASTT 500:  N3552F500R830V03
       c.  FAStT 200:  1RU - N3542-1RUR830V04
                       2RU - N3542-2RUR830V05
                                    
   Refer to the http://ssddom02.storage.ibm.com/techsup/webnav.nsf/support/disk
   IBM TotalStorage™ Disk Storage Systems Technical Support web site for the 
   latest released code levels.
          
=======================================================================
              
3.0   Installation and Setup Instructions
-----------------------------------------

3.1  Important: You must install the firmware update prior to downloading  
                the NVSRAM update.

   To download firmware, do the following: 
   
   a.  Open the Subsystem Management window. 
   b.  Click Storage Subsystem => Download => Firmware. 
       Follow the online instructions.

   To download NVSRAM, do the following: 
   
   a.  Open the Subsystem Management window. 
   b.  Click Storage Subsystem => Download => NVSRAM. 
       Follow the online instructions.

=======================================================================
                                
3.2  Helpful Hints
------------------

1. If you are unable to see the maximum number of drives during 
   Automatic Configuration, you should be able to use Manual 
   Configuration to select individual drives and select the maximum 
   number of drives allowed.

2. Depending on the storage subsystem that you have purchased, you
   may have to purchase the FAST storage partitioning premium feature
   option or an option to upgrade the number of supported partitions
   in a storage subsystem. Please see IBM Marketing representatives
   or IBM resellers for more information.
   
   - IBM FAStT600 storage subsystem (machine type 1722): The standard
     configuration does not have the FAST storage partitioning premium
     enabled. Four partition, eight partition and an upgrade from four
     to eight partition storage partitioning premium feature options 
     can be purchased.

   - IBM FAStT200, FAStT500, and FAStT700 storage subsystems (machine
     type 3542, 3552 and 1742 - models 1RU and 1RX, respectively): The 
     standard configuration has 64 partitions storage partitioning 
     premium option installed. No additional storage partitioning 
     premium feature options can be purchased for these storage
     subsystems.

   - IBM FAStT900 storage subsystem (machine type 1742 - models 90X and
     90U): The standard configuration has 16 partition storage partitioning
     premium option installed. An upgrade from 16 to 64 partition storage
     partitioning premium feature option can be purchased.

=======================================================================

4.0 Configuration Information
-----------------------------

        
4.1 Configuration Settings
--------------------------

1. By default the IBM FAStT Storage Manager 8.3 firmware does not 
   automatically map logical drives if storage partitioning feature is
   enabled. This means that the logical drives are not automatically 
   presented to host systems.

   For a new installation, after creating new arrays and logical drives; 
   a. If your host type is not Windows NT, create a partition with your 
      host type and map the logical drives to this partition. 
   b. If your host type is Windows NT, you can map your logical drives to the 
      "Default Host Group" or create a partition with a NT host type.   
                                 
   When upgrading from previous versions of IBM FAStT Storage 
   Manager to version 8.3. 
   a. If upgrading with no partitions created and you have an operating
      system other than Windows NT,  you will need to create a partition with
      your host type and map the logical drives from the "Default
      Host Group" to this partition.
   b. If upgrading with Storage Partitions and an operating system other 
      than Windows NT is accessing the default host group, you will need 
      to change the default host type.  After upgrading,  the default host 
      type is reset to Windows NT. 
              
   Refer to the IBM FAStT Storage Manager online help to learn
   more about creating storage partitions and changing host types.

2. When you are configuring IBM machine type 1722, 1742, 3542 or 3552 
   storage subsystems as boot devices, contact IBM support for supported 
   configurations and instructions for configuring LUNs in the IBM 
   storage subsystems as boot devices. 

3. Running script files for specific configurations. Apply the 
   appropriate scripts  to your subsystem based on the instructions you 
   have read in the publications or any instructions in the operating 
   system readme file. A description of each script is shown below.

   - SameWWN.scr: Setup RAID controllers to have the same World Wide 
     Names. The World Wide Names (node) will be the same for each 
     controller pair. The NVSRAM default sets the RAID controllers to have 
     the same World Wide Names.

   - DifferentWWN.scr:  Setup RAID controllers to have different World 
     Wide Names. The World Wide Names (node) will be different for each 
     controller pair. The NVSRAM default sets the RAID controllers to have 
     the same World Wide Names.

   - EnableDriveMigration.scr:  The Enable drive migration script scans 
     the drives for configurations when they are added to a storage system 
     and will also attempt to use configurations found on the newly added 
     drives. The NVSRAM default will enable drive migration.

   - DisableDriveMigration.scr:  The disable drive migration script 
     allows the addition of disk drives while the system is running. in 
     addition, it identifies the drives as unused capacity regardless of 
     past drive configuration. The NVSRAM default will enable drive 
     migration.
     
4. When you are configuring IBM machine type 1742 or 3552 storage
   controllers in host cluster Remote Mirror configurations, contact 
   IBM support for supported host cluster configurations and instructions
   for configuring IBM storage controllers in clustered Remote Mirror
   configurations. 

=======================================================================

4.2 Unsupported configurations
------------------------------

   The following lists configurations that are currently not being 
   supported with IBM FAStT Storage Manager 8.3.

   1. Fibre Channel loop environments with the IBM Fibre Channel Hub, 
      machine type 3523 and 3534, in conjunction with the IBM Fibre Channel 
      Switch, machine types 2109-S16, 2109-F16 or 2109-S8. In this 
      configuration, the hub is connected between the switch and the IBM 
      Fibre Channel RAID Controllers.

   2. The IBM Fibre Channel Hub, machine type 3523, connected to IBM 
      machine type 1722, 1742, 3542 and 3552.
      
   3."Direct connection of the FAStT600 to a host system running 
     using the IBM FAStT FC2-133 Host Bus Adapter (HBA), IBM option part 
     number 24P0960 or feature code 2104 with the last 6 digits of the 13 
     digit serial number of the HBA below H21160. For example, if 
     the serial number is FFC0308H21158, the last 6 digits will be 
     H21161, which indicates that this HBA do not meet the FAStT600 direct 
     connect prerequisite.  

=======================================================================

5.0   Unattended Mode
---------------------
        N/A

=======================================================================

6.0   WEB Sites and Support Phone Number
----------------------------------------

   6.1  IBM TotalStorage™ Disk Storage Systems Technical Support web site:
        http://ssddom02.storage.ibm.com/techsup/webnav.nsf/support/disk

   6.2  IBM TotalStorage™ Marketing Web Site:
        http://www.storage.ibm.com/hardsoft/disk/fastt/index.html

   6.3  If you have any questions about this update, or problem
        applying the update go to the following HelpCenter World
        Telephone Numbers URL:
        http://www.ibm.com/planetwide

=======================================================================

7.0   Trademarks and Notices
----------------------------

        7.1  The following terms are trademarks of the IBM Corporation
             in the United States or other countries or both:

                 IBM
                 
                 FAStT
                 
                 ToTalStorage™ 

                 the e-business logo

                 xSeries
                 
                 pSeries

                 HelpCenter

                 Microsoft, Windows, and Windows NT are trademarks of Microsoft
                 Corporation in the United States, other countries, or both.
                
                 Java and all Java-based trademarks and logos are trademarks or
                 registered trademarks of Sun Microsystems, Inc. in the United
                 states, other countries, or both.

                 UNIX is a registered trademark of The Open Group in the United 
                 States and other countries.

                 Linux is a registered trademark of Linus Torvalds.

                 Other company, product, and service names may be 
                 trademarks or service marks of others.

=======================================================================

8.0   Disclaimer
----------------

        8.1  THIS DOCUMENT IS PROVIDED "AS IS" WITHOUT WARRANTY OF
             ANY KIND. IBM DISCLAIMS ALL WARRANTIES, WHETHER EXPRESS
             OR IMPLIED, INCLUDING WITHOUT LIMITATION, THE IMPLIED
             WARRANTIES OF FITNESS FOR A PARTICULAR PURPOSE AND
             MERCHANTABILITY WITH RESPECT TO THE INFORMATION IN THIS
             DOCUMENT. BY FURNISHING THIS DOCUMENT, IBM GRANTS NO
             LICENSES TO ANY PATENTS OR COPYRIGHTS.


        8.2  Note to U.S. Government Users -- Documentation related to
             restricted rights -- Use, duplication or disclosure is
             subject to restrictions set forth in GSA ADP Schedule
             Contract with IBM Corporation.
