                 
                            File Name: README.TXT

       IBM xSeries 380 (8663) BIOS/FIRMWARE Version 1.3

                                
      CONTENTS
       ---------

    1.0   Overview
    2.0   Change History
    3.0   Installation and Setup Instructions
    4.0   Configuration Information
    5.0   Unattended Mode
    6.0   Web Sites and Support Phone Number
    7.0   Trademarks and Notices
    8.0   Disclaimer


    1.0  Overview: 
    --------------

       1.1   About this code
                  
             These files contain BIOS/FIRMWARE Version 1.3 code
             which supports the following Machine Type/Models 
             of IBM xSeries 380:
              
                   - 8683-1RX
                   - 8683-2RX                    

       1.2   Level of recommendations and prerequisites for the
             update:

         - The following Machine Type/Models of IBM xSeries 380
           require BIOS/FIRMWARE Version 1.0 or higher:
                  - 8683-1RX
                  - 8683-2RX
                                   
        1.3   Dependencies:

          - Determine the BIOS/FIRMWARE versions of your 
            server before trying to upgrade the BIOS and 
            Server management Firmware. 

          - Valid BIOS and Firmware combinations are listed in 
            the following table.
   
        BIOS# |  BMC Ver# | HSC Ver# | CBC Ver# | SDR Ver#
        ---------------------------------------------------
        B104  |  BMC 26	  | HSC 7    | CBC 02	| SDR 14 
        B100  |  BMC 24	  | HSC 7    | CBC 02	| SDR 14 
        B99   |  BMC 24	  | HSC 7    | CBC 02	| SDR 14    
        B83   |  BMC 22	  | HSC 7    | CBC 02	| SDR 13

          - IMPORTANT: Recommend upgrading to at least 
                       BMC Rev 24 before using BIOS-99.
        


    2.0   Change History
    --------------------
         2.1   IBM xSeries 380 BIOS/FIRMWARE Version 1.3. 
                   
        Includes: BIOS-104, BMC-26, HSC-07, CBC-02, SDR-14

            Date	         : 11/15/2001 
            Stamp	         : 0111151330
            BIOS Version         : S460AC4A.86B.0104.B  
            Processor Supported  : C0

         PAL/SAL/EFI REVISIONS
            PAL Version		        : 6.6.26			
            MSL Reference SAL Code	: 6.0 RC9
            SAL Specification Rev       : 3.0
            MSL Reference EFI Code	: 12.40
            EFI Specification Rev       : 1.02
            FPSWA Driver Version	: 1.9
            S460AC4.RCV Version         : 9

         2.2   IBM xSeries 380 BIOS/FIRMWARE Version 1.2. 
                   
        Includes: BIOS-100, BMC-24, HSC-07, CBC-02, SDR-14

            Date	         : 098/26/2001 
            Stamp	         : 0109252309
            BIOS Version         : S460AC4A.86B.0100.B  
            Processor Supported  : C0

         PAL/SAL/EFI REVISIONS
            PAL Version		        : 6.6.25			
            MSL Reference SAL Code	: 6.0 RC9
            SAL Specification Rev       : 3.0
            MSL Reference EFI Code	: 12.38
            EFI Specification Rev       : 1.02
            FPSWA Driver Version	: 1.6
            S460AC4.RCV Version         : 9


         2.3   IBM xSeries 380 BIOS/FIRMWARE Version 1.1. 
                   
        Includes: BIOS-99, BMC-24, HSC-07, CBC-02, SDR-14

            Date	         : 08/30/2001 
            Stamp	         : 0108300108301658
            BIOS Version         : S460AC4A.86B.0099.B 
            Processor Supported  : C0

         PAL/SAL/EFI REVISIONS
            PAL Version		        : 6.6.25			
            MSL Reference SAL Code	: 6.0 RC9
            SAL Specification Rev       : 3.0
            MSL Reference EFI Code	: 12.38
            EFI Specification Rev       : 1.02
            FPSWA Driver Version	: 1.6
            S460AC4.RCV Version         : 9

       
         2.4   IBM xSeries 380 BIOS/FIRMWARE Version 1.0. 
                    
        Includes: BIOS-83, BMC-22, HSC-07, CBC-02, SDR-13 
            
            Date	         : 06/07/2001 
            Stamp	         : 0106060029
            BIOS Version         : S460AC4A.86B.0083.B 
            Processor Supported  : C0

         PAL/SAL/EFI REVISIONS
            PAL Version		        : 6.6.23			
            MSL Reference SAL Code	: 6.0 RC9
            SAL Specification Rev       : 3.0 (Minimally)
            MSL Reference EFI Code	: 12.36
            EFI Specification Rev       : 1.02
            FPSWA Driver Version	: 1.6
            S460AC4.RCV Version         : 9

                      
    3.0   Installation and Setup Instructions
    -----------------------------------------

      3.1   Download and Media Creation. 
  
         1. To Build a CD.
           - Download the "iso" image of the IBM xSeries 380
             POST/FIRMWARE, from http://www.pc.ibm.com/support
           - Create a CD using instructions at following url: 
             from http://www.pc.ibm.com/qtechinfo/MIGR-4NJNJB
             or other CD creation Applications.

        Note: To update the SDR records all files have to be on  
              Read/write media, so copy all files from CD to the Hard
              Drive or LS120, and do the install.   

         2. To Build an LS-120 Diskette.
           - Download the 'zip' file of the IBM xSeries 380
             POST/FIRMWARE, from http://www.pc.ibm.com/support
           - Expand the 'zip' files and copy all files to 
             the LS-120. 
 
      3.2  Checking installed BIOS/FIRMWARE levels.

         1. Boot to EFI Shell 
           - Insert the LS-120 diskette or CD containing the 
             BIOS/FIRMWARE utilities.
           - Type: map -r  (Map's available devices)
             (find the file system (fsx:) defined to the specific 
              media being used) 
               Device:00 is LS-120,   Device:FF is CD
           - Type: fsx: (fsx:=fs0:, or fs1:, or fs2:) 
           - Type: load ipmi.efi (Load's ipmi driver)
         2. To check the Firmware levels installed.
           - From the EFI prompt (shell>), type ‘fwupdate /fwversion’ to find the FIRMWARE versions.
           - Read the ‘Op code’ numbers of BMC, HSC and CBC. They are the current versions on the system.
         3. To check the BIOS level installed. 
           - From the EFI prompt (shell>), type ‘ver’ to find the BIOS version.
           - You will find the following string: S460AC4A.86B.XXXX.B.yymmddhhmm
           - The BIOS version number is the ‘XXXX’ from the above string.
         4. To check the SDR level installed.
           - From the EFI prompt (shell>), type ‘FRUSDR -d sdr’ to find the SDR version.
           - The last SDR record will display the SDR version loaded on the system.
                    
       3.3  The procedure to update the BIOS/FIRMWARE is as follows:

         1. Boot to EFI Shell 
           - Insert the LS-120 diskette or CD containing the 
             BIOS/FIRMWARE utilities.
           - Type: map -r  (Map's available devices)
             (find the file system (fsx:) defined to the specific 
              media being used) 
               Device:00 is LS-120,   Device:FF is CD
           - Type: fsx: (fsx:=fs0:, or fs1:, or fs2:) 
           - Type: load ipmi.efi (Load's ipmi driver   
         2. To load BMC firmware release 26, 
            Type: fwupdate lnbmc26.hex /upload  
         3. If needed: To load HSC firmware release 07, 
            Type: fwupdate lonhsc07.hex /upload  
         4. If needed:  To load CBC firmware release 02,
            Type: fwupdate loncbc02.hex /upload 
         5. To load BIOS 104,
            Type: iflash64 oemfw104.bin  /update
       Note: To update the SDR records all these files have to be on  
          Read/write media, so copy all files from CD to Hard
          Drive or LS120, and do the install. 
           6. To load SDR release 14,
           - From the EFI prompt,
           - Type: frusdr -cfg srcfg08.cfg
           - Type:  1    (Load SDR from file)
           - This will update the SDR records on the system to SDR 14.              
         7. Once it is done, power off the system.
         8. Then clear the CMOS according to the following procedure:
           - Wait for 8 seconds after power off.
           - Hold the reset button for 4 seconds. 
           - While holding the reset button, press the power button 
             and release both at the same time. 
         Note: This procedure does not clear the password.
           - You will get "NVRAM cleared by Jumper" message.
           - Enter CMOS setup and set the date and time to current 
             date and time if needed.
           - Save settings. System will automatically reboot to EFI. 
       
    4.0   WEB Sites and Support Phone Number
    ----------------------------------------

       4.1   IBM Support Web Site:
             http://www.pc.ibm.com/support

       4.2   IBM Marketing eserver Web Site:
             http://www.ibm.com/eserver/xseries

       4.3   If you have any questions about this update, or
             problems applying the update go to the following 
             Help Center World Telephone Numbers URL:
             http://www.pc.ibm.com/qtechinfo/YAST-3P2QYL.html.
	     
    5.0   Trademarks and Notices
    ----------------------------

       5.1   IBM is a registered trademark of International Business
             Machines Corporation.

       5.2   Intel is a registered trademark and Itanium is a 
             registered trademark of Intel Corporation.

       5.3   Microsoft is a registered trademark and Windows NT, 
             Windows, are trademarks of Microsoft.

       5.4   Novell and NetWare are registered trademarks of
             Novell. Inc.

       5.5   SCO, SCO UNIX, Open Desktop, Open Server are registered 
             trademarks of Santa Cruz Operation, Inc.

       5.6   All other trademarks are the properties of their
             respective owners.

    6.0   Disclaimer
    ----------------------------

       6.1   THIS DOCUMENT IS PROVIDED "AS IS" WITHOUT WARRANTY OF
             ANY KIND.   IBM DISCLAIMS ALL WARRANTIES, WHETHER 
             EXPRESS OR IMPLIED, INCLUDING WITHOUT LIMITATION, THE
             IMPLIED WARRANTIES OF FITNESS FOR A PARTICULAR PURPOSE  
             AND MERCHANTABILITY WITH RESPECT TO THE INFORMATION IN 
             THIS DOCUMENT.   BY FURNISHING THIS DOCUMENT, IBM GRANTS
             NO LICENSES TO ANY PATENTS OR COPYRIGHTS.

       6.2   Note to Government Users
             Include the following note after the disclaimer 
             paragraph.

             Note to U. S. Government Users -- Documentation related
             to restricted rights -- Use, duplication or disclosure 
             is subject to restrictions set forth in GSA ADP Schedule
             Contract with IBM Corporation.















