IBM HS20 Fibre Channel Expansion Card Driver device driver version 6.0 for Linux

This directory contains 2 driver source files. 

i2LNX-v6.0-fo-dist.tgz:  The failover device driver for Multi-path I/O.
                         This device driver is configured by using FAStT MSJ.   

i2LNX-v6.0-dist.tgz: The non-failover version of the above device driver. 
