# Hot-spare configuration summary

If a hot-spare drive of the appropriate size is available, this column reports Yes.

If the logical drive is redundant (that is, RAID level-1, 1E, or 5), but a hot-spare drive of the appropriate size is not available, this column reports No (in red).

If the logical drive is RAID level-0, this column reports No (in black).

Glossary | Contents

x-2000-SRM-00-00-EN